(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 206)
    (no_connects 0)
    (area 128.194999 67.234999 190.575001 124.789001)
    (thickness 1.6)
    (drawings 79)
    (tracks 1139)
    (zones 0)
    (modules 76)
    (nets 107)
  )
  (page A4)
  (title_block
    (title "MixSID - C64 Stereo SID board")
    (date 2016-06-27)
    (rev 1)
    (company "Henning Bekel")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.18)
    (zone_clearance 0.127)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 "Net-(C4-Pad1)")
  (net 7 GND)
  (net 8 /+9V)
  (net 9 "Net-(C10-Pad2)")
  (net 10 "Net-(C9-Pad2)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 "Net-(C11-Pad1)")
  (net 13 "Net-(C11-Pad2)")
  (net 14 "Net-(C12-Pad1)")
  (net 15 "Net-(JP2-Pad2)")
  (net 16 "Net-(JP3-Pad2)")
  (net 17 "Net-(JP6-Pad2)")
  (net 18 "Net-(JP7-Pad2)")
  (net 19 /A5)
  (net 20 /A8)
  (net 21 /~IO1)
  (net 22 /~IO2)
  (net 23 /MS)
  (net 24 /~CS)
  (net 25 /RW)
  (net 26 "Net-(U1-Pad12)")
  (net 27 /~CS2)
  (net 28 /~CS1)
  (net 29 VCC)
  (net 30 /~RES)
  (net 31 /CLK)
  (net 32 /A0)
  (net 33 /A1)
  (net 34 /A2)
  (net 35 /A3)
  (net 36 /A4)
  (net 37 /D0)
  (net 38 /D1)
  (net 39 /D2)
  (net 40 /D3)
  (net 41 /D4)
  (net 42 /D5)
  (net 43 /D6)
  (net 44 /D7)
  (net 45 /POTY)
  (net 46 /POTX)
  (net 47 VDD)
  (net 48 "Net-(P4-Pad1)")
  (net 49 "Net-(P4-Pad2)")
  (net 50 "Net-(P4-Pad3)")
  (net 51 "Net-(P4-Pad4)")
  (net 52 "Net-(C13-Pad1)")
  (net 53 "Net-(C13-Pad2)")
  (net 54 "Net-(C14-Pad1)")
  (net 55 "Net-(C14-Pad2)")
  (net 56 /S1OUT)
  (net 57 /S2OUT)
  (net 58 /LEFT)
  (net 59 /RIGHT)
  (net 60 "Net-(C16-Pad2)")
  (net 61 /M0)
  (net 62 /M1)
  (net 63 "Net-(C17-Pad1)")
  (net 64 "Net-(C17-Pad2)")
  (net 65 /VEE)
  (net 66 /RIGHT_OUT)
  (net 67 /LEFT_OUT)
  (net 68 "Net-(U8-Pad6)")
  (net 69 "Net-(U8-Pad7)")
  (net 70 /+12V)
  (net 71 /PWR)
  (net 72 /S2IN)
  (net 73 "Net-(JP8-Pad3)")
  (net 74 /S1IN)
  (net 75 "Net-(JP11-Pad3)")
  (net 76 "Net-(R1-Pad2)")
  (net 77 "Net-(R10-Pad2)")
  (net 78 "Net-(RV1-Pad3)")
  (net 79 "Net-(RV2-Pad3)")
  (net 80 "Net-(C15-Pad1)")
  (net 81 "Net-(C20-Pad1)")
  (net 82 "Net-(C21-Pad2)")
  (net 83 "Net-(P6-Pad12)")
  (net 84 /MONO_OUT)
  (net 85 /PWR2)
  (net 86 /PWR1)
  (net 87 /VEXT)
  (net 88 /~IO1EN)
  (net 89 /~IO2EN)
  (net 90 "Net-(C19-Pad2)")
  (net 91 "Net-(C22-Pad2)")
  (net 92 /PS)
  (net 93 "Net-(U1-Pad14)")
  (net 94 /POTY2)
  (net 95 /POTX2)
  (net 96 /POTY1)
  (net 97 /POTX1)
  (net 98 "Net-(U7-Pad3)")
  (net 99 "Net-(U7-Pad4)")
  (net 100 "Net-(U7-Pad5)")
  (net 101 "Net-(JP12-Pad1)")
  (net 102 "Net-(JP12-Pad3)")
  (net 103 "Net-(JP13-Pad1)")
  (net 104 "Net-(JP13-Pad3)")
  (net 105 "Net-(U1-Pad18)")
  (net 106 "Net-(U1-Pad19)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.18)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A8)
    (add_net /CLK)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /LEFT)
    (add_net /LEFT_OUT)
    (add_net /M0)
    (add_net /M1)
    (add_net /MONO_OUT)
    (add_net /MS)
    (add_net /POTX)
    (add_net /POTX1)
    (add_net /POTX2)
    (add_net /POTY)
    (add_net /POTY1)
    (add_net /POTY2)
    (add_net /PS)
    (add_net /RIGHT)
    (add_net /RIGHT_OUT)
    (add_net /RW)
    (add_net /S1IN)
    (add_net /S1OUT)
    (add_net /S2IN)
    (add_net /S2OUT)
    (add_net /~CS)
    (add_net /~CS1)
    (add_net /~CS2)
    (add_net /~IO1)
    (add_net /~IO1EN)
    (add_net /~IO2)
    (add_net /~IO2EN)
    (add_net /~RES)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(JP11-Pad3)")
    (add_net "Net-(JP12-Pad1)")
    (add_net "Net-(JP12-Pad3)")
    (add_net "Net-(JP13-Pad1)")
    (add_net "Net-(JP13-Pad3)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(JP3-Pad2)")
    (add_net "Net-(JP6-Pad2)")
    (add_net "Net-(JP7-Pad2)")
    (add_net "Net-(JP8-Pad3)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P4-Pad4)")
    (add_net "Net-(P6-Pad12)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(RV2-Pad3)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U7-Pad3)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U8-Pad6)")
    (add_net "Net-(U8-Pad7)")
  )
  (net_class Power ""
    (clearance 0.18)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+12V)
    (add_net /+9V)
    (add_net /PWR)
    (add_net /PWR1)
    (add_net /PWR2)
    (add_net /VEE)
    (add_net /VEXT)
    (add_net GND)
    (add_net VCC)
    (add_net VDD)
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5733357A)
    (at 169.862 100.012)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 36.195 0) (layer F.SilkS) hide)
    (fp_text value BC547 (at 36.195 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(C15-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(C16-Pad2)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 70 /+12V))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 -0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5733357F)
    (at 174.942 100.012)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 23.495 0) (layer F.SilkS) hide)
    (fp_text value BC547 (at 23.495 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(C20-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(C21-Pad2)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 0.89916 1.50114) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 70 /+12V))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 -0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 57333A47)
    (at 163.195 69.85 180)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV1 (at -1.651 -2.54 270) (layer F.SilkS))
    (fp_text value 1M (at -1.397 -6.604 360) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(R10-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(RV1-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp (layer F.Cu) (tedit 57333A6B)
    (at 142.24 69.85 180)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV2 (at -1.651 -2.54 270) (layer F.SilkS))
    (fp_text value 1M (at -1.27 -6.604 360) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(R1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(RV2-Pad3)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x05 (layer F.Cu) (tedit 573335AB)
    (at 131.128 120.65 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -5.08 5.715 180) (layer F.SilkS) hide)
    (fp_text value INPUT (at -6.35 5.715 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A5))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A8))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /~IO1))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /~IO2))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 87 /VEXT))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 180 90))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 573335C9)
    (at 182.245 120.65 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -5.08 2.54 180) (layer F.SilkS) hide)
    (fp_text value OUTPUT (at -6.35 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /LEFT_OUT))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 /RIGHT_OUT))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 180 90))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x14 (layer B.Cu) (tedit 573336F3)
    (at 151.13 78.74 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -54.61 180) (layer B.SilkS) hide)
    (fp_text value "SOCKET LEFT" (at 0 -55.88 180) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 48 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 49 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 50 "Net-(P4-Pad3)"))
    (pad 4 thru_hole circle (at 0 -7.62 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 51 "Net-(P4-Pad4)"))
    (pad 5 thru_hole circle (at 0 -10.16 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 /~RES))
    (pad 6 thru_hole circle (at 0 -12.7 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 31 /CLK))
    (pad 7 thru_hole circle (at 0 -15.24 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 /RW))
    (pad 8 thru_hole circle (at 0 -17.78 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 /~CS))
    (pad 9 thru_hole circle (at 0 -20.32 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 32 /A0))
    (pad 10 thru_hole circle (at 0 -22.86 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 33 /A1))
    (pad 11 thru_hole circle (at 0 -25.4 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 34 /A2))
    (pad 12 thru_hole circle (at 0 -27.94 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 35 /A3))
    (pad 13 thru_hole circle (at 0 -30.48 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 36 /A4))
    (pad 14 thru_hole circle (at 0 -33.02 180) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x14.wrl
      (at (xyz 0 -0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x14 (layer B.Cu) (tedit 573336F6)
    (at 166.37 111.76)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0.635 21.59) (layer B.SilkS) hide)
    (fp_text value "SOCKET RIGHT" (at 0 22.86) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 37 /D0))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 38 /D1))
    (pad 3 thru_hole circle (at 0 -5.08) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 39 /D2))
    (pad 4 thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 40 /D3))
    (pad 5 thru_hole circle (at 0 -10.16) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 41 /D4))
    (pad 6 thru_hole circle (at 0 -12.7) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 42 /D5))
    (pad 7 thru_hole circle (at 0 -15.24) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 43 /D6))
    (pad 8 thru_hole circle (at 0 -17.78) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 44 /D7))
    (pad 9 thru_hole circle (at 0 -20.32) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 45 /POTY))
    (pad 10 thru_hole circle (at 0 -22.86) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 46 /POTX))
    (pad 11 thru_hole circle (at 0 -25.4) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 VCC))
    (pad 12 thru_hole circle (at 0 -27.94) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 83 "Net-(P6-Pad12)"))
    (pad 13 thru_hole circle (at 0 -30.48) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 84 /MONO_OUT))
    (pad 14 thru_hole circle (at 0 -33.02) (size 1.6 1.6) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 47 VDD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x14.wrl
      (at (xyz 0 -0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 5733339E)
    (at 169.862 94.9325)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C19 (at 24.13 -0.635) (layer F.SilkS) hide)
    (fp_text value 10uF (at 24.13 0.635) (layer F.Fab))
    (fp_text user + (at 0.7493 1.3335) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(C16-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(C19-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 0.8 0.8 1.18))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 573333D1)
    (at 174.942 94.996)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C22 (at 24.13 -0.635) (layer F.SilkS) hide)
    (fp_text value 10uF (at 24.13 0.635) (layer F.Fab))
    (fp_text user + (at 0.7493 1.3335) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(C21-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(C22-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 0.8 0.8 1.18))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 5733365A)
    (at 172.72 77.724)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C17 (at 3.175 19.685 90) (layer F.SilkS) hide)
    (fp_text value 10u (at 1.905 19.685 90) (layer F.Fab))
    (fp_text user + (at 0.7493 1.3335) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(C17-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 0.8 0.8 1.18))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 57333683)
    (at 172.72 82.296)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C18 (at 1.27 -19.685 90) (layer F.SilkS) hide)
    (fp_text value 10u (at 2.54 -19.685 90) (layer F.Fab))
    (fp_text user + (at 0.7493 1.3335) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 65 /VEE))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 0.8 0.8 1.18))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 573335A7)
    (at 164.465 120.65 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP4 (at 5.08 2.54 360) (layer F.SilkS) hide)
    (fp_text value BOARD (at 6.35 2.54 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 /PWR))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /+12V))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 VDD))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0.075 -0.15 0.05))
      (scale (xyz 0.381 0.381 0.381))
      (rotate (xyz 180 90 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3339P_Angular_ScrewUp (layer F.Cu) (tedit 57333766)
    (at 171.132 88.9)
    (descr "5/16, Round, Trimming, Potentiometer, Bourns, 3339")
    (tags "5/16, Round, Trimming, Potentiometer, Bourns, 3339")
    (fp_text reference RV3 (at 2.54 -0.762 180) (layer F.SilkS))
    (fp_text value 10k (at 2.54 1.143) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 58 /LEFT))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(C19-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3339P_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3339P_Angular_ScrewUp (layer F.Cu) (tedit 573B180E)
    (at 182.245 88.9)
    (descr "5/16, Round, Trimming, Potentiometer, Bourns, 3339")
    (tags "5/16, Round, Trimming, Potentiometer, Bourns, 3339")
    (fp_text reference RV4 (at 2.54 -0.635 180) (layer F.SilkS))
    (fp_text value 10k (at 2.54 1.143) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RIGHT))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(C22-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3339P_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:DIP-16_W7.62mm (layer F.Cu) (tedit 57610A20)
    (at 180.975 98.425)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U6 (at 0 32.385) (layer F.SilkS) hide)
    (fp_text value 4052 (at 3.81 8.89 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 58 /LEFT))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 58 /LEFT))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 66 /RIGHT_OUT))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RIGHT))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RIGHT))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 65 /VEE))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 62 /M1))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 61 /M0))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 58 /LEFT))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 58 /LEFT))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 67 /LEFT_OUT))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RIGHT))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 59 /RIGHT))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/packages3d/DIP16.wrl
      (at (xyz 0.15 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:DIP-16_W7.62mm (layer F.Cu) (tedit 57610A14)
    (at 153.67 91.44)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U7 (at 0 38.735) (layer F.SilkS) hide)
    (fp_text value 4053 (at 3.81 8.89 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 96 /POTY1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 94 /POTY2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(U7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(U7-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(U7-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 9 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 10 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 92 /PS))
    (pad 11 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 92 /PS))
    (pad 12 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 95 /POTX2))
    (pad 13 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 97 /POTX1))
    (pad 14 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 /POTX))
    (pad 15 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 /POTY))
    (pad 16 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:DIP-20_W7.62mm (layer F.Cu) (tedit 57610A08)
    (at 134.62 88.9)
    (descr "20-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0 41.275) (layer F.SilkS) hide)
    (fp_text value GAL16V8 (at 3.81 11.43 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 /MS))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 88 /~IO1EN))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 89 /~IO2EN))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RW))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /~CS))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 /~IO2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /~IO1))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /A5))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /A8))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 11 thru_hole oval (at 7.62 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 92 /PS))
    (pad 12 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U1-Pad12)"))
    (pad 13 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U1-Pad12)"))
    (pad 14 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(U1-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(U1-Pad14)"))
    (pad 16 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /~CS2))
    (pad 17 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 /~CS1))
    (pad 18 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(U1-Pad19)"))
    (pad 20 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (model Housings_DIP.3dshapes/DIP-20_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:DIP-28_W15.24mm (layer F.Cu) (tedit 573C1D96)
    (at 130.81 81.28)
    (descr "28-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U2 (at 0 48.895) (layer F.SilkS) hide)
    (fp_text value SID2 (at 7.62 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(JP3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(JP2-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 /~RES))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 /CLK))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RW))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 /~CS2))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 /A0))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 /A1))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 /A2))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /A3))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 /A4))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 /D0))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D1))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D2))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D3))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D4))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D5))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D6))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D7))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 94 /POTY2))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 95 /POTX2))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 72 /S2IN))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 57 /S2OUT))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 85 /PWR2))
    (model ${KIPRJMOD}/packages3d/DIP28-600-without-middle-and-bottom-bar.wrl
      (at (xyz 0.3 -0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:DIP-28_W15.24mm (layer F.Cu) (tedit 573C1D99)
    (at 148.59 81.28)
    (descr "28-lead dip package, row spacing 15.24 mm (600 mils)")
    (tags "dil dip 2.54 600")
    (fp_text reference U5 (at 0 48.895) (layer F.SilkS) hide)
    (fp_text value SID1 (at 7.62 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(JP7-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C11-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(JP6-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 /~RES))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 /CLK))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RW))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 /~CS1))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 /A0))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 /A1))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 /A2))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /A3))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 /A4))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 /D0))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 /D1))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /D2))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 /D3))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 /D4))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 /D5))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 /D6))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 /D7))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 96 /POTY1))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 97 /POTX1))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 74 /S1IN))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 56 /S1OUT))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 86 /PWR1))
    (model ${KIPRJMOD}/packages3d/DIP28-600-without-middle-bar.wrl
      (at (xyz 0.3 -0.65 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:DIP-8_W7.62mm (layer F.Cu) (tedit 57610A28)
    (at 185.42 76.2 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U8 (at 0 -30.48 360) (layer F.SilkS) hide)
    (fp_text value 7660 (at 3.81 3.81 540) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(C17-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(C17-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 65 /VEE))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(U8-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(U8-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0.1))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/packages3d/DIP8.wrl
      (at (xyz 0.15 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:TO-220 (layer F.Cu) (tedit 5733388A)
    (at 150.241 121.92 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U4 (at 0 -5.715 180) (layer F.SilkS) hide)
    (fp_text value 7809 (at 0 -6.985 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 8 /+9V))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 70 /+12V))
    (model ${KIPRJMOD}/packages3d/TO-220_Bipolar-BCE_Horizontal_Reverse.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.381 0.381 0.381))
      (rotate (xyz 0 180 0))
    )
  )
  (module Pinheaders:TO-220 (layer F.Cu) (tedit 5733388A)
    (at 173.736 121.92 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U3 (at 0 -5.715 180) (layer F.SilkS) hide)
    (fp_text value 7812 (at 0 -6.985 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 71 /PWR))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 87 /VEXT))
    (model ${KIPRJMOD}/packages3d/TO-220_Bipolar-BCE_Horizontal_Reverse.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.381 0.381 0.381))
      (rotate (xyz 0 180 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 142.24 83.82 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 470p (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 139.7 86.36)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.27 -1.397) (layer F.SilkS) hide)
    (fp_text value 22n (at 1.397 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 137.16 83.82 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 470p (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 134.62 86.36)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 1.27 -1.397) (layer F.SilkS) hide)
    (fp_text value 22n (at 1.397 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C3-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 178.816 122.936 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 1.27 -1.397 90) (layer F.SilkS) hide)
    (fp_text value 470p (at 1.397 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 87 /VEXT))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573B1856)
    (at 168.656 122.936 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 1.27 -1.397 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 71 /PWR))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 155.448 122.936 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 1.27 -1.397 90) (layer F.SilkS) hide)
    (fp_text value 470p (at 1.397 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 70 /+12V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573B1889)
    (at 145.288 122.936 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at 1.27 -1.397 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /+9V))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 158.75 83.82)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C9 (at 1.27 -1.397) (layer F.SilkS) hide)
    (fp_text value 470p (at 1.397 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C9-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 153.67 86.36)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C10 (at 1.27 -1.397) (layer F.SilkS) hide)
    (fp_text value 22n (at 1.397 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C10-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 153.67 83.82)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C11 (at 1.27 -1.397) (layer F.SilkS) hide)
    (fp_text value 470p (at 1.397 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C11-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C11-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 161.29 86.36 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C12 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 22n (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C12-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C11-Pad1)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 148.59 71.12 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C13 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(C13-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 169.545 71.12 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C14 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(C14-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 172.402 108.585 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C15 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 1n (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 177.482 108.585 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C20 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 1n (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 177.482 103.505 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C21 (at 1.27 -1.397 270) (layer F.SilkS) hide)
    (fp_text value 470p (at 1.397 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(C21-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573B1827)
    (at 187.96 81.28 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C23 (at 1.27 -1.397 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 158.75 88.9 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C24 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 186.055 95.25 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C25 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 172.402 103.505 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C16 (at 1.27 -1.397 270) (layer F.SilkS) hide)
    (fp_text value 470p (at 1.397 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(C16-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 573C1AFC)
    (at 169.545 73.66)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP9 (at 0 19.05 90) (layer F.Fab))
    (fp_text value NR1 (at 0 15.24 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 573C1D1A)
    (at 148.59 73.66)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP10 (at 0 19.05 90) (layer F.Fab))
    (fp_text value NR2 (at 0 15.24 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C13-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 0.381 0.381 0.381))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 573C6EF8)
    (at 169.545 80.645)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 19.05 90) (layer F.Fab))
    (fp_text value RAW (at 0 15.24 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 /S2OUT))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /S1OUT))
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 176.212 116.205 180)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R14 (at 0 0 180) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /S1OUT))
    (pad 2 thru_hole circle (at 1.27 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 /MONO_OUT))
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 171.132 116.205)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 /S2OUT))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 /MONO_OUT))
    (model ${KIPRJMOD}/packages3d/SIL4.wrl
      (at (xyz 0.1 0.15 -0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 174.942 104.775 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R12 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(C21-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 177.482 112.395 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R11 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /S1OUT))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 167.005 74.93 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R10 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 220k (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(JP11-Pad3)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(R10-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 147.32 68.58)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 100k (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(C13-Pad1)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 180.975 93.98 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R8 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 4k7 (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 /M1))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 188.595 93.98 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R7 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 4k7 (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 VCC))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 /M0))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 174.942 112.395 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R6 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(JP13-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 169.862 104.775 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R5 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(C16-Pad2)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 172.402 112.395 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R4 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 10k (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 /S2OUT))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 169.862 112.395 270)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(JP12-Pad1)"))
    (pad 2 thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 168.275 68.58)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value 100k (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(C14-Pad1)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:R1 (layer F.Cu) (tedit 573EEEF8)
    (at 146.05 74.93 90)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value 220k (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(JP8-Pad3)"))
    (pad 2 thru_hole circle (at 1.27 0 90) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(R1-Pad2)"))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 143.51 78.74)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C26 (at 1.27 -1.397) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.397 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 85 /PWR2))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:C_Disc_D3_P2.5 (layer F.Cu) (tedit 573427C0)
    (at 163.83 78.74 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C27 (at 1.27 -1.397 180) (layer F.SilkS) hide)
    (fp_text value 100n (at 1.397 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 86 /PWR1))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 0.8))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:DO-41 (layer F.Cu) (tedit 0)
    (at 173.736 118.618)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D1 (at 0 0) (layer F.SilkS))
    (fp_text value 1N4002 (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 87 /VEXT))
    (pad 2 thru_hole circle (at -5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 71 /PWR))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:DO-41 (layer F.Cu) (tedit 5742F0CB)
    (at 150.368 118.618)
    (descr "Diode 3 pas")
    (tags "DIODE DEV")
    (fp_text reference D2 (at 0 0) (layer F.SilkS))
    (fp_text value 1N4002 (at 0 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 70 /+12V))
    (pad 2 thru_hole circle (at -5.08 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask F.SilkS)
      (net 8 /+9V))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm (layer F.Cu) (tedit 57456A45)
    (at 132.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP3 (at 0 -5) (layer F.Fab))
    (fp_text value S2CAP1 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(JP3-Pad2)"))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C4-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.0375 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_1-2 (layer F.Cu) (tedit 57456A49)
    (at 134.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP2 (at 0 -5) (layer F.Fab))
    (fp_text value S2CAP2 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(JP2-Pad2)"))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.0375 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_1-2 (layer F.Cu) (tedit 57456A4F)
    (at 136.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP12 (at 0 -5) (layer F.Fab))
    (fp_text value J2R8 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 101 "Net-(JP12-Pad1)"))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 /S2OUT))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 102 "Net-(JP12-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.0375 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_2-3 (layer F.Cu) (tedit 57456A59)
    (at 151.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP5 (at 0 -5) (layer F.Fab))
    (fp_text value SUPPLY1 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 /+12V))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 /PWR1))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /+9V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.1175 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_2-3 (layer F.Cu) (tedit 57456A5D)
    (at 153.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP7 (at 0 -5) (layer F.Fab))
    (fp_text value S1CAP1 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C11-Pad2)"))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(JP7-Pad2)"))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C12-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.1175 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_2-3 (layer F.Cu) (tedit 57456A61)
    (at 155.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP6 (at 0 -5) (layer F.Fab))
    (fp_text value S1CAP2 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C9-Pad2)"))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(JP6-Pad2)"))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.1175 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_2-3 (layer F.Cu) (tedit 57456A66)
    (at 157.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP13 (at 0 -5) (layer F.Fab))
    (fp_text value J1R8 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 103 "Net-(JP13-Pad1)"))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 /S1OUT))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 104 "Net-(JP13-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.1175 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_1-2 (layer F.Cu) (tedit 57456A40)
    (at 130.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP1 (at 0 -5) (layer F.Fab))
    (fp_text value SUPPLY2 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 /+12V))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 /PWR2))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /+9V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.0375 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_1-2 (layer F.Cu) (tedit 57456A52)
    (at 138.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP8 (at 0 -5) (layer F.Fab))
    (fp_text value INPUT2 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(C13-Pad2)"))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 /S2IN))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(JP8-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.0375 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_1x03_Pitch2.00mm_Jumper_2-3 (layer F.Cu) (tedit 57456A6A)
    (at 159.5 70.5)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference JP11 (at 0 -5) (layer F.Fab))
    (fp_text value INPUT1 (at 0.31 -7.635) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(C14-Pad2)"))
    (pad 2 thru_hole circle (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /S1IN))
    (pad 3 thru_hole circle (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(JP11-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.078 0))
      (scale (xyz 0.78 0.78 0.78))
      (rotate (xyz 0 0 90))
    )
    (model ${KIPRJMOD}/packages3d/Jumper.wrl
      (at (xyz 0 -0.1175 0))
      (scale (xyz 0.32 0.32 0.32))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pinheaders:Pin_Header_Straight_2x06 (layer F.Cu) (tedit 5750437F)
    (at 175.26 72.39 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 7.366 6.35 180) (layer F.Fab))
    (fp_text value CONTROL (at 6.096 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /MS))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 92 /PS))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 88 /~IO1EN))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 89 /~IO2EN))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /M1))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /M0))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x06.wrl
      (at (xyz 0.05 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "Testing & Feedback by C0zmo, GI-Joe and GMP" (at 132.715 97.79 90) (layer F.SilkS))
  (gr_text GND (at 173.736 72.39) (layer F.SilkS))
  (gr_text SIGNAL (at 173.736 69.85) (layer F.SilkS))
  (gr_line (start 188.976 124.714) (end 129.794 124.714) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190.5 68.834) (end 190.5 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.794 67.31) (end 188.976 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 123.19) (end 128.27 68.834) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 129.794 123.19) (end 129.794 124.714) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 188.976 123.19) (end 190.5 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 188.976 68.834) (end 188.976 67.31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 129.794 68.834) (end 128.27 68.834) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 57.404 (width 0.3) (layer Dwgs.User)
    (gr_text "57,404 mm" (at 222.838 96.012 90) (layer Dwgs.User))
    (feature1 (pts (xy 190.5 67.31) (xy 224.188 67.31)))
    (feature2 (pts (xy 190.5 124.714) (xy 224.188 124.714)))
    (crossbar (pts (xy 221.488 124.714) (xy 221.488 67.31)))
    (arrow1a (pts (xy 221.488 67.31) (xy 222.074421 68.436504)))
    (arrow1b (pts (xy 221.488 67.31) (xy 220.901579 68.436504)))
    (arrow2a (pts (xy 221.488 124.714) (xy 222.074421 123.587496)))
    (arrow2b (pts (xy 221.488 124.714) (xy 220.901579 123.587496)))
  )
  (dimension 62.23 (width 0.3) (layer Dwgs.User)
    (gr_text "62,230 mm" (at 159.385 38.02) (layer Dwgs.User))
    (feature1 (pts (xy 190.5 67.31) (xy 190.5 36.67)))
    (feature2 (pts (xy 128.27 67.31) (xy 128.27 36.67)))
    (crossbar (pts (xy 128.27 39.37) (xy 190.5 39.37)))
    (arrow1a (pts (xy 190.5 39.37) (xy 189.373496 39.956421)))
    (arrow1b (pts (xy 190.5 39.37) (xy 189.373496 38.783579)))
    (arrow2a (pts (xy 128.27 39.37) (xy 129.396504 39.956421)))
    (arrow2b (pts (xy 128.27 39.37) (xy 129.396504 38.783579)))
  )
  (gr_text "SID1 CONFIG" (at 155.5 68) (layer F.SilkS))
  (gr_text "SID2 CONFIG" (at 134.5 68) (layer F.SilkS))
  (gr_text DGB (at 159.5 76.25) (layer F.SilkS))
  (gr_text DGB (at 138.5 76.25) (layer F.SilkS))
  (gr_text EXIN (at 159.5 69) (layer F.SilkS))
  (gr_text R8 (at 157.5 69) (layer F.SilkS))
  (gr_text FC2 (at 155.5 69) (layer F.SilkS))
  (gr_text FC1 (at 153.5 69) (layer F.SilkS))
  (gr_text VDD (at 151.5 69) (layer F.SilkS))
  (gr_text EXIN (at 138.5 69) (layer F.SilkS))
  (gr_text R8 (at 136.5 69) (layer F.SilkS))
  (gr_text FC2 (at 134.5 69) (layer F.SilkS))
  (gr_text FC1 (at 132.5 69) (layer F.SilkS))
  (gr_text 2 (at 167.767 80.645) (layer F.SilkS))
  (gr_text 1 (at 167.767 83.185) (layer F.SilkS))
  (gr_text "RAW\nOUT" (at 169.545 85.725) (layer F.SilkS))
  (gr_text BC547A (at 176.2125 98.7425) (layer F.SilkS))
  (gr_text BC547A (at 171.1325 98.7425) (layer F.SilkS))
  (gr_text "CONTROL SIGNALS" (at 181.61 74.422) (layer F.SilkS))
  (gr_text MODEL (at 154.682 76.851) (layer F.SilkS))
  (gr_text MODEL (at 133.727 76.851) (layer F.SilkS))
  (gr_text "MixSID Stereo SID Board Rev.1 ©2016 Henning Bekel" (at 129.159 97.79 90) (layer F.SilkS))
  (gr_text "BOARD SELECT" (at 161.925 117.475) (layer F.SilkS))
  (gr_text "VOLUME\nADJUST\n" (at 179.2 86.6) (layer F.SilkS))
  (gr_text 7809 (at 150.241 124.206) (layer F.SilkS))
  (gr_text 7812 (at 173.736 124.206) (layer F.SilkS))
  (gr_text "EXTERNAL SIGNALS" (at 136.2075 117.475) (layer F.SilkS))
  (gr_text R (at 189.23 120.65) (layer F.SilkS))
  (gr_text L (at 180.34 120.65) (layer F.SilkS))
  (gr_text "AUDIO OUT" (at 184.785 118.618) (layer F.SilkS))
  (gr_text NR1 (at 169.545 78.232) (layer F.SilkS))
  (gr_text NR2 (at 148.463 78.232) (layer F.SilkS))
  (gr_text 8580 (at 128.905 74.168 90) (layer F.SilkS))
  (gr_text 6581 (at 128.905 70.612 90) (layer F.SilkS))
  (gr_text NEW (at 164.465 118.745) (layer F.SilkS))
  (gr_text OLD (at 159.385 118.745) (layer F.SilkS))
  (gr_text VEXT (at 141.2875 118.745) (layer F.SilkS))
  (gr_text IO2 (at 138.7475 118.745) (layer F.SilkS))
  (gr_text IO1 (at 136.2075 118.745) (layer F.SilkS))
  (gr_text A8 (at 133.6675 118.745) (layer F.SilkS))
  (gr_text A5 (at 131.1275 118.745) (layer F.SilkS))
  (gr_text M0 (at 187.96 67.945) (layer F.SilkS))
  (gr_text M1 (at 185.42 67.945) (layer F.SilkS))
  (gr_text I2E (at 182.88 67.945) (layer F.SilkS))
  (gr_text I1E (at 180.34 67.945) (layer F.SilkS))
  (gr_text MS (at 175.26 67.945) (layer F.SilkS))
  (gr_text PS (at 177.8 67.945) (layer F.SilkS))
  (gr_text VDD (at 130.5 69) (layer F.SilkS))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 67.31) (xy 190.5 67.31) (xy 190.5 124.714) (xy 128.27 124.714)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 67.31) (xy 190.5 67.31) (xy 190.5 124.714) (xy 128.27 124.714)
      )
    )
  )
)
