<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="53.975" y2="0" width="0" layer="20"/>
<wire x1="53.975" y1="0" x2="53.975" y2="31.115" width="0" layer="20"/>
<wire x1="53.975" y1="31.115" x2="0" y2="31.115" width="0" layer="20"/>
<wire x1="0" y1="31.115" x2="0" y2="0" width="0" layer="20"/>
<text>Marky's House</text>
<text>LIVE</text>
<text>NEUTRAL</text>
<text>AC IN</text>
<text>DC OUT</text>
<text>from</text>
</plain>
<libraries>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SH32">
<description>&lt;b&gt;FUSE HOLDER&lt;/b&gt;&lt;p&gt; 6 x 32 mm, SH contact, SHH3N Schukat / Wickmann 102071 (Buerklin)</description>
</package>
</packages>
</library>
<library name="varistor">
<description>&lt;b&gt;Varistors/Thermistors&lt;/b&gt;&lt;p&gt;
Block, Siemens and generic&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="S14K11">
<description>&lt;b&gt;VARISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="captain-slow">
<description>Library provided by http://captain-slow.dk/&lt;br&gt;&lt;br&gt;
Find the newest version at https://github.com/blddk/EagleLbr/</description>
<packages>
<package name="HLK-PM01">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,6-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.6 mm, round</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="F1" library="fuse" package="SH32" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="varistor" package="S14K11" value="S14K11"/>
<element name="U$1" library="captain-slow" package="HLK-PM01" value="MAINS_CONVERTERS"/>
<element name="JP1" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,6-PAD" value="AC_N"/>
<element name="H2" library="holes" package="3,6-PAD" value="AC_L"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="AC_N"/>
<contactref element="H1" pad="B3,6"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="AC_L"/>
<contactref element="F1" pad="2A"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="VO-"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="VO+"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$3">
<contactref element="F1" pad="1A"/>
<contactref element="H2" pad="B3,6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
