(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 1247)
    (zones 0)
    (modules 117)
    (nets 191)
  )
  (page B)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu power hide)
    (2 In2.Cu power hide)
    (31 B.Cu power)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.5)
    (edge_width 0.5)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.2 0.6)
    (user_via 1.6 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +24V)
  (net 2 GND)
  (net 3 Earth)
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad1)")
  (net 7 "Net-(R1-Pad2)")
  (net 8 /LDAC)
  (net 9 /CS7)
  (net 10 /CS6)
  (net 11 /CS5)
  (net 12 /CS4)
  (net 13 /CS3)
  (net 14 /CS2)
  (net 15 /CS1)
  (net 16 "Net-(R3-Pad8)")
  (net 17 "Net-(R3-Pad7)")
  (net 18 "Net-(R3-Pad6)")
  (net 19 "Net-(R3-Pad5)")
  (net 20 "Net-(R3-Pad4)")
  (net 21 "Net-(R3-Pad3)")
  (net 22 "Net-(R3-Pad2)")
  (net 23 "Net-(R3-Pad1)")
  (net 24 "Net-(R4-Pad1)")
  (net 25 "Net-(R4-Pad2)")
  (net 26 "Net-(R4-Pad3)")
  (net 27 "Net-(R4-Pad4)")
  (net 28 "Net-(R4-Pad5)")
  (net 29 "Net-(R4-Pad6)")
  (net 30 "Net-(R4-Pad7)")
  (net 31 "Net-(R4-Pad8)")
  (net 32 /DB8)
  (net 33 /DB9)
  (net 34 /DB10)
  (net 35 /DB11)
  (net 36 /DB12)
  (net 37 /DB13)
  (net 38 /DB14)
  (net 39 /DB15)
  (net 40 "Net-(R5-Pad1)")
  (net 41 "Net-(R5-Pad2)")
  (net 42 "Net-(R5-Pad3)")
  (net 43 "Net-(R5-Pad4)")
  (net 44 "Net-(R5-Pad5)")
  (net 45 "Net-(R5-Pad6)")
  (net 46 "Net-(R5-Pad7)")
  (net 47 "Net-(R5-Pad8)")
  (net 48 /DB7)
  (net 49 /DB6)
  (net 50 /DB5)
  (net 51 /DB4)
  (net 52 /DB3)
  (net 53 /DB2)
  (net 54 /DB1)
  (net 55 /DB0)
  (net 56 "Net-(R18-Pad2)")
  (net 57 "Net-(R18-Pad1)")
  (net 58 "Net-(R22-Pad2)")
  (net 59 "Net-(U2-Pad4)")
  (net 60 "Net-(U2-Pad5)")
  (net 61 "Net-(U2-Pad6)")
  (net 62 "Net-(U2-Pad7)")
  (net 63 "Net-(U2-Pad8)")
  (net 64 "Net-(U2-Pad9)")
  (net 65 "Net-(U2-Pad10)")
  (net 66 "Net-(U2-Pad11)")
  (net 67 "Net-(U2-Pad12)")
  (net 68 "Net-(U2-Pad13)")
  (net 69 "Net-(U2-Pad14)")
  (net 70 "Net-(U2-Pad15)")
  (net 71 "Net-(U2-Pad16)")
  (net 72 "Net-(U2-Pad17)")
  (net 73 "Net-(U2-Pad18)")
  (net 74 "Net-(U2-Pad21)")
  (net 75 "Net-(U2-Pad22)")
  (net 76 "Net-(U2-Pad23)")
  (net 77 "Net-(U2-Pad24)")
  (net 78 "Net-(U2-Pad25)")
  (net 79 "Net-(U2-Pad26)")
  (net 80 "Net-(U2-Pad27)")
  (net 81 "Net-(U2-Pad28)")
  (net 82 "Net-(U2-Pad29)")
  (net 83 "Net-(U2-Pad30)")
  (net 84 "Net-(U2-Pad33)")
  (net 85 "Net-(U2-Pad34)")
  (net 86 "Net-(U2-Pad35)")
  (net 87 "Net-(U2-Pad36)")
  (net 88 "Net-(U2-Pad37)")
  (net 89 "Net-(U2-Pad38)")
  (net 90 "Net-(U2-Pad39)")
  (net 91 "Net-(U2-Pad40)")
  (net 92 "Net-(U2-Pad41)")
  (net 93 "Net-(U2-Pad42)")
  (net 94 "Net-(U2-Pad43)")
  (net 95 "Net-(U2-Pad44)")
  (net 96 "Net-(U2-Pad45)")
  (net 97 "Net-(U2-Pad46)")
  (net 98 "Net-(U2-Pad47)")
  (net 99 "Net-(U2-Pad48)")
  (net 100 "Net-(U2-Pad60)")
  (net 101 "Net-(U2-Pad59)")
  (net 102 "Net-(U2-Pad63)")
  (net 103 "Net-(U2-Pad98)")
  (net 104 "Net-(U2-Pad97)")
  (net 105 "Net-(U2-Pad92)")
  (net 106 "Net-(U2-Pad75)")
  (net 107 "Net-(U2-Pad91)")
  (net 108 "Net-(U2-Pad117)")
  (net 109 "Net-(U2-Pad101)")
  (net 110 "Net-(U2-Pad103)")
  (net 111 "Net-(U2-Pad104)")
  (net 112 "Net-(U2-Pad111)")
  (net 113 "Net-(U2-Pad112)")
  (net 114 "Net-(U2-Pad114)")
  (net 115 "Net-(U2-Pad105)")
  (net 116 "Net-(U2-Pad113)")
  (net 117 "Net-(U2-Pad110)")
  (net 118 "Net-(U2-Pad107)")
  (net 119 "Net-(U2-Pad102)")
  (net 120 "Net-(U2-Pad109)")
  (net 121 "Net-(U2-Pad115)")
  (net 122 "Net-(U2-Pad116)")
  (net 123 "Net-(U2-Pad56)")
  (net 124 "Net-(U2-Pad57)")
  (net 125 "Net-(U2-Pad58)")
  (net 126 "Net-(U2-Pad53)")
  (net 127 "Net-(U2-Pad55)")
  (net 128 "Net-(U2-Pad54)")
  (net 129 /CS0)
  (net 130 "Net-(U2-Pad64)")
  (net 131 "Net-(U2-Pad61)")
  (net 132 "Net-(U2-Pad76)")
  (net 133 +15V)
  (net 134 -15V)
  (net 135 +5V)
  (net 136 -24V)
  (net 137 "Net-(U2-Pad106)")
  (net 138 "Net-(R11-Pad1)")
  (net 139 "Net-(R7-Pad2)")
  (net 140 "Net-(R12-Pad1)")
  (net 141 "Net-(R8-Pad2)")
  (net 142 "Net-(R13-Pad1)")
  (net 143 "Net-(R9-Pad2)")
  (net 144 "Net-(R10-Pad1)")
  (net 145 "Net-(R10-Pad2)")
  (net 146 "Net-(R11-Pad2)")
  (net 147 "Net-(R12-Pad2)")
  (net 148 "Net-(R13-Pad2)")
  (net 149 "Net-(R14-Pad2)")
  (net 150 "Net-(R15-Pad1)")
  (net 151 "Net-(R15-Pad2)")
  (net 152 "Net-(R16-Pad1)")
  (net 153 "Net-(R16-Pad2)")
  (net 154 "Net-(R17-Pad1)")
  (net 155 "Net-(R17-Pad2)")
  (net 156 "Net-(R19-Pad2)")
  (net 157 "Net-(R20-Pad2)")
  (net 158 "Net-(R21-Pad2)")
  (net 159 "Net-(C9-Pad2)")
  (net 160 "Net-(C10-Pad2)")
  (net 161 "Net-(C11-Pad2)")
  (net 162 "Net-(C12-Pad2)")
  (net 163 "Net-(C13-Pad2)")
  (net 164 "Net-(C14-Pad2)")
  (net 165 "Net-(C15-Pad2)")
  (net 166 "Net-(C16-Pad2)")
  (net 167 "Net-(C17-Pad2)")
  (net 168 "Net-(C18-Pad2)")
  (net 169 "Net-(C19-Pad2)")
  (net 170 "Net-(C20-Pad2)")
  (net 171 "Net-(C21-Pad2)")
  (net 172 "Net-(C22-Pad2)")
  (net 173 "Net-(C23-Pad2)")
  (net 174 "Net-(C24-Pad2)")
  (net 175 "Net-(JP1-Pad1)")
  (net 176 "Net-(JP2-Pad1)")
  (net 177 "Net-(JP3-Pad1)")
  (net 178 "Net-(JP4-Pad1)")
  (net 179 "Net-(JP5-Pad1)")
  (net 180 "Net-(JP6-Pad1)")
  (net 181 "Net-(JP7-Pad1)")
  (net 182 "Net-(JP8-Pad1)")
  (net 183 "Net-(R2-Pad2)")
  (net 184 "Net-(R23-Pad2)")
  (net 185 "Net-(R24-Pad2)")
  (net 186 "Net-(R25-Pad2)")
  (net 187 "Net-(R26-Pad2)")
  (net 188 "Net-(R27-Pad2)")
  (net 189 "Net-(R28-Pad2)")
  (net 190 "Net-(R29-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net +24V)
    (add_net +5V)
    (add_net -15V)
    (add_net -24V)
    (add_net /CS0)
    (add_net /CS1)
    (add_net /CS2)
    (add_net /CS3)
    (add_net /CS4)
    (add_net /CS5)
    (add_net /CS6)
    (add_net /CS7)
    (add_net /DB0)
    (add_net /DB1)
    (add_net /DB10)
    (add_net /DB11)
    (add_net /DB12)
    (add_net /DB13)
    (add_net /DB14)
    (add_net /DB15)
    (add_net /DB2)
    (add_net /DB3)
    (add_net /DB4)
    (add_net /DB5)
    (add_net /DB6)
    (add_net /DB7)
    (add_net /DB8)
    (add_net /DB9)
    (add_net /LDAC)
    (add_net Earth)
    (add_net GND)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C13-Pad2)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad2)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C24-Pad2)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(JP5-Pad1)")
    (add_net "Net-(JP6-Pad1)")
    (add_net "Net-(JP7-Pad1)")
    (add_net "Net-(JP8-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R11-Pad2)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R13-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R16-Pad2)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R20-Pad2)")
    (add_net "Net-(R21-Pad2)")
    (add_net "Net-(R22-Pad2)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R27-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R3-Pad3)")
    (add_net "Net-(R3-Pad4)")
    (add_net "Net-(R3-Pad5)")
    (add_net "Net-(R3-Pad6)")
    (add_net "Net-(R3-Pad7)")
    (add_net "Net-(R3-Pad8)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R4-Pad3)")
    (add_net "Net-(R4-Pad4)")
    (add_net "Net-(R4-Pad5)")
    (add_net "Net-(R4-Pad6)")
    (add_net "Net-(R4-Pad7)")
    (add_net "Net-(R4-Pad8)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R5-Pad3)")
    (add_net "Net-(R5-Pad4)")
    (add_net "Net-(R5-Pad5)")
    (add_net "Net-(R5-Pad6)")
    (add_net "Net-(R5-Pad7)")
    (add_net "Net-(R5-Pad8)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad101)")
    (add_net "Net-(U2-Pad102)")
    (add_net "Net-(U2-Pad103)")
    (add_net "Net-(U2-Pad104)")
    (add_net "Net-(U2-Pad105)")
    (add_net "Net-(U2-Pad106)")
    (add_net "Net-(U2-Pad107)")
    (add_net "Net-(U2-Pad109)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad110)")
    (add_net "Net-(U2-Pad111)")
    (add_net "Net-(U2-Pad112)")
    (add_net "Net-(U2-Pad113)")
    (add_net "Net-(U2-Pad114)")
    (add_net "Net-(U2-Pad115)")
    (add_net "Net-(U2-Pad116)")
    (add_net "Net-(U2-Pad117)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad34)")
    (add_net "Net-(U2-Pad35)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad40)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad42)")
    (add_net "Net-(U2-Pad43)")
    (add_net "Net-(U2-Pad44)")
    (add_net "Net-(U2-Pad45)")
    (add_net "Net-(U2-Pad46)")
    (add_net "Net-(U2-Pad47)")
    (add_net "Net-(U2-Pad48)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad53)")
    (add_net "Net-(U2-Pad54)")
    (add_net "Net-(U2-Pad55)")
    (add_net "Net-(U2-Pad56)")
    (add_net "Net-(U2-Pad57)")
    (add_net "Net-(U2-Pad58)")
    (add_net "Net-(U2-Pad59)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad60)")
    (add_net "Net-(U2-Pad61)")
    (add_net "Net-(U2-Pad63)")
    (add_net "Net-(U2-Pad64)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad75)")
    (add_net "Net-(U2-Pad76)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U2-Pad91)")
    (add_net "Net-(U2-Pad92)")
    (add_net "Net-(U2-Pad97)")
    (add_net "Net-(U2-Pad98)")
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DD5A)
    (at 117.357 50.292 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R29 (at 3.565 0 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 190 "Net-(R29-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 182 "Net-(JP8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE12)
    (at 114.808 45.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C23 (at -2.794 -0.508 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 173 "Net-(C23-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6101DBF5)
    (at 122.682 46.482 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP8 (at -2.794 1.524 270) (layer F.SilkS))
    (fp_text value Bandwidth (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 173 "Net-(C23-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 182 "Net-(JP8-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DCA3)
    (at 113.792 42.418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L16 (at 1.27 -2.286 90) (layer F.SilkS))
    (fp_text value "100 nH" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 174 "Net-(C24-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 173 "Net-(C23-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE2D)
    (at 110.49 43.434 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C24 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value "47 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 174 "Net-(C24-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 6101DBBA)
    (at 112.776 39.116)
    (fp_text reference J12 (at 10.16 -10.16) (layer F.SilkS))
    (fp_text value DAC7 (at 0 -15.24) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 174 "Net-(C24-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
  )
  (module imported:SRR6603 (layer F.Cu) (tedit 6101DC81)
    (at 118.364 45.212 90)
    (fp_text reference L15 (at 4.572 3.556 180) (layer F.SilkS))
    (fp_text value "2.2 mH" (at 0.01524 -4.65328 90) (layer F.Fab))
    (pad 1 smd rect (at -2.775 0 180) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 182 "Net-(JP8-Pad1)"))
    (pad 2 smd rect (at 2.775 0) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 173 "Net-(C23-Pad2)"))
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DCC1)
    (at 139.192 42.418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L14 (at 1.27 -2.286 270) (layer F.SilkS))
    (fp_text value "100 nH" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 171 "Net-(C21-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 172 "Net-(C22-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE3A)
    (at 135.89 43.434 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C22 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value "47 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 172 "Net-(C22-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DD66)
    (at 142.757 50.292 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R28 (at 3.565 0 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 181 "Net-(JP7-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 189 "Net-(R28-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 6101DBAC)
    (at 138.176 39.116)
    (fp_text reference J11 (at 10.16 -10.16) (layer F.SilkS))
    (fp_text value DAC6 (at 0 -15.24) (layer F.Fab))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 172 "Net-(C22-Pad2)"))
  )
  (module imported:SRR6603 (layer F.Cu) (tedit 6101DC71)
    (at 143.764 45.212 90)
    (fp_text reference L13 (at 4.572 3.556 180) (layer F.SilkS))
    (fp_text value "2.2 mH" (at 0.01524 -4.65328 90) (layer F.Fab))
    (pad 2 smd rect (at 2.775 0) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 171 "Net-(C21-Pad2)"))
    (pad 1 smd rect (at -2.775 0 180) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 181 "Net-(JP7-Pad1)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE0A)
    (at 140.208 45.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C21 (at -2.794 -0.254 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 171 "Net-(C21-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6101DBFF)
    (at 148.082 46.482 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP7 (at -2.794 1.27 270) (layer F.SilkS))
    (fp_text value Bandwidth (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 181 "Net-(JP7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 "Net-(C21-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE46)
    (at 161.29 43.434 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C20 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value "47 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 170 "Net-(C20-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 6101DBA3)
    (at 163.576 39.116)
    (fp_text reference J10 (at 10.16 -10.16) (layer F.SilkS))
    (fp_text value DAC5 (at 0 -15.24) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 170 "Net-(C20-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DCD1)
    (at 164.592 42.418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L12 (at 1.27 -2.286 270) (layer F.SilkS))
    (fp_text value "100 nH" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 170 "Net-(C20-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 169 "Net-(C19-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DDFF)
    (at 165.608 45.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C19 (at -2.794 -0.254 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 169 "Net-(C19-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DD71)
    (at 168.157 50.292 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R27 (at 3.565 0 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 188 "Net-(R27-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 180 "Net-(JP6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6101DC08)
    (at 173.482 46.482 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP6 (at -3.048 1.27 270) (layer F.SilkS))
    (fp_text value Bandwidth (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 169 "Net-(C19-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 180 "Net-(JP6-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module imported:SRR6603 (layer F.Cu) (tedit 6101DC67)
    (at 169.164 45.212 90)
    (fp_text reference L11 (at 4.572 3.556 180) (layer F.SilkS))
    (fp_text value "2.2 mH" (at 0.01524 -4.65328 90) (layer F.Fab))
    (pad 1 smd rect (at -2.775 0 180) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 180 "Net-(JP6-Pad1)"))
    (pad 2 smd rect (at 2.775 0) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 169 "Net-(C19-Pad2)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DDEF)
    (at 191.008 45.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C17 (at -2.794 -0.254 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 167 "Net-(C17-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DCE3)
    (at 189.992 42.418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L10 (at 1.27 -2.286 270) (layer F.SilkS))
    (fp_text value "100 nH" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 167 "Net-(C17-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 168 "Net-(C18-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DD7B)
    (at 193.557 50.292 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R26 (at 3.565 0 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 179 "Net-(JP5-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 187 "Net-(R26-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6101DC11)
    (at 198.882 46.482 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP5 (at -3.048 1.27 270) (layer F.SilkS))
    (fp_text value Bandwidth (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 179 "Net-(JP5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 167 "Net-(C17-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE52)
    (at 186.69 43.434 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C18 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value "47 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 168 "Net-(C18-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 6101DB97)
    (at 188.976 39.116)
    (fp_text reference J9 (at 9.652 -10.16) (layer F.SilkS))
    (fp_text value DAC4 (at 0 -15.24) (layer F.Fab))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 168 "Net-(C18-Pad2)"))
  )
  (module imported:SRR6603 (layer F.Cu) (tedit 6101DC5F)
    (at 194.564 45.212 90)
    (fp_text reference L9 (at 4.572 3.302 180) (layer F.SilkS))
    (fp_text value "2.2 mH" (at 0.01524 -4.65328 90) (layer F.Fab))
    (pad 2 smd rect (at 2.775 0) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(C17-Pad2)"))
    (pad 1 smd rect (at -2.775 0 180) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 179 "Net-(JP5-Pad1)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DDE4)
    (at 216.408 45.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C15 (at -2.794 -0.254 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 165 "Net-(C15-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module imported:SRR6603 (layer F.Cu) (tedit 6101DC59)
    (at 219.964 45.212 90)
    (fp_text reference L7 (at 4.572 3.048 180) (layer F.SilkS))
    (fp_text value "2.2 mH" (at 0.01524 -4.65328 90) (layer F.Fab))
    (pad 1 smd rect (at -2.775 0 180) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 178 "Net-(JP4-Pad1)"))
    (pad 2 smd rect (at 2.775 0) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(C15-Pad2)"))
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DCF1)
    (at 215.392 42.418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L8 (at 1.27 -2.032 180) (layer F.SilkS))
    (fp_text value "100 nH" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 166 "Net-(C16-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 165 "Net-(C15-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DD88)
    (at 218.957 50.292 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R25 (at 3.565 0 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 186 "Net-(R25-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 178 "Net-(JP4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE5B)
    (at 212.09 43.434 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C16 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value "47 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 166 "Net-(C16-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 6101DB8D)
    (at 214.376 39.116)
    (fp_text reference J8 (at 9.652 -10.16) (layer F.SilkS))
    (fp_text value DAC3 (at 0 -15.24) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 166 "Net-(C16-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6101DC19)
    (at 224.282 46.482 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP4 (at -3.048 1.27 270) (layer F.SilkS))
    (fp_text value Bandwidth (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 "Net-(C15-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 178 "Net-(JP4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DD93)
    (at 244.357 50.292 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R24 (at 3.565 0 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 177 "Net-(JP3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 185 "Net-(R24-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module imported:SRR6603 (layer F.Cu) (tedit 6101DC4F)
    (at 245.364 45.212 90)
    (fp_text reference L5 (at 4.572 3.048 180) (layer F.SilkS))
    (fp_text value "2.2 mH" (at 0.01524 -4.65328 90) (layer F.Fab))
    (pad 2 smd rect (at 2.775 0) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(C13-Pad2)"))
    (pad 1 smd rect (at -2.775 0 180) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 177 "Net-(JP3-Pad1)"))
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DDD3)
    (at 241.808 45.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C13 (at -2.794 -0.254 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 163 "Net-(C13-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DCFD)
    (at 240.792 42.418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L6 (at 1.27 -2.032 180) (layer F.SilkS))
    (fp_text value "100 nH" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 163 "Net-(C13-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 164 "Net-(C14-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6101DC21)
    (at 249.682 46.482 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP3 (at -3.048 1.27 270) (layer F.SilkS))
    (fp_text value Bandwidth (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 177 "Net-(JP3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 163 "Net-(C13-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE64)
    (at 237.49 43.434 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C14 (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value "47 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 164 "Net-(C14-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 6101DB81)
    (at 239.776 39.116)
    (fp_text reference J7 (at 9.652 -10.16) (layer F.SilkS))
    (fp_text value DAC2 (at 0 -15.24) (layer F.Fab))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 164 "Net-(C14-Pad2)"))
  )
  (module imported:SRR6603 (layer F.Cu) (tedit 6101DC47)
    (at 270.764 45.212 90)
    (fp_text reference L3 (at 4.572 3.048 180) (layer F.SilkS))
    (fp_text value "2.2 mH" (at 0.01524 -4.65328 90) (layer F.Fab))
    (pad 1 smd rect (at -2.775 0 180) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 176 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 2.775 0) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 161 "Net-(C11-Pad2)"))
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DD06)
    (at 266.192 42.418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L4 (at 1.27 -2.032 180) (layer F.SilkS))
    (fp_text value "100 nH" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 162 "Net-(C12-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 161 "Net-(C11-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 6101DB71)
    (at 265.176 39.116)
    (fp_text reference J6 (at 9.652 -10.16) (layer F.SilkS))
    (fp_text value DAC1 (at 0 -15.24) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 162 "Net-(C12-Pad2)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6101DC2A)
    (at 275.082 46.482 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at -2.794 1.27 270) (layer F.SilkS))
    (fp_text value Bandwidth (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 161 "Net-(C11-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 176 "Net-(JP2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DDA0)
    (at 269.757 50.292 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R23 (at 3.565 0 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 184 "Net-(R23-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 176 "Net-(JP2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DE68)
    (at 262.89 43.434 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at 0 -2.286 90) (layer F.SilkS))
    (fp_text value "47 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 162 "Net-(C12-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 6101DDC9)
    (at 267.208 45.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at -2.794 -0.254 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 161 "Net-(C11-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EED9C)
    (at 286.512 49.53 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C27 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEF20)
    (at 261.112 49.53 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C28 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEF2B)
    (at 235.712 49.53 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C29 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEF31)
    (at 210.312 49.53 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C30 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEF47)
    (at 184.912 49.53 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C36 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEF4C)
    (at 159.512 49.53 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C37 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEF54)
    (at 134.112 49.53 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C38 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EED8C)
    (at 284.226 49.574167 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 3.600167 0 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 134 -15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEF10)
    (at 258.826 49.574167 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 3.600167 0 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 134 -15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEEF8)
    (at 233.426 49.574167 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C25 (at 3.600167 0 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 134 -15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEEF3)
    (at 208.026 49.574167 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C26 (at 3.600167 0 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 134 -15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEEE2)
    (at 182.626 49.574167 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C31 (at 3.600167 0 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 134 -15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEEDB)
    (at 157.226 49.574167 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C32 (at 3.600167 0 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 134 -15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEECF)
    (at 131.826 49.574167 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C33 (at 3.600167 0 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 134 -15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEDB4)
    (at 304.8 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at -3.683 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 138 "Net-(R11-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 139 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF08C)
    (at 279.4 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at -3.683 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 140 "Net-(R12-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 141 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF0A0)
    (at 254 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 142 "Net-(R13-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 143 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF0BD)
    (at 228.6 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 144 "Net-(R10-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 145 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF0E0)
    (at 203.2 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R15 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 150 "Net-(R15-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 151 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF0F6)
    (at 177.8 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R16 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 152 "Net-(R16-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 153 "Net-(R16-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF10F)
    (at 152.4 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R17 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 154 "Net-(R17-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 155 "Net-(R17-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 602EEDC7)
    (at 284.226 53.34)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U6 (at 14.986 -2.794) (layer F.SilkS))
    (fp_text value AD669 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "Net-(R11-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DB8))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 146 "Net-(R11-Pad2)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /DB9))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 139 "Net-(R7-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /DB10))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 183 "Net-(R2-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /DB11))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /DB12))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /LDAC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /DB13))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /DB0))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /DB14))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DB1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /DB15))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /DB2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 129 /CS0))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /DB3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /DB4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /DB5))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /DB6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 +15V))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /DB7))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 -15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 602EF056)
    (at 258.826 53.34)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U7 (at 14.986 -2.794) (layer F.SilkS))
    (fp_text value AD669 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 140 "Net-(R12-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DB8))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 147 "Net-(R12-Pad2)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /DB9))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 141 "Net-(R8-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /DB10))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 184 "Net-(R23-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /DB11))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /DB12))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /LDAC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /DB13))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /DB0))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /DB14))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DB1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /DB15))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /DB2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /CS1))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /DB3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /DB4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /DB5))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /DB6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 +15V))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /DB7))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 -15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 602EF04A)
    (at 233.426 53.34)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U8 (at 14.986 -2.794) (layer F.SilkS))
    (fp_text value AD669 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 "Net-(R13-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DB8))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 148 "Net-(R13-Pad2)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /DB9))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 143 "Net-(R9-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /DB10))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 185 "Net-(R24-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /DB11))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /DB12))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /LDAC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /DB13))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /DB0))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /DB14))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DB1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /DB15))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /DB2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /CS2))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /DB3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /DB4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /DB5))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /DB6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 +15V))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /DB7))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 -15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 602EF03F)
    (at 208.026 53.34)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U9 (at 14.986 -2.794) (layer F.SilkS))
    (fp_text value AD669 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 144 "Net-(R10-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DB8))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 149 "Net-(R14-Pad2)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /DB9))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 145 "Net-(R10-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /DB10))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 186 "Net-(R25-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /DB11))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /DB12))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /LDAC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /DB13))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /DB0))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /DB14))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DB1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /DB15))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /DB2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /CS3))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /DB3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /DB4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /DB5))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /DB6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 +15V))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /DB7))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 -15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 602EF032)
    (at 182.626 53.34)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U10 (at 14.986 -2.794) (layer F.SilkS))
    (fp_text value AD669 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 150 "Net-(R15-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DB8))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 156 "Net-(R19-Pad2)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /DB9))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 151 "Net-(R15-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /DB10))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 187 "Net-(R26-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /DB11))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /DB12))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /LDAC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /DB13))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /DB0))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /DB14))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DB1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /DB15))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /DB2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /CS4))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /DB3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /DB4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /DB5))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /DB6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 +15V))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /DB7))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 -15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 602EF029)
    (at 157.226 53.34)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U11 (at 14.986 -2.794) (layer F.SilkS))
    (fp_text value AD669 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 152 "Net-(R16-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DB8))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 157 "Net-(R20-Pad2)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /DB9))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 153 "Net-(R16-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /DB10))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 188 "Net-(R27-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /DB11))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /DB12))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /LDAC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /DB13))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /DB0))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /DB14))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DB1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /DB15))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /DB2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /CS5))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /DB3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /DB4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /DB5))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /DB6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 +15V))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /DB7))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 -15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 602EF025)
    (at 131.826 53.34)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U12 (at 14.732 -2.794) (layer F.SilkS))
    (fp_text value AD669 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 154 "Net-(R17-Pad1)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DB8))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 158 "Net-(R21-Pad2)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /DB9))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 155 "Net-(R17-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /DB10))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 189 "Net-(R28-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /DB11))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /DB12))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /LDAC))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /DB13))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /DB0))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /DB14))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DB1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /DB15))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /DB2))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /CS6))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /DB3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /DB4))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /DB5))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 +5V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /DB6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 +15V))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /DB7))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 -15V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EEDBA)
    (at 302.26 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at -3.683 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 146 "Net-(R11-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 138 "Net-(R11-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF091)
    (at 276.86 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at -3.683 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 147 "Net-(R12-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 140 "Net-(R12-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF0A6)
    (at 251.46 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R13 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 148 "Net-(R13-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 142 "Net-(R13-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF0C1)
    (at 226.06 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R14 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 149 "Net-(R14-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 144 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF0E8)
    (at 200.66 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R19 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 156 "Net-(R19-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 150 "Net-(R15-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF0FD)
    (at 175.26 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R20 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 157 "Net-(R20-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 152 "Net-(R16-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 602EF113)
    (at 149.86 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R21 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 158 "Net-(R21-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 154 "Net-(R17-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 5C18524C)
    (at 33.274 39.116)
    (fp_text reference J2 (at 9.652 -11.43) (layer F.SilkS))
    (fp_text value SYS_CLK (at 0 -15.24) (layer F.Fab))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
  )
  (module imported:XEM6001 (layer F.Cu) (tedit 5C7414E2)
    (at 74.676 134.62)
    (descr "Through hole straight pin header, 2x25, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x25 2.54mm double row")
    (fp_text reference U2 (at -48.768 -90.424) (layer F.SilkS))
    (fp_text value XEM6001 (at -47.752 -91.948) (layer F.Fab) hide)
    (fp_text user "Opal Kelly" (at -28.448 -44.196 90) (layer F.SilkS))
    (fp_text user XEM6001 (at -24.384 -43.18 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -48.26 -80.01) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 2 thru_hole oval (at -45.72 -80.01) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 3 thru_hole oval (at -48.26 -77.47) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad 4 thru_hole oval (at -45.72 -77.47) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad4)"))
    (pad 5 thru_hole oval (at -48.26 -74.93) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(U2-Pad5)"))
    (pad 6 thru_hole oval (at -45.72 -74.93) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(U2-Pad6)"))
    (pad 7 thru_hole oval (at -48.26 -72.39) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(U2-Pad7)"))
    (pad 8 thru_hole oval (at -45.72 -72.39) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(U2-Pad8)"))
    (pad 9 thru_hole oval (at -48.26 -69.85) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(U2-Pad9)"))
    (pad 10 thru_hole oval (at -45.72 -69.85) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(U2-Pad10)"))
    (pad 11 thru_hole oval (at -48.26 -67.31) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(U2-Pad11)"))
    (pad 12 thru_hole oval (at -45.72 -67.31) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(U2-Pad12)"))
    (pad 13 thru_hole oval (at -48.26 -64.77) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(U2-Pad13)"))
    (pad 14 thru_hole oval (at -45.72 -64.77) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(U2-Pad14)"))
    (pad 15 thru_hole oval (at -48.26 -62.23) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(U2-Pad15)"))
    (pad 16 thru_hole oval (at -45.72 -62.23) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(U2-Pad16)"))
    (pad 17 thru_hole oval (at -48.26 -59.69) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(U2-Pad17)"))
    (pad 18 thru_hole oval (at -45.72 -59.69) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(U2-Pad18)"))
    (pad 19 thru_hole oval (at -48.26 -57.15) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 20 thru_hole oval (at -45.72 -57.15) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 21 thru_hole oval (at -48.26 -54.61) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(U2-Pad21)"))
    (pad 22 thru_hole oval (at -45.72 -54.61) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 "Net-(U2-Pad22)"))
    (pad 23 thru_hole oval (at -48.26 -52.07) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "Net-(U2-Pad23)"))
    (pad 24 thru_hole oval (at -45.72 -52.07) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(U2-Pad24)"))
    (pad 25 thru_hole oval (at -48.26 -49.53) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 78 "Net-(U2-Pad25)"))
    (pad 26 thru_hole oval (at -45.72 -49.53) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(U2-Pad26)"))
    (pad 27 thru_hole oval (at -48.26 -46.99) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(U2-Pad27)"))
    (pad 28 thru_hole oval (at -45.72 -46.99) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(U2-Pad28)"))
    (pad 29 thru_hole oval (at -48.26 -44.45) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(U2-Pad29)"))
    (pad 30 thru_hole oval (at -45.72 -44.45) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(U2-Pad30)"))
    (pad 31 thru_hole oval (at -48.26 -41.91) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 32 thru_hole oval (at -45.72 -41.91) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 33 thru_hole oval (at -48.26 -39.37) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(U2-Pad33)"))
    (pad 34 thru_hole oval (at -45.72 -39.37) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(U2-Pad34)"))
    (pad 35 thru_hole oval (at -48.26 -36.83) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 "Net-(U2-Pad35)"))
    (pad 36 thru_hole oval (at -45.72 -36.83) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 "Net-(U2-Pad36)"))
    (pad 37 thru_hole oval (at -48.26 -34.29) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 "Net-(U2-Pad37)"))
    (pad 38 thru_hole oval (at -45.72 -34.29) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "Net-(U2-Pad38)"))
    (pad 39 thru_hole oval (at -48.26 -31.75) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "Net-(U2-Pad39)"))
    (pad 40 thru_hole oval (at -45.72 -31.75) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Net-(U2-Pad40)"))
    (pad 41 thru_hole oval (at -48.26 -29.21) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Net-(U2-Pad41)"))
    (pad 42 thru_hole oval (at -45.72 -29.21) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 "Net-(U2-Pad42)"))
    (pad 43 thru_hole oval (at -48.26 -26.67) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 "Net-(U2-Pad43)"))
    (pad 44 thru_hole oval (at -45.72 -26.67) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 "Net-(U2-Pad44)"))
    (pad 45 thru_hole oval (at -48.26 -24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "Net-(U2-Pad45)"))
    (pad 46 thru_hole oval (at -45.72 -24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 "Net-(U2-Pad46)"))
    (pad 47 thru_hole oval (at -48.26 -21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 "Net-(U2-Pad47)"))
    (pad 48 thru_hole oval (at -45.72 -21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(U2-Pad48)"))
    (pad 49 thru_hole oval (at -48.26 -19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 50 thru_hole oval (at -45.72 -19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 64 thru_hole oval (at -2.54 -64.77) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 "Net-(U2-Pad64)"))
    (pad 61 thru_hole oval (at -5.08 -67.31) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 131 "Net-(U2-Pad61)"))
    (pad 56 thru_hole oval (at -2.54 -74.93) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(U2-Pad56)"))
    (pad 57 thru_hole oval (at -5.08 -72.39) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(U2-Pad57)"))
    (pad 58 thru_hole oval (at -2.54 -72.39) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 "Net-(U2-Pad58)"))
    (pad 60 thru_hole oval (at -2.54 -69.85) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 "Net-(U2-Pad60)"))
    (pad 51 thru_hole rect (at -5.08 -80.01) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 52 thru_hole oval (at -2.54 -80.01) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 53 thru_hole oval (at -5.08 -77.47) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(U2-Pad53)"))
    (pad 55 thru_hole oval (at -5.08 -74.93) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(U2-Pad55)"))
    (pad 59 thru_hole oval (at -5.08 -69.85) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(U2-Pad59)"))
    (pad 54 thru_hole oval (at -2.54 -77.47) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(U2-Pad54)"))
    (pad 62 thru_hole oval (at -2.54 -67.31) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 63 thru_hole oval (at -5.08 -64.77) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(U2-Pad63)"))
    (pad 70 thru_hole oval (at -2.54 -57.15) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 85 thru_hole oval (at -5.08 -36.83) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(R4-Pad7)"))
    (pad 98 thru_hole oval (at -2.54 -21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 "Net-(U2-Pad98)"))
    (pad 69 thru_hole oval (at -5.08 -57.15) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 82 thru_hole oval (at -2.54 -41.91) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 83 thru_hole oval (at -5.08 -39.37) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(R4-Pad5)"))
    (pad 72 thru_hole oval (at -2.54 -54.61) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(R3-Pad6)"))
    (pad 97 thru_hole oval (at -5.08 -21.59) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 "Net-(U2-Pad97)"))
    (pad 86 thru_hole oval (at -2.54 -36.83) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(R4-Pad8)"))
    (pad 68 thru_hole oval (at -2.54 -59.69) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(R3-Pad3)"))
    (pad 95 thru_hole oval (at -5.08 -24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(R5-Pad7)"))
    (pad 79 thru_hole oval (at -5.08 -44.45) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(R4-Pad4)"))
    (pad 84 thru_hole oval (at -2.54 -39.37) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(R4-Pad6)"))
    (pad 71 thru_hole oval (at -5.08 -54.61) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(R3-Pad5)"))
    (pad 87 thru_hole oval (at -5.08 -34.29) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(R5-Pad2)"))
    (pad 67 thru_hole oval (at -5.08 -59.69) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(R3-Pad4)"))
    (pad 90 thru_hole oval (at -2.54 -31.75) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(R5-Pad3)"))
    (pad 96 thru_hole oval (at -2.54 -24.13) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(R5-Pad8)"))
    (pad 94 thru_hole oval (at -2.54 -26.67) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(R5-Pad6)"))
    (pad 80 thru_hole oval (at -2.54 -44.45) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(R4-Pad3)"))
    (pad 100 thru_hole oval (at -2.54 -19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 89 thru_hole oval (at -5.08 -31.75) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(R5-Pad4)"))
    (pad 88 thru_hole oval (at -2.54 -34.29) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(R5-Pad1)"))
    (pad 92 thru_hole oval (at -2.54 -29.21) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Net-(U2-Pad92)"))
    (pad 73 thru_hole oval (at -5.08 -52.07) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(R3-Pad7)"))
    (pad 75 thru_hole oval (at -5.08 -49.53) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Net-(U2-Pad75)"))
    (pad 81 thru_hole oval (at -5.08 -41.91) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 99 thru_hole oval (at -5.08 -19.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 77 thru_hole oval (at -5.08 -46.99) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(R4-Pad2)"))
    (pad 66 thru_hole oval (at -2.54 -62.23) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad1)"))
    (pad 78 thru_hole oval (at -2.54 -46.99) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(R4-Pad1)"))
    (pad 74 thru_hole oval (at -2.54 -52.07) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(R3-Pad8)"))
    (pad 65 thru_hole oval (at -5.08 -62.23) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(R3-Pad2)"))
    (pad 91 thru_hole oval (at -5.08 -29.21) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 "Net-(U2-Pad91)"))
    (pad 93 thru_hole oval (at -5.08 -26.67) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(R5-Pad5)"))
    (pad 76 thru_hole oval (at -2.54 -49.53) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 132 "Net-(U2-Pad76)"))
    (pad 118 thru_hole oval (at -12.7 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
    (pad 117 thru_hole oval (at -12.7 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Net-(U2-Pad117)"))
    (pad 101 thru_hole rect (at -33.02 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(U2-Pad101)"))
    (pad 119 thru_hole oval (at -10.16 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 103 thru_hole oval (at -30.48 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(U2-Pad103)"))
    (pad 120 thru_hole oval (at -10.16 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 104 thru_hole oval (at -30.48 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 "Net-(U2-Pad104)"))
    (pad 111 thru_hole oval (at -20.32 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Net-(U2-Pad111)"))
    (pad 112 thru_hole oval (at -20.32 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Net-(U2-Pad112)"))
    (pad 114 thru_hole oval (at -17.78 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 114 "Net-(U2-Pad114)"))
    (pad 108 thru_hole oval (at -25.4 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 105 thru_hole oval (at -27.94 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Net-(U2-Pad105)"))
    (pad 106 thru_hole oval (at -27.94 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(U2-Pad106)"))
    (pad 113 thru_hole oval (at -17.78 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 "Net-(U2-Pad113)"))
    (pad 110 thru_hole oval (at -22.86 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 117 "Net-(U2-Pad110)"))
    (pad 107 thru_hole oval (at -25.4 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 118 "Net-(U2-Pad107)"))
    (pad 102 thru_hole oval (at -33.02 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 "Net-(U2-Pad102)"))
    (pad 109 thru_hole oval (at -22.86 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 "Net-(U2-Pad109)"))
    (pad 115 thru_hole oval (at -15.24 -64.77 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(U2-Pad115)"))
    (pad 116 thru_hole oval (at -15.24 -67.31 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(U2-Pad116)"))
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 79.756 105.41)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference R5 (at 0 6.223) (layer F.SilkS))
    (fp_text value "8x 100" (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R5-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(R5-Pad3)"))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(R5-Pad4)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(R5-Pad5)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(R5-Pad6)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R5-Pad7)"))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(R5-Pad8)"))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /DB0))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /DB1))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 /DB2))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 /DB3))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /DB4))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /DB5))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 /DB6))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /DB7))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 5C18524C)
    (at 51.816 39.116)
    (fp_text reference J1 (at 9.652 -11.43) (layer F.SilkS))
    (fp_text value GCLK (at 0 -15.24) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 5C18524C)
    (at 70.358 39.116)
    (fp_text reference J3 (at 9.652 -11.43) (layer F.SilkS))
    (fp_text value TRIG (at 0 -15.24) (layer F.Fab))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad1)"))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 79.756 67.31 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 2.032 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 8 /LDAC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 79.756 77.724)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference R3 (at 0 6.223) (layer F.SilkS))
    (fp_text value "8x 100" (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /CS7))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /CS6))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS5))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /CS4))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /CS3))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /CS2))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /CS1))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 129 /CS0))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R3-Pad8)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R3-Pad7)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R3-Pad6)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R3-Pad5)"))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R3-Pad4)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R3-Pad3)"))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R3-Pad2)"))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 79.756 91.567)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference R4 (at 0 6.35) (layer F.SilkS))
    (fp_text value "8x 100" (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R4-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R4-Pad3)"))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R4-Pad4)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R4-Pad5)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R4-Pad6)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R4-Pad7)"))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R4-Pad8)"))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /DB8))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /DB9))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /DB10))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /DB11))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /DB12))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /DB13))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /DB14))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /DB15))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-28_W15.24mm (layer F.Cu) (tedit 5A02E8C5)
    (at 106.426 53.34)
    (descr "28-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U13 (at 14.732 -2.794) (layer F.SilkS))
    (fp_text value AD669 (at 7.62 35.35) (layer F.Fab))
    (fp_text user %R (at 7.62 16.51) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 -15V))
    (pad 15 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /DB7))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 +15V))
    (pad 16 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /DB6))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 +5V))
    (pad 17 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /DB5))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 18 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /DB4))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 19 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /DB3))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /CS7))
    (pad 20 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /DB2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /DB15))
    (pad 21 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 /DB1))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /DB14))
    (pad 22 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 /DB0))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /DB13))
    (pad 23 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /LDAC))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /DB12))
    (pad 24 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /DB11))
    (pad 25 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 190 "Net-(R29-Pad2)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /DB10))
    (pad 26 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(R18-Pad2)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /DB9))
    (pad 27 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(R22-Pad2)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /DB8))
    (pad 28 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(R18-Pad1)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-28_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 127 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R18 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 56 "Net-(R18-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 57 "Net-(R18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 124.46 54.483 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R22 (at -3.937 0 270) (layer F.SilkS))
    (fp_text value 50 (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 57 "Net-(R18-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 270) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 58 "Net-(R22-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 316.484 80.772 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at -0.508 2.032 270) (layer F.SilkS))
    (fp_text value 2.2UF (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +24V))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 313.436 85.344 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 1UF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 316.33821 98.615149 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.33UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 Earth))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 +24V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 316.33821 102.679149 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 Earth))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 135 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 316.484 66.548 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at -1.016 2.032 270) (layer F.SilkS))
    (fp_text value 2.2UF (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 136 -24V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 314.96 70.612)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at -4.064 0) (layer F.SilkS))
    (fp_text value 1UF (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 134 -15V))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 316.484 85.852 90)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at -3.556 0 90) (layer F.SilkS))
    (fp_text value SM4001 (at 0 2.1 90) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905 90) (layer F.Fab))
    (pad 1 smd rect (at -1.4 0 90) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 133 +15V))
    (pad 2 smd rect (at 1.4 0 90) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123F (layer F.Cu) (tedit 587F7769)
    (at 314.96 73.152)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D2 (at 0 2.032) (layer F.SilkS))
    (fp_text value SM4001 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.905) (layer F.Fab))
    (pad 2 smd rect (at 1.4 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 134 -15V))
    (pad 1 smd rect (at -1.4 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123F.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Molex:Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5A15A247)
    (at 336.042 113.538 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-03A example for new part number: 22-27-2031, 3 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 side entry")
    (fp_text reference J5 (at 1.016 4.826 180) (layer F.SilkS))
    (fp_text value "LINEAR AC/DC" (at 2.54 4.08 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -2.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 136 -24V))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.74 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 +24V))
    (model ${KISYS3DMOD}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-03A_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 323.85 113.538)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 Earth))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown (layer F.Cu) (tedit 5AC8BA0D)
    (at 319.532 80.264 270)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference U3 (at 9.144 -18.796 270) (layer F.SilkS))
    (fp_text value LM7815 (at 2.54 2 270) (layer F.Fab))
    (fp_text user %R (at -4.064 -1.524 270) (layer F.Fab))
    (pad "" np_thru_hole oval (at 2.54 -16.66 270) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 133 +15V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown (layer F.Cu) (tedit 5AC8BA0D)
    (at 319.532 98.044 270)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference U4 (at 9.398 -18.796 270) (layer F.SilkS))
    (fp_text value LM7805 (at 2.54 2 270) (layer F.Fab))
    (fp_text user %R (at 9.144 -1.524 270) (layer F.Fab))
    (pad "" np_thru_hole oval (at 2.54 -16.66 270) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 +24V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 Earth))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 135 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown (layer F.Cu) (tedit 5CB67F59)
    (at 319.532 66.548 270)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference U5 (at 9.144 -18.796 270) (layer F.SilkS))
    (fp_text value LM7915 (at 2.54 2 270) (layer F.Fab) hide)
    (fp_text user %R (at 9.144 -1.524 270) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 134 -15V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 136 -24V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole oval (at 2.54 -16.66 270) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 106.426 49.574167 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C34 (at 3.600167 0 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 134 -15V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 108.712 49.53 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C39 (at 0 2.286 90) (layer F.SilkS))
    (fp_text value 0.1UF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 133 +15V))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 292.608 45.72 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at -2.794 -0.254 180) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 159 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 288.29 43.434 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -2.286 90) (layer F.SilkS))
    (fp_text value "47 uF" (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 160 "Net-(C10-Pad2)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:BNC_HORZMOUNT (layer F.Cu) (tedit 5C18524C)
    (at 290.576 39.116)
    (fp_text reference J4 (at 9.652 -10.16) (layer F.SilkS))
    (fp_text value DAC0 (at 0 -15.24) (layer F.Fab))
    (pad "" thru_hole circle (at -5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 5.08 -5.08) (size 3.8 3.8) (drill 2.01) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -2.54 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.89) (layers *.Cu *.Mask)
      (net 160 "Net-(C10-Pad2)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 6101CEA5)
    (at 300.482 46.482 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at -3.048 1.27 270) (layer F.SilkS))
    (fp_text value Bandwidth (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 175 "Net-(JP1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 159 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module imported:SRR6603 (layer F.Cu) (tedit 6101C4B6)
    (at 296.164 45.212 90)
    (fp_text reference L1 (at 4.572 3.048 180) (layer F.SilkS))
    (fp_text value "2.2 mH" (at 0.01524 -4.65328 90) (layer F.Fab))
    (pad 2 smd rect (at 2.775 0) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 159 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -2.775 0 180) (size 3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 175 "Net-(JP1-Pad1)"))
  )
  (module Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 291.592 42.418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L2 (at 1.27 -2.032 180) (layer F.SilkS))
    (fp_text value "100 nH" (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 159 "Net-(C9-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 160 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 295.157 50.292 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 3.057 0 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.65 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 175 "Net-(JP1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 183 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "DAC7\n" (at 121.412 30.734) (layer F.SilkS))
  (gr_text "DAC6\n" (at 146.812 30.734) (layer F.SilkS))
  (gr_text "DAC5\n" (at 172.212 30.734) (layer F.SilkS))
  (gr_text "DAC4\n" (at 197.612 30.734) (layer F.SilkS))
  (gr_text "DAC3\n" (at 223.012 30.734) (layer F.SilkS))
  (gr_text "DAC2\n" (at 248.412 30.734) (layer F.SilkS))
  (gr_text "DAC1\n" (at 273.812 30.734) (layer F.SilkS))
  (gr_text "DAC0\n" (at 299.212 30.734) (layer F.SilkS))
  (gr_text "Bandwidth Jumpers\nOpen: Low\nClosed: High\n" (at 325.882 41.656) (layer F.SilkS))
  (gr_text "DAC Board\nRev. 2 07.30.2021" (at 325.374 32.258) (layer F.SilkS))
  (gr_text GND (at 333.502 118.364) (layer F.SilkS))
  (gr_text -24V (at 338.328 118.364) (layer F.SilkS))
  (gr_text +24V (at 328.676 118.364) (layer F.SilkS))
  (gr_line (start 23.368 26.924) (end 340.868 26.924) (layer Edge.Cuts) (width 0.5))
  (gr_line (start 340.868 26.924) (end 340.868 119.888) (layer Edge.Cuts) (width 0.5))
  (gr_line (start 23.368 119.888) (end 340.868 119.888) (layer Edge.Cuts) (width 0.5))
  (gr_line (start 23.368 26.924) (end 23.368 119.888) (layer Edge.Cuts) (width 0.5))
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.368 26.924) (xy 91.44 26.924) (xy 91.44 119.888) (xy 23.368 119.888)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 340.614 59.436) (xy 340.868 59.436) (xy 340.868 88.9) (xy 309.372 88.9) (xy 309.372 59.436)
        (xy 305.181 59.436) (xy 300.736 63.881) (xy 298.196 63.881) (xy 293.751 59.436) (xy 279.781 59.436)
        (xy 275.336 63.881) (xy 272.796 63.881) (xy 268.351 59.436) (xy 254.381 59.436) (xy 249.936 63.881)
        (xy 247.396 63.881) (xy 242.951 59.436) (xy 228.981 59.436) (xy 224.536 63.881) (xy 221.996 63.881)
        (xy 217.551 59.436) (xy 203.581 59.436) (xy 199.136 63.881) (xy 196.596 63.881) (xy 192.151 59.436)
        (xy 178.181 59.436) (xy 173.736 63.881) (xy 171.196 63.881) (xy 166.751 59.436) (xy 152.781 59.436)
        (xy 148.336 63.881) (xy 145.796 63.881) (xy 141.351 59.436) (xy 127.381 59.436) (xy 122.936 63.881)
        (xy 120.396 63.881) (xy 115.951 59.436) (xy 97.028 59.436) (xy 97.028 26.924) (xy 340.868 26.924)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.634 65.024) (xy 303.784 65.024) (xy 303.784 119.888) (xy 89.154 119.888) (xy 89.154 65.024)
        (xy 115.062 65.024)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107.696 60.579) (xy 105.156 60.579) (xy 99.695 66.04) (xy 113.157 66.04)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.096 60.579) (xy 130.556 60.579) (xy 125.095 66.04) (xy 138.557 66.04)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.496 60.579) (xy 155.956 60.579) (xy 150.495 66.04) (xy 163.957 66.04)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.896 60.579) (xy 181.356 60.579) (xy 175.895 66.04) (xy 189.357 66.04)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 209.296 60.579) (xy 206.756 60.579) (xy 201.295 66.04) (xy 214.757 66.04)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.696 60.579) (xy 232.156 60.579) (xy 226.695 66.04) (xy 240.157 66.04)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 260.096 60.579) (xy 257.556 60.579) (xy 252.095 66.04) (xy 265.557 66.04)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 285.496 60.579) (xy 282.956 60.579) (xy 277.495 66.04) (xy 290.957 66.04)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 325.628 88.646) (xy 325.628 120.142) (xy 340.868 120.142) (xy 340.868 88.646)
      )
    )
  )
  (zone (net 3) (net_name Earth) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 301.244 94.488) (xy 322.072 94.488) (xy 322.072 119.888) (xy 301.244 119.888)
      )
    )
  )
  (zone (net 135) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 301.752 94.488) (xy 322.072 94.488) (xy 322.072 119.888) (xy 301.752 119.888)
      )
    )
  )
  (zone (net 133) (net_name +15V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.028 26.924) (xy 97.028 59.436) (xy 340.868 59.436) (xy 340.868 26.924)
      )
    )
  )
  (zone (net 134) (net_name -15V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 340.868 119.888) (xy 325.628 119.888) (xy 325.628 88.9) (xy 309.372 88.9) (xy 309.372 59.436)
        (xy 97.028 59.436) (xy 97.028 26.924) (xy 340.868 26.924)
      )
    )
  )
  (zone (net 135) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23.368 26.924) (xy 23.368 67.056) (xy 91.44 67.056) (xy 91.44 26.924)
      )
    )
  )
  (zone (net 135) (net_name +5V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 303.784 119.888) (xy 23.368 119.888) (xy 23.368 65.024) (xy 303.784 65.024)
      )
    )
  )
  (zone (net 133) (net_name +15V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 340.868 119.888) (xy 340.868 88.392) (xy 325.628 88.392) (xy 325.628 119.888)
      )
    )
  )
  (zone (net 133) (net_name +15V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 309.372 88.9) (xy 340.868 88.9) (xy 340.868 26.924) (xy 309.372 26.924)
      )
    )
  )
)
