(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gbr/")
    )
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U1-Pad2)")
  (net 3 "unconnected-(U1-Pad8)")
  (net 4 "unconnected-(U1-Pad9)")
  (net 5 "unconnected-(U1-Pad12)")
  (net 6 "unconnected-(U1-Pad13)")
  (net 7 "Net-(U1-Pad3)")
  (net 8 "Net-(U1-Pad5)")
  (net 9 "Net-(U1-Pad6)")
  (net 10 "Net-(U1-Pad7)")
  (net 11 "GND")
  (net 12 "Net-(U1-Pad14)")
  (net 13 "Net-(U1-Pad15)")
  (net 14 "Net-(U1-Pad16)")
  (net 15 "Net-(U1-Pad18)")
  (net 16 "Net-(U1-Pad19)")
  (net 17 "-15V")
  (net 18 "+15V")
  (net 19 "Net-(U2-Pad4)")
  (net 20 "Net-(U2-Pad13)")
  (footprint "Library:SSOP-20_4.4x6.5mm_P0.65mm" (layer "F.Cu")
    (tedit 62126013)
    (at 144.78 76.2)
    (descr "SSOP20: plastic shrink small outline package; 20 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot266-1_po.pdf)")
    (tags "SSOP 0.65")
    (property "Sheetfile" "ssm2040 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.3) (layer "F.SilkS") hide)
    (fp_text value "SSI2140" (at 0 -0.023183 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -2.85 -2.925) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(U1-Pad1)") (pinfunction "OUT2") (pintype "passive"))
    (pad "2" smd rect (at -2.85 -2.275) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(U1-Pad2)") (pinfunction "CAP2") (pintype "passive"))
    (pad "3" smd rect (at -2.85 -1.625) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(U1-Pad3)") (pinfunction "IN2") (pintype "passive"))
    (pad "4" smd rect (at -2.85 -0.975) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(U2-Pad4)") (pinfunction "OUT1") (pintype "passive"))
    (pad "5" smd rect (at -2.85 -0.325) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(U1-Pad5)") (pinfunction "CAP1") (pintype "passive"))
    (pad "6" smd rect (at -2.85 0.325) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(U1-Pad6)") (pinfunction "IN1") (pintype "passive"))
    (pad "7" smd rect (at -2.85 0.975) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(U1-Pad7)") (pinfunction "EXPO_CTRL") (pintype "passive"))
    (pad "8" smd rect (at -2.85 1.625) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "unconnected-(U1-Pad8)") (pinfunction "TEMPCO") (pintype "power_in+no_connect"))
    (pad "9" smd rect (at -2.85 2.275) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "unconnected-(U1-Pad9)") (pinfunction "QVCA_OUT") (pintype "power_in+no_connect"))
    (pad "10" smd rect (at -2.85 2.925) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd rect (at 2.85 2.925) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd rect (at 2.85 2.275) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(U1-Pad12)") (pinfunction "QCTRL") (pintype "passive+no_connect"))
    (pad "13" smd rect (at 2.85 1.625) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(U1-Pad13)") (pinfunction "QVCA_IN+") (pintype "passive+no_connect"))
    (pad "14" smd rect (at 2.85 0.975) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(U1-Pad14)") (pinfunction "OUT4") (pintype "passive"))
    (pad "15" smd rect (at 2.85 0.325) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(U1-Pad15)") (pinfunction "CAP4") (pintype "passive"))
    (pad "16" smd rect (at 2.85 -0.325) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(U1-Pad16)") (pinfunction "IN4") (pintype "passive"))
    (pad "17" smd rect (at 2.85 -0.975) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(U2-Pad13)") (pinfunction "OUT3") (pintype "passive"))
    (pad "18" smd rect (at 2.85 -1.625) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(U1-Pad18)") (pinfunction "CAP3") (pintype "passive"))
    (pad "19" smd rect (at 2.85 -2.275) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(U1-Pad19)") (pinfunction "IN3") (pintype "passive"))
    (pad "20" smd rect (at 2.85 -2.925) (size 0.9 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "+15V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-20_4.4x6.5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Library:DIP-16_W7.62mm-5" (layer "F.Cu")
    (tedit 62391062)
    (at 140.98 67.31)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "ssm2040 adapter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS") hide)
    (fp_text value "SSM2040" (at 3.81 20.11) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "B.Cu" "B.Mask")
      (pinfunction "CAP4") (pintype "passive"))
    (pad "" np_thru_hole oval (at 7.62 7.62) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu)
      (zone_connect 0))
    (pad "" np_thru_hole oval (at 0 7.62) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu)
      (zone_connect 0))
    (pad "" np_thru_hole oval (at 7.62 10.16) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu)
      (zone_connect 0))
    (pad "" np_thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers "B.Cu" "B.Mask")
      (pinfunction "CAP4") (pintype "passive"))
    (pad "" np_thru_hole oval (at 7.62 12.79195) (size 1.6 1.6) (drill 0.8) (layers "B.Cu" "B.Mask")
      (pinfunction "CAP4") (pintype "passive"))
    (pad "" np_thru_hole oval (at 0 10.16) (size 0.8 0.8) (drill 0.8) (layers F&B.Cu)
      (zone_connect 0))
    (pad "" np_thru_hole oval (at 7.62 5.17195) (size 1.6 1.6) (drill 0.8) (layers "B.Cu" "B.Mask")
      (pinfunction "CAP4") (pintype "passive"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(U1-Pad1)") (pinfunction "OUT2") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad2)") (pinfunction "CAP2") (pintype "passive"))
    (pad "3" smd roundrect (at 0 5.08) (size 1.6 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
      (chamfer_ratio 0.5) (chamfer bottom_right)
      (net 7 "Net-(U1-Pad3)") (pinfunction "IN2") (pintype "passive"))
    (pad "6" smd roundrect (at 0 12.7) (size 1.6 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
      (chamfer_ratio 0.5) (chamfer top_right)
      (net 9 "Net-(U1-Pad6)") (pinfunction "IN1") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad7)") (pinfunction "CNTL_IN") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "9" smd roundrect (at 7.62 12.79195) (size 1.6 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
      (chamfer_ratio 0.5) (chamfer top_left)
      (net 17 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "10" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad14)") (pinfunction "OUT4") (pintype "passive"))
    (pad "14" smd roundrect (at 7.62 5.17195) (size 1.6 1.6) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.5)
      (chamfer_ratio 0.5) (chamfer bottom_left)
      (net 15 "Net-(U1-Pad18)") (pinfunction "CAP3") (pintype "passive"))
    (pad "15" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad19)") (pinfunction "IN3") (pintype "passive"))
    (pad "16" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "+15V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_poly
    (pts
      (arc (start 139.7 86.106) (mid 139.774395 86.285605) (end 139.954 86.36))
      (arc (start 149.606 86.36) (mid 149.785605 86.285605) (end 149.86 86.106))
      (arc (start 149.86 66.294) (mid 149.785605 66.114395) (end 149.606 66.04))
      (xy 145.796 66.04)
      (xy 145.793554 66.139826)
      (xy 145.754604 66.335643)
      (xy 145.6782 66.520098)
      (xy 145.567279 66.686103)
      (xy 145.426103 66.827279)
      (xy 145.260098 66.9382)
      (xy 145.075643 67.014604)
      (xy 144.879826 67.053554)
      (xy 144.680174 67.053554)
      (xy 144.484357 67.014604)
      (xy 144.299902 66.9382)
      (xy 144.133897 66.827279)
      (xy 143.992721 66.686103)
      (xy 143.8818 66.520098)
      (xy 143.805396 66.335643)
      (xy 143.766446 66.139826)
      (xy 143.764 66.04)
      (arc (start 139.954 66.04) (mid 139.774395 66.114395) (end 139.7 66.294))
    ) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "G.Müller\nCC BY-NC" (at 144.78 85.09) (layer "F.SilkS"))
  (zone (net 11) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads no (clearance 0.128))
    (min_thickness 0.128) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.128))
    (polygon
      (pts
        (xy 149.86 86.36)
        (xy 139.7 86.36)
        (xy 139.7 66.04)
        (xy 149.86 66.04)
      )
    )
  )
)
