(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 40)
    (no_connects 1)
    (area 75.442857 77.325 124.557143 131.000001)
    (thickness 1.6)
    (drawings 12)
    (tracks 126)
    (zones 0)
    (modules 31)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.33)
    (user_trace_width 0.33)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 GND)
  (net 5 "Net-(D1-Pad1)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D3-Pad1)")
  (net 8 "Net-(D4-Pad1)")
  (net 9 "Net-(D5-Pad1)")
  (net 10 "Net-(D6-Pad1)")
  (net 11 "Net-(D7-Pad1)")
  (net 12 "Net-(D8-Pad1)")
  (net 13 "Net-(D10-Pad2)")
  (net 14 "Net-(D10-Pad1)")
  (net 15 "Net-(D11-Pad2)")
  (net 16 "Net-(J1-Pad1)")
  (net 17 "Net-(D12-Pad1)")
  (net 18 "Net-(D13-Pad1)")
  (net 19 "Net-(D14-Pad1)")
  (net 20 "Net-(D15-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(J1-Pad1)")
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 100 81.5)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0.09124 -4.42878) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 85 115)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at -11.10124 -26.52672) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 109.4 115.2 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.08602 -1.69334 180) (layer B.SilkS))
    (fp_text value 1.0uF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 104.2 115.6)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.27082 -1.75466) (layer B.SilkS))
    (fp_text value 2.2uF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 100 115 180)
    (fp_text reference D1 (at -28.07442 -2.6401 180) (layer F.SilkS))
    (fp_text value LED (at 0 -4 180) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 180) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.5 0 180) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 106.51 113.51 205.7)
    (fp_text reference D2 (at -19.590747 -4.269963 205.7) (layer F.SilkS))
    (fp_text value LED (at 0 -4 205.7) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 205.7) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.5 0 205.7) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 111.73 109.35 231.4)
    (fp_text reference D3 (at -10.77781 -6.163913 231.4) (layer F.SilkS))
    (fp_text value LED (at 0 -4 231.4) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 231.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.5 0 231.4) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 114.62 103.34 257.1)
    (fp_text reference D4 (at -9.65225 -7.146688 257.1) (layer F.SilkS))
    (fp_text value LED (at 0 -4 257.1) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 257.1) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.5 0 257.1) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 114.62 96.66 282.8)
    (fp_text reference D5 (at -7.244994 -4.008553 282.8) (layer F.SilkS))
    (fp_text value LED (at 0 -4 282.8) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 282.8) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.5 0 282.8) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 111.73 90.65 308.5)
    (fp_text reference D6 (at -2.829421 -5.982401 308.5) (layer F.SilkS))
    (fp_text value LED (at 0 -4 308.5) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 308.5) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.5 0 308.5) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D5-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 106.51 86.49 334.2)
    (fp_text reference D7 (at 3.203369 -6.136388 334.2) (layer F.SilkS))
    (fp_text value LED (at 0 -4 334.2) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 334.2) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 0.5 0 334.2) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 100 85)
    (fp_text reference D8 (at -31.90006 2.8459) (layer F.SilkS))
    (fp_text value LED (at 0 -4) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 0.5 0) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D7-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 93.49 86.49 25.7)
    (fp_text reference D9 (at -7.587548 -7.364575 25.7) (layer F.SilkS))
    (fp_text value LED (at 0 -4 25.7) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 25.7) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 0.5 0 25.7) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 88.27 90.65 51.4)
    (fp_text reference D10 (at -9.912392 -7.869302 51.4) (layer F.SilkS))
    (fp_text value LED (at 0 -4 51.4) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 51.4) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 0.5 0 51.4) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D10-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Angled_1x03 (layer F.Cu) (tedit 0)
    (at 93.54 119.4 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -0.66008 -30.56186 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDParts:Inductor (layer B.Cu) (tedit 5F0F719F)
    (at 109.2 122 180)
    (fp_text reference L1 (at -4.63518 0.1308 180) (layer B.SilkS))
    (fp_text value 33uH (at 0 3 180) (layer B.Fab))
    (pad 1 smd rect (at -2.7 0 180) (size 1.2 6.6) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at 2.7 0 180) (size 1.2 6.6) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D11-Pad2)"))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 98.8 117.2 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 1R33 (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 109.35 111.73 38.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2.1 38.5) (layer B.SilkS))
    (fp_text value R250 (at 0 -2.1 38.5) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 38.5) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 38.5) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 115 100 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value R250 (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 109.35 88.27 141.4)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 2.1 141.4) (layer B.SilkS))
    (fp_text value R250 (at 0 -2.1 321.4) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 141.4) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.95 0 141.4) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 96.66 85.38 192.8)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 2.1 192.8) (layer B.SilkS))
    (fp_text value R250 (at 0 -2.1 192.8) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 192.8) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 0.95 0 192.8) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 86.49 93.49 244.2)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 2.1 244.2) (layer B.SilkS))
    (fp_text value R250 (at 0 -2.1 244.2) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 244.2) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 0.95 0 244.2) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer B.Cu) (tedit 583F3A3F)
    (at 99 121.4 90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U1 (at 0.15056 -2.31744 90) (layer B.SilkS))
    (fp_text value AL8805 (at 0 -2.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 3 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J1-Pad1)"))
    (pad 4 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 85.38 96.66 77.1)
    (fp_text reference D12 (at -3.143434 -7.923836 77.1) (layer F.SilkS))
    (fp_text value LED (at 0 -4 77.1) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 77.1) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 0.5 0 77.1) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 85.38 103.34 102.8)
    (fp_text reference D13 (at 3.152908 -10.093754 102.8) (layer F.SilkS))
    (fp_text value LED (at 0 -4 102.8) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 102.8) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 0.5 0 102.8) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D12-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 88.27 109.35 128.5)
    (fp_text reference D14 (at 10.737019 -9.923266 128.5) (layer F.SilkS))
    (fp_text value LED (at 0.370501 -3.233581 128.5) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 128.5) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 0.5 0 128.5) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
  )
  (module LEDParts:OSRAMLED (layer F.Cu) (tedit 5F0F6F5A)
    (at 93.49 113.51 154.2)
    (fp_text reference D15 (at -30.565752 14.127114 154.2) (layer F.SilkS))
    (fp_text value LED (at -0.894605 -3.708458 154.2) (layer F.Fab))
    (pad 1 smd rect (at -0.65 0 154.2) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 0.5 0 154.2) (size 1 0.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D14-Pad1)"))
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 86.49 106.51 295.7)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 2.1 295.7) (layer B.SilkS))
    (fp_text value R250 (at 0 -2.1 295.7) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 295.7) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 0.95 0 295.7) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 58307B54)
    (at 96.66 114.62 347.1)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 2.1 347.1) (layer B.SilkS))
    (fp_text value R250 (at -6 -0.424999 347.1) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 347.1) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 0.95 0 347.1) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SMA_Standard (layer B.Cu) (tedit 586432E5)
    (at 103.2 120.6 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D11 (at 0 3.81 270) (layer B.SilkS))
    (fp_text value D_Shockley (at 0 -4.3 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D11-Pad2)"))
    (model Diodes_SMD.3dshapes/D_SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5F160723)
    (at 115 115)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 11.64186 -13.98928) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad "" np_thru_hole circle (at -0.2 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_text "mds - 2020" (at 107.6579 120.57888) (layer F.SilkS))
  (gr_text rev0.0 (at 107.2896 118.41988) (layer F.SilkS))
  (gr_text ADJ (at 93.6625 116.3955 90) (layer F.SilkS))
  (gr_text GND (at 91.11234 116.21262 90) (layer F.SilkS))
  (gr_text +12-24v (at 88.51138 114.70894 90) (layer F.SilkS))
  (gr_arc (start 100 100) (end 82 100) (angle 80.702) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100 81.5) (end 102.908 82.2365) (angle -208.422) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 82 126) (end 82 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118 126) (end 82 126) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118 100) (end 118 126) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100 100) (end 118 100) (angle -80.702) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 100 100) (end 112.5 100) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120 80) (xy 120 130) (xy 79 130) (xy 80 80)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121 79) (xy 121 131) (xy 78 131) (xy 79 79)
      )
    )
  )
)
