(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g0214c9d)")
  (general
    (thickness 1.6)
    (drawings 46)
    (tracks 200)
    (zones 0)
    (modules 10)
    (nets 15)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1778)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.25)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010f4_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /belamini_cape_B2_2/SCL)
  (net 3 /belamini_cape_B2_2/SDA)
  (net 4 /belamini_cape_B2_2/A0)
  (net 5 /belamini_cape_B2_2/D0)
  (net 6 /belamini_cape_B2_2/D1)
  (net 7 /belamini_cape_B2_2/A1)
  (net 8 /belamini_cape_B2_2/D2)
  (net 9 /belamini_cape_B2_2/A2)
  (net 10 /belamini_cape_B2_2/A3)
  (net 11 /belamini_cape_B2_2/D3)
  (net 12 /belamini_cape_B2_2/D4)
  (net 13 /belamini_cape_B2_2/A4)
  (net 14 +3V3)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /belamini_cape_B2_2/A0)
    (add_net /belamini_cape_B2_2/A1)
    (add_net /belamini_cape_B2_2/A2)
    (add_net /belamini_cape_B2_2/A3)
    (add_net /belamini_cape_B2_2/A4)
    (add_net /belamini_cape_B2_2/D0)
    (add_net /belamini_cape_B2_2/D1)
    (add_net /belamini_cape_B2_2/D2)
    (add_net /belamini_cape_B2_2/D3)
    (add_net /belamini_cape_B2_2/D4)
    (add_net /belamini_cape_B2_2/SCL)
    (add_net /belamini_cape_B2_2/SDA)
    (add_net GND)
  )
  (module belamini_cape_B2:1X10_analog (layer Top) (tedit 5CA63B31)
    (at 153.5811 90.297 180)
    (fp_text reference J1 (at -1.6129 0.889 90) (layer F.SilkS))
    (fp_text value M10SILK_FEMALE_PTH (at -1.27 3.175) (layer F.Fab))
    (pad 10 thru_hole circle (at 22.86 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 /belamini_cape_B2_2/A0) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /belamini_cape_B2_2/A1) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /belamini_cape_B2_2/A2) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /belamini_cape_B2_2/A3) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /belamini_cape_B2_2/A4) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module belamini_cape_B2:2X18_P2 (layer Top) (tedit 5C8A35CF)
    (at 152.3111 86.4489)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference P2 (at 24.3459 0.8001 90) (layer F.SilkS))
    (fp_text value PINHD-2X18 (at -22.86 4.445) (layer F.Fab))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 +3V3) (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 /belamini_cape_B2_2/SDA) (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 /belamini_cape_B2_2/SCL) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /belamini_cape_B2_2/D4) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /belamini_cape_B2_2/D3) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /belamini_cape_B2_2/D2) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /belamini_cape_B2_2/D1) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 /belamini_cape_B2_2/D0) (solder_mask_margin 0.1016))
  )
  (module belamini_cape_B2:2X18_P1 (layer Top) (tedit 5C8A35AF)
    (at 152.3111 111.8489)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference P1 (at 24.4729 0.7366 90) (layer F.SilkS))
    (fp_text value PINHD-2X18 (at -22.86 4.445) (layer F.Fab))
    (pad 36 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 35 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 34 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 33 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 32 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 31 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 30 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 29 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 28 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 27 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 26 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 25 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 24 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 23 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 22 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 21 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 20 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 19 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 18 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 17 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -21.59 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer Bottom) (tedit 58D3FE32)
    (at 149.352 81.534)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J6 (at 3.0226 -4.191) (layer B.SilkS))
    (fp_text value Grove_4x2mm (at 3 -7.25) (layer B.Fab))
    (fp_text user %R (at 3 -2.5) (layer B.Fab))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 /belamini_cape_B2_2/D4))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 13 /belamini_cape_B2_2/A4))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer Bottom) (tedit 58D3FE32)
    (at 169.037 116.7 180)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J10 (at 2.921 -4.191 180) (layer B.SilkS))
    (fp_text value Grove_4x2mm (at 3.0988 -7.239 180) (layer B.Fab))
    (fp_text user %R (at 3 -2.5 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 /belamini_cape_B2_2/A2))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 /belamini_cape_B2_2/D2))
    (pad 3 thru_hole oval (at 4 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 6 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer Bottom) (tedit 58D3FE32)
    (at 155.321 116.7 180)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J9 (at 2.984 -4.191 180) (layer B.SilkS))
    (fp_text value Grove_4x2mm (at 3 -7.25 180) (layer B.Fab))
    (fp_text user %R (at 3 -2.5 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 6 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (pad 3 thru_hole oval (at 4 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 /belamini_cape_B2_2/D1))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 /belamini_cape_B2_2/A1))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer Bottom) (tedit 58D3FE32)
    (at 141.605 116.7 180)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J8 (at 3.048 -4.191 180) (layer B.SilkS))
    (fp_text value Grove_4x2mm (at 3 -7.25 180) (layer B.Fab))
    (fp_text user %R (at 3 -2.5 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 6 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (pad 3 thru_hole oval (at 4 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 5 /belamini_cape_B2_2/D0))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 4 /belamini_cape_B2_2/A0))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer Bottom) (tedit 58D3FE32)
    (at 135.636 81.534)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J5 (at 3.1877 -4.1275) (layer B.SilkS))
    (fp_text value Grove_4x2mm (at 3 -7.25) (layer B.Fab))
    (fp_text user %R (at 3 -2.5) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 /belamini_cape_B2_2/SCL))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 3 /belamini_cape_B2_2/SDA))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST:JST_PH_S4B-PH-K_04x2.00mm_Angled (layer Bottom) (tedit 58D3FE32)
    (at 163.068 81.534)
    (descr "JST PH series connector, S4B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference J7 (at 3.0734 -4.064) (layer B.SilkS))
    (fp_text value Grove_4x2mm (at 3 -7.25) (layer B.Fab))
    (fp_text user %R (at 3 -2.5) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 /belamini_cape_B2_2/A3))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 /belamini_cape_B2_2/D3))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.7) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 +3V3))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S4B-PH-K_04x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module belamini_cape_B2:Untitled (layer Top) (tedit 0)
    (at 151.384 99.568)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text SCL (at 135.5725 78.74 270) (layer F.SilkS))
  (gr_text GND (at 139.573 78.6765 270) (layer F.SilkS))
  (gr_text SDA (at 137.541 78.6765 270) (layer F.SilkS))
  (gr_text 3.3V (at 141.5415 78.486 270) (layer F.SilkS))
  (gr_text 3.3V (at 155.2575 78.486 270) (layer F.SilkS))
  (gr_text GND (at 153.289 78.6765 270) (layer F.SilkS))
  (gr_text "D4\n" (at 151.257 79.1845 270) (layer F.SilkS))
  (gr_text A4 (at 149.2885 79.248 270) (layer F.SilkS))
  (gr_text 3.3V (at 168.91 78.486 270) (layer F.SilkS))
  (gr_text GND (at 166.9415 78.6765 270) (layer F.SilkS))
  (gr_text "D3\n" (at 164.9095 79.1845 270) (layer F.SilkS))
  (gr_text A3 (at 162.941 79.248 270) (layer F.SilkS))
  (gr_text A2 (at 169.037 118.872 90) (layer F.SilkS))
  (gr_text 3.3V (at 163.068 119.634 90) (layer F.SilkS))
  (gr_text D2 (at 167.0685 118.9355 90) (layer F.SilkS))
  (gr_text GND (at 165.0365 119.4435 90) (layer F.SilkS))
  (gr_text A1 (at 155.321 118.872 90) (layer F.SilkS))
  (gr_text 3.3V (at 149.352 119.634 90) (layer F.SilkS))
  (gr_text D1 (at 153.3525 118.9355 90) (layer F.SilkS))
  (gr_text GND (at 151.3205 119.4435 90) (layer F.SilkS))
  (gr_text S0 (at 138.7475 122.7) (layer F.SilkS))
  (gr_text A0 (at 141.605 118.872 90) (layer F.SilkS))
  (gr_text D0 (at 139.6365 118.9355 90) (layer F.SilkS))
  (gr_text GND (at 137.6045 119.4435 90) (layer F.SilkS))
  (gr_text 3.3V (at 135.636 119.634 90) (layer F.SilkS))
  (gr_text "08/18\n" (at 165.1508 107.5) (layer F.SilkS))
  (gr_text bela.io (at 135.5725 107.5) (layer F.SilkS))
  (gr_text S4 (at 152.146 75.438 180) (layer F.SilkS))
  (gr_text S3 (at 166.116 75.438 180) (layer F.SilkS))
  (gr_text S2 (at 165.989 122.7) (layer F.SilkS))
  (gr_text S1 (at 152.4 122.7) (layer F.SilkS))
  (gr_text I2C (at 138.684 75.438 180) (layer F.SilkS))
  (gr_arc (start 169.796424 84.193999) (end 179.8066 84.3026) (angle -90.62158096) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.796424 84.193999) (end 134.796424 74.193999) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.796424 74.193999) (end 134.796424 74.193999) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.958 90.1446) (end 171.958 108.1659) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.593001 108.127801) (end 172.6184 108.7628) (angle 92.29061004) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.593 90.169999) (end 172.618399 89.535) (angle -92.29061004) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.8066 84.167032) (end 179.8066 89.5223) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.7812 89.535) (end 172.6184 89.535) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.8066 108.7628) (end 172.6438 108.7628) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.8066 114.0968) (end 179.8066 108.7755) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.8111 124.1038) (end 134.8111 124.1038) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 134.8111 114.1038) (end 134.8111 124.1038) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.8156 114.0968) (end 124.7902 84.0232) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 169.8111 114.1038) (end 179.8066 114.0968) (angle 90.0401251) (layer Edge.Cuts) (width 0.15))
)
