<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0.4064" layer="20" curve="90"/>
<wire x1="0.635" y1="0" x2="26.035" y2="0" width="0.4064" layer="20"/>
<wire x1="26.035" y1="0" x2="26.67" y2="0.635" width="0.4064" layer="20" curve="90"/>
<wire x1="26.67" y1="0.635" x2="26.67" y2="33.655" width="0.4064" layer="20"/>
<wire x1="26.67" y1="33.655" x2="26.035" y2="34.29" width="0.4064" layer="20" curve="90"/>
<wire x1="26.035" y1="34.29" x2="0.635" y2="34.29" width="0.4064" layer="20"/>
<wire x1="0.635" y1="34.29" x2="0" y2="33.655" width="0.4064" layer="20" curve="90"/>
<wire x1="0" y1="33.655" x2="0" y2="0.635" width="0.4064" layer="20"/>
<text>433MHz</text>
<text>868MHz</text>
<text>Tinkerman 2016
RN2483
MOTEINO SHIELD
v0.2.20161127</text>
<hole x="7.62" y="26.035" drill="0.6"/>
<hole x="7.62" y="27.305" drill="0.6"/>
<hole x="7.62" y="29.845" drill="0.6"/>
<hole x="7.62" y="31.115" drill="0.6"/>
<hole x="8.89" y="29.845" drill="0.6"/>
<hole x="17.78" y="29.845" drill="0.6"/>
<hole x="17.78" y="31.115" drill="0.6"/>
<hole x="17.78" y="32.385" drill="0.6"/>
<hole x="19.05" y="32.385" drill="0.6"/>
<hole x="19.05" y="31.115" drill="0.6"/>
<hole x="19.05" y="29.845" drill="0.6"/>
<hole x="19.05" y="28.575" drill="0.6"/>
<hole x="19.05" y="27.305" drill="0.6"/>
<hole x="19.05" y="26.035" drill="0.6"/>
<hole x="19.05" y="24.765" drill="0.6"/>
<hole x="17.78" y="24.765" drill="0.6"/>
<hole x="19.05" y="23.495" drill="0.6"/>
<hole x="17.78" y="23.495" drill="0.6"/>
<hole x="8.89" y="24.765" drill="0.6"/>
<hole x="8.89" y="23.495" drill="0.6"/>
<hole x="8.89" y="31.115" drill="0.6"/>
<hole x="7.62" y="23.495" drill="0.6"/>
<hole x="7.62" y="24.765" drill="0.6"/>
<hole x="8.89" y="22.225" drill="0.6"/>
<hole x="10.16" y="22.225" drill="0.6"/>
<hole x="11.43" y="22.225" drill="0.6"/>
<hole x="12.7" y="22.225" drill="0.6"/>
<hole x="13.97" y="22.225" drill="0.6"/>
<hole x="15.24" y="22.225" drill="0.6"/>
<hole x="16.51" y="22.225" drill="0.6"/>
<hole x="17.78" y="22.225" drill="0.6"/>
<hole x="19.05" y="22.225" drill="0.6"/>
<hole x="8.89" y="33.655" drill="0.6"/>
<hole x="17.78" y="33.655" drill="0.6"/>
<hole x="7.62" y="33.655" drill="0.6"/>
<hole x="19.05" y="33.655" drill="0.6"/>
</plain>
<libraries>
<library name="xose">
<packages>
<package name="0805">
</package>
<package name="SJ_3">
</package>
<package name="1X13_SMD">
</package>
</packages>
</library>
<library name="tobias">
<packages>
<package name="RN2483">
<description>Full package

Adapted from: https://github.com/Octanis1/Octanis1-Electronics/blob/ae493cac28c100e20856abe563dfe8824e9cc4bd/lib/Octanis1.lbr</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="U.FL">
</package>
<package name="SMA_EDGELAUNCH">
</package>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="xose" package="0805" value=""/>
<element name="RN2483" library="tobias" package="RN2483" value=""/>
<element name="SJ1" library="xose" package="SJ_3" value=""/>
<element name="X2" library="adafruit" package="U.FL" value=""/>
<element name="X4" library="adafruit" package="SMA_EDGELAUNCH" value=""/>
<element name="U$1" library="xose" package="1X13_SMD" value=""/>
<element name="U$2" library="xose" package="1X13_SMD" value=""/>
<element name="CN1" library="adafruit" package="JST-PH-2-SMT-RA" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="X2" pad="1"/>
<contactref element="X2" pad="2"/>
<contactref element="RN2483" pad="GND"/>
<contactref element="RN2483" pad="GND1"/>
<contactref element="RN2483" pad="GND2"/>
<contactref element="RN2483" pad="GND3"/>
<contactref element="RN2483" pad="GND4"/>
<contactref element="RN2483" pad="GND5"/>
<contactref element="RN2483" pad="GND6"/>
<contactref element="RN2483" pad="GND7"/>
<contactref element="RN2483" pad="GND8"/>
<contactref element="RN2483" pad="GND9"/>
<contactref element="RN2483" pad="GND10"/>
<contactref element="RN2483" pad="GND11"/>
<contactref element="RN2483" pad="GND12"/>
<contactref element="X4" pad="GND@4"/>
<contactref element="X4" pad="GND@2"/>
<contactref element="X4" pad="GND@3"/>
<contactref element="X4" pad="GND@1"/>
<contactref element="C1" pad="2"/>
<contactref element="U$2" pad="P$13"/>
<contactref element="CN1" pad="2"/>
</signal>
<signal name="RFL">
<contactref element="RN2483" pad="RFL"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="RFH">
<contactref element="RN2483" pad="RFH"/>
<contactref element="SJ1" pad="3"/>
</signal>
<signal name="3V3">
<contactref element="RN2483" pad="VDD"/>
<contactref element="RN2483" pad="VDD2"/>
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="P$11"/>
</signal>
<signal name="RST">
<contactref element="U$1" pad="P$13"/>
</signal>
<signal name="N$2">
<contactref element="X2" pad="3"/>
<contactref element="X4" pad="P"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="D2">
<contactref element="U$1" pad="P$12"/>
</signal>
<signal name="D3">
<contactref element="U$1" pad="P$11"/>
<contactref element="RN2483" pad="UART_TX"/>
</signal>
<signal name="D4">
<contactref element="U$1" pad="P$10"/>
<contactref element="RN2483" pad="UART_RX"/>
</signal>
<signal name="D5">
<contactref element="U$1" pad="P$9"/>
<contactref element="RN2483" pad="RESET°"/>
</signal>
<signal name="D6">
<contactref element="U$1" pad="P$8"/>
</signal>
<signal name="D7">
<contactref element="U$1" pad="P$7"/>
</signal>
<signal name="D8">
<contactref element="U$1" pad="P$6"/>
</signal>
<signal name="D9">
<contactref element="U$1" pad="P$5"/>
</signal>
<signal name="D10">
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="D11">
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="D12">
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="D13">
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="VIN">
<contactref element="U$2" pad="P$12"/>
<contactref element="CN1" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U$2" pad="P$10"/>
</signal>
<signal name="RX">
<contactref element="U$2" pad="P$9"/>
</signal>
<signal name="A7">
<contactref element="U$2" pad="P$8"/>
</signal>
<signal name="A6">
<contactref element="U$2" pad="P$7"/>
</signal>
<signal name="A5">
<contactref element="U$2" pad="P$6"/>
</signal>
<signal name="A4">
<contactref element="U$2" pad="P$5"/>
</signal>
<signal name="A3">
<contactref element="U$2" pad="P$4"/>
</signal>
<signal name="A2">
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="A1">
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="A0">
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
