(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad3)")
  (net 3 "Net-(J1-Pad12)")
  (net 4 "Net-(J1-Pad11)")
  (net 5 "Net-(J1-Pad10)")
  (net 6 "Net-(J1-Pad8)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J1-Pad15)")
  (footprint "Package_DIP:DIP-16_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 82.55 83.82 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "SSC Jumper Block.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 3.81 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x08_Counter_Clockwise" (at 3.81 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 8.89 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad3)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad12)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad11)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad10)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad8)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad15)") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl" hide
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 101.6 85.09) (end 81.28 85.09) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 81.28 74.93) (end 101.6 74.93) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 81.28 85.09) (end 81.28 74.93) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 101.6 74.93) (end 101.6 85.09) (layer "Edge.Cuts") (width 0.1))
  (gr_text "Apple SSC\nModem/Terminal\nJumper Block" (at 91.44 80.01) (layer "B.SilkS"))
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84.9376 82.23)
        (xy 84.928746 82.416057)
        (xy 84.903599 82.569476)
        (xy 84.864275 82.697335)
        (xy 84.812893 82.806713)
        (xy 84.751572 82.904689)
        (xy 84.682428 82.998341)
        (xy 84.607581 83.094749)
        (xy 84.529149 83.20099)
        (xy 84.449249 83.324144)
        (xy 84.37 83.471289)
        (xy 85.09 84.22)
        (xy 85.81 83.471289)
        (xy 85.73075 83.324144)
        (xy 85.65085 83.20099)
        (xy 85.572418 83.094749)
        (xy 85.497571 82.998341)
        (xy 85.428427 82.904689)
        (xy 85.367106 82.806713)
        (xy 85.315724 82.697335)
        (xy 85.2764 82.569476)
        (xy 85.251253 82.416057)
        (xy 85.2424 82.23)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pad10)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.9424 77.79)
        (xy 97.951253 77.603942)
        (xy 97.9764 77.450523)
        (xy 98.015724 77.322664)
        (xy 98.067106 77.213286)
        (xy 98.128427 77.11531)
        (xy 98.197571 77.021658)
        (xy 98.272418 76.92525)
        (xy 98.35085 76.819009)
        (xy 98.43075 76.695855)
        (xy 98.51 76.548711)
        (xy 97.79 75.8)
        (xy 97.07 76.548711)
        (xy 97.149249 76.695855)
        (xy 97.229149 76.819009)
        (xy 97.307581 76.92525)
        (xy 97.382428 77.021658)
        (xy 97.451572 77.11531)
        (xy 97.512893 77.213286)
        (xy 97.564275 77.322664)
        (xy 97.603599 77.450523)
        (xy 97.628746 77.603942)
        (xy 97.6376 77.79)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pad13)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.3224 77.79)
        (xy 90.331253 77.603942)
        (xy 90.3564 77.450523)
        (xy 90.395724 77.322664)
        (xy 90.447106 77.213286)
        (xy 90.508427 77.11531)
        (xy 90.577571 77.021658)
        (xy 90.652418 76.92525)
        (xy 90.73085 76.819009)
        (xy 90.81075 76.695855)
        (xy 90.89 76.548711)
        (xy 90.17 75.8)
        (xy 89.45 76.548711)
        (xy 89.529249 76.695855)
        (xy 89.609149 76.819009)
        (xy 89.687581 76.92525)
        (xy 89.762428 77.021658)
        (xy 89.831572 77.11531)
        (xy 89.892893 77.213286)
        (xy 89.944275 77.322664)
        (xy 89.983599 77.450523)
        (xy 90.008746 77.603942)
        (xy 90.0176 77.79)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pad11)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.0976 82.23)
        (xy 95.088746 82.416057)
        (xy 95.063599 82.569476)
        (xy 95.024275 82.697335)
        (xy 94.972893 82.806713)
        (xy 94.911572 82.904689)
        (xy 94.842428 82.998341)
        (xy 94.767581 83.094749)
        (xy 94.689149 83.20099)
        (xy 94.609249 83.324144)
        (xy 94.53 83.471289)
        (xy 95.25 84.22)
        (xy 95.97 83.471289)
        (xy 95.89075 83.324144)
        (xy 95.81085 83.20099)
        (xy 95.732418 83.094749)
        (xy 95.657571 82.998341)
        (xy 95.588427 82.904689)
        (xy 95.527106 82.806713)
        (xy 95.475724 82.697335)
        (xy 95.4364 82.569476)
        (xy 95.411253 82.416057)
        (xy 95.4024 82.23)
      )
    )
  )
  (zone (net 7) (net_name "Net-(J1-Pad13)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.7824 77.79)
        (xy 87.791253 77.603942)
        (xy 87.8164 77.450523)
        (xy 87.855724 77.322664)
        (xy 87.907106 77.213286)
        (xy 87.968427 77.11531)
        (xy 88.037571 77.021658)
        (xy 88.112418 76.92525)
        (xy 88.19085 76.819009)
        (xy 88.27075 76.695855)
        (xy 88.35 76.548711)
        (xy 87.63 75.8)
        (xy 86.91 76.548711)
        (xy 86.989249 76.695855)
        (xy 87.069149 76.819009)
        (xy 87.147581 76.92525)
        (xy 87.222428 77.021658)
        (xy 87.291572 77.11531)
        (xy 87.352893 77.213286)
        (xy 87.404275 77.322664)
        (xy 87.443599 77.450523)
        (xy 87.468746 77.603942)
        (xy 87.4776 77.79)
      )
    )
  )
  (zone (net 5) (net_name "Net-(J1-Pad10)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 97.6376 82.23)
        (xy 97.628746 82.416057)
        (xy 97.603599 82.569476)
        (xy 97.564275 82.697335)
        (xy 97.512893 82.806713)
        (xy 97.451572 82.904689)
        (xy 97.382428 82.998341)
        (xy 97.307581 83.094749)
        (xy 97.229149 83.20099)
        (xy 97.149249 83.324144)
        (xy 97.07 83.471289)
        (xy 97.79 84.22)
        (xy 98.51 83.471289)
        (xy 98.43075 83.324144)
        (xy 98.35085 83.20099)
        (xy 98.272418 83.094749)
        (xy 98.197571 82.998341)
        (xy 98.128427 82.904689)
        (xy 98.067106 82.806713)
        (xy 98.015724 82.697335)
        (xy 97.9764 82.569476)
        (xy 97.951253 82.416057)
        (xy 97.9424 82.23)
      )
    )
  )
  (zone (net 8) (net_name "Net-(J1-Pad15)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 85.2424 77.79)
        (xy 85.251253 77.603942)
        (xy 85.2764 77.450523)
        (xy 85.315724 77.322664)
        (xy 85.367106 77.213286)
        (xy 85.428427 77.11531)
        (xy 85.497571 77.021658)
        (xy 85.572418 76.92525)
        (xy 85.65085 76.819009)
        (xy 85.73075 76.695855)
        (xy 85.81 76.548711)
        (xy 85.09 75.8)
        (xy 84.37 76.548711)
        (xy 84.449249 76.695855)
        (xy 84.529149 76.819009)
        (xy 84.607581 76.92525)
        (xy 84.682428 77.021658)
        (xy 84.751572 77.11531)
        (xy 84.812893 77.213286)
        (xy 84.864275 77.322664)
        (xy 84.903599 77.450523)
        (xy 84.928746 77.603942)
        (xy 84.9376 77.79)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pad8)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.4824 77.79)
        (xy 100.491253 77.603942)
        (xy 100.5164 77.450523)
        (xy 100.555724 77.322664)
        (xy 100.607106 77.213286)
        (xy 100.668427 77.11531)
        (xy 100.737571 77.021658)
        (xy 100.812418 76.92525)
        (xy 100.89085 76.819009)
        (xy 100.97075 76.695855)
        (xy 101.05 76.548711)
        (xy 100.33 75.8)
        (xy 99.61 76.548711)
        (xy 99.689249 76.695855)
        (xy 99.769149 76.819009)
        (xy 99.847581 76.92525)
        (xy 99.922428 77.021658)
        (xy 99.991572 77.11531)
        (xy 100.052893 77.213286)
        (xy 100.104275 77.322664)
        (xy 100.143599 77.450523)
        (xy 100.168746 77.603942)
        (xy 100.1776 77.79)
      )
    )
  )
  (zone (net 8) (net_name "Net-(J1-Pad15)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.7024 77.79)
        (xy 82.711253 77.603942)
        (xy 82.7364 77.450523)
        (xy 82.775724 77.322664)
        (xy 82.827106 77.213286)
        (xy 82.888427 77.11531)
        (xy 82.957571 77.021658)
        (xy 83.032418 76.92525)
        (xy 83.11085 76.819009)
        (xy 83.19075 76.695855)
        (xy 83.27 76.548711)
        (xy 82.55 75.8)
        (xy 81.83 76.548711)
        (xy 81.909249 76.695855)
        (xy 81.989149 76.819009)
        (xy 82.067581 76.92525)
        (xy 82.142428 77.021658)
        (xy 82.211572 77.11531)
        (xy 82.272893 77.213286)
        (xy 82.324275 77.322664)
        (xy 82.363599 77.450523)
        (xy 82.388746 77.603942)
        (xy 82.3976 77.79)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pad12)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.5576 82.23)
        (xy 92.548746 82.416057)
        (xy 92.523599 82.569476)
        (xy 92.484275 82.697335)
        (xy 92.432893 82.806713)
        (xy 92.371572 82.904689)
        (xy 92.302428 82.998341)
        (xy 92.227581 83.094749)
        (xy 92.149149 83.20099)
        (xy 92.069249 83.324144)
        (xy 91.99 83.471289)
        (xy 92.71 84.22)
        (xy 93.43 83.471289)
        (xy 93.35075 83.324144)
        (xy 93.27085 83.20099)
        (xy 93.192418 83.094749)
        (xy 93.117571 82.998341)
        (xy 93.048427 82.904689)
        (xy 92.987106 82.806713)
        (xy 92.935724 82.697335)
        (xy 92.8964 82.569476)
        (xy 92.871253 82.416057)
        (xy 92.8624 82.23)
      )
    )
  )
  (zone (net 6) (net_name "Net-(J1-Pad8)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.1776 82.23)
        (xy 100.168746 82.416057)
        (xy 100.143599 82.569476)
        (xy 100.104275 82.697335)
        (xy 100.052893 82.806713)
        (xy 99.991572 82.904689)
        (xy 99.922428 82.998341)
        (xy 99.847581 83.094749)
        (xy 99.769149 83.20099)
        (xy 99.689249 83.324144)
        (xy 99.61 83.471289)
        (xy 100.33 84.22)
        (xy 101.05 83.471289)
        (xy 100.97075 83.324144)
        (xy 100.89085 83.20099)
        (xy 100.812418 83.094749)
        (xy 100.737571 82.998341)
        (xy 100.668427 82.904689)
        (xy 100.607106 82.806713)
        (xy 100.555724 82.697335)
        (xy 100.5164 82.569476)
        (xy 100.491253 82.416057)
        (xy 100.4824 82.23)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad3)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.4776 82.23)
        (xy 87.468746 82.416057)
        (xy 87.443599 82.569476)
        (xy 87.404275 82.697335)
        (xy 87.352893 82.806713)
        (xy 87.291572 82.904689)
        (xy 87.222428 82.998341)
        (xy 87.147581 83.094749)
        (xy 87.069149 83.20099)
        (xy 86.989249 83.324144)
        (xy 86.91 83.471289)
        (xy 87.63 84.22)
        (xy 88.35 83.471289)
        (xy 88.27075 83.324144)
        (xy 88.19085 83.20099)
        (xy 88.112418 83.094749)
        (xy 88.037571 82.998341)
        (xy 87.968427 82.904689)
        (xy 87.907106 82.806713)
        (xy 87.855724 82.697335)
        (xy 87.8164 82.569476)
        (xy 87.791253 82.416057)
        (xy 87.7824 82.23)
      )
    )
  )
  (zone (net 4) (net_name "Net-(J1-Pad11)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 95.4024 77.79)
        (xy 95.411253 77.603942)
        (xy 95.4364 77.450523)
        (xy 95.475724 77.322664)
        (xy 95.527106 77.213286)
        (xy 95.588427 77.11531)
        (xy 95.657571 77.021658)
        (xy 95.732418 76.92525)
        (xy 95.81085 76.819009)
        (xy 95.89075 76.695855)
        (xy 95.97 76.548711)
        (xy 95.25 75.8)
        (xy 94.53 76.548711)
        (xy 94.609249 76.695855)
        (xy 94.689149 76.819009)
        (xy 94.767581 76.92525)
        (xy 94.842428 77.021658)
        (xy 94.911572 77.11531)
        (xy 94.972893 77.213286)
        (xy 95.024275 77.322664)
        (xy 95.063599 77.450523)
        (xy 95.088746 77.603942)
        (xy 95.0976 77.79)
      )
    )
  )
  (zone (net 2) (net_name "Net-(J1-Pad3)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 90.0176 82.23)
        (xy 90.008746 82.416057)
        (xy 89.983599 82.569476)
        (xy 89.944275 82.697335)
        (xy 89.892893 82.806713)
        (xy 89.831572 82.904689)
        (xy 89.762428 82.998341)
        (xy 89.687581 83.094749)
        (xy 89.609149 83.20099)
        (xy 89.529249 83.324144)
        (xy 89.45 83.471289)
        (xy 90.17 84.22)
        (xy 90.89 83.471289)
        (xy 90.81075 83.324144)
        (xy 90.73085 83.20099)
        (xy 90.652418 83.094749)
        (xy 90.577571 82.998341)
        (xy 90.508427 82.904689)
        (xy 90.447106 82.806713)
        (xy 90.395724 82.697335)
        (xy 90.3564 82.569476)
        (xy 90.331253 82.416057)
        (xy 90.3224 82.23)
      )
    )
  )
  (zone (net 3) (net_name "Net-(J1-Pad12)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.8624 77.79)
        (xy 92.871253 77.603942)
        (xy 92.8964 77.450523)
        (xy 92.935724 77.322664)
        (xy 92.987106 77.213286)
        (xy 93.048427 77.11531)
        (xy 93.117571 77.021658)
        (xy 93.192418 76.92525)
        (xy 93.27085 76.819009)
        (xy 93.35075 76.695855)
        (xy 93.43 76.548711)
        (xy 92.71 75.8)
        (xy 91.99 76.548711)
        (xy 92.069249 76.695855)
        (xy 92.149149 76.819009)
        (xy 92.227581 76.92525)
        (xy 92.302428 77.021658)
        (xy 92.371572 77.11531)
        (xy 92.432893 77.213286)
        (xy 92.484275 77.322664)
        (xy 92.523599 77.450523)
        (xy 92.548746 77.603942)
        (xy 92.5576 77.79)
      )
    )
  )
  (zone (net 1) (net_name "Net-(J1-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (priority 16962)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.3976 82.23)
        (xy 82.388746 82.416057)
        (xy 82.363599 82.569476)
        (xy 82.324275 82.697335)
        (xy 82.272893 82.806713)
        (xy 82.211572 82.904689)
        (xy 82.142428 82.998341)
        (xy 82.067581 83.094749)
        (xy 81.989149 83.20099)
        (xy 81.909249 83.324144)
        (xy 81.83 83.471289)
        (xy 82.55 84.22)
        (xy 83.27 83.471289)
        (xy 83.19075 83.324144)
        (xy 83.11085 83.20099)
        (xy 83.032418 83.094749)
        (xy 82.957571 82.998341)
        (xy 82.888427 82.904689)
        (xy 82.827106 82.806713)
        (xy 82.775724 82.697335)
        (xy 82.7364 82.569476)
        (xy 82.711253 82.416057)
        (xy 82.7024 82.23)
      )
    )
  )
)
