(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 0.63)
    (drawings 6)
    (tracks 24)
    (zones 0)
    (modules 18)
    (nets 5)
  )
  (page A4)
  (title_block
    (title "dc506 anniversary badge")
    (date 2018-09-28)
    (rev beta)
    (company @defcon506)
    (comment 1 "design by cedric (@thecedricz)")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.006)
    (trace_clearance 0.006)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.027)
    (via_drill 0.013)
    (via_min_size 0.02)
    (via_min_drill 0.01)
    (uvia_size 0.2)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.6 2.6)
    (pad_drill 1.99898)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(BAT1-Pad1)")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.006)
    (trace_width 0.006)
    (via_dia 0.027)
    (via_drill 0.013)
    (uvia_dia 0.2)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(BAT1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 142.24 99.06)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 154.94 106.68)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module digikey-footprints:Battery_Holder_Coin_2032_BS-7 (layer B.Cu) (tedit 5BAEBE4E)
    (at 147.32 133.35 90)
    (descr http://www.memoryprotectiondevices.com/datasheets/BS-7-datasheet.pdf)
    (fp_text reference BAT1 (at 7.52856 12.3063 90) (layer B.SilkS))
    (fp_text value BS-7 (at 7.4676 -13.56 90) (layer B.Fab))
    (fp_text user %R (at 7.4676 0 90) (layer B.Fab))
    (pad 2 thru_hole rect (at 0 0 90) (size 2.17 2.17) (drill 1.17) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 20 0 90) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(BAT1-Pad1)"))
  )
  (module LED_THT:LED_D8.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 152.4 77.47)
    (descr "LED, diameter 8.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED8MMGE_LED8MMGN_LED8MMRT%23KIN.pdf")
    (tags "LED diameter 8.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -5.56) (layer F.SilkS))
    (fp_text value LED (at 1.27 5.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D8.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D8.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 142.24 77.47 180)
    (descr "LED, diameter 8.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LED8MMGE_LED8MMGN_LED8MMRT%23KIN.pdf")
    (tags "LED diameter 8.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -5.56 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 5.56 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D8.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 120.65 82.55 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 0.95 -1.92 270) (layer F.SilkS))
    (fp_text value 1KΩ (at 0.95 1.92 270) (layer F.Fab))
    (fp_text user %R (at 0.95 -1.92 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(BAT1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 173.99 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 0.95 -1.92 270) (layer F.SilkS))
    (fp_text value 1KΩ (at 0.95 1.92 270) (layer F.Fab))
    (fp_text user %R (at 0.95 -1.92 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(BAT1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module dc506:dclogo (layer F.Cu) (tedit 0)
    (at 148.59 97.79)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 163.83 95.25)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 290.83 60.96)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 142.24 100.33)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 293.37 59.69)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 219.71 60.96)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 154.94 96.52)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 205.74 52.07)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 148.59 102.87)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module dc506:dc506_logo (layer F.Cu) (tedit 0)
    (at 147.32 96.52)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill2mm (layer F.Cu) (tedit 5BAEE83B)
    (at 167.64 73.025)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_1x01_Drill2mm (at 0 3.81) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 1.99898) (layers *.Cu *.Mask))
  )
  (gr_text ® (at 177.165 109.855) (layer F.SilkS))
  (gr_text @thecedricz (at 147.32 139.065) (layer B.SilkS))
  (gr_text "hack the planet!" (at 147.32 99.695) (layer B.SilkS))
  (gr_text "0x1 year!" (at 147.32 127.635) (layer F.SilkS))
  (gr_text @defcon506 (at 146.685 123.19) (layer F.SilkS))
  (gr_circle (center 147.240703 101.6) (end 149.780703 60.96) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.425 53.975) (xy 189.23 53.975) (xy 189.865 146.685) (xy 98.425 146.685)
      )
    )
  )
  (zone (net 2) (net_name "Net-(BAT1-Pad1)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.425 53.975) (xy 189.23 53.975) (xy 189.865 146.685) (xy 98.425 146.685)
      )
    )
  )
)
