(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "Net-(IC1A-14M)")
  (net 4 "/DRD13")
  (net 5 "/DRD12")
  (net 6 "/DRD11")
  (net 7 "/DRD10")
  (net 8 "/DRD9")
  (net 9 "/DRD8")
  (net 10 "/DRD7")
  (net 11 "/DRD6")
  (net 12 "/DRD5")
  (net 13 "/DRD4")
  (net 14 "/DRD3")
  (net 15 "/DRD2")
  (net 16 "/DRD1")
  (net 17 "/DRD0")
  (net 18 "Net-(IC1A-~{RESET})")
  (net 19 "Net-(IC1A-~{INTRQ})")
  (net 20 "Net-(IC1A-DMAL)")
  (net 21 "Net-(IC1A-~{BLISS})")
  (net 22 "Net-(IC1A-~{BLIT})")
  (net 23 "Net-(IC1A-~{WE})")
  (net 24 "Net-(IC1A-R~{W})")
  (net 25 "Net-(IC1A-~{REGEN})")
  (net 26 "Net-(IC1A-~{AS})")
  (net 27 "Net-(IC1A-~{RAMEN})")
  (net 28 "/RGA8")
  (net 29 "/RGA7")
  (net 30 "/RGA6")
  (net 31 "/RGA5")
  (net 32 "/RGA4")
  (net 33 "/RGA3")
  (net 34 "/RGA2")
  (net 35 "/RGA1")
  (net 36 "Net-(IC1A-28M)")
  (net 37 "/A20")
  (net 38 "Net-(IC1A-~{CDAC})")
  (net 39 "Net-(IC1A-7M)")
  (net 40 "Net-(IC1A-CCKQ)")
  (net 41 "Net-(IC1A-CCK)")
  (net 42 "/DRA0")
  (net 43 "/DRA1")
  (net 44 "/DRA2")
  (net 45 "/DRA3")
  (net 46 "/DRA4")
  (net 47 "/DRA5")
  (net 48 "/DRA6")
  (net 49 "/DRA7")
  (net 50 "/DRA8")
  (net 51 "Net-(IC1A-~{LDS})")
  (net 52 "Net-(IC1A-~{UDS})")
  (net 53 "Net-(IC1A-~{CASL})")
  (net 54 "Net-(IC1A-~{CASU})")
  (net 55 "/DRA9")
  (net 56 "Net-(IC1A-~{RAS1})")
  (net 57 "Net-(IC1A-~{RAS0})")
  (net 58 "/A19")
  (net 59 "/A1")
  (net 60 "/A2")
  (net 61 "/A3")
  (net 62 "/A4")
  (net 63 "/A5")
  (net 64 "/A6")
  (net 65 "/A7")
  (net 66 "/A8")
  (net 67 "/A9")
  (net 68 "/A10")
  (net 69 "/A11")
  (net 70 "/A12")
  (net 71 "/A13")
  (net 72 "/A14")
  (net 73 "/A15")
  (net 74 "/A16")
  (net 75 "/A17")
  (net 76 "/A18")
  (net 77 "Net-(IC1A-~{LPEN})")
  (net 78 "Net-(IC1A-~{VSYNC})")
  (net 79 "Net-(IC1A-~{CSYNC})")
  (net 80 "Net-(IC1A-~{HSYNC})")
  (net 81 "/DRD15")
  (net 82 "/DRD14")
  (net 83 "unconnected-(IC2-PAL{slash}NTSC-Pad41)")
  (net 84 "Net-(IC2-~{RAS})")
  (footprint "Package_LCC:PLCC-84_SMD-Socket" (layer "F.Cu")
    (at 149.0425 103.38)
    (descr "PLCC, 84 pins, surface mount")
    (tags "plcc smt")
    (property "Sheetfile" "AgnusAdaptorv2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC1" (at 0 -19) (layer "F.SilkS") hide)
    (fp_text value "~" (at 0 19) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at 0 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/DRD13") (pinfunction "DRD13") (pintype "bidirectional"))
    (pad "2" smd rect (at -1.27 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/DRD12") (pinfunction "DRD12") (pintype "bidirectional"))
    (pad "3" smd rect (at -2.54 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/DRD11") (pinfunction "DRD11") (pintype "bidirectional"))
    (pad "4" smd rect (at -3.81 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "/DRD10") (pinfunction "DRD10") (pintype "bidirectional"))
    (pad "5" smd rect (at -5.08 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/DRD9") (pinfunction "DRD9") (pintype "bidirectional"))
    (pad "6" smd rect (at -6.35 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/DRD8") (pinfunction "DRD8") (pintype "bidirectional"))
    (pad "7" smd rect (at -7.62 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/DRD7") (pinfunction "DRD7") (pintype "bidirectional"))
    (pad "8" smd rect (at -8.89 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/DRD6") (pinfunction "DRD6") (pintype "bidirectional"))
    (pad "9" smd rect (at -10.16 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/DRD5") (pinfunction "DRD5") (pintype "bidirectional"))
    (pad "10" smd rect (at -11.43 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/DRD4") (pinfunction "DRD4") (pintype "bidirectional"))
    (pad "11" smd rect (at -12.7 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/DRD3") (pinfunction "DRD3") (pintype "bidirectional"))
    (pad "12" smd rect (at -14.2125 -12.7) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/DRD2") (pinfunction "DRD2") (pintype "bidirectional"))
    (pad "13" smd rect (at -14.2125 -11.43) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/DRD1") (pinfunction "DRD1") (pintype "bidirectional"))
    (pad "14" smd rect (at -14.2125 -10.16) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/DRD0") (pinfunction "DRD0") (pintype "bidirectional"))
    (pad "15" smd rect (at -14.2125 -8.89) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "16" smd rect (at -14.2125 -7.62) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(IC1A-~{RESET})") (pinfunction "~{RESET}") (pintype "input"))
    (pad "17" smd rect (at -14.2125 -6.35) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(IC1A-~{INTRQ})") (pinfunction "~{INTRQ}") (pintype "output"))
    (pad "18" smd rect (at -14.2125 -5.08) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(IC1A-DMAL)") (pinfunction "DMAL") (pintype "input"))
    (pad "19" smd rect (at -14.2125 -3.81) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(IC1A-~{BLISS})") (pinfunction "~{BLISS}") (pintype "output"))
    (pad "20" smd rect (at -14.2125 -2.54) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(IC1A-~{BLIT})") (pinfunction "~{BLIT}") (pintype "output"))
    (pad "21" smd rect (at -14.2125 -1.27) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(IC1A-~{WE})") (pinfunction "~{WE}") (pintype "output"))
    (pad "22" smd rect (at -14.2125 0) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(IC1A-R~{W})") (pinfunction "R~{W}") (pintype "input"))
    (pad "23" smd rect (at -14.2125 1.27) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(IC1A-~{REGEN})") (pinfunction "~{REGEN}") (pintype "output"))
    (pad "24" smd rect (at -14.2125 2.54) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(IC1A-~{AS})") (pinfunction "~{AS}") (pintype "input"))
    (pad "25" smd rect (at -14.2125 3.81) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(IC1A-~{RAMEN})") (pinfunction "~{RAMEN}") (pintype "output"))
    (pad "26" smd rect (at -14.2125 5.08) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "/RGA8") (pinfunction "RGA8") (pintype "output"))
    (pad "27" smd rect (at -14.2125 6.35) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "/RGA7") (pinfunction "RGA7") (pintype "output"))
    (pad "28" smd rect (at -14.2125 7.62) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "/RGA6") (pinfunction "RGA6") (pintype "output"))
    (pad "29" smd rect (at -14.2125 8.89) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/RGA5") (pinfunction "RGA5") (pintype "output"))
    (pad "30" smd rect (at -14.2125 10.16) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/RGA4") (pinfunction "RGA4") (pintype "output"))
    (pad "31" smd rect (at -14.2125 11.43) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/RGA3") (pinfunction "RGA3") (pintype "output"))
    (pad "32" smd rect (at -14.2125 12.7) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/RGA2") (pinfunction "RGA2") (pintype "output"))
    (pad "33" smd rect (at -12.7 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/RGA1") (pinfunction "RGA1") (pintype "output"))
    (pad "34" smd rect (at -11.43 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "Net-(IC1A-28M)") (pinfunction "28M") (pintype "input"))
    (pad "35" smd rect (at -10.16 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/A20") (pinfunction "A20") (pintype "input"))
    (pad "36" smd rect (at -8.89 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(IC1A-~{CDAC})") (pinfunction "~{CDAC}") (pintype "output"))
    (pad "37" smd rect (at -7.62 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "Net-(IC1A-7M)") (pinfunction "7M") (pintype "output"))
    (pad "38" smd rect (at -6.35 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(IC1A-CCKQ)") (pinfunction "CCKQ") (pintype "output"))
    (pad "39" smd rect (at -5.08 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(IC1A-CCK)") (pinfunction "CCK") (pintype "output"))
    (pad "40" smd rect (at -3.81 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(IC1A-14M)") (pinfunction "14M") (pintype "output"))
    (pad "41" smd rect (at -2.54 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND@1") (pintype "power_in"))
    (pad "42" smd rect (at -1.27 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/DRA0") (pinfunction "DRA0") (pintype "output"))
    (pad "43" smd rect (at 0 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "/DRA1") (pinfunction "DRA1") (pintype "output"))
    (pad "44" smd rect (at 1.27 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/DRA2") (pinfunction "DRA2") (pintype "output"))
    (pad "45" smd rect (at 2.54 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/DRA3") (pinfunction "DRA3") (pintype "output"))
    (pad "46" smd rect (at 3.81 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/DRA4") (pinfunction "DRA4") (pintype "output"))
    (pad "47" smd rect (at 5.08 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/DRA5") (pinfunction "DRA5") (pintype "output"))
    (pad "48" smd rect (at 6.35 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/DRA6") (pinfunction "DRA6") (pintype "output"))
    (pad "49" smd rect (at 7.62 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/DRA7") (pinfunction "DRA7") (pintype "output"))
    (pad "50" smd rect (at 8.89 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/DRA8") (pinfunction "DRA8") (pintype "output"))
    (pad "51" smd rect (at 10.16 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(IC1A-~{LDS})") (pinfunction "~{LDS}") (pintype "input"))
    (pad "52" smd rect (at 11.43 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(IC1A-~{UDS})") (pinfunction "~{UDS}") (pintype "input"))
    (pad "53" smd rect (at 12.7 14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(IC1A-~{CASL})") (pinfunction "~{CASL}") (pintype "output"))
    (pad "54" smd rect (at 14.2125 12.7) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(IC1A-~{CASU})") (pinfunction "~{CASU}") (pintype "output"))
    (pad "55" smd rect (at 14.2125 11.43) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/DRA9") (pinfunction "DRA9") (pintype "output"))
    (pad "56" smd rect (at 14.2125 10.16) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(IC1A-~{RAS1})") (pinfunction "~{RAS1}") (pintype "output"))
    (pad "57" smd rect (at 14.2125 8.89) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(IC1A-~{RAS0})") (pinfunction "~{RAS0}") (pintype "output"))
    (pad "58" smd rect (at 14.2125 7.62) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND@2") (pintype "power_in"))
    (pad "59" smd rect (at 14.2125 6.35) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/A19") (pinfunction "A19") (pintype "input"))
    (pad "60" smd rect (at 14.2125 5.08) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "61" smd rect (at 14.2125 3.81) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "62" smd rect (at 14.2125 2.54) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/A3") (pinfunction "A3") (pintype "input"))
    (pad "63" smd rect (at 14.2125 1.27) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/A4") (pinfunction "A4") (pintype "input"))
    (pad "64" smd rect (at 14.2125 0) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/A5") (pinfunction "A5") (pintype "input"))
    (pad "65" smd rect (at 14.2125 -1.27) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/A6") (pinfunction "A6") (pintype "input"))
    (pad "66" smd rect (at 14.2125 -2.54) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/A7") (pinfunction "A7") (pintype "input"))
    (pad "67" smd rect (at 14.2125 -3.81) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/A8") (pinfunction "A8") (pintype "input"))
    (pad "68" smd rect (at 14.2125 -5.08) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/A9") (pinfunction "A9") (pintype "input"))
    (pad "69" smd rect (at 14.2125 -6.35) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/A10") (pinfunction "A10") (pintype "input"))
    (pad "70" smd rect (at 14.2125 -7.62) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/A11") (pinfunction "A11") (pintype "input"))
    (pad "71" smd rect (at 14.2125 -8.89) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/A12") (pinfunction "A12") (pintype "input"))
    (pad "72" smd rect (at 14.2125 -10.16) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/A13") (pinfunction "A13") (pintype "input"))
    (pad "73" smd rect (at 14.2125 -11.43) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/A14") (pinfunction "A14") (pintype "input"))
    (pad "74" smd rect (at 14.2125 -12.7) (size 1.925 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/A15") (pinfunction "A15") (pintype "input"))
    (pad "75" smd rect (at 12.7 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/A16") (pinfunction "A16") (pintype "input"))
    (pad "76" smd rect (at 11.43 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/A17") (pinfunction "A17") (pintype "input"))
    (pad "77" smd rect (at 10.16 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/A18") (pinfunction "A18") (pintype "input"))
    (pad "78" smd rect (at 8.89 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "Net-(IC1A-~{LPEN})") (pinfunction "~{LPEN}") (pintype "input"))
    (pad "79" smd rect (at 7.62 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "Net-(IC1A-~{VSYNC})") (pinfunction "~{VSYNC}") (pintype "output"))
    (pad "80" smd rect (at 6.35 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "Net-(IC1A-~{CSYNC})") (pinfunction "~{CSYNC}") (pintype "output"))
    (pad "81" smd rect (at 5.08 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(IC1A-~{HSYNC})") (pinfunction "~{HSYNC}") (pintype "output"))
    (pad "82" smd rect (at 3.81 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND@3") (pintype "power_in"))
    (pad "83" smd rect (at 2.54 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/DRD15") (pinfunction "DRD15") (pintype "bidirectional"))
    (pad "84" smd rect (at 1.27 -14.2125) (size 0.7 1.925) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/DRD14") (pinfunction "DRD14") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_LCC.3dshapes/PLCC-84_SMD-Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "AgnusAdaptorv2:CAPC2012X110" (layer "B.Cu")
    (at 146.9854 112.65)
    (descr "Chip, 2.00 X 1.25 X 1.10 mm body\n<p>Chip package with body size 2.00 X 1.25 X 1.10 mm</p>")
    (property "Sheetfile" "AgnusAdaptorv2.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C2" (at 0.0046 2.69) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 0 -1.6817) (layer "B.Fab"))
    (pad "1" smd rect (at -0.8754 0) (size 1.1646 1.4653) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "Net-(IC1A-14M)") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
    (pad "2" smd rect (at 0.8754 0) (size 1.1646 1.4653) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
  )
  (footprint "AgnusAdaptorv2:SOT23-5" (layer "B.Cu")
    (at 157.42 111.29 180)
    (descr "<b>Small Outline Transistor</b><p>\nSOT753 - Philips Semiconductors<br>\nSource: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf")
    (property "Sheetfile" "AgnusAdaptorv2.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "IC4" (at -1.44 -3.93) (layer "B.SilkS"))
    (fp_text value "~" (at -2.54 -3.81) (layer "B.Fab") hide)
    (pad "1" smd rect (at -0.95 -1.29 180) (size 0.69 0.99) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 56 "Net-(IC1A-~{RAS1})") (pinfunction "I0") (pintype "input") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
    (pad "2" smd rect (at 0 -1.29 180) (size 0.69 0.99) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 57 "Net-(IC1A-~{RAS0})") (pinfunction "I1") (pintype "input") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
    (pad "3" smd rect (at 0.95 -1.29 180) (size 0.69 0.99) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
    (pad "4" smd rect (at 0.95 1.3 180) (size 0.69 0.99) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "Net-(IC2-~{RAS})") (pinfunction "O") (pintype "output") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
    (pad "5" smd rect (at -0.95 1.3 180) (size 0.69 0.99) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
  )
  (footprint "AgnusAdaptorv2:APW" (layer "B.Cu")
    (at 149.035 103.38 180)
    (descr "PLCC plug, 84 pins, surface mount")
    (tags "plcc smt")
    (property "Sheetfile" "AgnusAdaptorv2.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC2" (at 0 19.3) (layer "B.SilkS") hide)
    (fp_text value "A3000 Agnus Socket" (at 0 -19.8) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -0.525) (layer "B.Fab"))
    (pad "1" smd rect (at 0 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "/DRD13") (pinfunction "DRD13") (pintype "bidirectional"))
    (pad "2" smd rect (at 1.27 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "/DRD12") (pinfunction "DRD12") (pintype "bidirectional"))
    (pad "3" smd rect (at 2.54 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/DRD11") (pinfunction "DRD11") (pintype "bidirectional"))
    (pad "4" smd rect (at 3.81 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/DRD10") (pinfunction "DRD10") (pintype "bidirectional"))
    (pad "5" smd rect (at 5.08 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 8 "/DRD9") (pinfunction "DRD9") (pintype "bidirectional"))
    (pad "6" smd rect (at 6.35 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "/DRD8") (pinfunction "DRD8") (pintype "bidirectional"))
    (pad "7" smd rect (at 7.62 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 10 "/DRD7") (pinfunction "DRD7") (pintype "bidirectional"))
    (pad "8" smd rect (at 8.89 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "/DRD6") (pinfunction "DRD6") (pintype "bidirectional"))
    (pad "9" smd rect (at 10.16 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "/DRD5") (pinfunction "DRD5") (pintype "bidirectional"))
    (pad "10" smd rect (at 11.43 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "/DRD4") (pinfunction "DRD4") (pintype "bidirectional"))
    (pad "11" smd rect (at 12.7 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 14 "/DRD3") (pinfunction "DRD3") (pintype "bidirectional"))
    (pad "12" smd rect (at 16.025 12.7 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "/DRD2") (pinfunction "DRD2") (pintype "bidirectional"))
    (pad "13" smd rect (at 16.025 11.43 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 16 "/DRD1") (pinfunction "DRD1") (pintype "bidirectional"))
    (pad "14" smd rect (at 16.025 10.16 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "/DRD0") (pinfunction "DRD0") (pintype "bidirectional"))
    (pad "15" smd rect (at 16.025 8.89 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "16" smd rect (at 16.025 7.62 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "Net-(IC1A-~{RESET})") (pinfunction "~{RESET}") (pintype "input"))
    (pad "17" smd rect (at 16.025 6.35 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "Net-(IC1A-~{INTRQ})") (pinfunction "~{INTR}") (pintype "output"))
    (pad "18" smd rect (at 16.025 5.08 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "Net-(IC1A-DMAL)") (pinfunction "DMAL") (pintype "input"))
    (pad "19" smd rect (at 16.025 3.81 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "Net-(IC1A-~{BLISS})") (pinfunction "~{BLISS}") (pintype "input"))
    (pad "20" smd rect (at 16.025 2.54 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "Net-(IC1A-~{BLIT})") (pinfunction "~{BLIT}") (pintype "output"))
    (pad "21" smd rect (at 16.025 1.27 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "Net-(IC1A-~{WE})") (pinfunction "~{WE}") (pintype "output"))
    (pad "22" smd rect (at 16.025 0 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "Net-(IC1A-R~{W})") (pinfunction "R/~{W}") (pintype "input"))
    (pad "23" smd rect (at 16.025 -1.27 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "Net-(IC1A-~{REGEN})") (pinfunction "~{REGEN}") (pintype "input"))
    (pad "24" smd rect (at 16.025 -2.54 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "Net-(IC1A-~{AS})") (pinfunction "~{AS}") (pintype "input"))
    (pad "25" smd rect (at 16.025 -3.81 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "Net-(IC1A-~{RAMEN})") (pinfunction "~{RAMEN}") (pintype "input"))
    (pad "26" smd rect (at 16.025 -5.08 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/RGA8") (pinfunction "RGA8") (pintype "bidirectional"))
    (pad "27" smd rect (at 16.025 -6.35 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "/RGA7") (pinfunction "RGA7") (pintype "bidirectional"))
    (pad "28" smd rect (at 16.025 -7.62 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/RGA6") (pinfunction "RGA6") (pintype "bidirectional"))
    (pad "29" smd rect (at 16.025 -8.89 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "/RGA5") (pinfunction "RGA5") (pintype "bidirectional"))
    (pad "30" smd rect (at 16.025 -10.16 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "/RGA4") (pinfunction "RGA4") (pintype "bidirectional"))
    (pad "31" smd rect (at 16.025 -11.43 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "/RGA3") (pinfunction "RGA3") (pintype "bidirectional"))
    (pad "32" smd rect (at 16.025 -12.7 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/RGA2") (pinfunction "RGA2") (pintype "bidirectional"))
    (pad "33" smd rect (at 12.7 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/RGA1") (pinfunction "RGA1") (pintype "bidirectional"))
    (pad "34" smd rect (at 11.43 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "Net-(IC1A-28M)") (pinfunction "28MHZ") (pintype "input"))
    (pad "35" smd rect (at 10.16 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "/A20") (pinfunction "A20") (pintype "input"))
    (pad "36" smd rect (at 8.89 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VCC") (pinfunction "~{XCLKEN}") (pintype "input"))
    (pad "37" smd rect (at 7.62 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "Net-(IC1A-~{CDAC})") (pinfunction "~{CDAC}") (pintype "output"))
    (pad "38" smd rect (at 6.35 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "Net-(IC1A-7M)") (pinfunction "7MHZ") (pintype "output"))
    (pad "39" smd rect (at 5.08 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "Net-(IC1A-CCKQ)") (pinfunction "CCKQ") (pintype "output"))
    (pad "40" smd rect (at 3.81 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "Net-(IC1A-CCK)") (pinfunction "CCK") (pintype "output"))
    (pad "41" smd rect (at 2.54 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "unconnected-(IC2-PAL{slash}NTSC-Pad41)") (pinfunction "PAL/NTSC") (pintype "input"))
    (pad "42" smd rect (at 1.27 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "VSS1") (pintype "power_in"))
    (pad "43" smd rect (at 0 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "/DRA0") (pinfunction "DRA0") (pintype "output"))
    (pad "44" smd rect (at -1.27 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "/DRA1") (pinfunction "DRA1") (pintype "output"))
    (pad "45" smd rect (at -2.54 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "/DRA2") (pinfunction "DRA2") (pintype "output"))
    (pad "46" smd rect (at -3.81 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 45 "/DRA3") (pinfunction "DRA3") (pintype "output"))
    (pad "47" smd rect (at -5.08 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 46 "/DRA4") (pinfunction "DRA4") (pintype "output"))
    (pad "48" smd rect (at -6.35 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 47 "/DRA5") (pinfunction "DRA5") (pintype "output"))
    (pad "49" smd rect (at -7.62 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 48 "/DRA6") (pinfunction "DRA6") (pintype "output"))
    (pad "50" smd rect (at -8.89 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "/DRA7") (pinfunction "DRA7") (pintype "output"))
    (pad "51" smd rect (at -10.16 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 50 "/DRA8") (pinfunction "DRA8") (pintype "output"))
    (pad "52" smd rect (at -11.43 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "Net-(IC1A-~{LDS})") (pinfunction "~{LDS}") (pintype "input"))
    (pad "53" smd rect (at -12.7 -16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "Net-(IC1A-~{UDS})") (pinfunction "~{UDS}") (pintype "input"))
    (pad "54" smd rect (at -16.025 -12.7 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 53 "Net-(IC1A-~{CASL})") (pinfunction "~{CASL}") (pintype "output"))
    (pad "55" smd rect (at -16.025 -11.43 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 54 "Net-(IC1A-~{CASU})") (pinfunction "~{CASU}") (pintype "output"))
    (pad "56" smd rect (at -16.025 -10.16 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 55 "/DRA9") (pinfunction "DRA9") (pintype "output"))
    (pad "57" smd rect (at -16.025 -8.89 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "Net-(IC2-~{RAS})") (pinfunction "~{RAS}") (pintype "output"))
    (pad "58" smd rect (at -16.025 -7.62 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "VSS2") (pintype "power_in"))
    (pad "59" smd rect (at -16.025 -6.35 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 58 "/A19") (pinfunction "A19") (pintype "input"))
    (pad "60" smd rect (at -16.025 -5.08 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 59 "/A1") (pinfunction "A1") (pintype "input"))
    (pad "61" smd rect (at -16.025 -3.81 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 60 "/A2") (pinfunction "A2") (pintype "input"))
    (pad "62" smd rect (at -16.025 -2.54 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "/A3") (pinfunction "A3") (pintype "input"))
    (pad "63" smd rect (at -16.025 -1.27 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "/A4") (pinfunction "A4") (pintype "input"))
    (pad "64" smd rect (at -16.025 0 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "/A5") (pinfunction "A5") (pintype "input"))
    (pad "65" smd rect (at -16.025 1.27 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 64 "/A6") (pinfunction "A6") (pintype "input"))
    (pad "66" smd rect (at -16.025 2.54 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "/A7") (pinfunction "A7") (pintype "input"))
    (pad "67" smd rect (at -16.025 3.81 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "/A8") (pinfunction "A8") (pintype "input"))
    (pad "68" smd rect (at -16.025 5.08 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 67 "/A9") (pinfunction "A9") (pintype "input"))
    (pad "69" smd rect (at -16.025 6.35 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "/A10") (pinfunction "A10") (pintype "input"))
    (pad "70" smd rect (at -16.025 7.62 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 69 "/A11") (pinfunction "A11") (pintype "input"))
    (pad "71" smd rect (at -16.025 8.89 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "/A12") (pinfunction "A12") (pintype "input"))
    (pad "72" smd rect (at -16.025 10.16 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "/A13") (pinfunction "A13") (pintype "input"))
    (pad "73" smd rect (at -16.025 11.43 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "/A14") (pinfunction "A14") (pintype "input"))
    (pad "74" smd rect (at -16.025 12.7 180) (size 4.55 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "/A15") (pinfunction "A15") (pintype "input"))
    (pad "75" smd rect (at -12.7 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "/A16") (pinfunction "A16") (pintype "input"))
    (pad "76" smd rect (at -11.43 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "/A17") (pinfunction "A17") (pintype "input"))
    (pad "77" smd rect (at -10.16 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "/A18") (pinfunction "A18") (pintype "input"))
    (pad "78" smd rect (at -8.89 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "Net-(IC1A-~{LPEN})") (pinfunction "~{LPEN}") (pintype "input"))
    (pad "79" smd rect (at -7.62 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "Net-(IC1A-~{VSYNC})") (pinfunction "~{VSYNC}") (pintype "output"))
    (pad "80" smd rect (at -6.35 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "Net-(IC1A-~{CSYNC})") (pinfunction "~{CSYNC}") (pintype "output"))
    (pad "81" smd rect (at -5.08 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "Net-(IC1A-~{HSYNC})") (pinfunction "~{HSYNC}") (pintype "output"))
    (pad "82" smd rect (at -3.81 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "VSS3") (pintype "power_in"))
    (pad "83" smd rect (at -2.54 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "/DRD15") (pinfunction "DRD15") (pintype "bidirectional"))
    (pad "84" smd rect (at -1.27 16.025 180) (size 0.9 4.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "/DRD14") (pinfunction "DRD14") (pintype "bidirectional"))
    (model "${KISYS3DMOD}/Package_LCC.3dshapes/PLCC-84_SMD-Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "AgnusAdaptorv2:CAPC2012X110" (layer "B.Cu")
    (at 141.8554 112.64)
    (descr "Chip, 2.00 X 1.25 X 1.10 mm body\n<p>Chip package with body size 2.00 X 1.25 X 1.10 mm</p>")
    (property "Sheetfile" "AgnusAdaptorv2.kicad_sch")
    (property "Sheetname" "")
    (fp_text reference "C1" (at -0.0654 2.7) (layer "B.SilkS"))
    (fp_text value "0.1uF" (at 36.509716 -27.6085) (layer "B.Fab"))
    (pad "1" smd rect (at -0.8754 0) (size 1.1646 1.4653) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "VCC") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
    (pad "2" smd rect (at 0.8754 0) (size 1.1646 1.4653) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762) (thermal_bridge_angle 45))
  )
  (gr_line (start 168.148 126.1618) (end 143.7005 126.1618)
    (layer "Edge.Cuts"))
  (gr_line (start 129.2329 124.178) (end 129.2329 86.062)
    (layer "Edge.Cuts"))
  (gr_line (start 149.99 83.84) (end 168.148 83.8454)
    (layer "Edge.Cuts"))
  (gr_line (start 131.465 83.85) (end 129.2329 86.062)
    (layer "Edge.Cuts"))
  (gr_arc (start 149.99 83.84) (mid 148.96 84.87) (end 147.93 83.84)
    (layer "Edge.Cuts"))
  (gr_line (start 143.7005 124.206) (end 129.2329 124.178)
    (layer "Edge.Cuts"))
  (gr_line (start 168.148 83.8454) (end 168.148 126.1618)
    (layer "Edge.Cuts"))
  (gr_line (start 131.465 83.85) (end 147.93 83.84)
    (layer "Edge.Cuts"))
  (gr_line (start 143.7005 126.1618) (end 143.7005 124.206)
    (layer "Edge.Cuts"))
  (gr_text "C1: 0.1uF\nC2: 0.1uF (vbb Only)\nIC4: 74AHC1G08DBV" (at 158.369 93.4466) (layer "B.SilkS"))
  (gr_text "A500+ / A600 Agnus \n8375  (390544)" (at 151.44 124.71) (layer "F.SilkS"))
  (gr_text "Design By Mike Taylor / Stefan Reinauer 2023" (at 144.61 125.68) (layer "F.Mask"))
  (gr_text "A3000 Agnus Adapter V2" (at 130.39 123.53) (layer "F.Mask"))
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.0762) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2024) (thermal_bridge_width 0.2024))
    (polygon
      (pts
        (xy 168.0845 126.0475)
        (xy 128.9685 126.0475)
        (xy 128.9685 83.9343)
        (xy 168.0845 83.9343)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.0762) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2024) (thermal_bridge_width 0.2024))
    (polygon
      (pts
        (xy 168.0845 126.0475)
        (xy 128.9685 126.0475)
        (xy 128.9685 83.9343)
        (xy 168.0845 83.9343)
      )
    )
  )
)
