(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 19)
    (no_connects 0)
    (area 145.280667 100.449 163.303 116.803)
    (thickness 1.6)
    (drawings 6)
    (tracks 63)
    (zones 0)
    (modules 10)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu jumper)
    (31 B.Cu signal hide)
    (37 F.SilkS user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.1524 0.1524)
    (mod_text_width 0.0381)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(LA1-Pad2)")
  (net 5 "Net-(R1-Pad2)")
  (net 6 "Net-(R2-Pad1)")
  (net 7 "Net-(R4-Pad2)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(LA1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net VCC)
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 586C7D55)
    (at 156.464 108.458)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 -1.27) (layer F.SilkS) hide)
    (fp_text value LMV358 (at 0 0) (layer F.SilkS))
    (pad 8 smd rect (at -1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 1 VCC))
    (pad 7 smd rect (at -0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 4 "Net-(LA1-Pad2)"))
    (pad 6 smd rect (at 0.635 -3.175) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.175) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 7 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at -0.635 3.175) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -1.905 3.175) (size 0.508 1.143) (layers F.Cu F.Mask)
      (net 6 "Net-(R2-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586C7D39)
    (at 152.654 105.664 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586C7D19)
    (at 154.686 113.284 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 180) (layer F.SilkS) hide)
    (fp_text value 1u (at 0 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch1.27mm (layer F.Cu) (tedit 586C7D4A)
    (at 149.606 103.886 90)
    (descr "Through hole straight pin header, 1x02, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.27mm single row")
    (fp_text reference LA1 (at 0 -1.755 90) (layer F.SilkS) hide)
    (fp_text value Lamp (at -1.524 0.508 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 "Net-(LA1-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 586C7CCF)
    (at 150.368 113.284 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.93 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586C7D31)
    (at 160.02 104.648 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 1M (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586C7D3F)
    (at 152.654 109.982 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.9 90) (layer F.SilkS) hide)
    (fp_text value 470k (at 0 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 6 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586C7CEE)
    (at 156.718 103.378)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 2.2M (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 4 "Net-(LA1-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 5 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586C7D28)
    (at 160.274 108.966 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.9 270) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 6 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 7 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586C7D12)
    (at 158.496 113.284)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.9) (layer F.SilkS) hide)
    (fp_text value 100K (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 7 "Net-(R4-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 148.082 113.284) (layer F.SilkS))
  (gr_text +3V (at 148.082 110.744) (layer F.SilkS))
  (gr_line (start 147.32 101.6) (end 147.32 115.316) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 161.29 101.6) (end 147.32 101.6) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 161.29 115.316) (end 161.29 101.6) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 147.32 115.316) (end 161.29 115.316) (angle 90) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 115.316) (xy 147.32 115.316) (xy 147.32 101.6) (xy 161.29 101.6)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161.29 115.316) (xy 161.29 101.6) (xy 147.32 101.6) (xy 147.32 115.316)
      )
    )
  )
)
