(kicad_pcb (version 20171130) (host pcbnew "(5.1.9-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 130)
    (zones 0)
    (modules 17)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.2 2.2)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C3-Pad2)")
  (net 3 "Net-(C4-Pad2)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 /V12)
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(U2-Pad9)")
  (net 8 /V5)
  (net 9 "Net-(C3-Pad1)")
  (net 10 "Net-(R1-Pad1)")
  (net 11 "Net-(C1-Pad2)")
  (net 12 "Net-(C1-Pad1)")
  (net 13 /VS+)
  (net 14 "Net-(C2-Pad1)")
  (net 15 "Net-(J2-Pad5)")
  (net 16 "Net-(J2-Pad6)")
  (net 17 "Net-(J2-Pad2)")
  (net 18 "Net-(J2-Pad1)")
  (net 19 "Net-(U1-Pad31)")
  (net 20 "Net-(U1-Pad30)")
  (net 21 "Net-(U1-Pad27)")
  (net 22 "Net-(U1-Pad26)")
  (net 23 "Net-(U1-Pad25)")
  (net 24 "Net-(U1-Pad24)")
  (net 25 "Net-(U1-Pad23)")
  (net 26 "Net-(U1-Pad22)")
  (net 27 "Net-(U1-Pad21)")
  (net 28 "Net-(U1-Pad20)")
  (net 29 "Net-(U1-Pad19)")
  (net 30 "Net-(U1-Pad18)")
  (net 31 "Net-(U1-Pad17)")
  (net 32 "Net-(U1-Pad14)")
  (net 33 "Net-(U1-Pad13)")
  (net 34 "Net-(U1-Pad12)")
  (net 35 "Net-(U1-Pad11)")
  (net 36 "Net-(U1-Pad10)")
  (net 37 "Net-(U1-Pad9)")
  (net 38 "Net-(U1-Pad8)")
  (net 39 "Net-(U1-Pad7)")
  (net 40 "Net-(U1-Pad6)")
  (net 41 "Net-(U1-Pad5)")
  (net 42 "Net-(U1-Pad3)")
  (net 43 "Net-(U1-Pad1)")
  (net 44 "Net-(U2-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net /V12)
    (add_net /V5)
    (add_net /VS+)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
  )
  (module lk201_parts:MDJ-006 (layer F.Cu) (tedit 603C0CA2)
    (at 27.94 -50.165 180)
    (fp_text reference J2 (at 0.3 -1.27) (layer F.SilkS))
    (fp_text value Mini-DIN-6 (at 0 -1.1) (layer F.Fab))
    (pad 6 thru_hole circle (at -3.4 -11 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad6)"))
    (pad 5 thru_hole circle (at 3.4 -11 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad5)"))
    (pad 3 thru_hole circle (at 3.4 -8.5 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.4 -8.5 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 /V5))
    (pad 2 thru_hole circle (at -1.3 -8.5 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 1.3 -8.5 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad1)"))
    (pad SH thru_hole circle (at -6.75 -5.5 180) (size 3.2 3.2) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole circle (at 6.75 -5.5 180) (size 3.2 3.2) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad SH thru_hole circle (at 0 -4.7 180) (size 3.2 3.2) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../lk201_parts/MDJ-00x.step
      (offset (xyz -7 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:Itsy (layer F.Cu) (tedit 5FEF9B3B)
    (at 2.54 -38.735 270)
    (fp_text reference U1 (at 16.51 -6.985 90) (layer F.SilkS))
    (fp_text value Itsy_Bitsy_5V (at 16.51 -8.89 90) (layer F.Fab))
    (fp_text user RX (at 31.9 -14 135) (layer F.SilkS))
    (fp_text user BAT (at 0.1 -13.4 90) (layer F.SilkS))
    (fp_text user TX (at 30.2 -13.4 90) (layer F.SilkS))
    (fp_text user SDA (at 27.9 -13.4 90) (layer F.SilkS))
    (fp_text user SCL (at 25.4 -13.4 90) (layer F.SilkS))
    (fp_text user 5 (at 22.9 -13.4 90) (layer F.SilkS))
    (fp_text user 7 (at 20.3 -13.4 90) (layer F.SilkS))
    (fp_text user 9 (at 17.8 -13.4 90) (layer F.SilkS))
    (fp_text user 10 (at 15.2 -13.4 90) (layer F.SilkS))
    (fp_text user 11 (at 12.7 -13.4 90) (layer F.SilkS))
    (fp_text user 12 (at 10.2 -13.4 90) (layer F.SilkS))
    (fp_text user 13 (at 7.6 -13.4 90) (layer F.SilkS))
    (fp_text user USB (at 5.1 -13.4 90) (layer F.SilkS))
    (fp_text user G (at 7.681816 -1) (layer F.SilkS))
    (fp_text user 4 (at 31.3 -12.1) (layer F.SilkS))
    (fp_text user 6 (at 31.3 -9.549207) (layer F.SilkS))
    (fp_text user 8 (at 31.3 -6.998414) (layer F.SilkS))
    (fp_text user G (at 31.3 -4.4) (layer F.SilkS))
    (fp_text user En (at 31.3 -2.2) (layer F.SilkS))
    (fp_text user MI (at 30.1 -1) (layer F.SilkS))
    (fp_text user MO (at 27.9 -1) (layer F.SilkS))
    (fp_text user SCLK (at 25.37272 -1) (layer F.SilkS))
    (fp_text user A5 (at 22.845448 -1) (layer F.SilkS))
    (fp_text user A4 (at 20.318176 -1) (layer F.SilkS))
    (fp_text user A3 (at 17.790904 -1) (layer F.SilkS))
    (fp_text user A2 (at 15.263632 -1) (layer F.SilkS))
    (fp_text user A1 (at 12.73636 -1) (layer F.SilkS))
    (fp_text user A0 (at 10.209088 -1) (layer F.SilkS))
    (fp_text user RST (at 0.1 -1) (layer F.SilkS))
    (fp_text user 5V (at 2.627272 -1) (layer F.SilkS))
    (fp_text user Aref (at 5.154544 -1) (layer F.SilkS))
    (fp_text user G (at 7.681816 -1) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /V5))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at 15.24 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at 17.78 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at 20.32 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at 22.86 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at 25.4 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 27.94 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at 30.48 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at 33.02 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at 33.02 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 33.02 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 17 thru_hole circle (at 33.02 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at 33.02 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 33.02 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 33.02 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad20)"))
    (pad 21 thru_hole circle (at 30.48 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at 27.94 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at 25.4 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at 22.86 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at 20.32 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at 17.78 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at 15.24 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad27)"))
    (pad 28 thru_hole circle (at 12.7 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad1)"))
    (pad 29 thru_hole circle (at 10.16 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad5)"))
    (pad 30 thru_hole circle (at 7.62 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad30)"))
    (pad 31 thru_hole circle (at 5.08 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad31)"))
    (pad 32 thru_hole circle (at 2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 33 thru_hole circle (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /V12))
    (model :USER3DMOD:Itsy.step
      (offset (xyz -132.1 112.6 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:RJ22 (layer F.Cu) (tedit 5FEF9014)
    (at 41.91 -24.13 90)
    (fp_text reference J1 (at 0 1.27 90) (layer F.SilkS))
    (fp_text value RJ22 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -1.905 -6.35 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -0.635 -8.89 90) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /V12))
    (pad 3 thru_hole circle (at 0.635 -6.35 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 1.905 -8.89 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad "" np_thru_hole circle (at 3.81 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Mask F.Cu))
    (pad "" np_thru_hole circle (at -3.81 0 90) (size 3.2 3.2) (drill 3.2) (layers *.Mask F.Cu))
    (model ${KIPRJMOD}/../lk201_parts/modular_jack_a-20040.step
      (offset (xyz 0 -10.5 1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 180))
    )
  )
  (module lk201_parts:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 48.26 -2.54)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module lk201_parts:PS1420_buzzer (layer F.Cu) (tedit 5EC6900F)
    (at 43.18 -38.735)
    (fp_text reference LS1 (at 0 -1.905 180) (layer F.SilkS))
    (fp_text value PS1420 (at 0 -1.905 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 2.5 0) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at -2.5 0) (size 1.524 1.524) (drill 1) (layers *.Cu *.Mask)
      (net 13 /VS+))
    (model ${KISYS3DMOD}/Buzzer_Beeper.3dshapes/Buzzer_15x7.5RM7.6.step
      (offset (xyz -3.6 0 0))
      (scale (xyz 0.93 0.93 1.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:DIP-16_296_ELL (layer F.Cu) (tedit 5EC68F95)
    (at 34.29 -10.845)
    (fp_text reference U2 (at 6.985 0.05 -180) (layer F.SilkS))
    (fp_text value ICL3232CPZ (at 0 0 180) (layer F.Fab))
    (pad 16 thru_hole oval (at -8.89 -3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /V5))
    (pad 1 thru_hole oval (at -8.89 3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C1-Pad1)"))
    (pad 15 thru_hole oval (at -6.35 -3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at -6.35 3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VS+))
    (pad 14 thru_hole oval (at -3.81 -3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 3 thru_hole oval (at -3.81 3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C1-Pad2)"))
    (pad 13 thru_hole oval (at -1.27 -3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 4 thru_hole oval (at -1.27 3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (pad 12 thru_hole oval (at 1.27 -3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad20)"))
    (pad 5 thru_hole oval (at 1.27 3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C3-Pad2)"))
    (pad 11 thru_hole oval (at 3.81 -3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad21)"))
    (pad 6 thru_hole oval (at 3.81 3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 10 thru_hole oval (at 6.35 -3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad26)"))
    (pad 7 thru_hole oval (at 6.35 3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (pad 9 thru_hole oval (at 8.89 -3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(U2-Pad9)"))
    (pad 8 thru_hole oval (at 8.89 3.76) (size 1.2 2) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U2-Pad8)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-16_W7.62mm.step
      (offset (xyz 8.890000000000001 3.81 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module lk201_parts:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 26.67 -19.05 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.37 90) (layer F.SilkS))
    (fp_text value 3.3k (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5FECF770)
    (at 22.225 -15.875 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /V5))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5FECF770)
    (at 22.225 -10.795 270)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C5 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VS+))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5FECF770)
    (at 40.64 -3.175 180)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C4 (at -1.905 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5FECF770)
    (at 31.75 -3.175)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 3.175 1.905) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5FECF770)
    (at 31.75 -32.385 90)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 1.25 -2.5 90) (layer F.SilkS))
    (fp_text value 0.01uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /VS+))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lk201_parts:C_Rect_L4.0mm_W2.5mm_P2.54mm (layer F.Cu) (tedit 5FECF770)
    (at 25.4 -3.175)
    (descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
    (fp_text reference C1 (at -1.905 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.5) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LK201:AK_Design_9mm (layer F.Cu) (tedit 5EC6EF5E)
    (at 48.895 -5.715 90)
    (fp_text reference REF** (at 0 0.5 90) (layer F.SilkS) hide)
    (fp_text value AK_Design_9mm (at 0 -0.5 90) (layer F.Fab) hide)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 56D1B4CB)
    (at 2.54 -2.54)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5FEE21E3)
    (at 2.54 -35.56)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 -12.7) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5FEE2185)
    (at 48.26 -35.56)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 -12.7) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (gr_text "AK-004 C" (at 13.97 -1.905) (layer B.Cu))
  (gr_text "AK-004 C" (at 6.35 -1.905) (layer F.Cu))
  (gr_text "LK201 emulator by\nPaul Koning\nApril 2021" (at 5.08 -47.625) (layer F.SilkS))
  (gr_line (start 50.8 0) (end 0 0) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 50.8 -50.8) (end 50.8 0) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 0 -50.8) (end 50.8 -50.8) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 0 0) (end 0 -50.8) (layer Edge.Cuts) (width 0.12))
)
