(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 30)
    (no_connects 0)
    (area 90.094999 92.634999 118.185001 110.565001)
    (thickness 1.6)
    (drawings 22)
    (tracks 66)
    (zones 0)
    (modules 10)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(CS1-Pad2)")
  (net 3 "Net-(CT1-Pad2)")
  (net 4 VCC)
  (net 5 "Net-(P1-Pad5)")
  (net 6 "Net-(P2-Pad2)")
  (net 7 "Net-(P2-Pad3)")
  (net 8 "Net-(P2-Pad4)")
  (net 9 "Net-(P2-Pad5)")
  (net 10 "Net-(P2-Pad6)")
  (net 11 "Net-(P2-Pad7)")
  (net 12 "Net-(P2-Pad8)")
  (net 13 "Net-(P2-Pad9)")
  (net 14 "Net-(P3-Pad3)")
  (net_class Default "Toto je výchozí třída sítě."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class 1mm ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(CS1-Pad2)")
    (add_net "Net-(CT1-Pad2)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P2-Pad6)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(P2-Pad8)")
    (add_net "Net-(P2-Pad9)")
    (add_net "Net-(P3-Pad3)")
    (add_net VCC)
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Small (layer F.Cu) (tedit 583C8C2C)
    (at 105.41 97.79)
    (descr "Mesurement Point, Square, Trough Hole,  1.5mm x 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Square Trough Hole 1.5x1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference "" (at 0 -2) (layer F.SilkS) hide)
    (fp_text value " " (at 0 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.5 0.8) (drill 0.3 (offset 0 0.2)) (layers *.Cu *.Mask))
  )
  (module Measurement_Points:Measurement_Point_Square-TH_Small (layer F.Cu) (tedit 583C8C50)
    (at 113.03 97.79)
    (descr "Mesurement Point, Square, Trough Hole,  1.5mm x 1.5mm, Drill 0.8mm,")
    (tags "Mesurement Point Square Trough Hole 1.5x1.5mm Drill 0.8mm")
    (attr virtual)
    (fp_text reference "" (at 0 -2) (layer F.SilkS) hide)
    (fp_text value "" (at 0 2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 0.5 0.8) (drill 0.3 (offset 0 0.2)) (layers *.Cu *.Mask))
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 583C8151)
    (at 96.52 106.68 90)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value 74HC595 (at 3.81 6.35 180) (layer F.SilkS))
    (fp_text user 1 (at 1.27 0 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(P3-Pad3)"))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(CT1-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(CS1-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(P2-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 583C75A1)
    (at 96.52 96.52)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference "C2 D" (at 2.54 0) (layer F.SilkS))
    (fp_text value C (at 2.5 3.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(CS1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 583C75B1)
    (at 96.52 93.98)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference "C1 L" (at 2.54 0) (layer F.SilkS))
    (fp_text value C (at 2.5 3.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 5 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(CT1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer B.Cu) (tedit 583C7E49)
    (at 91.44 106.68)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 5.1) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 0 10.16) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole oval (at 0 -5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(CS1-Pad2)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(CT1-Pad2)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x10 (layer B.Cu) (tedit 583C7E4F)
    (at 91.44 109.22)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 0 5.1) (layer B.SilkS))
    (fp_text value CONN_01X10 (at 0 11.43) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(P2-Pad8)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(P2-Pad9)"))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 VCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x10.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05 (layer B.Cu) (tedit 583C7E2A)
    (at 116.84 106.68)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 5.1) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 0 10.16) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 VCC))
    (pad 3 thru_hole oval (at 0 -5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(P3-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(CT1-Pad2)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad5)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 583C7529)
    (at 104.14 96.52)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference "R2 DAT" (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(CS1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(P1-Pad5)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 583C7536)
    (at 106.68 93.98)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference "R1 LAT" (at 3.81 0) (layer F.SilkS))
    (fp_text value R (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(CT1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(P1-Pad5)"))
  )
  (gr_text CL (at 114.3 96.52) (layer B.SilkS))
  (gr_text CL (at 114.3 96.52) (layer F.SilkS))
  (gr_text + (at 114.3 104.14) (layer F.SilkS))
  (gr_text + (at 114.3 104.14) (layer B.SilkS))
  (gr_text DO (at 114.3 101.6) (layer B.SilkS))
  (gr_text DO (at 114.3 101.6) (layer F.SilkS))
  (gr_text + (at 93.98 104.14) (layer B.SilkS))
  (gr_text CL (at 93.98 96.52) (layer B.SilkS))
  (gr_text LA (at 93.98 99.06) (layer B.SilkS))
  (gr_text DI (at 93.98 101.6) (layer B.SilkS))
  (gr_text - (at 93.98 106.68) (layer B.SilkS))
  (gr_text CL (at 93.98 96.52) (layer F.SilkS))
  (gr_text LA (at 93.98 99.06) (layer F.SilkS))
  (gr_text DI (at 93.98 101.6) (layer F.SilkS))
  (gr_text - (at 93.98 106.68) (layer F.SilkS))
  (gr_text + (at 93.98 104.14) (layer F.SilkS))
  (gr_line (start 90.17 92.71) (end 118.11 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.17 110.49) (end 90.17 92.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 110.49) (end 90.17 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.11 92.71) (end 118.11 110.49) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 17.78 (width 0.3) (layer B.Paste)
    (gr_text "17,780 mm" (at 83.74 101.6 270) (layer B.Paste))
    (feature1 (pts (xy 87.63 110.49) (xy 82.39 110.49)))
    (feature2 (pts (xy 87.63 92.71) (xy 82.39 92.71)))
    (crossbar (pts (xy 85.09 92.71) (xy 85.09 110.49)))
    (arrow1a (pts (xy 85.09 110.49) (xy 84.503579 109.363496)))
    (arrow1b (pts (xy 85.09 110.49) (xy 85.676421 109.363496)))
    (arrow2a (pts (xy 85.09 92.71) (xy 84.503579 93.836504)))
    (arrow2b (pts (xy 85.09 92.71) (xy 85.676421 93.836504)))
  )
  (dimension 27.94 (width 0.3) (layer B.Paste)
    (gr_text "27,940 mm" (at 104.14 85.01) (layer B.Paste))
    (feature1 (pts (xy 118.11 90.17) (xy 118.11 83.66)))
    (feature2 (pts (xy 90.17 90.17) (xy 90.17 83.66)))
    (crossbar (pts (xy 90.17 86.36) (xy 118.11 86.36)))
    (arrow1a (pts (xy 118.11 86.36) (xy 116.983496 86.946421)))
    (arrow1b (pts (xy 118.11 86.36) (xy 116.983496 85.773579)))
    (arrow2a (pts (xy 90.17 86.36) (xy 91.296504 86.946421)))
    (arrow2b (pts (xy 90.17 86.36) (xy 91.296504 85.773579)))
  )
)
