(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 52)
    (no_connects 0)
    (area 128.194999 90.094999 146.125001 128.345001)
    (thickness 1.6)
    (drawings 41)
    (tracks 183)
    (zones 0)
    (modules 10)
    (nets 31)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.2032)
    (zone_clearance 0.32)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6096)
    (via_drill 0.4064)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.2032)
    (pcb_text_size 0.889 0.889)
    (mod_edge_width 0.15)
    (mod_text_size 0.889 0.889)
    (mod_text_width 0.2032)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 3V3)
  (net 2 Earth)
  (net 3 RAW)
  (net 4 MISO)
  (net 5 SCK)
  (net 6 MOSI)
  (net 7 RESET)
  (net 8 INT1)
  (net 9 PD4)
  (net 10 SDA1)
  (net 11 SCL1)
  (net 12 PB6)
  (net 13 PB7)
  (net 14 PD5)
  (net 15 PD6)
  (net 16 PB0)
  (net 17 PB1)
  (net 18 SS0)
  (net 19 SS1)
  (net 20 MOSI1)
  (net 21 MISO1)
  (net 22 SCK1)
  (net 23 PC2)
  (net 24 PC3)
  (net 25 SDA0)
  (net 26 SCL0)
  (net 27 RXD0)
  (net 28 TXD0)
  (net 29 INT0)
  (net 30 PD7)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.254)
    (via_dia 0.6096)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net INT0)
    (add_net INT1)
    (add_net MISO)
    (add_net MISO1)
    (add_net MOSI)
    (add_net MOSI1)
    (add_net PB0)
    (add_net PB1)
    (add_net PB6)
    (add_net PB7)
    (add_net PC2)
    (add_net PC3)
    (add_net PD4)
    (add_net PD5)
    (add_net PD6)
    (add_net PD7)
    (add_net RESET)
    (add_net RXD0)
    (add_net SCK)
    (add_net SCK1)
    (add_net SCL0)
    (add_net SCL1)
    (add_net SDA0)
    (add_net SDA1)
    (add_net SS0)
    (add_net SS1)
    (add_net TXD0)
  )
  (net_class power ""
    (clearance 0.2032)
    (trace_width 0.381)
    (via_dia 0.6096)
    (via_drill 0.4064)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3V3)
    (add_net Earth)
    (add_net RAW)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B87DC4D)
    (at 143.002 110.49 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.27 90) (layer Dwgs.User))
    (fp_text value 0.1uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B87DC13)
    (at 131.318 110.49 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.127 1.143 270) (layer Dwgs.User))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer B.Cu) (tedit 5B87C8A6)
    (at 129.54 91.44 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 2.159 180) (layer Dwgs.User))
    (fp_text value CONN_01X15 (at 0 3.1 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 2 Earth))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 7 RESET))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 27 RXD0))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 28 TXD0))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 29 INT0))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 8 INT1))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 9 PD4))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 10 SDA1))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 11 SCL1))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 12 PB6))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 13 PB7))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 14 PD5))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 15 PD6))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 30 PD7))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 16 PB0))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer B.Cu) (tedit 5B87C8AC)
    (at 144.78 91.44 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 2.286 180) (layer Dwgs.User))
    (fp_text value CONN_01X15 (at 0 3.1 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 3 RAW))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 1 3V3))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 26 SCL0))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 25 SDA0))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 24 PC3))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 23 PC2))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 22 SCK1))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 21 MISO1))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 20 MOSI1))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 19 SS1))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 5 SCK))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 4 MISO))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 6 MOSI))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 18 SS0))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask B.SilkS)
      (net 17 PB1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 5B87C8B5)
    (at 139.7 91.44 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.159 2.54 360) (layer Dwgs.User))
    (fp_text value CONN_02X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 MISO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 3V3))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MOSI))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 Earth))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B87C825)
    (at 134.112 99.06 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.413 0 360) (layer F.SilkS))
    (fp_text value 1.0uF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 RAW))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5B87C819)
    (at 140.208 99.06 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.413 0 180) (layer F.SilkS))
    (fp_text value 1.0uF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5B88E7CA)
    (at 137.16 102.489 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.524 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 RESET))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 5B88E7C4)
    (at 137.16 110.49)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 0.127) (layer F.SilkS))
    (fp_text value Atmega328PB (at 0 6.05) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 INT1))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 PD4))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 SDA1))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 SCL1))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 PB6))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 PB7))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 PD5))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 PD6))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 PD7))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 PB0))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 PB1))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 SS0))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 MISO))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 SCK))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 SS1))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 MOSI1))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 MISO1))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 SCK1))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 PC2))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 PC3))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 SDA0))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 SCL0))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 RESET))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 RXD0))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 TXD0))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 INT0))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT-23-5 (layer F.Cu) (tedit 5B87C769)
    (at 137.16 99.06 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value APE8865Y5-33-HF-3 (at -0.05 2.35 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 RAW))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 RAW))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 328PB (at 137.16 125.73) (layer F.SilkS))
  (gr_text B1 (at 142.621 127) (layer F.SilkS))
  (gr_text B2 (at 142.621 124.46) (layer F.SilkS))
  (gr_text B3 (at 142.621 121.92) (layer F.SilkS))
  (gr_text B4 (at 142.621 119.38) (layer F.SilkS))
  (gr_text B5 (at 142.621 116.84) (layer F.SilkS))
  (gr_text E2 (at 142.621 114.427) (layer F.SilkS))
  (gr_text E3 (at 143.002 113.03 90) (layer F.SilkS))
  (gr_text C0 (at 143.002 107.95 90) (layer F.SilkS))
  (gr_text C1 (at 142.621 106.553) (layer F.SilkS))
  (gr_text C2 (at 142.621 104.14) (layer F.SilkS))
  (gr_text C3 (at 142.621 101.6) (layer F.SilkS))
  (gr_text C4 (at 142.621 99.06) (layer F.SilkS))
  (gr_text C5 (at 142.621 96.647) (layer F.SilkS))
  (gr_text 3V3 (at 142.367 93.98) (layer F.SilkS))
  (gr_text RAW (at 142.24 91.821) (layer F.SilkS))
  (gr_text B0 (at 131.572 127) (layer F.SilkS))
  (gr_text D7 (at 131.572 124.46) (layer F.SilkS))
  (gr_text D6 (at 131.572 121.92) (layer F.SilkS))
  (gr_text D5 (at 131.572 119.38) (layer F.SilkS))
  (gr_text B7 (at 131.572 116.84) (layer F.SilkS))
  (gr_text B6 (at 131.572 114.427) (layer F.SilkS))
  (gr_text E1 (at 131.318 113.03 90) (layer F.SilkS))
  (gr_text E0 (at 131.318 107.95 90) (layer F.SilkS))
  (gr_text D4 (at 131.572 106.553) (layer F.SilkS))
  (gr_text D3 (at 131.572 104.14) (layer F.SilkS))
  (gr_text D2 (at 131.572 101.6) (layer F.SilkS))
  (gr_text TX (at 131.572 99.06) (layer F.SilkS))
  (gr_text RX (at 131.572 96.647) (layer F.SilkS))
  (gr_text RST (at 131.953 93.98) (layer F.SilkS))
  (gr_text GND (at 132.08 91.44) (layer F.SilkS))
  (dimension 38.1 (width 0.3) (layer Dwgs.User)
    (gr_text "1.5000 in" (at 152.226 109.22 270) (layer Dwgs.User))
    (feature1 (pts (xy 146.05 128.27) (xy 153.576 128.27)))
    (feature2 (pts (xy 146.05 90.17) (xy 153.576 90.17)))
    (crossbar (pts (xy 150.876 90.17) (xy 150.876 128.27)))
    (arrow1a (pts (xy 150.876 128.27) (xy 150.289579 127.143496)))
    (arrow1b (pts (xy 150.876 128.27) (xy 151.462421 127.143496)))
    (arrow2a (pts (xy 150.876 90.17) (xy 150.289579 91.296504)))
    (arrow2b (pts (xy 150.876 90.17) (xy 151.462421 91.296504)))
  )
  (dimension 17.78 (width 0.3) (layer Dwgs.User)
    (gr_text "0.7000 in" (at 137.16 83.613) (layer Dwgs.User))
    (feature1 (pts (xy 146.05 90.17) (xy 146.05 82.263)))
    (feature2 (pts (xy 128.27 90.17) (xy 128.27 82.263)))
    (crossbar (pts (xy 128.27 84.963) (xy 146.05 84.963)))
    (arrow1a (pts (xy 146.05 84.963) (xy 144.923496 85.549421)))
    (arrow1b (pts (xy 146.05 84.963) (xy 144.923496 84.376579)))
    (arrow2a (pts (xy 128.27 84.963) (xy 129.396504 85.549421)))
    (arrow2b (pts (xy 128.27 84.963) (xy 129.396504 84.376579)))
  )
  (gr_line (start 128.27 128.27) (end 128.27 128.143) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 128.27) (end 128.27 128.27) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 128.143) (end 146.05 128.27) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 90.17) (end 146.05 90.297) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 90.17) (end 146.05 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 90.297) (end 128.27 90.17) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 128.143) (end 128.27 90.297) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.05 90.297) (end 146.05 128.143) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.32))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.524 90.551) (xy 145.796 90.551) (xy 146.05 128.143) (xy 128.27 128.27) (xy 128.524 90.551)
      )
    )
  )
)
