(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 664)
    (zones 0)
    (modules 41)
    (nets 64)
  )
  (page USLetter portrait)
  (title_block
    (title "Shutdown - PowerBoard")
    (rev 7a)
    (company "Formula U")
    (comment 1 "Author: Jesse Koker")
  )
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.143)
    (user_trace_width 1.524)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FF7FFF7)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Plot/"))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 "Net-(Q2-Pad2)")
  (net 3 "Net-(Q3-Pad2)")
  (net 4 "Net-(Q4-Pad4)")
  (net 5 "Net-(Q4-Pad2)")
  (net 6 "Net-(C1-Pad1)")
  (net 7 "Net-(R6-Pad2)")
  (net 8 "Net-(R7-Pad2)")
  (net 9 "Net-(R7-Pad1)")
  (net 10 "Net-(R9-Pad2)")
  (net 11 GND)
  (net 12 "Net-(R10-Pad1)")
  (net 13 "Net-(U1-Pad7)")
  (net 14 "Net-(Q4-Pad7)")
  (net 15 /TO_PRE)
  (net 16 /+12VF)
  (net 17 /IMD_ON)
  (net 18 /APPS_BSE_ON)
  (net 19 /BMS_ON)
  (net 20 /BSPD_ON)
  (net 21 /TO_GO)
  (net 22 /FROM_BTNS)
  (net 23 "Net-(Q1-Pad2)")
  (net 24 /BSPD_DASH_ERR)
  (net 25 /BMS_DASH_ERR)
  (net 26 "Net-(Q5-Pad4)")
  (net 27 "Net-(Q5-Pad2)")
  (net 28 /A&B_DASH_ERR)
  (net 29 "Net-(D1-Pad1)")
  (net 30 "Net-(D2-Pad2)")
  (net 31 "Net-(D2-Pad1)")
  (net 32 "Net-(D3-Pad2)")
  (net 33 "Net-(D3-Pad1)")
  (net 34 "Net-(D4-Pad2)")
  (net 35 "Net-(D4-Pad1)")
  (net 36 "Net-(D5-Pad2)")
  (net 37 "Net-(D5-Pad1)")
  (net 38 "Net-(D6-Pad1)")
  (net 39 "Net-(D7-Pad2)")
  (net 40 "Net-(D7-Pad1)")
  (net 41 "Net-(K1-Pad7)")
  (net 42 "Net-(K1-Pad2)")
  (net 43 "Net-(K1-Pad6)")
  (net 44 "Net-(K1-Pad5)")
  (net 45 "Net-(K1-Pad4)")
  (net 46 "Net-(K2-Pad7)")
  (net 47 "Net-(K2-Pad2)")
  (net 48 "Net-(K2-Pad6)")
  (net 49 "Net-(K2-Pad5)")
  (net 50 "Net-(K2-Pad4)")
  (net 51 "Net-(K3-Pad7)")
  (net 52 "Net-(K3-Pad2)")
  (net 53 "Net-(K3-Pad6)")
  (net 54 "Net-(K3-Pad5)")
  (net 55 "Net-(K3-Pad4)")
  (net 56 "Net-(K4-Pad7)")
  (net 57 "Net-(K4-Pad2)")
  (net 58 "Net-(K4-Pad6)")
  (net 59 "Net-(K4-Pad5)")
  (net 60 "Net-(K5-Pad7)")
  (net 61 "Net-(K5-Pad2)")
  (net 62 "Net-(K5-Pad4)")
  (net 63 "Net-(K5-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /+12VF)
    (add_net /A&B_DASH_ERR)
    (add_net /APPS_BSE_ON)
    (add_net /BMS_DASH_ERR)
    (add_net /BMS_ON)
    (add_net /BSPD_DASH_ERR)
    (add_net /BSPD_ON)
    (add_net /FROM_BTNS)
    (add_net /IMD_ON)
    (add_net /TO_GO)
    (add_net /TO_PRE)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(K1-Pad2)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(K1-Pad5)")
    (add_net "Net-(K1-Pad6)")
    (add_net "Net-(K1-Pad7)")
    (add_net "Net-(K2-Pad2)")
    (add_net "Net-(K2-Pad4)")
    (add_net "Net-(K2-Pad5)")
    (add_net "Net-(K2-Pad6)")
    (add_net "Net-(K2-Pad7)")
    (add_net "Net-(K3-Pad2)")
    (add_net "Net-(K3-Pad4)")
    (add_net "Net-(K3-Pad5)")
    (add_net "Net-(K3-Pad6)")
    (add_net "Net-(K3-Pad7)")
    (add_net "Net-(K4-Pad2)")
    (add_net "Net-(K4-Pad5)")
    (add_net "Net-(K4-Pad6)")
    (add_net "Net-(K4-Pad7)")
    (add_net "Net-(K5-Pad2)")
    (add_net "Net-(K5-Pad3)")
    (add_net "Net-(K5-Pad4)")
    (add_net "Net-(K5-Pad7)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q4-Pad4)")
    (add_net "Net-(Q4-Pad7)")
    (add_net "Net-(Q5-Pad2)")
    (add_net "Net-(Q5-Pad4)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad7)")
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer F.Cu) (tedit 5B82E1AD)
    (at 84.4 120.2 90)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN5 (at 0 -2.8 90) (layer F.SilkS))
    (fp_text value 10k (at 0 2.8 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.7 -1.27 90) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 19 /BMS_ON))
    (pad 3 smd rect (at -0.7 0.4 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /BSPD_ON))
    (pad 2 smd rect (at -0.7 -0.4 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /IMD_ON))
    (pad 4 smd rect (at -0.7 1.27 90) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 18 /APPS_BSE_ON))
    (pad 7 smd rect (at 0.7 -0.4 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(Q5-Pad2)"))
    (pad 8 smd rect (at 0.7 -1.27 90) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(Q1-Pad2)"))
    (pad 6 smd rect (at 0.7 0.4 90) (size 0.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(Q2-Pad2)"))
    (pad 5 smd rect (at 0.7 1.27 90) (size 0.7 0.64) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(Q3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer B.Cu) (tedit 5B82E1AD)
    (at 84.4 120.2 270)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 2.8 90) (layer B.SilkS))
    (fp_text value 1M (at 0 -2.8 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.7 1.27 270) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 3 smd rect (at -0.7 -0.4 270) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 2 smd rect (at -0.7 0.4 270) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 4 smd rect (at -0.7 -1.27 270) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 11 GND))
    (pad 7 smd rect (at 0.7 0.4 270) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 17 /IMD_ON))
    (pad 8 smd rect (at 0.7 1.27 270) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 19 /BMS_ON))
    (pad 6 smd rect (at 0.7 -0.4 270) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 20 /BSPD_ON))
    (pad 5 smd rect (at 0.7 -1.27 270) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 18 /APPS_BSE_ON))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_Array_Convex_4x0612 (layer B.Cu) (tedit 5B82E1AD)
    (at 85.3 96.8 90)
    (descr "Precision Thin Film Chip Resistor Array, VISHAY (see http://www.vishay.com/docs/28770/acasat.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 1.9 0 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -2.8 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.7 1.27 90) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V))
    (pad 3 smd rect (at -0.7 -0.4 90) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V))
    (pad 2 smd rect (at -0.7 0.4 90) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V))
    (pad 4 smd rect (at -0.7 -1.27 90) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 1 +12V))
    (pad 7 smd rect (at 0.7 0.4 90) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(D4-Pad2)"))
    (pad 8 smd rect (at 0.7 1.27 90) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D7-Pad2)"))
    (pad 6 smd rect (at 0.7 -0.4 90) (size 0.7 0.5) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D3-Pad2)"))
    (pad 5 smd rect (at 0.7 -1.27 90) (size 0.7 0.64) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x0612.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HomeBrew:Panasonic_AGQ_Relay-THT (layer F.Cu) (tedit 5E549643)
    (at 99.25 134.8 180)
    (fp_text reference K2 (at -6.5 0 90) (layer F.SilkS))
    (fp_text value AGQ_Relay (at 0 0) (layer F.Fab))
    (pad 8 thru_hole circle (at -4.3 -2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 33 "Net-(D3-Pad1)"))
    (pad 1 thru_hole circle (at -4.3 2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 7 thru_hole circle (at -1.1 -2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 46 "Net-(K2-Pad7)"))
    (pad 2 thru_hole circle (at -1.1 2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 47 "Net-(K2-Pad2)"))
    (pad 6 thru_hole circle (at 1.1 -2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 48 "Net-(K2-Pad6)"))
    (pad 3 thru_hole circle (at 1.1 2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 45 "Net-(K1-Pad4)"))
    (pad 5 thru_hole circle (at 3.3 -2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 49 "Net-(K2-Pad5)"))
    (pad 4 thru_hole circle (at 3.3 2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 50 "Net-(K2-Pad4)"))
  )
  (module HomeBrew:Panasonic_AGQ_Relay-THT (layer F.Cu) (tedit 5E549643)
    (at 87.55 134.8 180)
    (fp_text reference K3 (at 5.8 3.5 90) (layer F.SilkS))
    (fp_text value AGQ_Relay (at 0 0) (layer F.Fab))
    (pad 8 thru_hole circle (at -4.3 -2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 35 "Net-(D4-Pad1)"))
    (pad 1 thru_hole circle (at -4.3 2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 7 thru_hole circle (at -1.1 -2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 51 "Net-(K3-Pad7)"))
    (pad 2 thru_hole circle (at -1.1 2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 52 "Net-(K3-Pad2)"))
    (pad 6 thru_hole circle (at 1.1 -2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 53 "Net-(K3-Pad6)"))
    (pad 3 thru_hole circle (at 1.1 2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 50 "Net-(K2-Pad4)"))
    (pad 5 thru_hole circle (at 3.3 -2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 54 "Net-(K3-Pad5)"))
    (pad 4 thru_hole circle (at 3.3 2.54 180) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 55 "Net-(K3-Pad4)"))
  )
  (module HomeBrew:Panasonic_AGQ_Relay-THT (layer F.Cu) (tedit 5E549643)
    (at 88.55 126.85)
    (fp_text reference K4 (at -6.4 0 90) (layer F.SilkS))
    (fp_text value AGQ_Relay (at 0 0) (layer F.Fab))
    (pad 8 thru_hole circle (at -4.3 -2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 37 "Net-(D5-Pad1)"))
    (pad 1 thru_hole circle (at -4.3 2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 7 thru_hole circle (at -1.1 -2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 56 "Net-(K4-Pad7)"))
    (pad 2 thru_hole circle (at -1.1 2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 57 "Net-(K4-Pad2)"))
    (pad 6 thru_hole circle (at 1.1 -2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 58 "Net-(K4-Pad6)"))
    (pad 3 thru_hole circle (at 1.1 2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 55 "Net-(K3-Pad4)"))
    (pad 5 thru_hole circle (at 3.3 -2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 59 "Net-(K4-Pad5)"))
    (pad 4 thru_hole circle (at 3.3 2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 15 /TO_PRE))
  )
  (module HomeBrew:Panasonic_AGQ_Relay-THT (layer F.Cu) (tedit 5E549643)
    (at 100.25 126.85)
    (fp_text reference K5 (at 2.8 -4.6 180) (layer F.SilkS))
    (fp_text value AGQ_Relay (at 0 0) (layer F.Fab))
    (pad 8 thru_hole circle (at -4.3 -2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 40 "Net-(D7-Pad1)"))
    (pad 1 thru_hole circle (at -4.3 2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 22 /FROM_BTNS))
    (pad 7 thru_hole circle (at -1.1 -2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 60 "Net-(K5-Pad7)"))
    (pad 2 thru_hole circle (at -1.1 2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 61 "Net-(K5-Pad2)"))
    (pad 6 thru_hole circle (at 1.1 -2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 15 /TO_PRE))
    (pad 3 thru_hole circle (at 1.1 2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 63 "Net-(K5-Pad3)"))
    (pad 5 thru_hole circle (at 3.3 -2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 21 /TO_GO))
    (pad 4 thru_hole circle (at 3.3 2.54) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 62 "Net-(K5-Pad4)"))
  )
  (module HomeBrew:Panasonic_AGQ_Relay-THT (layer F.Cu) (tedit 5E549643)
    (at 109.45 127.2 270)
    (fp_text reference K1 (at -5.8 4.55 90) (layer F.SilkS))
    (fp_text value AGQ_Relay (at 0 0 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 3.3 2.54 270) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 45 "Net-(K1-Pad4)"))
    (pad 5 thru_hole circle (at 3.3 -2.54 270) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 44 "Net-(K1-Pad5)"))
    (pad 3 thru_hole circle (at 1.1 2.54 270) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 22 /FROM_BTNS))
    (pad 6 thru_hole circle (at 1.1 -2.54 270) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 43 "Net-(K1-Pad6)"))
    (pad 2 thru_hole circle (at -1.1 2.54 270) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 42 "Net-(K1-Pad2)"))
    (pad 7 thru_hole circle (at -1.1 -2.54 270) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 41 "Net-(K1-Pad7)"))
    (pad 1 thru_hole circle (at -4.3 2.54 270) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 8 thru_hole circle (at -4.3 -2.54 270) (size 1.4 1.4) (drill 0.85) (layers *.Cu *.Mask)
      (net 31 "Net-(D2-Pad1)"))
  )
  (module Connector_JST:JST_GH_SM04B-GHS-TB_1x04-1MP_P1.25mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 95.75 95.1 180)
    (descr "JST GH series connector, SM04B-GHS-TB (http://www.jst-mfg.com/product/pdf/eng/eGH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST GH top entry")
    (attr smd)
    (fp_text reference J2 (at 0 -3.9) (layer F.SilkS))
    (fp_text value Conn_01x04_Female (at 0 3.9) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad MP smd roundrect (at 3.725 1.35 180) (size 1 2.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad MP smd roundrect (at -3.725 1.35 180) (size 1 2.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at 1.875 -1.85 180) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 3 smd roundrect (at 0.625 -1.85 180) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /A&B_DASH_ERR))
    (pad 2 smd roundrect (at -0.625 -1.85 180) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /BMS_DASH_ERR))
    (pad 1 smd roundrect (at -1.875 -1.85 180) (size 0.6 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /BSPD_DASH_ERR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_GH_SM04B-GHS-TB_1x04-1MP_P1.25mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1210_3225Metric (layer F.Cu) (tedit 5B301BBE)
    (at 90.85 120.15 180)
    (descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.9 0 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 2.28) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 2.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HomeBrew:5x20_FuseBlank locked (layer F.Cu) (tedit 5E537535)
    (at 98.55 111.06 270)
    (fp_text reference F1 (at 3.69 -3.6 270) (layer F.SilkS))
    (fp_text value 5A (at 0.02 3.48 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -10.16 0 270) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 1 thru_hole rect (at -5.36 0 270) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole rect (at 5.36 0 90) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask)
      (net 16 /+12VF))
    (pad 2 thru_hole rect (at 10.16 0 90) (size 2.3 2.3) (drill 1.65) (layers *.Cu *.Mask)
      (net 16 /+12VF))
  )
  (module Connector_JST:JST_ZE_SM06B-ZESS-TB_1x06-1MP_P1.50mm_Horizontal (layer F.Cu) (tedit 5C2814BC)
    (at 106.95 107 90)
    (descr "JST ZE series connector, SM06B-ZESS-TB (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator")
    (tags "connector JST ZE horizontal")
    (attr smd)
    (fp_text reference J3 (at -5.55 -3 90) (layer F.SilkS))
    (fp_text value Conn_01x06_Female (at 0 6.68 270) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad MP smd roundrect (at 6.35 2.125 90) (size 1.8 3.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889))
    (pad MP smd roundrect (at -6.35 2.125 90) (size 1.8 3.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.138889))
    (pad 6 smd roundrect (at 3.75 -2.575 90) (size 0.8 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 5 smd roundrect (at 2.25 -2.575 90) (size 0.8 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (pad 4 smd roundrect (at 0.75 -2.575 90) (size 0.8 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /+12VF))
    (pad 3 smd roundrect (at -0.75 -2.575 90) (size 0.8 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /FROM_BTNS))
    (pad 2 smd roundrect (at -2.25 -2.575 90) (size 0.8 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /TO_PRE))
    (pad 1 smd roundrect (at -3.75 -2.575 90) (size 0.8 2.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 /TO_GO))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_ZE_SM06B-ZESS-TB_1x06-1MP_P1.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 89.9 96.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 94.15 126.75 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /TO_PRE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A429)
    (at 79 121.18 180)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference J5 (at 0 2.77) (layer B.SilkS))
    (fp_text value Conn_01x04_Male (at 0 -10.39) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 270) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /APPS_BSE_ON))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /BSPD_ON))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /IMD_ON))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /BMS_ON))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A420)
    (at 79 101.3 180)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.77) (layer B.SilkS))
    (fp_text value Conn_01x02_Male (at 0 -5.31) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SO-8_5.3x6.2mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 80.4 112.4 270)
    (descr "8-Lead Plastic Small Outline, 5.3x6.2mm Body (http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -4.13 90) (layer F.SilkS))
    (fp_text value LM393 (at 0 4.13 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 3.7 -1.905 270) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 7 smd rect (at 3.7 -0.635 270) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at 3.7 0.635 270) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R10-Pad1)"))
    (pad 5 smd rect (at 3.7 1.905 270) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R9-Pad2)"))
    (pad 4 smd rect (at -3.7 1.905 270) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 3 smd rect (at -3.7 0.635 270) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at -3.7 -0.635 270) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(R7-Pad1)"))
    (pad 1 smd rect (at -3.7 -1.905 270) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(Q5-Pad4)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-8_5.3x6.2mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 85.85 102.6 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference Q3 (at 0 3.4) (layer B.SilkS))
    (fp_text value FDS4897C (at 0 -3.4) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 8 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(D5-Pad1)"))
    (pad 7 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(D5-Pad1)"))
    (pad 6 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /A&B_DASH_ERR))
    (pad 5 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 28 /A&B_DASH_ERR))
    (pad 4 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(D5-Pad1)"))
    (pad 3 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (pad 2 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(Q3-Pad2)"))
    (pad 1 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 101.75 96.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 0 1.65 90) (layer B.SilkS))
    (fp_text value 470 (at -2.8 1.6 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 101.75 96.5 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at -2.45 0) (layer F.SilkS))
    (fp_text value BTNS (at 2.3 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /FROM_BTNS))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 80.4 112.35 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference Q5 (at 0 3.4 90) (layer B.SilkS))
    (fp_text value FDS6930B (at 0 -3.4 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 8 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(D3-Pad1)"))
    (pad 7 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(D3-Pad1)"))
    (pad 6 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(D7-Pad1)"))
    (pad 5 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(D7-Pad1)"))
    (pad 4 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(Q5-Pad4)"))
    (pad 3 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 2 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(Q5-Pad2)"))
    (pad 1 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 85.85 102.6)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference Q4 (at 0 3.4) (layer F.SilkS))
    (fp_text value FDS6930B (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(Q4-Pad7)"))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(Q4-Pad7)"))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(Q4-Pad2)"))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(Q4-Pad2)"))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(Q4-Pad4)"))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(Q4-Pad2)"))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 91.75 114 270)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference Q2 (at 0 -3.4 90) (layer F.SilkS))
    (fp_text value FDS4897C (at 0 3.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(D4-Pad1)"))
    (pad 7 smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(D4-Pad1)"))
    (pad 6 smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /BSPD_DASH_ERR))
    (pad 5 smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /BSPD_DASH_ERR))
    (pad 4 smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(D4-Pad1)"))
    (pad 3 smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (pad 2 smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(Q2-Pad2)"))
    (pad 1 smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 91.8 114 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference Q1 (at 0 3.4 90) (layer B.SilkS))
    (fp_text value FDS4897C (at 0 -3.4 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 8 smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D2-Pad1)"))
    (pad 7 smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D2-Pad1)"))
    (pad 6 smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 /BMS_DASH_ERR))
    (pad 5 smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 25 /BMS_DASH_ERR))
    (pad 4 smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D2-Pad1)"))
    (pad 3 smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (pad 2 smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(Q1-Pad2)"))
    (pad 1 smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_SMD:Potentiometer_Bourns_3214G_Horizontal (layer F.Cu) (tedit 5A3D7171)
    (at 109.5 118 180)
    (descr "Potentiometer, horizontal, Bourns 3214G, https://www.bourns.com/docs/Product-Datasheets/3214.pdf")
    (tags "Potentiometer horizontal Bourns 3214G")
    (attr smd)
    (fp_text reference RV1 (at 4.2 0.1 90) (layer F.SilkS))
    (fp_text value 100k (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 2.6 1.15 180) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 2 smd rect (at -2.6 0 180) (size 1.3 2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R7-Pad2)"))
    (pad 1 smd rect (at 2.6 -1.15 180) (size 1.3 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (model "D:/Users/John Praxious/Documents/KiCad/HomeBrew/3D/Bourns_3224G_Horiz.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 86.35 111.75 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 5k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(R10-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 85.35 115.45 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 5k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(R9-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 87.1 107.9 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 5k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(Q5-Pad4)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 98.55 112.9)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 1.65) (layer B.SilkS))
    (fp_text value 5k (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(R7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 92.6375 106.05 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 5k (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 92.6125 101.45 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(Q4-Pad7)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 103.05 120.4 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 1.65 270) (layer B.SilkS))
    (fp_text value 100k (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C1-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /TO_PRE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 92.65 106.05 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.65) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(Q4-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 +12V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 101.85 126.95)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.65 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(Q4-Pad4)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /TO_PRE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 103.9 96.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0.9 -1.7 90) (layer B.SilkS))
    (fp_text value 470 (at 2.3 0) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 106.05 96.5 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D7 (at -2.45 0 180) (layer F.SilkS))
    (fp_text value GO (at 2.3 0) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(D7-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 103.9 96.5 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D6 (at -2.45 0 180) (layer F.SilkS))
    (fp_text value PRE (at 3.6 0) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /TO_PRE))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(D6-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 89.9 96.5 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D5 (at -2.45 0 180) (layer F.SilkS))
    (fp_text value A&B (at 3.6 0) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 87.75 96.5 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at -2.45 0 180) (layer F.SilkS))
    (fp_text value BSPD (at 2.3 0) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 85.6 96.5 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at -2.45 0 180) (layer F.SilkS))
    (fp_text value IMD (at 3.6 0) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0805_2012Metric (layer F.Cu) (tedit 5B36C52C)
    (at 83.45 96.5 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at -2.45 0 180) (layer F.SilkS))
    (fp_text value BMS (at 2.3 0) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Shutdown Power Board v2020.1" (at 94.7 135.85) (layer B.SilkS))
  (gr_text "GND RTN" (at 93.85 94 270) (layer B.SilkS))
  (gr_text "FROM BTNS" (at 108.45 107.75) (layer B.SilkS))
  (gr_text "TO BTNS" (at 109.45 104.75) (layer B.SilkS))
  (gr_text "+12V IN" (at 109.65 106.25) (layer B.SilkS))
  (gr_text "TO PRE" (at 109.9 109.25) (layer B.SilkS))
  (gr_text "TO GO" (at 110.3 110.75) (layer B.SilkS))
  (gr_text "GND IN" (at 110.05 103.25) (layer B.SilkS))
  (gr_text "BSPD GO" (at 97.6 94.1 270) (layer B.SilkS))
  (gr_text "BMS GO" (at 96.35 93.75 270) (layer B.SilkS))
  (gr_text "A&B GO" (at 95.1 93.75 270) (layer B.SilkS))
  (gr_text GO (at 105.9 93.9 90) (layer F.SilkS))
  (gr_text PRE (at 103.6 93.5 90) (layer F.SilkS))
  (gr_text BTNS (at 101.3 93.1 90) (layer F.SilkS))
  (gr_text A&B (at 90.6 93.35 90) (layer F.SilkS))
  (gr_text BSPD (at 88.35 93.05 90) (layer F.SilkS))
  (gr_text IMD (at 85.95 93.7 90) (layer F.SilkS))
  (gr_text BMS (at 83.7 93.45 90) (layer F.SilkS))
  (dimension 3 (width 0.15) (layer Dwgs.User)
    (gr_text "3.000 mm" (at 77.5 135.75) (layer Dwgs.User))
    (feature1 (pts (xy 79 128.8) (xy 79 135.036421)))
    (feature2 (pts (xy 76 128.8) (xy 76 135.036421)))
    (crossbar (pts (xy 76 134.45) (xy 79 134.45)))
    (arrow1a (pts (xy 79 134.45) (xy 77.873496 135.036421)))
    (arrow1b (pts (xy 79 134.45) (xy 77.873496 133.863579)))
    (arrow2a (pts (xy 76 134.45) (xy 77.126504 135.036421)))
    (arrow2b (pts (xy 76 134.45) (xy 77.126504 133.863579)))
  )
  (dimension 10 (width 0.15) (layer Dwgs.User)
    (gr_text "10.000 mm" (at 70.1 133.8 90) (layer Dwgs.User))
    (feature1 (pts (xy 76 128.8) (xy 70.813579 128.8)))
    (feature2 (pts (xy 76 138.8) (xy 70.813579 138.8)))
    (crossbar (pts (xy 71.4 138.8) (xy 71.4 128.8)))
    (arrow1a (pts (xy 71.4 128.8) (xy 71.986421 129.926504)))
    (arrow1b (pts (xy 71.4 128.8) (xy 70.813579 129.926504)))
    (arrow2a (pts (xy 71.4 138.8) (xy 71.986421 137.673496)))
    (arrow2b (pts (xy 71.4 138.8) (xy 70.813579 137.673496)))
  )
  (dimension 3 (width 0.12) (layer Dwgs.User)
    (gr_text "3.000 mm" (at 77.5 84.53) (layer Dwgs.User))
    (feature1 (pts (xy 79 101.3) (xy 79 85.213579)))
    (feature2 (pts (xy 76 101.3) (xy 76 85.213579)))
    (crossbar (pts (xy 76 85.8) (xy 79 85.8)))
    (arrow1a (pts (xy 79 85.8) (xy 77.873496 86.386421)))
    (arrow1b (pts (xy 79 85.8) (xy 77.873496 85.213579)))
    (arrow2a (pts (xy 76 85.8) (xy 77.126504 86.386421)))
    (arrow2b (pts (xy 76 85.8) (xy 77.126504 85.213579)))
  )
  (dimension 10 (width 0.12) (layer Dwgs.User)
    (gr_text "10.000 mm" (at 70.28 96.3 270) (layer Dwgs.User))
    (feature1 (pts (xy 76 101.3) (xy 70.963579 101.3)))
    (feature2 (pts (xy 76 91.3) (xy 70.963579 91.3)))
    (crossbar (pts (xy 71.55 91.3) (xy 71.55 101.3)))
    (arrow1a (pts (xy 71.55 101.3) (xy 70.963579 100.173496)))
    (arrow1b (pts (xy 71.55 101.3) (xy 72.136421 100.173496)))
    (arrow2a (pts (xy 71.55 91.3) (xy 70.963579 92.426504)))
    (arrow2b (pts (xy 71.55 91.3) (xy 72.136421 92.426504)))
  )
  (dimension 47.5 (width 0.12) (layer Dwgs.User)
    (gr_text "47.500 mm" (at 72.731534 115.05 270) (layer Dwgs.User))
    (feature1 (pts (xy 76 138.8) (xy 73.415113 138.8)))
    (feature2 (pts (xy 76 91.3) (xy 73.415113 91.3)))
    (crossbar (pts (xy 74.001534 91.3) (xy 74.001534 138.8)))
    (arrow1a (pts (xy 74.001534 138.8) (xy 73.415113 137.673496)))
    (arrow1b (pts (xy 74.001534 138.8) (xy 74.587955 137.673496)))
    (arrow2a (pts (xy 74.001534 91.3) (xy 73.415113 92.426504)))
    (arrow2b (pts (xy 74.001534 91.3) (xy 74.587955 92.426504)))
  )
  (dimension 37.5 (width 0.12) (layer Dwgs.User)
    (gr_text "37.500 mm" (at 94.75 87.279936) (layer Dwgs.User))
    (feature1 (pts (xy 113.5 91.3) (xy 113.5 87.963515)))
    (feature2 (pts (xy 76 91.3) (xy 76 87.963515)))
    (crossbar (pts (xy 76 88.549936) (xy 113.5 88.549936)))
    (arrow1a (pts (xy 113.5 88.549936) (xy 112.373496 89.136357)))
    (arrow1b (pts (xy 113.5 88.549936) (xy 112.373496 87.963515)))
    (arrow2a (pts (xy 76 88.549936) (xy 77.126504 89.136357)))
    (arrow2b (pts (xy 76 88.549936) (xy 77.126504 87.963515)))
  )
  (gr_circle (center 110.3 94.5) (end 112 94.5) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 110.3 135.6) (end 112 135.6) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 79.2 135.6) (end 80.9 135.6) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 79.2 94.5) (end 80.9 94.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.5 138.8) (end 76 138.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.5 91.3) (end 113.5 138.8) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76 91.3) (end 113.5 91.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 76 138.8) (end 76 91.3) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.4 97.7) (xy 76 97.7) (xy 76 91.3) (xy 82.4 91.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.4 138.8) (xy 76 138.8) (xy 76 132.4) (xy 82.4 132.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.5 138.8) (xy 107.1 138.8) (xy 107.1 132.4) (xy 113.5 132.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.5 97.7) (xy 107.1 97.7) (xy 107.1 91.3) (xy 113.5 91.3)
      )
    )
  )
)
