(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 23)
    (no_connects 0)
    (area 145.842667 79.24328 178.007334 132.609599)
    (thickness 1.6)
    (drawings 16)
    (tracks 99)
    (zones 0)
    (modules 5)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 4.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 MISO)
  (net 4 MOSI)
  (net 5 SCK)
  (net 6 NSS)
  (net 7 RESET)
  (net 8 DIO0)
  (net 9 DIO1)
  (net 10 DIO2)
  (net 11 DIO3)
  (net 12 DIO4)
  (net 13 DIO5)
  (net 14 ANT)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net ANT)
    (add_net DIO0)
    (add_net DIO1)
    (add_net DIO2)
    (add_net DIO3)
    (add_net DIO4)
    (add_net DIO5)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net NSS)
    (add_net RESET)
    (add_net SCK)
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58F85E5C)
    (at 150.114 88.884 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 58F85E7A)
    (at 149.86 93.98)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at 1.016 22.098) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 MISO))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 MOSI))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 SCK))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 NSS))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 RESET))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 58F85E77)
    (at 172.72 93.98)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at 0.254 20.574) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 DIO0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 DIO1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 DIO2))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 DIO3))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 DIO4))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 DIO5))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Antenna:SMA-RF+HOLE (layer F.Cu) (tedit 58F85FCD)
    (at 170.12 87.63)
    (fp_text reference U1 (at -16.2814 -5.6134) (layer F.SilkS))
    (fp_text value SMA-RF+HOLE (at -12.07008 -7.41172) (layer F.Fab))
    (pad 2 thru_hole trapezoid (at 0 0) (size 1.6 4.2) (drill 0.8 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 14 ANT))
    (pad 1 smd rect (at -2.6 0) (size 1.6 4.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.6 0) (size 1.6 4.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -2.6 0) (size 1.6 4.2) (layers B.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.6 0) (size 1.6 4.2) (layers B.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module RFM69:RFM69HCW (layer F.Cu) (tedit 58F77996)
    (at 154.37 109.345 90)
    (fp_text reference U2 (at -19.01698 -2.33972 90) (layer F.SilkS))
    (fp_text value RFM69HCW (at -19.01698 -3.33972 90) (layer F.Fab))
    (fp_text user IC (at 3.937 1.48844 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole rect (at 0 2 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 MISO))
    (pad 3 thru_hole rect (at 0 4 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 MOSI))
    (pad 4 thru_hole rect (at 0 6 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 SCK))
    (pad 5 thru_hole rect (at 0 8 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 NSS))
    (pad 6 thru_hole rect (at 0 10 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 RESET))
    (pad 7 thru_hole rect (at 0 12 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 DIO5))
    (pad 8 thru_hole rect (at 0 14 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 16 thru_hole rect (at 16 0 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 DIO2))
    (pad 15 thru_hole rect (at 16 2 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 DIO1))
    (pad 14 thru_hole rect (at 16 4 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 DIO0))
    (pad 13 thru_hole rect (at 16 6 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 12 thru_hole rect (at 16 8 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 DIO4))
    (pad 11 thru_hole rect (at 16 10 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 DIO3))
    (pad 10 thru_hole rect (at 16 12 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole rect (at 16 14 90) (size 3 1) (drill 0.762) (layers *.Cu *.Mask)
      (net 14 ANT))
  )
  (gr_text "By Eikacy\nUC 2017/04\n" (at 158.496 88.392) (layer B.Cu))
  (gr_text DIO0 (at 171.704 91.694) (layer B.SilkS))
  (gr_text GND (at 170.18 109.474 90) (layer B.SilkS))
  (gr_text RST (at 152.4 109.728 90) (layer B.SilkS))
  (gr_text VCC (at 150.622 91.694) (layer B.SilkS))
  (gr_text "GND\nMISO\nMOSI\nSCK\nNSS" (at 151.638 101.6) (layer B.SilkS))
  (gr_text "DIO1\nDIO2\nDIO3\nDIO4\nDIO5" (at 168.402 101.6) (layer B.SilkS))
  (gr_arc (start 173.482 110.998) (end 173.99 110.998) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.098 110.998) (end 149.098 111.506) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 149.098 85.852) (end 148.59 85.852) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.482 85.852) (end 173.482 85.344) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "RFM69 Breakout" (at 159.258 88.392) (layer F.SilkS))
  (gr_line (start 173.482 85.344) (end 149.098 85.344) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.99 110.998) (end 173.99 85.852) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 110.998) (end 148.59 85.852) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.482 111.506) (end 149.098 111.506) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 173.736 111.252) (xy 148.844 111.252) (xy 148.844 85.598) (xy 173.736 85.598)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.844 111.252) (xy 173.736 111.252) (xy 173.736 85.598) (xy 148.844 85.598)
      )
    )
  )
)
