(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 96)
    (zones 0)
    (modules 10)
    (nets 14)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4064)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(S1-Pad11)")
  (net 2 "Net-(X1-Pad1)")
  (net 3 "Net-(+5V1-Pad1)")
  (net 4 "Net-(COM1-Pad1)")
  (net 5 "Net-(B1-Pad1)")
  (net 6 "Net-(A1-Pad1)")
  (net 7 "Net-(S1-Pad16)")
  (net 8 "Net-(S1-Pad3)")
  (net 9 "Net-(S1-Pad4)")
  (net 10 "Net-(S1-Pad1)")
  (net 11 "Net-(S1-Pad2)")
  (net 12 "Net-(X1-Pad6)")
  (net 13 "Net-(X1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.4064)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(+5V1-Pad1)")
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(B1-Pad1)")
    (add_net "Net-(COM1-Pad1)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(S1-Pad11)")
    (add_net "Net-(S1-Pad16)")
    (add_net "Net-(S1-Pad2)")
    (add_net "Net-(S1-Pad3)")
    (add_net "Net-(S1-Pad4)")
    (add_net "Net-(X1-Pad1)")
    (add_net "Net-(X1-Pad3)")
    (add_net "Net-(X1-Pad6)")
  )
  (module "Encoder Inverting Connector:SMD1,27-2,54" (layer Bottom) (tedit 5BB2638C)
    (at 152.654 105.664)
    (descr "<b>SMD PAD</b>")
    (fp_text reference +5V (at 0.47 -5.194 90) (layer B.SilkS))
    (fp_text value SMD2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 3 "Net-(+5V1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:SMD1,27-2,54" (layer Bottom) (tedit 5BB26397)
    (at 155.829 105.664)
    (descr "<b>SMD PAD</b>")
    (fp_text reference A (at 0.597 -3.035 90) (layer B.SilkS))
    (fp_text value SMD2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 6 "Net-(A1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:SMD1,27-2,54" (layer Bottom) (tedit 5BB26366)
    (at 141.224 105.664)
    (descr "<b>SMD PAD</b>")
    (fp_text reference B (at 0.597 -3.035 90) (layer B.SilkS))
    (fp_text value SMD2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 5 "Net-(B1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:SMD1,27-2,54" (layer Bottom) (tedit 5BB26382)
    (at 150.495 105.664)
    (descr "<b>SMD PAD</b>")
    (fp_text reference COM (at 0.47 -5.194 90) (layer B.SilkS))
    (fp_text value SMD2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 4 "Net-(COM1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:CHS-08B" (layer Top) (tedit 0)
    (at 144.018 101.473)
    (descr "8 bits, gull wing")
    (fp_text reference S1 (at -1.905 2.54 90) (layer F.SilkS) hide)
    (fp_text value CHS-08TB (at 12.065 2.54 90) (layer F.Fab) hide)
    (fp_text user O (at 0.3175 -1.5875 90) (layer F.SilkS))
    (fp_text user N (at 1.5875 -1.5875 90) (layer F.SilkS))
    (fp_text user 1 (at 0.3175 1.905 90) (layer F.SilkS))
    (fp_text user 2 (at 1.5875 1.905 90) (layer F.SilkS))
    (fp_text user 3 (at 2.8575 1.905 90) (layer F.SilkS))
    (fp_text user 4 (at 4.1275 1.905 90) (layer F.SilkS))
    (fp_text user 5 (at 5.3975 1.905 90) (layer F.SilkS))
    (fp_text user 6 (at 6.6675 1.905 90) (layer F.SilkS))
    (fp_text user 7 (at 7.9375 1.905 90) (layer F.SilkS))
    (fp_text user 8 (at 9.2075 1.905 90) (layer F.SilkS))
    (pad 1 smd rect (at 0 3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 10 "Net-(S1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 1.27 3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 11 "Net-(S1-Pad2)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at 3.81 3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 9 "Net-(S1-Pad4)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 2.54 3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 8 "Net-(S1-Pad3)") (solder_mask_margin 0.1016))
    (pad 5 smd rect (at 5.08 3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 11 "Net-(S1-Pad2)") (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 6.35 3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 10 "Net-(S1-Pad1)") (solder_mask_margin 0.1016))
    (pad 7 smd rect (at 7.62 3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 9 "Net-(S1-Pad4)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at 8.89 3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 8 "Net-(S1-Pad3)") (solder_mask_margin 0.1016))
    (pad 9 smd rect (at 8.89 -3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 7 "Net-(S1-Pad16)") (solder_mask_margin 0.1016))
    (pad 10 smd rect (at 7.62 -3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 5 "Net-(B1-Pad1)") (solder_mask_margin 0.1016))
    (pad 11 smd rect (at 6.35 -3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 1 "Net-(S1-Pad11)") (solder_mask_margin 0.1016))
    (pad 12 smd rect (at 5.08 -3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 6 "Net-(A1-Pad1)") (solder_mask_margin 0.1016))
    (pad 13 smd rect (at 3.81 -3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 6 "Net-(A1-Pad1)") (solder_mask_margin 0.1016))
    (pad 14 smd rect (at 2.54 -3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 1 "Net-(S1-Pad11)") (solder_mask_margin 0.1016))
    (pad 15 smd rect (at 1.27 -3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 5 "Net-(B1-Pad1)") (solder_mask_margin 0.1016))
    (pad 16 smd rect (at 0 -3.81) (size 0.76 1.27) (layers Top F.Paste F.Mask)
      (net 7 "Net-(S1-Pad16)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:M09D" (layer Top) (tedit 5BB26457)
    (at 148.48205 117.856 180)
    (descr <b>SUB-D</b>)
    (fp_text reference X1 (at -11.15 6.7 180) (layer F.SilkS) hide)
    (fp_text value 172-E09-103R001 (at 1.27 10.16 180) (layer F.Fab) hide)
    (fp_text user 1 (at 4.85 2.1786 180) (layer F.SilkS) hide)
    (fp_text user 5 (at -6.1 2.2 180) (layer F.SilkS) hide)
    (fp_text user 9 (at -3.5 2.1966 180) (layer B.SilkS) hide)
    (fp_text user 6 (at 4.55 2.2 180) (layer B.SilkS) hide)
    (fp_text user Board (at 11.43 2.54 180) (layer Cmts.User))
    (fp_text user M09D (at -7.62 -5.969 180) (layer F.Fab))
    (fp_text user "Board " (at -16.51 2.54 180) (layer Cmts.User))
    (pad 1 smd rect (at 5.4862 6.0448 180) (size 1.7 3.5) (layers Top F.Paste F.Mask)
      (net 2 "Net-(X1-Pad1)") (solder_mask_margin 0.1016))
    (pad 2 smd rect (at 2.75 6.05 180) (size 1.7 3.5) (layers Top F.Paste F.Mask)
      (net 4 "Net-(COM1-Pad1)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at 0 6.045 180) (size 1.7 3.5) (layers Top F.Paste F.Mask)
      (net 13 "Net-(X1-Pad3)") (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -2.7434 6.0448 180) (size 1.7 3.5) (layers Top F.Paste F.Mask)
      (net 10 "Net-(S1-Pad1)") (solder_mask_margin 0.1016))
    (pad 5 smd rect (at -5.5 6.05 180) (size 1.7 3.5) (layers Top F.Paste F.Mask)
      (net 8 "Net-(S1-Pad3)") (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 4.1 6.05 180) (size 1.7 3.5) (layers Bottom B.Paste B.Mask)
      (net 12 "Net-(X1-Pad6)") (solder_mask_margin 0.1016))
    (pad 7 smd rect (at 1.35 6.0452 180) (size 1.7 3.5) (layers Bottom B.Paste B.Mask)
      (net 11 "Net-(S1-Pad2)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -1.4 6.0452 180) (size 1.7 3.5) (layers Bottom B.Paste B.Mask)
      (net 9 "Net-(S1-Pad4)") (solder_mask_margin 0.1016))
    (pad 9 smd rect (at -4.15 6.05 180) (size 1.7 3.5) (layers Bottom B.Paste B.Mask)
      (net 3 "Net-(+5V1-Pad1)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:SMD1,27-2,54" (layer Bottom) (tedit 5BB2636F)
    (at 145.288 105.664)
    (descr "<b>SMD PAD</b>")
    (fp_text reference X (at 0.597 -3.035 90) (layer B.SilkS))
    (fp_text value SMD2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 12 "Net-(X1-Pad6)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:SMD1,27-2,54" (layer Bottom) (tedit 5BB263A0)
    (at 158.115 105.664)
    (descr "<b>SMD PAD</b>")
    (fp_text reference ~A~ (at 0.597 -3.035 90) (layer B.SilkS))
    (fp_text value SMD2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 1 "Net-(S1-Pad11)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:SMD1,27-2,54" (layer Bottom) (tedit 5BB2635B)
    (at 138.938 105.664)
    (descr "<b>SMD PAD</b>")
    (fp_text reference ~B~ (at 0.597 -3.035 90) (layer B.SilkS))
    (fp_text value SMD2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 7 "Net-(S1-Pad16)") (solder_mask_margin 0.1016))
  )
  (module "Encoder Inverting Connector:SMD1,27-2,54" (layer Bottom) (tedit 5BB26378)
    (at 147.447 105.664)
    (descr "<b>SMD PAD</b>")
    (fp_text reference ~X~ (at 0.597 -3.035 90) (layer B.SilkS))
    (fp_text value SMD2 (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 13 "Net-(X1-Pad3)") (solder_mask_margin 0.1016))
  )
  (gr_line (start 138.9761 113.6396) (end 157.988 113.6396) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.432223 98.3996) (end 158.7881 98.3996) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.2141 98.399602) (end 139.569977 98.3996) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.4521 99.161602) (end 137.4521 112.115602) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.9868 96.367602) (end 143.0154 96.367602) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.5501 112.115602) (end 159.5501 99.161602) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.9761 112.115602) (end 137.4521 112.115602) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 138.2141 99.161602) (end 138.2141 98.399602) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.56998 95.224603) (end 139.569981 98.399602) (angle -61.061402) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.015399 97.129604) (end 143.0154 96.367602) (angle -61.061494) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 153.986798 97.129602) (end 154.653659 96.760893) (angle -61.061608) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157.432224 95.224604) (end 154.653659 96.760893) (angle -61.061339) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.7881 99.161602) (end 159.5501 99.161602) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 158.0261 112.115602) (end 158.0261 113.639602) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text "1-4 ON/5-8 OFF\nNORMAL\n1-4 OFF/5-8 ON\nINVERTED" (at 154.686 103.886 90) (layer F.SilkS))
  (gr_text "CENTROID\nENCODER\nADAPTER" (at 141.478 105.791 90) (layer F.SilkS))
)
