(kicad_pcb (version 20171130) (host pcbnew "(5.1.0)-1")
  (general
    (thickness 1.2)
    (drawings 36)
    (tracks 58)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 7)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerberFinalFinal"))
  )
  (net 0 "")
  (net 1 /+3.3)
  (net 2 GND)
  (net 3 /INT)
  (net 4 /CLK)
  (net 5 /DO)
  (net 6 /DI)
  (net 7 /CS)
  (net 8 "Net-(J1-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+3.3)
    (add_net /CLK)
    (add_net /CS)
    (add_net /DI)
    (add_net /DO)
    (add_net /INT)
    (add_net GND)
    (add_net "Net-(J1-Pad8)")
  )
  (module gc_sp2:SP2_FootPrint (layer F.Cu) (tedit 5BB4D81F)
    (at 75.5 115.9)
    (attr smd)
    (fp_text reference P1 (at -0.5 4.75) (layer F.SilkS))
    (fp_text value SerialPort (at 4.5 4.75) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1.5 7) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3))
    (pad 2 smd rect (at 1 0) (size 1.5 7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2 0) (size 1.5 7) (layers F.Cu F.Paste F.Mask)
      (net 3 /INT))
    (pad 4 smd rect (at 3 0) (size 1.5 7) (layers B.Cu B.Adhes B.Mask)
      (net 4 /CLK))
    (pad 5 smd rect (at 4 0) (size 1.5 7) (layers F.Cu F.Paste F.Mask)
      (net 6 /DI))
    (pad 6 smd rect (at 5 0) (size 1.5 7) (layers B.Cu B.Paste B.Mask)
      (net 5 /DO))
    (pad 7 smd rect (at 6 0) (size 1.5 7) (layers F.Cu F.Paste F.Mask)
      (net 7 /CS))
    (pad 8 smd rect (at 7 0) (size 1.5 7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
  )
  (module gc_sp2:1050270001 (layer F.Cu) (tedit 5BB4CF60)
    (at 96.1 110.3 180)
    (attr smd)
    (fp_text reference J1 (at 9 -8) (layer F.SilkS))
    (fp_text value Micro_SD_Card (at 4 -3.9 180) (layer F.Fab))
    (pad 8 smd rect (at 0 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad8)"))
    (pad 7 smd rect (at 1.1 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /DO))
    (pad 6 smd rect (at 2.2 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 3.3 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /CLK))
    (pad "" smd rect (at 4.05 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 4.75 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3))
    (pad 3 smd rect (at 5.5 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /DI))
    (pad 2 smd rect (at 6.6 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /CS))
    (pad 1 smd rect (at 7.7 0 180) (size 0.5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /INT))
    (pad 9 smd rect (at 9 -1.61 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 9 -6.06 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -1.3 -1.61 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -1.3 -6.06 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5BB4D9BD)
    (at 80.92 106.83)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 4.01 0.07 90) (layer F.SilkS))
    (fp_text value .1 (at 3.1 0) (layer F.Fab) hide)
    (fp_text user %R (at 4.03 0.16 -90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 /+3.3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 75.1 119.4) (end 74.5 119.4) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 82.9 119.4) (end 82.9 120) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text DI (at 80.5 111.6 90) (layer B.SilkS))
  (gr_text CLK (at 78.6 110.9 90) (layer B.SilkS))
  (gr_text GND (at 76.6 110.9 90) (layer B.SilkS))
  (gr_text GND (at 82.6 110.8 90) (layer B.SilkS))
  (gr_text +3.3 (at 75.5 110.9 90) (layer F.SilkS))
  (gr_text INT (at 77.6 111.4 90) (layer F.SilkS))
  (gr_text DO (at 79.6 111.5 90) (layer F.SilkS))
  (gr_text CS (at 81.5 111.5 90) (layer F.SilkS))
  (gr_text 7 (at 95 109.05) (layer F.SilkS))
  (gr_text 6 (at 93.9 109) (layer F.SilkS))
  (gr_text 5 (at 92.85 109) (layer F.SilkS))
  (gr_text 4 (at 91.4 109) (layer F.SilkS))
  (gr_text 3 (at 90.6 109) (layer F.SilkS))
  (gr_text 2 (at 89.5 109) (layer F.SilkS))
  (gr_text 1 (at 88.45 109) (layer F.SilkS))
  (gr_text 8 (at 96.1 109.05) (layer F.SilkS))
  (gr_text "SD2SP2 1.2a" (at 68.49 110.42) (layer F.SilkS))
  (gr_text @citrus3000psi (at 69.25 111.7) (layer F.SilkS))
  (gr_text "THIS SIDE FACE\nOUTSIDE" (at 73.55 105.7) (layer B.SilkS))
  (gr_line (start 83.75 105.5) (end 83.75 100.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.5 105.5) (end 83.75 105.5) (layer Edge.Cuts) (width 0.15))
  (gr_text "THIS SIDE FACE \nINSIDE" (at 74.05 105.7) (layer F.SilkS))
  (gr_line (start 75.1 120) (end 82.9 120) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.5 113) (end 74.5 119.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.5 113) (end 74.5 113) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.5 113) (end 83.5 119.4) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.5 113) (end 85.5 113) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 85.5 120) (end 85.5 113) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.5 120) (end 72.5 113) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.5 120) (end 85.5 120) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63 120) (end 72.5 120) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63 120) (end 63 100.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.5 105.5) (end 99.5 120) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63 100.5) (end 83.75 100.5) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 120) (xy 72.5 120) (xy 72.5 113) (xy 85.5 113) (xy 85.5 120)
        (xy 99.5 120) (xy 99.5 105.5) (xy 83.75 105.5) (xy 83.75 100.5) (xy 63 100.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 120) (xy 72.5 120) (xy 72.5 113) (xy 85.5 113) (xy 85.5 120)
        (xy 99.4 120) (xy 99.5 105.5) (xy 83.75 105.5) (xy 83.75 100.5) (xy 63 100.5)
      )
    )
  )
)
