(kicad_pcb (version 20171130) (host pcbnew 5.1.5)
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 146)
    (zones 0)
    (modules 23)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 35 31)
    (grid_origin 35 31)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/daniel/kicad/gerber/4/rgb_trinitron/"))
  )
  (net 0 "")
  (net 1 "Net-(C5-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C10-Pad2)")
  (net 4 "Net-(RV2-Pad2)")
  (net 5 "Net-(RV3-Pad2)")
  (net 6 /RIN)
  (net 7 "Net-(C1-Pad1)")
  (net 8 "Net-(C2-Pad1)")
  (net 9 /GIN)
  (net 10 /BIN)
  (net 11 "Net-(C3-Pad1)")
  (net 12 "Net-(C4-Pad2)")
  (net 13 /COMPOSITE)
  (net 14 +15V)
  (net 15 /VBIAS)
  (net 16 "Net-(C8-Pad1)")
  (net 17 -15V)
  (net 18 +9V)
  (net 19 "Net-(J1-Pad1)")
  (net 20 /R)
  (net 21 "Net-(J1-Pad3)")
  (net 22 /L)
  (net 23 "Net-(J1-Pad8)")
  (net 24 "Net-(J1-Pad10)")
  (net 25 "Net-(J1-Pad12)")
  (net 26 "Net-(J1-Pad16)")
  (net 27 "Net-(J1-Pad19)")
  (net 28 /CSYNC)
  (net 29 /BOUT)
  (net 30 /GOUT)
  (net 31 /ROUT)
  (net 32 "Net-(J3-Pad4)")
  (net 33 "Net-(J3-Pad2)")
  (net 34 "Net-(RV4-Pad2)")
  (net 35 "Net-(U2-Pad7)")
  (net 36 "Net-(U2-Pad3)")
  (net 37 "Net-(U2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +15V)
    (add_net +9V)
    (add_net -15V)
    (add_net /BIN)
    (add_net /BOUT)
    (add_net /COMPOSITE)
    (add_net /CSYNC)
    (add_net /GIN)
    (add_net /GOUT)
    (add_net /L)
    (add_net /R)
    (add_net /RIN)
    (add_net /ROUT)
    (add_net /VBIAS)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(RV2-Pad2)")
    (add_net "Net-(RV3-Pad2)")
    (add_net "Net-(RV4-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad7)")
  )
  (module pcb:teapot (layer B.Cu) (tedit 0)
    (at 109 43 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 119.6 54.8)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 1-10uF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /RIN))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 119.6 47.2)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 1-10uF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /GIN))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 119.6 39.6)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 1-10uF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /BIN))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 122.6 61.4 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C4 (at 2.2 2.4) (layer F.SilkS))
    (fp_text value 2.2nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D4.0mm_P2.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 114.8 35.6)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C5 (at -2.6 0.6) (layer F.SilkS))
    (fp_text value 0.1uF (at 1 3.31) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 /COMPOSITE))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 104.6 21.2 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C6 (at 2.4 2.6) (layer F.SilkS))
    (fp_text value 2.2nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 +15V))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 117.6 66.6)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C7 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 2.2nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VBIAS))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D4.0mm_P2.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 110.8 19.2)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 4mm Electrolytic Capacitor")
    (fp_text reference C8 (at -3 -1.2) (layer F.SilkS))
    (fp_text value 0.1uF (at 1 3.31) (layer F.Fab))
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 16 "Net-(C8-Pad1)"))
    (pad 2 thru_hole circle (at 2 0) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D4.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 99.6 26.4)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C9 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 2.2nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 -15V))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 120.6 21.8 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C10 (at 2.5 -2.56 90) (layer F.SilkS))
    (fp_text value 510pF (at 2.5 2.56 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 99.6 31.4)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C11 (at 2.5 -2.56) (layer F.SilkS))
    (fp_text value 2.2nF (at 2.5 2.56) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +9V))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pcb2:SCART-F (layer F.Cu) (tedit 5E45562F)
    (at 133.4 47.2 90)
    (descr "TV SCART <B>CONNECTOR</B>")
    (fp_text reference J1 (at -25.4 -3.937 90) (layer F.SilkS))
    (fp_text value SCART-F (at -11.557 9.271 90) (layer F.Fab))
    (fp_text user 3,0 (at 24.765 7.112 90) (layer Dwgs.User))
    (fp_text user 1 (at 19.939 2.286 90) (layer F.SilkS))
    (fp_text user 21 (at -21.336 2.286 90) (layer F.SilkS))
    (fp_text user long (at 31.877 7.62 90) (layer Dwgs.User))
    (fp_text user SCART-F (at -9.779 5.08 90) (layer F.SilkS))
    (fp_text user 3,0~ (at -28.067 7.112 90) (layer Dwgs.User))
    (fp_text user long~ (at -29.083 7.747 90) (layer Dwgs.User))
    (pad 1 thru_hole oval (at 19.05 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 17.145 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 20 /R))
    (pad 3 thru_hole oval (at 15.24 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 13.335 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 11.43 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 9.525 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 22 /L))
    (pad 7 thru_hole oval (at 7.62 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 10 /BIN))
    (pad 8 thru_hole oval (at 5.715 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 3.81 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 1.905 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 9 /GIN))
    (pad 12 thru_hole oval (at -1.905 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at -3.81 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 14 thru_hole oval (at -5.715 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 15 thru_hole oval (at -7.62 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 6 /RIN))
    (pad 16 thru_hole oval (at -9.525 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at -11.43 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at -13.335 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 19 thru_hole oval (at -15.24 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad19)"))
    (pad 20 thru_hole oval (at -17.145 0 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 13 /COMPOSITE))
    (pad 21 thru_hole oval (at -19.05 -5.08 90) (size 1.9812 3.9624) (drill 1.3208) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad None np_thru_hole circle (at 26.416 -0.254 90) (size 3.0226 3.0226) (drill 3.0226) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at 26.416 3.302 90) (size 3.0226 3.0226) (drill 3.0226) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -26.416 -0.254 90) (size 3.0226 3.0226) (drill 3.0226) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -26.416 3.302 90) (size 3.0226 3.0226) (drill 3.0226) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 96.4 74.4 180)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /CSYNC))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /R))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /L))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /BOUT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /GOUT))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /ROUT))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x06_Pitch2.54mm.wrl
      (offset (xyz 0 -6.349999904632568 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 96.4 21.2)
    (descr "Through hole straight socket strip, 1x05, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +9V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 -15V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 +15V))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x05_Pitch2.54mm.wrl
      (offset (xyz 0 -5.079999923706055 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 115.6 19.2)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 2.54 -1.86) (layer F.SilkS))
    (fp_text value 680K (at 2.54 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(C8-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 120.6 29.2 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 -1.86 90) (layer F.SilkS))
    (fp_text value 620 (at 2.54 1.86 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(C5-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(C10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 107.4 56.4)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value TL084 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VBIAS))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /GOUT))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VBIAS))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(RV3-Pad2)"))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VBIAS))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 -15V))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 +15V))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VBIAS))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /VBIAS))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(RV4-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(RV2-Pad2)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /BOUT))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /ROUT))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 117 31.4 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value LM1881 (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +9V))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U2-Pad7)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad3)"))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(C8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C10-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad5)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /CSYNC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_ACP_CA9h2.5_Vertical_Px2.5mm_Py5.0mm (layer F.Cu) (tedit 58826B0A)
    (at 100.4 46.8)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, Vishay T73XX Single, Vishay T73XX Single, Vishay T73YP Single, Piher PT-6h Single, Piher PT-6v Single, Piher PT-6v Single, Piher PT-10h2.5 Single, Piher PT-10h5 Single, Piher PT-101h3.8 Single, Piher PT-10v10 Single, Piher PT-10v10 Single, Piher PT-10v5 Single, Piher PT-15h5 Single, Piher PT-15h2.5 Single, Piher PT-15B Single, Piher PT-15hc5 Single, Piher PT-15v12.5 Single, Piher PT-15v12.5 Single, Piher PT-15v15 Single, Piher PT-15v15 Single, ACP CA6h Single, ACP CA6v Single, ACP CA6v Single, ACP CA6VSMD Single, ACP CA6VSMD Single, ACP CA9h2.5 Single, http://www.acptechnologies.com/wp-content/uploads/2016/12/ACP-CAT%C3%81LOGO-ENTERO-2016.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single  Vishay T73XX Single  Vishay T73XX Single  Vishay T73YP Single  Piher PT-6h Single  Piher PT-6v Single  Piher PT-6v Single  Piher PT-10h2.5 Single  Piher PT-10h5 Single  Piher PT-101h3.8 Single  Piher PT-10v10 Single  Piher PT-10v10 Single  Piher PT-10v5 Single  Piher PT-15h5 Single  Piher PT-15h2.5 Single  Piher PT-15B Single  Piher PT-15hc5 Single  Piher PT-15v12.5 Single  Piher PT-15v12.5 Single  Piher PT-15v15 Single  Piher PT-15v15 Single  ACP CA6h Single  ACP CA6v Single  ACP CA6v Single  ACP CA6VSMD Single  ACP CA6VSMD Single  ACP CA9h2.5 Single")
    (fp_text reference RV1 (at 2.8 -6.6) (layer F.SilkS))
    (fp_text value "POT_TRIM 50K" (at 0 8.65) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.5 2.5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 12 "Net-(C4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 14 +15V))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA9h2.5_Vertical_Px2.5mm_Py5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_ACP_CA9h2.5_Vertical_Px2.5mm_Py5.0mm (layer F.Cu) (tedit 58826B0A)
    (at 100.4 57.6)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, Vishay T73XX Single, Vishay T73XX Single, Vishay T73YP Single, Piher PT-6h Single, Piher PT-6v Single, Piher PT-6v Single, Piher PT-10h2.5 Single, Piher PT-10h5 Single, Piher PT-101h3.8 Single, Piher PT-10v10 Single, Piher PT-10v10 Single, Piher PT-10v5 Single, Piher PT-15h5 Single, Piher PT-15h2.5 Single, Piher PT-15B Single, Piher PT-15hc5 Single, Piher PT-15v12.5 Single, Piher PT-15v12.5 Single, Piher PT-15v15 Single, Piher PT-15v15 Single, ACP CA6h Single, ACP CA6v Single, ACP CA6v Single, ACP CA6VSMD Single, ACP CA6VSMD Single, ACP CA9h2.5 Single, http://www.acptechnologies.com/wp-content/uploads/2016/12/ACP-CAT%C3%81LOGO-ENTERO-2016.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single  Vishay T73XX Single  Vishay T73XX Single  Vishay T73YP Single  Piher PT-6h Single  Piher PT-6v Single  Piher PT-6v Single  Piher PT-10h2.5 Single  Piher PT-10h5 Single  Piher PT-101h3.8 Single  Piher PT-10v10 Single  Piher PT-10v10 Single  Piher PT-10v5 Single  Piher PT-15h5 Single  Piher PT-15h2.5 Single  Piher PT-15B Single  Piher PT-15hc5 Single  Piher PT-15v12.5 Single  Piher PT-15v12.5 Single  Piher PT-15v15 Single  Piher PT-15v15 Single  ACP CA6h Single  ACP CA6v Single  ACP CA6v Single  ACP CA6VSMD Single  ACP CA6VSMD Single  ACP CA9h2.5 Single")
    (fp_text reference RV2 (at 2.8 -15.8) (layer F.SilkS))
    (fp_text value "POT_TRIM 50K" (at 0 8.65) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 31 /ROUT))
    (pad 2 thru_hole circle (at 2.5 2.5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(RV2-Pad2)"))
    (pad 3 thru_hole circle (at 0 5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(C1-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA9h2.5_Vertical_Px2.5mm_Py5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_ACP_CA9h2.5_Vertical_Px2.5mm_Py5.0mm (layer F.Cu) (tedit 58826B0A)
    (at 100.5 68.4)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, Vishay T73XX Single, Vishay T73XX Single, Vishay T73YP Single, Piher PT-6h Single, Piher PT-6v Single, Piher PT-6v Single, Piher PT-10h2.5 Single, Piher PT-10h5 Single, Piher PT-101h3.8 Single, Piher PT-10v10 Single, Piher PT-10v10 Single, Piher PT-10v5 Single, Piher PT-15h5 Single, Piher PT-15h2.5 Single, Piher PT-15B Single, Piher PT-15hc5 Single, Piher PT-15v12.5 Single, Piher PT-15v12.5 Single, Piher PT-15v15 Single, Piher PT-15v15 Single, ACP CA6h Single, ACP CA6v Single, ACP CA6v Single, ACP CA6VSMD Single, ACP CA6VSMD Single, ACP CA9h2.5 Single, http://www.acptechnologies.com/wp-content/uploads/2016/12/ACP-CAT%C3%81LOGO-ENTERO-2016.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single  Vishay T73XX Single  Vishay T73XX Single  Vishay T73YP Single  Piher PT-6h Single  Piher PT-6v Single  Piher PT-6v Single  Piher PT-10h2.5 Single  Piher PT-10h5 Single  Piher PT-101h3.8 Single  Piher PT-10v10 Single  Piher PT-10v10 Single  Piher PT-10v5 Single  Piher PT-15h5 Single  Piher PT-15h2.5 Single  Piher PT-15B Single  Piher PT-15hc5 Single  Piher PT-15v12.5 Single  Piher PT-15v12.5 Single  Piher PT-15v15 Single  Piher PT-15v15 Single  ACP CA6h Single  ACP CA6v Single  ACP CA6v Single  ACP CA6VSMD Single  ACP CA6VSMD Single  ACP CA9h2.5 Single")
    (fp_text reference RV3 (at 2.7 -25) (layer F.SilkS))
    (fp_text value "POT_TRIM 50K" (at 0 8.65) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 2.5) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(RV3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 /GOUT))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA9h2.5_Vertical_Px2.5mm_Py5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Trimmer_ACP_CA9h2.5_Vertical_Px2.5mm_Py5.0mm (layer F.Cu) (tedit 58826B0A)
    (at 119.4 75 90)
    (descr "Potentiometer, vertically mounted, Omeg PC16PU, Omeg PC16PU, Omeg PC16PU, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GJ/249GJ Single, Vishay/Spectrol 248GH/249GH Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148/149 Single, Vishay/Spectrol 148A/149A Single with mounting plates, Vishay/Spectrol 148/149 Double, Vishay/Spectrol 148A/149A Double with mounting plates, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16 Single, Piher PC-16SV Single, Piher PC-16 Double, Piher PC-16 Triple, Piher T16H Single, Piher T16L Single, Piher T16H Double, Alps RK163 Single, Alps RK163 Double, Alps RK097 Single, Alps RK097 Double, Bourns PTV09A-2 Single with mounting sleve Single, Bourns PTV09A-1 with mounting sleve Single, Bourns PRS11S Single, Alps RK09K Single with mounting sleve Single, Alps RK09K with mounting sleve Single, Alps RK09L Single, Alps RK09L Single, Alps RK09L Double, Alps RK09L Double, Alps RK09Y Single, Bourns 3339S Single, Bourns 3339S Single, Bourns 3339P Single, Bourns 3339H Single, Vishay T7YA Single, Suntan TSR-3386H Single, Suntan TSR-3386H Single, Suntan TSR-3386P Single, Vishay T73XX Single, Vishay T73XX Single, Vishay T73YP Single, Piher PT-6h Single, Piher PT-6v Single, Piher PT-6v Single, Piher PT-10h2.5 Single, Piher PT-10h5 Single, Piher PT-101h3.8 Single, Piher PT-10v10 Single, Piher PT-10v10 Single, Piher PT-10v5 Single, Piher PT-15h5 Single, Piher PT-15h2.5 Single, Piher PT-15B Single, Piher PT-15hc5 Single, Piher PT-15v12.5 Single, Piher PT-15v12.5 Single, Piher PT-15v15 Single, Piher PT-15v15 Single, ACP CA6h Single, ACP CA6v Single, ACP CA6v Single, ACP CA6VSMD Single, ACP CA6VSMD Single, ACP CA9h2.5 Single, http://www.acptechnologies.com/wp-content/uploads/2016/12/ACP-CAT%C3%81LOGO-ENTERO-2016.pdf")
    (tags "Potentiometer vertical  Omeg PC16PU  Omeg PC16PU  Omeg PC16PU  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GJ/249GJ Single  Vishay/Spectrol 248GH/249GH Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148/149 Single  Vishay/Spectrol 148A/149A Single with mounting plates  Vishay/Spectrol 148/149 Double  Vishay/Spectrol 148A/149A Double with mounting plates  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16 Single  Piher PC-16SV Single  Piher PC-16 Double  Piher PC-16 Triple  Piher T16H Single  Piher T16L Single  Piher T16H Double  Alps RK163 Single  Alps RK163 Double  Alps RK097 Single  Alps RK097 Double  Bourns PTV09A-2 Single with mounting sleve Single  Bourns PTV09A-1 with mounting sleve Single  Bourns PRS11S Single  Alps RK09K Single with mounting sleve Single  Alps RK09K with mounting sleve Single  Alps RK09L Single  Alps RK09L Single  Alps RK09L Double  Alps RK09L Double  Alps RK09Y Single  Bourns 3339S Single  Bourns 3339S Single  Bourns 3339P Single  Bourns 3339H Single  Vishay T7YA Single  Suntan TSR-3386H Single  Suntan TSR-3386H Single  Suntan TSR-3386P Single  Vishay T73XX Single  Vishay T73XX Single  Vishay T73YP Single  Piher PT-6h Single  Piher PT-6v Single  Piher PT-6v Single  Piher PT-10h2.5 Single  Piher PT-10h5 Single  Piher PT-101h3.8 Single  Piher PT-10v10 Single  Piher PT-10v10 Single  Piher PT-10v5 Single  Piher PT-15h5 Single  Piher PT-15h2.5 Single  Piher PT-15B Single  Piher PT-15hc5 Single  Piher PT-15v12.5 Single  Piher PT-15v12.5 Single  Piher PT-15v15 Single  Piher PT-15v15 Single  ACP CA6h Single  ACP CA6v Single  ACP CA6v Single  ACP CA6VSMD Single  ACP CA6VSMD Single  ACP CA9h2.5 Single")
    (fp_text reference RV4 (at 0 -3.65 90) (layer F.SilkS))
    (fp_text value "POT_TRIM 50K" (at 0 8.65 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 /BOUT))
    (pad 2 thru_hole circle (at 2.5 2.5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 34 "Net-(RV4-Pad2)"))
    (pad 3 thru_hole circle (at 0 5 90) (size 2.34 2.34) (drill 1.3) (layers *.Cu *.Mask)
      (net 11 "Net-(C3-Pad1)"))
    (model Potentiometers.3dshapes/Potentiometer_Trimmer_ACP_CA9h2.5_Vertical_Px2.5mm_Py5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "+15\nNC\n-15\nNC\n+9" (at 96 37) (layer F.SilkS))
  (gr_text "S\nR\nL\nB\nG\nR" (at 98.4 68.2) (layer F.SilkS))
  (dimension 45 (width 0.15) (layer Dwgs.User)
    (gr_text "45.000 mm" (at 116.5 86.3) (layer Dwgs.User))
    (feature1 (pts (xy 139 78) (xy 139 85.586421)))
    (feature2 (pts (xy 94 78) (xy 94 85.586421)))
    (crossbar (pts (xy 94 85) (xy 139 85)))
    (arrow1a (pts (xy 139 85) (xy 137.873496 85.586421)))
    (arrow1b (pts (xy 139 85) (xy 137.873496 84.413579)))
    (arrow2a (pts (xy 94 85) (xy 95.126504 85.586421)))
    (arrow2b (pts (xy 94 85) (xy 95.126504 84.413579)))
  )
  (dimension 62 (width 0.15) (layer Dwgs.User)
    (gr_text "62.000 mm" (at 147.3 47 270) (layer Dwgs.User))
    (feature1 (pts (xy 139 78) (xy 146.586421 78)))
    (feature2 (pts (xy 139 16) (xy 146.586421 16)))
    (crossbar (pts (xy 146 16) (xy 146 78)))
    (arrow1a (pts (xy 146 78) (xy 145.413579 76.873496)))
    (arrow1b (pts (xy 146 78) (xy 146.586421 76.873496)))
    (arrow2a (pts (xy 146 16) (xy 145.413579 17.126504)))
    (arrow2b (pts (xy 146 16) (xy 146.586421 17.126504)))
  )
  (gr_text "RGB2CRT_SCART\nFor Sony BA-6 Chassis\n20200213\ncom64@0x64.ca" (at 109.6 44.4 90) (layer F.SilkS))
  (gr_text B (at 121.8 75) (layer B.SilkS))
  (gr_text G (at 100.4 71) (layer B.SilkS))
  (gr_text R (at 100.4 60.2) (layer B.SilkS))
  (gr_text VB (at 100.4 49.4) (layer B.SilkS))
  (gr_text +9 (at 102.2 31.4) (layer B.SilkS))
  (gr_text "-15\n" (at 102.2 26.4) (layer B.SilkS))
  (gr_text +15 (at 102.2 21) (layer B.SilkS))
  (gr_line (start 94 16) (end 139 16) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 94 78) (end 94 16) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 78) (end 94 78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 77) (end 139 78) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139 16) (end 139 77) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 139 78) (xy 94 78) (xy 94 16) (xy 139 16)
      )
    )
  )
)
