(kicad_pcb (version 20171130) (host pcbnew "(5.1.0-0)")
  (general
    (thickness 1.6)
    (drawings 103)
    (tracks 1075)
    (zones 0)
    (modules 104)
    (nets 84)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.4318)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (user_via 0.762 0.381)
    (user_via 1.016 0.635)
    (user_via 1.27 0.889)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.254)
    (uvia_min_drill 0.254)
    (edge_width 0.1016)
    (segment_width 0.3048)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.1524)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.1524)
    (pad_size 0.8 1.9)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance -0.07)
    (aux_axis_origin 30 120)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f4_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 2.000000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 100.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(R1-Pad2)")
  (net 3 VBUS)
  (net 4 /WINC_EN)
  (net 5 /~WINC_RST)
  (net 6 /WINC_MISO)
  (net 7 /~WINC_SS)
  (net 8 /WINC_SCK)
  (net 9 /WINC_MOSI)
  (net 10 /~WINC_IRQ)
  (net 11 /WINC_WAKE)
  (net 12 "Net-(C16-Pad2)")
  (net 13 /D6)
  (net 14 /USB_N)
  (net 15 /USB_P)
  (net 16 /A5)
  (net 17 /~RESET~)
  (net 18 /SWCLK)
  (net 19 /SWDIO)
  (net 20 "Net-(C15-Pad2)")
  (net 21 "Net-(C9-Pad1)")
  (net 22 +5V)
  (net 23 "Net-(C19-Pad2)")
  (net 24 "Net-(C20-Pad2)")
  (net 25 LINE)
  (net 26 NEUT)
  (net 27 /ALM)
  (net 28 /P2)
  (net 29 /P1)
  (net 30 /A6)
  (net 31 /A0)
  (net 32 /A1)
  (net 33 "Net-(Q2-Pad3)")
  (net 34 /A2)
  (net 35 /A3)
  (net 36 /PR1)
  (net 37 /A4)
  (net 38 /D7)
  (net 39 "Net-(C4-Pad1)")
  (net 40 "Net-(C7-Pad2)")
  (net 41 "Net-(D2-Pad4)")
  (net 42 "Net-(D2-Pad3)")
  (net 43 "Net-(D3-Pad1)")
  (net 44 "Net-(D3-Pad2)")
  (net 45 "Net-(D5-Pad1)")
  (net 46 "Net-(D7-Pad1)")
  (net 47 "Net-(D8-Pad1)")
  (net 48 "Net-(D9-Pad2)")
  (net 49 "Net-(J4-Pad5)")
  (net 50 "Net-(J4-Pad3)")
  (net 51 "Net-(J4-Pad1)")
  (net 52 "Net-(J5-Pad6)")
  (net 53 "Net-(J6-Pad3)")
  (net 54 /D4)
  (net 55 /D0)
  (net 56 /D1)
  (net 57 /D2)
  (net 58 "Net-(J6-Pad16)")
  (net 59 "Net-(J6-Pad17)")
  (net 60 "Net-(J7-Pad10)")
  (net 61 "Net-(Q3-Pad1)")
  (net 62 "Net-(Q4-Pad2)")
  (net 63 /SDA)
  (net 64 /MISO)
  (net 65 "Net-(J6-Pad18)")
  (net 66 /MOSI)
  (net 67 "Net-(R6-Pad2)")
  (net 68 "Net-(R7-Pad2)")
  (net 69 "Net-(R12-Pad2)")
  (net 70 "Net-(R19-Pad1)")
  (net 71 "Net-(R20-Pad1)")
  (net 72 VCC)
  (net 73 "Net-(R25-Pad2)")
  (net 74 /VSUPPLY)
  (net 75 +12V)
  (net 76 /SCK)
  (net 77 /AREF)
  (net 78 "Net-(D4-Pad2)")
  (net 79 "Net-(D10-Pad2)")
  (net 80 "Net-(R28-Pad2)")
  (net 81 "Net-(R29-Pad2)")
  (net 82 "Net-(R26-Pad2)")
  (net 83 "Net-(Q1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +12V)
    (add_net +5V)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /ALM)
    (add_net /AREF)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D4)
    (add_net /D6)
    (add_net /D7)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /P1)
    (add_net /P2)
    (add_net /PR1)
    (add_net /SCK)
    (add_net /SDA)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /USB_N)
    (add_net /USB_P)
    (add_net /VSUPPLY)
    (add_net /WINC_EN)
    (add_net /WINC_MISO)
    (add_net /WINC_MOSI)
    (add_net /WINC_SCK)
    (add_net /WINC_WAKE)
    (add_net /~RESET~)
    (add_net /~WINC_IRQ)
    (add_net /~WINC_RST)
    (add_net /~WINC_SS)
    (add_net GND)
    (add_net LINE)
    (add_net NEUT)
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D2-Pad3)")
    (add_net "Net-(D2-Pad4)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J6-Pad16)")
    (add_net "Net-(J6-Pad17)")
    (add_net "Net-(J6-Pad18)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J7-Pad10)")
    (add_net "Net-(Q1-Pad3)")
    (add_net "Net-(Q2-Pad3)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R12-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(R28-Pad2)")
    (add_net "Net-(R29-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net VBUS)
    (add_net VCC)
  )
  (net_class +3V3 ""
    (clearance 0.1524)
    (trace_width 0.508)
    (via_dia 1.016)
    (via_drill 0.635)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module RF_Module-ML:Microchip_ATWINC1500-MR210UB (layer B.Cu) (tedit 5CCE040B)
    (at 90.75 48.25 90)
    (attr smd)
    (fp_text reference U6 (at -8 -4 90) (layer B.SilkS))
    (fp_text value ATWINC1500-MR210UB (at 0 -5 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at 7.365 0) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 7.365 1.016) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at 7.365 2.032) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 7.365 3.048) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 5 /~WINC_RST))
    (pad 5 smd rect (at 7.365 7.112) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 7.365 9.144) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at 7.365 10.16) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 7.365 11.176) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at 7.365 12.192) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -7.365 10.154) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 72 VCC))
    (pad 11 smd rect (at -7.365 9.138) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 11 /WINC_WAKE))
    (pad 12 smd rect (at -7.365 8.122) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at -7.365 7.106) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 10 /~WINC_IRQ))
    (pad 14 smd rect (at -7.365 6.09) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at -7.365 5.074) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /WINC_MOSI))
    (pad 16 smd rect (at -7.365 4.058) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 7 /~WINC_SS))
    (pad 17 smd rect (at -7.365 3.042) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /WINC_MISO))
    (pad 18 smd rect (at -7.365 2.026) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /WINC_SCK))
    (pad 19 smd rect (at -7.365 1.01) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at -5.465 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 72 VCC))
    (pad 21 smd rect (at -2.417 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 22 smd rect (at -1.401 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 4 /WINC_EN))
    (pad 23 smd rect (at -0.385 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 72 VCC))
    (pad 24 smd rect (at 0.631 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C15-Pad2)"))
    (pad 25 smd rect (at 1.647 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask))
    (pad 26 smd rect (at 2.663 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(R20-Pad1)"))
    (pad 27 smd rect (at 3.679 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(R19-Pad1)"))
    (pad 28 smd rect (at 4.695 -2.67 270) (size 0.8 1.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 29 smd rect (at -0.485 3.6 90) (size 3.7 3.7) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 29 thru_hole circle (at -0.485 3.6 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 29 thru_hole circle (at -1.685 3.6 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 29 thru_hole circle (at 0.715 3.6 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 29 thru_hole circle (at -1.685 4.8 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 29 thru_hole circle (at -0.485 4.8 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 29 thru_hole circle (at 0.715 4.8 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 29 thru_hole circle (at -1.685 2.4 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 29 thru_hole circle (at -0.485 2.4 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 29 thru_hole circle (at 0.715 2.4 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model ${KIML3DMOD}/RF_Module-ML.3dshapes/ATWINC1500-MR210UB--3DModel-STEP-56544.STEP
      (offset (xyz 0 8.18 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3339P_Vertical (layer F.Cu) (tedit 5CCB24E4)
    (at 88.225 69.58 90)
    (descr "Potentiometer, vertical, Bourns 3339P, http://www.bourns.com/docs/Product-Datasheets/3339.pdf")
    (tags "Potentiometer vertical Bourns 3339P")
    (fp_text reference RV1 (at 4.937 -2.5 180) (layer F.SilkS))
    (fp_text value 10k (at 0 2.52 90) (layer F.Fab))
    (fp_text user %R (at -3.018 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask)
      (net 53 "Net-(J6-Pad3)"))
    (pad 3 thru_hole circle (at 0 -5.08 90) (size 1.26 1.26) (drill 0.7) (layers *.Cu *.Mask)
      (net 22 +5V))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3339P_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-6-3.5-H_1x06_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F41)
    (at 100 86 90)
    (descr "Terminal Block Phoenix PT-1,5-6-3.5-H, 6 pins, pitch 3.5mm, size 21x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-6-3.5-H pitch 3.5mm size 21x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J4 (at -2.773 -2.591 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x06 (at 8.75 5.56 90) (layer F.Fab))
    (fp_text user %R (at 8.75 2.4 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 51 "Net-(J4-Pad1)"))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 7 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 50 "Net-(J4-Pad3)"))
    (pad 4 thru_hole circle (at 10.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 14 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "Net-(J4-Pad5)"))
    (pad 6 thru_hole circle (at 17.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/packages3d/pxc_1984659_01_PT-1-5-6-3-5-H_3D.stp
      (offset (xyz -1.778 -4.064 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo_19x20mm_SilkScreen locked (layer F.Cu) (tedit 5A615485)
    (at 99.75 49.75)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference "#LOGO1" (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_19x20mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module holes-ml:6-32_NPTH_Mounting_Hole locked (layer F.Cu) (tedit 5AF0FBD8)
    (at 54 64)
    (fp_text reference MK2 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7084 3.7084) (drill 3.7084) (layers *.Cu *.Mask)
      (solder_mask_margin 1.9558) (clearance 1.9558))
  )
  (module holes-ml:6-32_NPTH_Mounting_Hole locked (layer F.Cu) (tedit 5AF1072D)
    (at 106 112)
    (fp_text reference MK4 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7084 3.7084) (drill 3.7084) (layers *.Cu *.Mask)
      (solder_mask_margin 1.9558) (clearance 1.9558))
  )
  (module holes-ml:6-32_NPTH_Mounting_Hole locked (layer F.Cu) (tedit 5AF10726)
    (at 54 112)
    (fp_text reference MK3 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.7084 3.7084) (drill 3.7084) (layers *.Cu *.Mask)
      (solder_mask_margin 1.9558) (clearance 1.9558))
  )
  (module Symbols:OSHW-Logo_19x20mm_SilkScreen locked (layer B.Cu) (tedit 5A615485)
    (at 47 85 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference "#LOGO1" (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_19x20mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_3pol (layer F.Cu) (tedit 5AF887F2)
    (at 94.5 37.75 180)
    (descr "3-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J8 (at 9.918 3.714 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 3.5 6 180) (layer F.Fab) hide)
    (fp_text user %R (at 3.5 0 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 72 VCC))
    (pad 3 thru_hole circle (at 7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 57 /D2))
    (model ${KIPRJMOD}/packages3d/pxc_1984620_01_PT-1-5-3-3-5-H_3D.stp
      (offset (xyz -1.778 -4.064 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-3.5mm_2pol (layer F.Cu) (tedit 5AF88826)
    (at 37 112)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference J2 (at 6.307 -2.399) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 1.75 6) (layer F.Fab) hide)
    (fp_text user %R (at 1.75 0) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 LINE))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 NEUT))
    (model ${KIPRJMOD}/packages3d/pxc_1984617_01_PT-1-5-2-3-5-H_3D.stp
      (offset (xyz -1.778 -4.064 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_10x10.5 (layer F.Cu) (tedit 5BCA39D1)
    (at 36.620357 53.899169 180)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1010, 10.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C1 (at -5.543643 5.512169) (layer F.SilkS))
    (fp_text value 330uF (at 0 -6.46 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -4.2 0 180) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 75 +12V))
    (pad 2 smd roundrect (at 4.2 0 180) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_10x10.5 (layer F.Cu) (tedit 5BCA39D1)
    (at 36.620357 41.399169 180)
    (descr "SMD capacitor, aluminum electrolytic, Vishay 1010, 10.0x10.5mm, http://www.vishay.com/docs/28395/150crz.pdf")
    (tags "capacitor electrolytic")
    (attr smd)
    (fp_text reference C2 (at -5.543643 5.458169 180) (layer F.SilkS))
    (fp_text value 330uF (at 0 -6.46 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 4.2 0 180) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 1 GND))
    (pad 1 smd roundrect (at -4.2 0 180) (size 4.4 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.1)
      (net 75 +12V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 47 59)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.677 0.055) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.65) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 /VSUPPLY))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 43.561 54.6735 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 3.3nF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(C4-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 49.75 54.75 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.495 -1.685 270) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.65 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 68.458 66 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -1.865 0.005) (layer B.SilkS))
    (fp_text value 1nF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VBUS))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 65.558 66 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -1.865 0.026) (layer B.SilkS))
    (fp_text value 1nF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(C7-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 47 48.25)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -2.677 0.01) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.65) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 74 /VSUPPLY))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 43.688 43.942 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 3.3nF (at 0 -1.43 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(C9-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 49.75 44 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 0 -1.558 270) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.65 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 +5V))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 69.75 41.275 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -2.794 0.027 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 63.627 45.974)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at -2.794 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 66.75 53.34 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 1.322 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 76.2 46.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 84.5 45.847)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -2.839 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C15-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 63.246 47.498)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at -2.794 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C16-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer B.Cu) (tedit 5B36C52B)
    (at 84.5 47.619 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 2.966 -0.006 180) (layer B.SilkS))
    (fp_text value 22uF (at 0 -1.65 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(C15-Pad2)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 84.5 49.403)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -2.839 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 64.491847 38.75 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at -2.809 -0.024153 270) (layer B.SilkS))
    (fp_text value 15pF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C19-Pad2)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 66.891847 38.75 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at -2.809 -0.037153 270) (layer B.SilkS))
    (fp_text value 15pF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C20-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 94.5 34 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 71.25 62 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C22 (at -0.024 -1.394 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /~RESET~))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_PowerDI-123 (layer B.Cu) (tedit 588FC24C)
    (at 38.5 45 180)
    (descr http://www.diodes.com/_files/datasheets/ds30497.pdf)
    (tags "PowerDI diode vishay")
    (attr smd)
    (fp_text reference D1 (at 0 2 180) (layer B.SilkS))
    (fp_text value DFLS130 (at 0 -2.5 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 2 180) (layer B.Fab))
    (pad 1 smd rect (at -0.85 0) (size 2.4 1.5) (layers B.Cu B.Paste B.Mask)
      (net 74 /VSUPPLY))
    (pad 2 smd rect (at 1.525 0) (size 1.05 1.5) (layers B.Cu B.Paste B.Mask)
      (net 75 +12V))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_PowerDI-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:Diode_Bridge_Vishay_DFS (layer F.Cu) (tedit 5A4F675E)
    (at 41 65.5 270)
    (descr "SMD diode bridge DFS, see http://www.vishay.com/docs/88854/padlayouts.pdf")
    (tags DFS)
    (attr smd)
    (fp_text reference D2 (at -2.508 -5.482) (layer F.SilkS))
    (fp_text value D_Bridge_+-AA (at 0 5.2 270) (layer F.Fab))
    (fp_text user %R (at 0 -0.065 270) (layer F.Fab))
    (pad 1 smd rect (at -4.37 -2.55 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 75 +12V))
    (pad 2 smd rect (at -4.37 2.55 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 4.37 2.55 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D2-Pad3)"))
    (pad 4 smd rect (at 4.37 -2.55 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D2-Pad4)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/Diode_Bridge_Vishay_DFS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 95.5 82.5)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D3 (at 2 -1.5) (layer B.SilkS))
    (fp_text value TPD2E2U06 (at 0 -2.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D3-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 95.5 75.5)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D4 (at 2 -1.5) (layer B.SilkS))
    (fp_text value TPD2E2U06 (at 0 -2.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 101.5 64.75)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D5 (at 0 -2.5) (layer B.SilkS))
    (fp_text value TPD2E2U06 (at 0 -2.5) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(D5-Pad1)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-143 (layer B.Cu) (tedit 5A02FF57)
    (at 74.25 66.75)
    (descr SOT-143)
    (tags SOT-143)
    (attr smd)
    (fp_text reference D6 (at 0 -2.25 180) (layer B.SilkS))
    (fp_text value PRTR5V0U2X (at -0.28 -2.48) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.77 90) (size 1.2 1.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 -0.95 90) (size 1 1.4) (layers B.Cu B.Paste B.Mask)
      (net 15 /USB_P))
    (pad 3 smd rect (at 1.1 -0.95 90) (size 1 1.4) (layers B.Cu B.Paste B.Mask)
      (net 14 /USB_N))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1 1.4) (layers B.Cu B.Paste B.Mask)
      (net 3 VBUS))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-143.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 70.104 76.454)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D7 (at -2.921 0 90) (layer F.SilkS))
    (fp_text value Yellow (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(D7-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 70.104 73.914)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D8 (at -2.921 0 90) (layer F.SilkS))
    (fp_text value Green (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(D8-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 70.104 81.534)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D9 (at -2.921 0 90) (layer F.SilkS))
    (fp_text value Red (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(D9-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 70.104 78.994)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D10 (at -2.921 0 270) (layer F.SilkS))
    (fp_text value Blue (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(D10-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 /D7))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-2-3.5-H_1x02_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F3F)
    (at 70 109.5)
    (descr "Terminal Block Phoenix PT-1,5-2-3.5-H, 2 pins, pitch 3.5mm, size 7x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-2-3.5-H pitch 3.5mm size 7x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J1 (at 6.327 -2.566) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 1.75 5.56) (layer F.Fab) hide)
    (fp_text user %R (at 1.75 2.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 /PR1))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 26 NEUT))
    (model ${KIPRJMOD}/packages3d/pxc_1984617_01_PT-1-5-2-3-5-H_3D.stp
      (offset (xyz -1.778 -4.064 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_PT-1,5-3-3.5-H_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B294F3F)
    (at 84.4828 111.5)
    (descr "Terminal Block Phoenix PT-1,5-3-3.5-H, 3 pins, pitch 3.5mm, size 10.5x7.6mm^2, drill diamater 1.2mm, pad diameter 2.4mm, see , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix PT-1,5-3-3.5-H pitch 3.5mm size 10.5x7.6mm^2 drill 1.2mm pad 2.4mm")
    (fp_text reference J3 (at -2.8218 -2.534) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 3.5 5.56) (layer F.Fab) hide)
    (fp_text user %R (at 3.5 2.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 /ALM))
    (pad 2 thru_hole circle (at 3.5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 /P1))
    (pad 3 thru_hole circle (at 7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 /P2))
    (model ${KIPRJMOD}/packages3d/pxc_1984620_01_PT-1-5-3-3-5-H_3D.stp
      (offset (xyz -1.778 -4.064 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Adafruit-ML:GWT-C1627A-RGB locked (layer F.Cu) (tedit 5AF73905)
    (at 38 32.5)
    (fp_text reference J6 (at -2 0) (layer F.SilkS))
    (fp_text value GWT-C1627A-RGB (at 22.86 -0.5) (layer F.Fab) hide)
    (pad 18 thru_hole circle (at 43.18 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "Net-(J6-Pad18)"))
    (pad 17 thru_hole circle (at 40.64 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 "Net-(J6-Pad17)"))
    (pad 16 thru_hole circle (at 38.1 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 "Net-(J6-Pad16)"))
    (pad 15 thru_hole circle (at 35.56 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 +5V))
    (pad 14 thru_hole circle (at 33.02 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /A6))
    (pad 13 thru_hole circle (at 30.48 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 /A5))
    (pad 12 thru_hole circle (at 27.94 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 77 /AREF))
    (pad 11 thru_hole circle (at 25.4 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /A0))
    (pad 10 thru_hole circle (at 22.86 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 17.78 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 15.24 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 12.7 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /A2))
    (pad 5 thru_hole circle (at 10.16 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /A1))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 "Net-(J6-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 +5V))
    (pad "" np_thru_hole circle (at 69.5 31) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 0.9125) (clearance 0.9125))
    (pad "" np_thru_hole circle (at -5.5 31) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 0.9125) (clearance 0.9125))
    (pad "" np_thru_hole circle (at 69.5 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 0.9125) (clearance 0.9125))
    (pad "" np_thru_hole circle (at -5.5 0) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask)
      (solder_mask_margin 0.9125) (clearance 0.9125))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model "${KIPRJMOD}/packages3d/User Library-AC162B.STEP"
      (offset (xyz 31.75 -15.494 12.7))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/packages3d/SSW-118-01-G-S.stp
      (offset (xyz 21.59 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/packages3d/TSW-118-14-G-S.stp
      (offset (xyz 21.336 0 12.7))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
    (model ${KIPRJMOD}/packages3d/keystone-PN2027.STEP
      (offset (xyz -5.588 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/packages3d/keystone-PN2027.STEP
      (offset (xyz 69.46899999999999 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/packages3d/keystone-PN2027.STEP
      (offset (xyz -5.588 -30.988 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/packages3d/keystone-PN2027.STEP
      (offset (xyz 69.46899999999999 -30.988 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "${KIPRJMOD}/packages3d/User Library-User Library-4-40 x _125 sems.STEP"
      (offset (xyz -5.588 0 1.524))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
    (model "${KIPRJMOD}/packages3d/User Library-User Library-4-40 x _125 sems.STEP"
      (offset (xyz 69.46899999999999 0 1.524))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
    (model "${KIPRJMOD}/packages3d/User Library-User Library-4-40 x _125 sems.STEP"
      (offset (xyz -5.588 -30.988 1.524))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
    (model "${KIPRJMOD}/packages3d/User Library-User Library-4-40 x _125 sems.STEP"
      (offset (xyz 69.46899999999999 -30.988 1.524))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
    (model "${KIPRJMOD}/packages3d/User Library-User Library-4-40 x _125 sems.STEP"
      (offset (xyz -5.588 0 11.1252))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "${KIPRJMOD}/packages3d/User Library-User Library-4-40 x _125 sems.STEP"
      (offset (xyz 69.4182 0 11.1252))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "${KIPRJMOD}/packages3d/User Library-User Library-4-40 x _125 sems.STEP"
      (offset (xyz -5.588 -30.988 11.1252))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "${KIPRJMOD}/packages3d/User Library-User Library-4-40 x _125 sems.STEP"
      (offset (xyz 69.4182 -30.988 11.1252))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 59FED6E3)
    (at 59 39 270)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J7 (at -2.551 4.009) (layer F.SilkS))
    (fp_text value "Cortex Debug" (at 0 4.235 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 72 VCC))
    (pad 2 smd rect (at 1.95 -2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 19 /SWDIO))
    (pad 3 smd rect (at -1.95 -1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.95 -1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 18 /SWCLK))
    (pad 5 smd rect (at -1.95 0 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 1.95 0 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.95 1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 1.95 1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -1.95 2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 1.95 2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(J7-Pad10)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1206_3216Metric (layer B.Cu) (tedit 5B301BBE)
    (at 67.008 68.707 180)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 0 -1.778 180) (layer B.SilkS))
    (fp_text value 1k@1MHz (at 0 -1.82 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 40 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 3 VBUS))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 100.5 64.75 180)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L2 (at 0 1.758 180) (layer F.SilkS))
    (fp_text value 1k@1MHz (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 +5V))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 45 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 70.375 67.25 270)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L3 (at -1.972 0.017) (layer B.SilkS))
    (fp_text value 470@1MHz (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(J5-Pad6)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 73.66 78.994 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.5 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 55 /D0))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 78.74 85.598 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.53 0.02 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 76 /SCK))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 63.008 64 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.548 180) (layer B.SilkS))
    (fp_text value DMG2305UX (at 0 -2.5 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(C7-Pad2)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 74 /VSUPPLY))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-363_SC-70-6 (layer B.Cu) (tedit 5A02FF57)
    (at 59.817 64 270)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference Q4 (at 2.413 0) (layer B.SilkS))
    (fp_text value BCM857BS (at 0 -2 90) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0.65 270) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(C7-Pad2)"))
    (pad 3 smd rect (at -0.95 -0.65 270) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(Q3-Pad1)"))
    (pad 5 smd rect (at 0.95 0 270) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(Q4-Pad2)"))
    (pad 2 smd rect (at -0.95 0 270) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(Q4-Pad2)"))
    (pad 4 smd rect (at 0.95 -0.65 270) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 74 /VSUPPLY))
    (pad 6 smd rect (at 0.95 0.65 270) (size 0.65 0.4) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 76 35.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at -2.5 0 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 35 /A3))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(J6-Pad16)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 79.5 35.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at -2.5 0 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 /A4))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(J6-Pad17)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 83 35.5 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q7 (at -2.5 0 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(J6-Pad18)"))
    (pad 2 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 63 /SDA))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 78.74 78.486 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at -2.54 0 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 54 /D4))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 78.74 82.042 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q9 (at -2.54 0 180) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(Q2-Pad3)"))
    (pad 2 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 56 /D1))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 48 52 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 1.21M (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 44.704 52 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 383k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 76.2 78.994 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2.159 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 55 /D0))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 70.104 78.994 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 1.143) (layer B.SilkS))
    (fp_text value 169 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 +5V))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 79 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 70.75 53.627 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 2.634 0.011 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 /D7))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 86.63 106.47 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -3.54 -0.083 180) (layer F.SilkS))
    (fp_text value 22k (at 0 1.82 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 29 /P1))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 67 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 48 41.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 232k (at 0 -1.43 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(R7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 44.704 41.25 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0 1.43 180) (layer B.SilkS))
    (fp_text value 44.2k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 68 "Net-(R7-Pad2)"))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 59.817 60.833 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.413 0 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(Q4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 61.976 60.706 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.921 0 90) (layer B.SilkS))
    (fp_text value 47k (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(Q3-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 72.75 53.627 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 3.142 -0.021 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 /MISO))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 95.48 106.47)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 3.961 -0.044) (layer F.SilkS))
    (fp_text value 22k (at 0 1.82) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 69 "Net-(R12-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 28 /P2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 93.98 86)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 22k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 51 "Net-(J4-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 45 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 96 86 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 3.544 0.021 180) (layer B.SilkS))
    (fp_text value 22k (at 0 -1.82 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 43 "Net-(D3-Pad1)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 51 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 96 79 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 3.417 -0.121 180) (layer B.SilkS))
    (fp_text value 22k (at 0 -1.82 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 50 "Net-(J4-Pad3)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 44 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 93.98 79)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 22k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 45 "Net-(D5-Pad1)"))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 50 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 93.98 72)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 22k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 49 "Net-(J4-Pad5)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 45 "Net-(D5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer B.Cu) (tedit 5B301BBD)
    (at 96 72 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 3.544 -0.009 180) (layer B.SilkS))
    (fp_text value 22k (at 0 -1.82 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 49 "Net-(J4-Pad5)"))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.2)
      (net 78 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 70.104 76.454 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 0 1.143) (layer B.SilkS))
    (fp_text value 130 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(D7-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 70 "Net-(R19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 70.104 73.914 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at 0 1.143) (layer B.SilkS))
    (fp_text value 130 (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(D8-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 71 "Net-(R20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 70.104 81.534)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 0 -1.27 180) (layer B.SilkS))
    (fp_text value 130 (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 /D6))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(D9-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 91 33.945 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at 0 1.43 270) (layer B.SilkS))
    (fp_text value 4.7k (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 57 /D2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 68 62 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 2.818 0.072 90) (layer B.SilkS))
    (fp_text value 39 (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /~RESET~))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(J7-Pad10)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 69.75 62 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at 2.818 -0.027 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /~RESET~))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 66.25 62 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at -2.818 -0.044 270) (layer B.SilkS))
    (fp_text value 330 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 73 "Net-(R25-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /~RESET~))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 87.5 82.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at -0.003 -1.32 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.43 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 82 "Net-(R26-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 67.31 84.455 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R28 (at 2.921 0 270) (layer B.SilkS))
    (fp_text value 698 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 80 "Net-(R28-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 83 "Net-(Q1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 73.279 84.455 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R29 (at 2.794 0 270) (layer B.SilkS))
    (fp_text value 698 (at 0 -1.43 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 33 "Net-(Q2-Pad3)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 81 "Net-(R29-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_THT-ML:Relay_IXYS_PowerSIP (layer F.Cu) (tedit 5CC88E7A)
    (at 70 94 270)
    (fp_text reference RL1 (at -8.382 -2.286 270) (layer F.SilkS))
    (fp_text value CPC1511Y (at -8.128 2.794 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -8.89 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 80 "Net-(R28-Pad2)"))
    (pad 2 thru_hole circle (at -6.35 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 22 +5V))
    (pad 3 thru_hole circle (at 3.81 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 25 LINE))
    (pad 4 thru_hole circle (at 8.89 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 36 /PR1))
    (model ${KIML3DMOD}/Relay_THT-ML/CPC1511Y--3DModel-STEP-56544.STEP
      (offset (xyz 0 0 6.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Relay_THT-ML:Relay_IXYS_PowerSIP (layer F.Cu) (tedit 5CC88E7A)
    (at 75.5 94 270)
    (fp_text reference RL2 (at -8.382 -2.286 270) (layer F.SilkS))
    (fp_text value CPC1511Y (at -8.128 2.794 270) (layer F.Fab) hide)
    (pad 4 thru_hole circle (at 8.89 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 27 /ALM))
    (pad 3 thru_hole circle (at 3.81 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 25 LINE))
    (pad 2 thru_hole circle (at -6.35 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 22 +5V))
    (pad 1 thru_hole rect (at -8.89 0 270) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 81 "Net-(R29-Pad2)"))
    (model ${KIML3DMOD}/Relay_THT-ML/CPC1511Y--3DModel-STEP-56544.STEP
      (offset (xyz 0 0 6.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_B3U-1000P (layer F.Cu) (tedit 5A02FC95)
    (at 66 68 270)
    (descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
    (tags "Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at -2.849 -0.04) (layer F.SilkS))
    (fp_text value Reset (at 0 2.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1.7 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(R25-Pad2)"))
    (pad 2 smd rect (at 1.7 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 5A02FC95)
    (at 85.725 81.915 270)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW2 (at 0.085 -5.025 180) (layer F.SilkS))
    (fp_text value Pump (at 6.45 0) (layer F.Fab) hide)
    (fp_text user %R (at 0 -4.05 270) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.98 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R26-Pad2)"))
    (pad 1 smd rect (at 3.98 -2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 82 "Net-(R26-Pad2)"))
    (pad 2 smd rect (at 3.98 2.25 270) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/packages3d/PTS645SL70SMTR92-LFS.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Transformer_THT-ML:Triad_VPP_5.0VA locked (layer F.Cu) (tedit 5CC8E879)
    (at 47.127 88 180)
    (descr "Transformer, Power, THT")
    (fp_text reference T1 (at 1.27 0.5 180) (layer F.SilkS))
    (fp_text value VPP-XFMR (at 1.27 -0.5 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -12.7 -10.16 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 25 LINE))
    (pad 3 thru_hole circle (at -12.7 -5.08 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 26 NEUT))
    (pad 4 thru_hole circle (at -12.7 5.08 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 25 LINE))
    (pad 6 thru_hole circle (at -12.7 10.16 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 26 NEUT))
    (pad 7 thru_hole circle (at 12.7 -10.16 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 41 "Net-(D2-Pad4)"))
    (pad 9 thru_hole circle (at 12.7 -5.08 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 42 "Net-(D2-Pad3)"))
    (pad 10 thru_hole circle (at 12.7 5.08 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 41 "Net-(D2-Pad4)"))
    (pad 12 thru_hole circle (at 12.7 10.16 180) (size 2.54 2.54) (drill 1.27) (layers *.Cu *.Mask)
      (net 42 "Net-(D2-Pad3)"))
    (model ${KIML3DMOD}/Transformer_THT-ML/Triad-VPP16-310.step
      (offset (xyz 0 0 9.398))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5010-5014_Multipurpose (layer F.Cu) (tedit 5A0F774F)
    (at 107.315 90.551)
    (descr "Keystone Miniature THM Test Point 5010-5014, http://www.keyelco.com/product-pdf.cfm?p=1319")
    (tags "Through Hole Mount Test Points")
    (fp_text reference TP3 (at -3.556 0) (layer F.SilkS))
    (fp_text value GND (at 0 2.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.8 2.8) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/packages3d/keystone-PN5126.STEP
      (offset (xyz -0.1524 0.254 2.0574))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Converter_DCDC-ML:Converter_DCDC_Texas-SIL0008E (layer B.Cu) (tedit 5CC79879)
    (at 46.75 55.5 270)
    (attr smd)
    (fp_text reference U1 (at 2.031 -3.034) (layer B.SilkS))
    (fp_text value LMZ21700 (at 0 2.7 270) (layer B.Fab) hide)
    (pad 10 thru_hole rect (at 0.55 0 270) (size 0.8 1.9) (drill 0.254) (layers *.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -10))
    (pad 9 thru_hole rect (at -0.55 0 270) (size 0.8 1.9) (drill 0.254) (layers *.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -10))
    (pad 8 smd rect (at 1.475 1.2 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 74 /VSUPPLY) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 1.475 0.4 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 74 /VSUPPLY) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 1.475 -0.4 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 72 VCC) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.475 -1.2 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 4 smd rect (at -1.475 -1.2 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 72 VCC) (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.475 -0.4 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.475 0.4 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(R1-Pad2)") (solder_mask_margin 0.07))
    (pad 1 smd rect (at -1.475 1.2 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(C4-Pad1)") (solder_mask_margin 0.07))
    (model /Users/mike/Documents/KiCAD/Libraries/packages3d/ti-ml.3dshapes/MicroSIP.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /Users/mike/Documents/KiCad/Libraries/packages3d/Converter_DCDC-ML.3dshapes/MicroSIP.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Converter_DCDC-ML:Converter_DCDC_Texas-SIL0008E (layer B.Cu) (tedit 5CC79879)
    (at 46.75 44.75 270)
    (attr smd)
    (fp_text reference U2 (at 1.986 -3.161) (layer B.SilkS))
    (fp_text value LMZ21700 (at 0 2.7 270) (layer B.Fab) hide)
    (pad 1 smd rect (at -1.475 1.2 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(C9-Pad1)") (solder_mask_margin 0.07))
    (pad 2 smd rect (at -1.475 0.4 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(R7-Pad2)") (solder_mask_margin 0.07))
    (pad 3 smd rect (at -1.475 -0.4 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.07))
    (pad 4 smd rect (at -1.475 -1.2 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V) (solder_mask_margin 0.07))
    (pad 5 smd rect (at 1.475 -1.2 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.07))
    (pad 6 smd rect (at 1.475 -0.4 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 22 +5V) (solder_mask_margin 0.07))
    (pad 7 smd rect (at 1.475 0.4 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 74 /VSUPPLY) (solder_mask_margin 0.07))
    (pad 8 smd rect (at 1.475 1.2 270) (size 0.45 0.4) (layers B.Cu B.Paste B.Mask)
      (net 74 /VSUPPLY) (solder_mask_margin 0.07))
    (pad 9 thru_hole rect (at -0.55 0 270) (size 0.8 1.9) (drill 0.254) (layers *.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -10))
    (pad 10 thru_hole rect (at 0.55 0 270) (size 0.8 1.9) (drill 0.254) (layers *.Cu B.Paste B.Mask)
      (net 1 GND) (solder_mask_margin 0.07) (solder_paste_margin -10))
    (model /Users/mike/Documents/KiCAD/Libraries/packages3d/ti-ml.3dshapes/MicroSIP.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /Users/mike/Documents/KiCad/Libraries/packages3d/Converter_DCDC-ML.3dshapes/MicroSIP.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:SMDIP-8_W9.53mm (layer F.Cu) (tedit 5A02E8C5)
    (at 89 98.75 90)
    (descr "8-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)")
    (tags "SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil")
    (attr smd)
    (fp_text reference U3 (at -3.25 -6.45 180) (layer F.SilkS))
    (fp_text value MID400 (at 0 6.14 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.765 -3.81 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(R6-Pad2)"))
    (pad 5 smd rect (at 4.765 3.81 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.765 -1.27 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 4.765 1.27 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 38 /D7))
    (pad 3 smd rect (at -4.765 1.27 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 26 NEUT))
    (pad 7 smd rect (at 4.765 -1.27 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -4.765 3.81 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 4.765 -3.81 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/SMDIP-8_W9.53mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:SMDIP-8_W9.53mm (layer F.Cu) (tedit 5A02E8C5)
    (at 100.75 98.75 90)
    (descr "8-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)")
    (tags "SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil")
    (attr smd)
    (fp_text reference U4 (at -3.25 6.438 180) (layer F.SilkS))
    (fp_text value MID400 (at 0 6.14 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd rect (at 4.765 -3.81 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 22 +5V))
    (pad 4 smd rect (at -4.765 3.81 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 4.765 -1.27 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.765 1.27 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 26 NEUT))
    (pad 6 smd rect (at 4.765 1.27 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 64 /MISO))
    (pad 2 smd rect (at -4.765 -1.27 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 4.765 3.81 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -4.765 -3.81 90) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(R12-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/SMDIP-8_W9.53mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer B.Cu) (tedit 5A02FF57)
    (at 91.5 82.5 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U5 (at 1.711 2.363 180) (layer B.SilkS))
    (fp_text value 74LVC2G14 (at 0 -2.9 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 72 VCC))
    (pad 6 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 56 /D1))
    (pad 4 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 76 /SCK))
    (pad 3 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer B.Cu) (tedit 5A02FF57)
    (at 91.5 75.5 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U7 (at 1.711 2.348 180) (layer B.SilkS))
    (fp_text value 74LVC2G14 (at 0 -2.9 180) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(R26-Pad2)"))
    (pad 4 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 66 /MOSI))
    (pad 6 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 54 /D4))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 72 VCC))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm (layer B.Cu) (tedit 5C26A111)
    (at 70 47.25 270)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U8 (at -3.435 5.103) (layer B.SilkS))
    (fp_text value SAMD21G18-M (at 0 -4.82 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 49 smd roundrect (at 0 0 270) (size 5.15 5.15) (layers B.Cu B.Mask) (roundrect_rratio 0.048544))
    (pad "" smd roundrect (at -1.935 1.935 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 270) (size 1.04 1.04) (layers B.Paste) (roundrect_rratio 0.240385))
    (pad 1 smd roundrect (at -3.4375 2.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C19-Pad2)"))
    (pad 2 smd roundrect (at -3.4375 2.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(C20-Pad2)"))
    (pad 3 smd roundrect (at -3.4375 1.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 31 /A0))
    (pad 4 smd roundrect (at -3.4375 1.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 77 /AREF))
    (pad 5 smd roundrect (at -3.4375 0.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 6 smd roundrect (at -3.4375 0.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 7 smd roundrect (at -3.4375 -0.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 /WINC_WAKE))
    (pad 8 smd roundrect (at -3.4375 -0.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 /~WINC_IRQ))
    (pad 9 smd roundrect (at -3.4375 -1.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 /A3))
    (pad 10 smd roundrect (at -3.4375 -1.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 /A4))
    (pad 11 smd roundrect (at -3.4375 -2.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 /A5))
    (pad 12 smd roundrect (at -3.4375 -2.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 30 /A6))
    (pad 13 smd roundrect (at -2.75 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 63 /SDA))
    (pad 14 smd roundrect (at -2.25 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at -1.75 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 57 /D2))
    (pad 16 smd roundrect (at -1.25 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 17 smd roundrect (at -0.75 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 18 smd roundrect (at -0.25 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 19 smd roundrect (at 0.25 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 54 /D4))
    (pad 20 smd roundrect (at 0.75 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 21 smd roundrect (at 1.25 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 /WINC_MOSI))
    (pad 22 smd roundrect (at 1.75 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 /WINC_SCK))
    (pad 23 smd roundrect (at 2.25 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 /~WINC_SS))
    (pad 24 smd roundrect (at 2.75 -3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 /WINC_MISO))
    (pad 25 smd roundrect (at 3.4375 -2.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 66 /MOSI))
    (pad 26 smd roundrect (at 3.4375 -2.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 76 /SCK))
    (pad 27 smd roundrect (at 3.4375 -1.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 28 smd roundrect (at 3.4375 -1.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 64 /MISO))
    (pad 29 smd roundrect (at 3.4375 -0.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 /D6))
    (pad 30 smd roundrect (at 3.4375 -0.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 38 /D7))
    (pad 31 smd roundrect (at 3.4375 0.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 55 /D0))
    (pad 32 smd roundrect (at 3.4375 0.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 56 /D1))
    (pad 33 smd roundrect (at 3.4375 1.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 /USB_N))
    (pad 34 smd roundrect (at 3.4375 1.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 /USB_P))
    (pad 35 smd roundrect (at 3.4375 2.25 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 36 smd roundrect (at 3.4375 2.75 270) (size 0.875 0.25) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 37 smd roundrect (at 2.75 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 38 smd roundrect (at 2.25 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25))
    (pad 39 smd roundrect (at 1.75 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 /~WINC_RST))
    (pad 40 smd roundrect (at 1.25 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 /~RESET~))
    (pad 41 smd roundrect (at 0.75 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 /WINC_EN))
    (pad 42 smd roundrect (at 0.25 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 43 smd roundrect (at -0.25 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C16-Pad2)"))
    (pad 44 smd roundrect (at -0.75 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 72 VCC))
    (pad 45 smd roundrect (at -1.25 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 /SWCLK))
    (pad 46 smd roundrect (at -1.75 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 /SWDIO))
    (pad 47 smd roundrect (at -2.25 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 32 /A1))
    (pad 48 smd roundrect (at -2.75 3.4375 270) (size 0.25 0.875) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 34 /A2))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal-ML:Crystal_SMD_Abracon_ABS07-2Pin_3.2x1.5mm (layer B.Cu) (tedit 5ABE15CC)
    (at 65.691847 41.5)
    (fp_text reference Y1 (at -2.445847 -0.098 90) (layer B.SilkS))
    (fp_text value 32.768kHz (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at -1.2 0) (size 1.1 1.9) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(C19-Pad2)"))
    (pad 2 smd rect (at 1.2 0) (size 1.1 1.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(C20-Pad2)"))
    (model /Users/mike/Documents/KiCAD/packages3d/abracon-ml.3dshapes/ABS07.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model "${KIML3DMOD}/Crystal-ML.3dshapes/Abracon ABS07.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MountingHole-ML:6-32_PTH_Mounting_Hole locked (layer F.Cu) (tedit 5AF109A3)
    (at 93 64)
    (fp_text reference MK1 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole_PAD (at 0.09906 3.59918) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.35 6.35) (drill 3.7084) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.635) (clearance 0.635))
  )
  (module Connector_USB:USB_Micro-B_Wuerth_614105150721_Vertical_CircularHoles (layer F.Cu) (tedit 5A142044)
    (at 75.25 70.5 180)
    (descr "USB Micro-B receptacle, through-hole, vertical, http://katalog.we-online.de/em/datasheet/614105150721.pdf")
    (tags "usb micro receptacle vertical")
    (fp_text reference J5 (at -2.347 2.936 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 1.3 2.92 180) (layer F.Fab))
    (fp_text user %R (at 1.3 0.22 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 3 VBUS))
    (pad 2 thru_hole circle (at 0.65 1 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 14 /USB_N))
    (pad 3 thru_hole circle (at 1.3 0 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 15 /USB_P))
    (pad 4 thru_hole circle (at 1.95 1 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 2.6 0 180) (size 0.84 0.84) (drill 0.44) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.275 0.22 180) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 52 "Net-(J5-Pad6)"))
    (pad 6 thru_hole circle (at 4.875 0.22 180) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask)
      (net 52 "Net-(J5-Pad6)"))
    (model ${KIML3DMOD}/Connector_USB/614105150721.stp
      (offset (xyz 1.2954 -0.2032 1.651))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 51.5 50.292)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.998) (layer F.SilkS))
    (fp_text value 3.3V (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 72 VCC))
  )
  (module TestPoint:TestPoint_THTPad_2.0x2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 51.5 39)
    (descr "THT rectangular pad as test Point, square 2.0mm_Drill1.0mm  side length, hole diameter 1.0mm")
    (tags "test point THT pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0 -1.998) (layer F.SilkS))
    (fp_text value 5V (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 22 +5V))
  )
  (gr_text Sense (at 95 119.5 90) (layer F.SilkS))
  (gr_text Alarm (at 80.75 119.5 90) (layer F.SilkS))
  (gr_text GND (at 108.204 95.504 90) (layer F.SilkS))
  (gr_text "Pump Relay" (at 66.04 119.5 90) (layer F.SilkS))
  (gr_text "VAC In" (at 33 114.25 90) (layer F.SilkS))
  (gr_text 1-Wire (at 101.5 36.5) (layer F.SilkS))
  (gr_text "by Mike Lawrence" (at 52.191 55.915) (layer F.SilkS))
  (gr_text "Rev 1.1 May 2019\n" (at 52.191 58.455) (layer F.SilkS))
  (gr_text "WiFi Septic Controller" (at 52.191 53.228) (layer F.SilkS))
  (gr_text "Pump\nToggle" (at 85.75 89.25) (layer F.SilkS))
  (gr_text Alarm (at 72.009 81.534) (layer F.SilkS))
  (dimension 52 (width 0.3048) (layer Dwgs.User)
    (gr_text "52.000 mm" (at 80 130.1336) (layer Dwgs.User))
    (feature1 (pts (xy 106 112) (xy 106 128.586421)))
    (feature2 (pts (xy 54 112) (xy 54 128.586421)))
    (crossbar (pts (xy 54 128) (xy 106 128)))
    (arrow1a (pts (xy 106 128) (xy 104.873496 128.586421)))
    (arrow1b (pts (xy 106 128) (xy 104.873496 127.413579)))
    (arrow2a (pts (xy 54 128) (xy 55.126504 128.586421)))
    (arrow2b (pts (xy 54 128) (xy 55.126504 127.413579)))
  )
  (dimension 39 (width 0.3048) (layer Dwgs.User)
    (gr_text "39.000 mm" (at 73.5 125.1336) (layer Dwgs.User))
    (feature1 (pts (xy 93 64) (xy 93 123.586421)))
    (feature2 (pts (xy 54 64) (xy 54 123.586421)))
    (crossbar (pts (xy 54 123) (xy 93 123)))
    (arrow1a (pts (xy 93 123) (xy 91.873496 123.586421)))
    (arrow1b (pts (xy 93 123) (xy 91.873496 122.413579)))
    (arrow2a (pts (xy 54 123) (xy 55.126504 123.586421)))
    (arrow2b (pts (xy 54 123) (xy 55.126504 122.413579)))
  )
  (gr_line (start 96.774 97.409) (end 105.41 97.409) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 96.774 99.949) (end 105.41 99.949) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 96.774 98.679) (end 95.504 98.679) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 96.774 98.679) (end 96.774 99.949) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 92.837 98.679) (end 94.107 98.679) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 92.837 98.679) (end 92.837 97.409) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 77.47 90.805) (end 74.93 90.805) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 77.47 93.345) (end 74.93 93.345) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 70.485 92.075) (end 71.755 92.075) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 74.93 92.075) (end 74.93 93.345) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 74.93 92.075) (end 73.66 92.075) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 70.485 92.075) (end 70.485 90.805) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 82.55 99.949) (end 92.837 99.949) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 82.55 97.409) (end 92.837 97.409) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 105.41 98.679) (end 106.68 98.679) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 105.41 98.679) (end 105.41 97.409) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 78.74 96.139) (end 78.74 94.615) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 81.28 94.615) (end 81.28 96.139) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 82.55 96.139) (end 82.55 99.949) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 77.47 94.615) (end 77.47 90.805) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 54.61 71.755) (end 62.23 71.755) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 62.23 74.295) (end 54.61 74.295) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 62.23 75.565) (end 63.5 75.565) (angle -90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 54.61 73.025) (end 53.34 73.025) (angle -90) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 66.04 75.565) (end 66.04 89.535) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 63.5 89.535) (end 63.5 75.565) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 70.485 93.345) (end 67.31 93.345) (layer Edge.Cuts) (width 0.1016))
  (gr_line (start 67.31 90.805) (end 70.485 90.805) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 67.31 89.535) (end 67.31 90.805) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 77.47 94.615) (end 77.47 93.345) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 82.55 96.139) (end 82.55 97.409) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 67.31 89.535) (end 67.31 93.345) (angle 90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 54.61 73.025) (end 54.61 71.755) (angle -90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 62.23 75.565) (end 66.04 75.565) (angle -90) (layer Edge.Cuts) (width 0.1016))
  (gr_text Pump (at 72.009 78.994) (layer F.SilkS))
  (gr_text Act (at 72.009 76.454) (layer F.SilkS))
  (gr_text Net (at 72.009 73.914) (layer F.SilkS))
  (gr_text Contrast (at 85.685 75.295) (layer F.SilkS))
  (gr_text W (at 91 32.9 90) (layer F.SilkS))
  (gr_text V (at 94.5 32.8 90) (layer F.SilkS))
  (gr_text G (at 87.5 33 90) (layer F.SilkS))
  (gr_text PR2 (at 73.5 119.5 90) (layer F.SilkS))
  (gr_text PR1 (at 70 119.5 90) (layer F.SilkS))
  (gr_text N (at 40.5 119.5 90) (layer F.SilkS))
  (gr_text L (at 37 119.5 90) (layer F.SilkS))
  (gr_text AL (at 84.5 119.5 90) (layer F.SilkS))
  (gr_text BA1 (at 104.25 86) (layer F.SilkS))
  (gr_text BA1 (at 104.25 82.5) (layer F.SilkS))
  (gr_text FA2 (at 104.25 79) (layer F.SilkS))
  (gr_text FA1 (at 104.25 75.5) (layer F.SilkS))
  (gr_text AA2 (at 104.25 72) (layer F.SilkS))
  (gr_text AA1 (at 104.25 68.5) (layer F.SilkS))
  (gr_text Reset (at 69.342 71.12) (layer F.SilkS))
  (dimension 48 (width 0.3048) (layer Dwgs.User)
    (gr_text "48.000 mm" (at 24.8664 88 90) (layer Dwgs.User))
    (feature1 (pts (xy 54 64) (xy 26.413579 64)))
    (feature2 (pts (xy 54 112) (xy 26.413579 112)))
    (crossbar (pts (xy 27 112) (xy 27 64)))
    (arrow1a (pts (xy 27 64) (xy 27.586421 65.126504)))
    (arrow1b (pts (xy 27 64) (xy 26.413579 65.126504)))
    (arrow2a (pts (xy 27 112) (xy 27.586421 110.873496)))
    (arrow2b (pts (xy 27 112) (xy 26.413579 110.873496)))
  )
  (dimension 2.5 (width 0.3048) (layer Dwgs.User)
    (gr_text "2.500 mm" (at 24.8664 31.25 90) (layer Dwgs.User))
    (feature1 (pts (xy 29 30) (xy 26.413579 30)))
    (feature2 (pts (xy 29 32.5) (xy 26.413579 32.5)))
    (crossbar (pts (xy 27 32.5) (xy 27 30)))
    (arrow1a (pts (xy 27 30) (xy 27.586421 31.126504)))
    (arrow1b (pts (xy 27 30) (xy 26.413579 31.126504)))
    (arrow2a (pts (xy 27 32.5) (xy 27.586421 31.373496)))
    (arrow2b (pts (xy 27 32.5) (xy 26.413579 31.373496)))
  )
  (gr_text S2 (at 91.5 119.75 90) (layer F.SilkS))
  (gr_text S1 (at 88 119.75 90) (layer F.SilkS))
  (dimension 31 (width 0.3048) (layer Dwgs.User)
    (gr_text "31.000 mm" (at 24.8664 48 90) (layer Dwgs.User))
    (feature1 (pts (xy 29 32.5) (xy 26.413579 32.5)))
    (feature2 (pts (xy 29 63.5) (xy 26.413579 63.5)))
    (crossbar (pts (xy 27 63.5) (xy 27 32.5)))
    (arrow1a (pts (xy 27 32.5) (xy 27.586421 33.626504)))
    (arrow1b (pts (xy 27 32.5) (xy 26.413579 33.626504)))
    (arrow2a (pts (xy 27 63.5) (xy 27.586421 62.373496)))
    (arrow2b (pts (xy 27 63.5) (xy 26.413579 62.373496)))
  )
  (gr_arc (start 107.5 117.5) (end 107.5 120) (angle -90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 32.5 32.5) (end 32.5 30) (angle -90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 107.5 32.5) (end 110 32.5) (angle -90) (layer Edge.Cuts) (width 0.1016))
  (gr_arc (start 32 118) (end 30 118) (angle -90) (layer Edge.Cuts) (width 0.1016))
  (dimension 75 (width 0.3048) (layer Dwgs.User)
    (gr_text "75.000 mm" (at 70 24.8664) (layer Dwgs.User))
    (feature1 (pts (xy 107.5 29) (xy 107.5 26.413579)))
    (feature2 (pts (xy 32.5 29) (xy 32.5 26.413579)))
    (crossbar (pts (xy 32.5 27) (xy 107.5 27)))
    (arrow1a (pts (xy 107.5 27) (xy 106.373496 27.586421)))
    (arrow1b (pts (xy 107.5 27) (xy 106.373496 26.413579)))
    (arrow2a (pts (xy 32.5 27) (xy 33.626504 27.586421)))
    (arrow2b (pts (xy 32.5 27) (xy 33.626504 26.413579)))
  )
  (gr_line (start 32 120) (end 107.5 120) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "by Mike Lawrence" (at 63.876 103.952) (layer B.SilkS))
  (gr_text "Rev 1.1 May 2019\n" (at 63.876 106.492) (layer B.SilkS))
  (gr_text "WiFi Septic Controller" (at 63.876 101.412) (layer B.SilkS))
  (dimension 80 (width 0.3048) (layer Dwgs.User)
    (gr_text "80.000 mm" (at 70 19.866557) (layer Dwgs.User))
    (feature1 (pts (xy 30 29) (xy 30 21.413736)))
    (feature2 (pts (xy 110 29) (xy 110 21.413736)))
    (crossbar (pts (xy 110 22.000157) (xy 30 22.000157)))
    (arrow1a (pts (xy 30 22.000157) (xy 31.126504 21.413736)))
    (arrow1b (pts (xy 30 22.000157) (xy 31.126504 22.586578)))
    (arrow2a (pts (xy 110 22.000157) (xy 108.873496 21.413736)))
    (arrow2b (pts (xy 110 22.000157) (xy 108.873496 22.586578)))
  )
  (dimension 90 (width 0.3048) (layer Dwgs.User)
    (gr_text "90.000 mm" (at 115.1336 75 270) (layer Dwgs.User))
    (feature1 (pts (xy 110 120) (xy 113.586421 120)))
    (feature2 (pts (xy 110 30) (xy 113.586421 30)))
    (crossbar (pts (xy 113 30) (xy 113 120)))
    (arrow1a (pts (xy 113 120) (xy 112.413579 118.873496)))
    (arrow1b (pts (xy 113 120) (xy 113.586421 118.873496)))
    (arrow2a (pts (xy 113 30) (xy 112.413579 31.126504)))
    (arrow2b (pts (xy 113 30) (xy 113.586421 31.126504)))
  )
  (gr_line (start 32.5 30) (end 107.5 30) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 30 32.5) (end 30 118) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110 32.5) (end 110 117.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254003) (thermal_bridge_width 0.254003))
    (polygon
      (pts
        (xy 109.972 61.972) (xy 95.988002 61.972) (xy 29.972 61.972) (xy 29.972 29.972) (xy 109.972 29.972)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2286))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30 40) (xy 35.75 40) (xy 35.75 55.5) (xy 30 55.5)
      )
    )
  )
  (zone (net 75) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2286))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.25 40) (xy 42.75 40) (xy 42.75 55.5) (xy 36.25 55.5)
      )
    )
  )
  (zone (net 72) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2286))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.752 52.705) (xy 47.751 54.356) (xy 52.833 54.356) (xy 52.832 52.705)
      )
    )
  )
  (zone (net 74) (net_name /VSUPPLY) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41.75 46) (xy 46.55 46) (xy 46.55 49.5) (xy 41.75 49.5) (xy 41.75 56.75)
        (xy 46.55 56.75) (xy 46.55 60.25) (xy 39 60.25) (xy 39 44.25) (xy 41.75 44.25)
      )
    )
  )
  (zone (net 22) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.2286))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47.75 42) (xy 47.75 43.5) (xy 50.75 43.5) (xy 50.75 42)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2286))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42 40) (xy 50.5 40) (xy 50.5 62) (xy 42 62)
      )
    )
  )
  (zone (net 72) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.2794) (thermal_bridge_width 0.2794))
    (polygon
      (pts
        (xy 30 30) (xy 110 30) (xy 110 62) (xy 30 62)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.8398 60.198) (xy 96.1644 60.198) (xy 96.1644 64.008) (xy 89.8398 64.008)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 37.5) (xy 54 37.5) (xy 54 62) (xy 41 62)
      )
    )
  )
)
