<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="-2.54" y1="0" x2="25.07" y2="0" width="0" layer="20"/>
<wire x1="25.07" y1="0" x2="24.985340625" y2="56.6343375" width="0" layer="20"/>
<wire x1="24.985340625" y1="56.6343375" x2="-2.624659375" y2="56.6343375" width="0" layer="20"/>
<wire x1="-2.624659375" y1="56.6343375" x2="-2.54" y2="0" width="0" layer="20"/>
<text>Buzz Fly FPV bridge</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="PNA460XM">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74ttl-din">
<description>&lt;b&gt;TTL Devices with DIN Symbols&lt;/b&gt;&lt;p&gt;
CadSoft and the author do not warrant that this library is free from error
or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Created by Holger Bettenbühl, hol.bet.@rhein-main.net&lt;/author&gt;</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="INPUTBRIDGE" library="adafruit" package="1X03" value=""/>
<element name="OUTPUTBRIDGE" library="adafruit" package="1X03" value=""/>
<element name="SWITCH" library="pinhead" package="1X02" value=""/>
<element name="U$1" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="U$2" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="U$3" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="U$4" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="U$5" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="U$6" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="U$7" library="adafruit" package="PNA460XM" value="PNA460XM"/>
<element name="V1" library="74ttl-din" package="DIL14" value="7421N"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="V1" pad="6"/>
<contactref element="V1" pad="9"/>
</signal>
<signal name="VCC">
<contactref element="OUTPUTBRIDGE" pad="3"/>
<contactref element="INPUTBRIDGE" pad="3"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$5" pad="3"/>
<contactref element="U$6" pad="3"/>
<contactref element="V1" pad="14"/>
<contactref element="U$7" pad="3"/>
</signal>
<signal name="OUT">
<contactref element="V1" pad="8"/>
<contactref element="OUTPUTBRIDGE" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="U$5" pad="2"/>
<contactref element="U$6" pad="2"/>
<contactref element="V1" pad="7"/>
<contactref element="OUTPUTBRIDGE" pad="2"/>
<contactref element="U$7" pad="2"/>
<contactref element="INPUTBRIDGE" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="V1" pad="5"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="V1" pad="4"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="V1" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="V1" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="V1" pad="13"/>
<contactref element="INPUTBRIDGE" pad="1"/>
<contactref element="SWITCH" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U$6" pad="1"/>
<contactref element="V1" pad="12"/>
</signal>
<signal name="S$1">
<contactref element="V1" pad="10"/>
<contactref element="U$7" pad="1"/>
</signal>
<signal name="S$2">
<contactref element="U$5" pad="1"/>
<contactref element="SWITCH" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
