(kicad_pcb (version 20171130) (host pcbnew 5.1.12)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 136)
    (zones 0)
    (modules 4)
    (nets 24)
  )
  (page A4)
  (title_block
    (title nwX287)
    (date 2021-12-15)
    (rev 1a)
    (company Necroware)
    (comment 1 "by Scorp")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.15)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed yes)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./gerber"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 SQW)
  (net 4 AD7)
  (net 5 AD6)
  (net 6 AD5)
  (net 7 AD4)
  (net 8 INT)
  (net 9 AD3)
  (net 10 RST)
  (net 11 AD2)
  (net 12 DS)
  (net 13 AD1)
  (net 14 AD0)
  (net 15 RW)
  (net 16 AS)
  (net 17 CS)
  (net 18 BC)
  (net 19 X2)
  (net 20 X1)
  (net 21 CEO)
  (net 22 CEI)
  (net 23 VOUT)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net AD0)
    (add_net AD1)
    (add_net AD2)
    (add_net AD3)
    (add_net AD4)
    (add_net AD5)
    (add_net AD6)
    (add_net AD7)
    (add_net AS)
    (add_net CEI)
    (add_net CEO)
    (add_net CS)
    (add_net DS)
    (add_net INT)
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad3)")
    (add_net RST)
    (add_net RW)
    (add_net SQW)
    (add_net VOUT)
    (add_net X1)
    (add_net X2)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BC)
    (add_net GND)
    (add_net VCC)
  )
  (module nwX287:BatteryHolder_CR1220 (layer F.Cu) (tedit 60A7B985)
    (at 134.62 98.425 180)
    (fp_text reference BT1 (at -3.048 8.636) (layer F.SilkS))
    (fp_text value CR1220 (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 8 180) (size 2.3 4) (layers F.Cu F.Paste F.Mask)
      (net 18 BC))
    (pad 2 smd rect (at 0 -8 180) (size 2.3 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at 0 -3.6 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu F.SilkS))
    (pad "" thru_hole circle (at 0 3.9 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu F.SilkS))
  )
  (module Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm (layer B.Cu) (tedit 5D9F72B1)
    (at 134.62 99.568 180)
    (descr "SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at -3.6195 8.8265) (layer B.SilkS))
    (fp_text value bq4285 (at 0 -0.635 180) (layer B.SilkS))
    (fp_text user bq3285 (at 0 1.27) (layer B.SilkS))
    (pad 24 smd roundrect (at 4.65 6.985 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 23 smd roundrect (at 4.65 5.715 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 SQW))
    (pad 22 smd roundrect (at 4.65 4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 21 CEO))
    (pad 21 smd roundrect (at 4.65 3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 22 CEI))
    (pad 20 smd roundrect (at 4.65 1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 18 BC))
    (pad 19 smd roundrect (at 4.65 0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 8 INT))
    (pad 18 smd roundrect (at 4.65 -0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 10 RST))
    (pad 17 smd roundrect (at 4.65 -1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 12 DS))
    (pad 16 smd roundrect (at 4.65 -3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 15 smd roundrect (at 4.65 -4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 15 RW))
    (pad 14 smd roundrect (at 4.65 -5.715 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 AS))
    (pad 13 smd roundrect (at 4.65 -6.985 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 17 CS))
    (pad 12 smd roundrect (at -4.65 -6.985 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at -4.65 -5.715 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 AD7))
    (pad 10 smd roundrect (at -4.65 -4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 5 AD6))
    (pad 9 smd roundrect (at -4.65 -3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 AD5))
    (pad 8 smd roundrect (at -4.65 -1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 AD4))
    (pad 7 smd roundrect (at -4.65 -0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 9 AD3))
    (pad 6 smd roundrect (at -4.65 0.635 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 11 AD2))
    (pad 5 smd roundrect (at -4.65 1.905 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 13 AD1))
    (pad 4 smd roundrect (at -4.65 3.175 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 AD0))
    (pad 3 smd roundrect (at -4.65 4.445 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 19 X2))
    (pad 2 smd roundrect (at -4.65 5.715 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 20 X1))
    (pad 1 smd roundrect (at -4.65 6.985 180) (size 2.05 0.6) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 23 VOUT))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-24_W15.24mm_Socket (layer F.Cu) (tedit 60A81ED2)
    (at 127 79.459001)
    (descr "24-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
    (fp_text reference U2 (at 7.62 -2.33) (layer F.SilkS) hide)
    (fp_text value socket (at 7.62 30.27) (layer F.Fab) hide)
    (fp_text user %R (at 7.62 13.97) (layer F.Fab) hide)
    (pad 24 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 23 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 SQW))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 AD7))
    (pad 22 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 CEO))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 AD6))
    (pad 21 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 CEI))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 AD5))
    (pad 20 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 AD4))
    (pad 19 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 INT))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 AD3))
    (pad 18 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 RST))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 AD2))
    (pad 17 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 DS))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 AD1))
    (pad 16 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 AD0))
    (pad 15 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 RW))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 AS))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 CS))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 VOUT))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W15.24mm_Socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_FrontierElectronics_FM206 (layer B.Cu) (tedit 5A1AD604)
    (at 134.6073 86.3346)
    (descr "SMD Watch Crystal FrontierElectronics FM206 6.0mm length 1.9mm diameter http://www.chinafronter.com/wp-content/uploads/2013/12/FM206.pdf")
    (tags ['FM206'])
    (attr smd)
    (fp_text reference Y1 (at 0 -5.842 180) (layer B.SilkS))
    (fp_text value "32.768kHz 6pF" (at -3.1115 -0.889 90) (layer B.SilkS))
    (fp_text user %R (at 0 -0.3 180) (layer B.Fab))
    (pad 3 smd rect (at 0 -3.05) (size 3 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.27 3.5) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 20 X1))
    (pad 1 smd rect (at -1.27 3.5) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 19 X2))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_FrontierElectronics_FM206.wrl
      (offset (xyz 0 0.224999996200839 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 4 (at 137.668 79.629) (layer F.SilkS))
  (gr_text 3 (at 131.572 79.629) (layer F.SilkS))
  (gr_line (start 125.476 77.9145) (end 133.604 77.9145) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 134.62 77.978) (end 133.604 77.9145) (angle -187.1526687) (layer Edge.Cuts) (width 0.05))
  (gr_text rev.1a (at 138.811 107.823) (layer F.SilkS))
  (gr_line (start 125.476 108.966) (end 125.476 77.9145) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.764 108.966) (end 125.476 108.966) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.764 77.9145) (end 143.764 108.966) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.636 77.9145) (end 143.764 77.9145) (layer Edge.Cuts) (width 0.05))
  (gr_text "by Necroware" (at 134.62 85.344) (layer F.Mask))
  (gr_text nwX287 (at 134.747 82.55) (layer F.Mask))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.3195 108.712) (xy 125.9205 108.712) (xy 125.9205 78.232) (xy 143.3195 78.232)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.3195 108.712) (xy 125.9205 108.712) (xy 125.9205 78.232) (xy 143.3195 78.232)
      )
    )
  )
)
