(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 63)
    (no_connects 0)
    (area 135.814999 85.014999 165.175001 124.535001)
    (thickness 1.6)
    (drawings 20)
    (tracks 295)
    (zones 0)
    (modules 24)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.06 0.65)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEEF3F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 USB_VCC)
  (net 4 LED2)
  (net 5 "Net-(D1-Pad1)")
  (net 6 LED1)
  (net 7 "Net-(D2-Pad1)")
  (net 8 "Net-(IC1-Pad1)")
  (net 9 "Net-(IC1-Pad2)")
  (net 10 "Net-(IC1-Pad3)")
  (net 11 RESET)
  (net 12 "Net-(IC1-Pad5)")
  (net 13 "Net-(IC1-Pad6)")
  (net 14 "Net-(IC1-Pad7)")
  (net 15 "Net-(IC1-Pad9)")
  (net 16 "Net-(IC1-Pad10)")
  (net 17 SW2)
  (net 18 SW1)
  (net 19 STATUS_LED)
  (net 20 "Net-(IC1-Pad15)")
  (net 21 USB_DM)
  (net 22 SWCLK)
  (net 23 SWDIO)
  (net 24 "Net-(IC1-Pad22)")
  (net 25 "Net-(IC1-Pad23)")
  (net 26 "Net-(IC1-Pad24)")
  (net 27 "Net-(IC3-Pad2)")
  (net 28 "Net-(IC3-Pad3)")
  (net 29 "Net-(IC3-Pad4)")
  (net 30 "Net-(IC3-Pad5)")
  (net 31 "Net-(IC3-Pad7)")
  (net 32 "Net-(IC3-Pad8)")
  (net 33 "Net-(IC1-Pad25)")
  (net 34 "Net-(IC1-Pad26)")
  (net 35 "Net-(IC1-Pad27)")
  (net 36 "Net-(IC1-Pad28)")
  (net 37 "Net-(R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
    (add_net LED1)
    (add_net LED2)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad15)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(IC3-Pad2)")
    (add_net "Net-(IC3-Pad3)")
    (add_net "Net-(IC3-Pad4)")
    (add_net "Net-(IC3-Pad5)")
    (add_net "Net-(IC3-Pad7)")
    (add_net "Net-(IC3-Pad8)")
    (add_net "Net-(R1-Pad1)")
    (add_net RESET)
    (add_net STATUS_LED)
    (add_net SW1)
    (add_net SW2)
    (add_net SWCLK)
    (add_net SWDIO)
    (add_net USB_DM)
    (add_net USB_VCC)
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 143.51 100.33)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 USB_VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 141.986 109.093 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 158.262 101.6)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A3AF6F3)
    (at 158.222 104.14)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -0.02 -1.27) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at -0.0435 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A3AF6FC)
    (at 158.262 106.68)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0.0435 -1.143) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0.02 0) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 142.113 113.9825 90)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 -1.75 90) (layer F.SilkS))
    (fp_text value 100uF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.5 0 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803)
    (at 153.2255 110.236 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 LED2))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803)
    (at 149.86 110.236 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 LED1))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module DRV8835DSSR:SON50P200X300X80-13N (layer F.Cu) (tedit 5A29B73A)
    (at 146.27 112.55)
    (descr "DSS (R-PWSON-N12)")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC3 (at 0 0) (layer F.SilkS))
    (fp_text value DRV8835DSSR (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.05 -1.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.05 -0.75 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC3-Pad2)"))
    (pad 3 smd rect (at -1.05 -0.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC3-Pad3)"))
    (pad 4 smd rect (at -1.05 0.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(IC3-Pad4)"))
    (pad 5 smd rect (at -1.05 0.75 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC3-Pad5)"))
    (pad 6 smd rect (at -1.05 1.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 1.05 1.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC3-Pad7)"))
    (pad 8 smd rect (at 1.05 0.75 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC3-Pad8)"))
    (pad 9 smd rect (at 1.05 0.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 LED1))
    (pad 10 smd rect (at 1.05 -0.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad7)"))
    (pad 11 smd rect (at 1.05 -0.75 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad6)"))
    (pad 12 smd rect (at 1.05 -1.25 90) (size 0.3 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 13 smd rect (at 0 0) (size 1 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module libraries:usb-PCB (layer F.Cu) (tedit 542BB0AF)
    (at 149.86 85.09 180)
    (attr virtual)
    (fp_text reference P1 (at 0.13 -7.85 180) (layer F.SilkS) hide)
    (fp_text value USB_A (at 0.29 -10.13 180) (layer F.SilkS) hide)
    (pad 1 connect rect (at 3.81 -4.9 180) (size 1.9 8) (layers F.Cu F.Mask)
      (net 3 USB_VCC))
    (pad 4 connect rect (at -3.81 -4.9 180) (size 1.9 8) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 connect rect (at -1.3 -5.15 180) (size 2 7.5) (layers F.Cu F.Mask)
      (net 22 SWCLK))
    (pad 2 connect rect (at 1.3 -5.15 180) (size 2 7.5) (layers F.Cu F.Mask)
      (net 21 USB_DM))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 162.56 115.697 180)
    (descr "Through hole straight socket strip, 1x07, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x07 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value "Expansion Port" (at 0 17.57 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(IC1-Pad22)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(IC1-Pad23)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(IC1-Pad24)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(IC1-Pad25)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(IC1-Pad26)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(IC1-Pad27)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(IC1-Pad28)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 5A3B260B)
    (at 138.43 100.33)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P4 (at 0.127 -1.8415) (layer F.SilkS))
    (fp_text value "Program Port" (at 0 12.49) (layer F.Fab))
    (fp_text user %R (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 RESET))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 SWDIO))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 SWCLK))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5A3AF6A6)
    (at 142.24 104.14 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 2.2k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 153.2255 114.173 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 330Ohm (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0.32 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 149.9235 114.173 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65 270) (layer F.SilkS))
    (fp_text value 330Ohm (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 146.1135 103.378)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 100ohm (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Switches:TACTILE_SWITCH_SMD_6.2MM_TALL (layer F.Cu) (tedit 5A3B2508)
    (at 144.94256 120.3579 180)
    (descr "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 6.2MM SQUARE")
    (tags "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 6.2MM SQUARE")
    (attr smd)
    (fp_text reference FIRE! (at 0 -3.556 180) (layer F.SilkS))
    (fp_text value Select (at 0 3.683 180) (layer F.SilkS))
    (pad A1 smd rect (at -3.97256 2.2479 270) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 17 SW2) (solder_mask_margin 0.1016))
    (pad A2 smd rect (at 3.97256 2.2479 270) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 17 SW2) (solder_mask_margin 0.1016))
    (pad B1 smd rect (at -3.97256 -2.2479 270) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad B2 smd rect (at 3.97256 -2.2479 270) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module Switches:TACTILE_SWITCH_SMD_6.2MM_TALL (layer F.Cu) (tedit 5A3B250E)
    (at 155.702 120.3579 180)
    (descr "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 6.2MM SQUARE")
    (tags "MOMENTARY SWITCH (PUSHBUTTON) - SPST - SMD, 6.2MM SQUARE")
    (attr smd)
    (fp_text reference Select (at 0 -3.556 180) (layer F.SilkS))
    (fp_text value FIRE! (at 0 3.683 180) (layer F.SilkS))
    (pad A1 smd rect (at -3.97256 2.2479 270) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 18 SW1) (solder_mask_margin 0.1016))
    (pad A2 smd rect (at 3.97256 2.2479 270) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 18 SW1) (solder_mask_margin 0.1016))
    (pad B1 smd rect (at -3.97256 -2.2479 270) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad B2 smd rect (at 3.97256 -2.2479 270) (size 1.29794 1.5494) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5A3B0DE9)
    (at 145.3515 106.6165 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value MCP73831-2-OT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 19 STATUS_LED))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 USB_VCC))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A3B2611)
    (at 162.56 121.92 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference BT1 (at -0.0635 -1.905 180) (layer F.SilkS))
    (fp_text value Battery (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5A381D56)
    (at 157.5435 111.76)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "Ext Clock" (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(IC1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(IC1-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 138.43 114.3)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference L1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value L_Small (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(IC3-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(IC3-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module STM32F042G6U6:QFN50P400X400X60-28N (layer F.Cu) (tedit 5A2E0DE5)
    (at 151.5585 104.9065)
    (descr UFQFPN28)
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference IC1 (at 0 0) (layer F.SilkS))
    (fp_text value STM32F042G6U6 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.1 -1.5 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -2.1 -1 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -2.1 -0.5 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -2.1 0 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 RESET))
    (pad 5 smd rect (at -2.1 0.5 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad5)"))
    (pad 6 smd rect (at -2.1 1 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at -2.1 1.5 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -1.5 2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 LED1))
    (pad 9 smd rect (at -1 2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -0.5 2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 0 2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 SW2))
    (pad 12 smd rect (at 0.5 2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 SW1))
    (pad 13 smd rect (at 1 2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 LED2))
    (pad 14 smd rect (at 1.5 2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 STATUS_LED))
    (pad 15 smd rect (at 2.1 1.5 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad15)"))
    (pad 16 smd rect (at 2.1 1 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 2.1 0.5 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 18 smd rect (at 2.1 0 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 19 smd rect (at 2.1 -0.5 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 USB_DM))
    (pad 20 smd rect (at 2.1 -1 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 SWCLK))
    (pad 21 smd rect (at 2.1 -1.5 90) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 SWDIO))
    (pad 22 smd rect (at 1.5 -2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 1 -2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad23)"))
    (pad 24 smd rect (at 0.5 -2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad24)"))
    (pad 25 smd rect (at 0 -2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at -0.5 -2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at -1 -2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at -1.5 -2.1) (size 0.3 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC1-Pad28)"))
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 140.1445 120.65 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_text + (at 160.401 121.8565) (layer B.SilkS))
  (gr_text - (at 160.3375 119.1895) (layer B.SilkS))
  (gr_text "RickMagSpoof v2" (at 149.9235 99.8855) (layer B.SilkS))
  (gr_text WR (at 138.8745 120.5865) (layer F.SilkS))
  (gr_line (start 155.956 97.536) (end 155.956 97.282) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 156.21 97.536) (end 156.21 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.764 97.536) (end 143.764 97.282) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 143.51 97.536) (end 143.764 97.536) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.956 85.09) (end 155.956 97.282) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.764 85.09) (end 155.956 85.09) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.764 97.282) (end 143.764 85.09) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.16 99.06) (end 135.89 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.16 123.19) (end 137.16 124.46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 163.83 123.19) (end 165.1 123.19) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 163.83 99.06) (end 163.83 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.21 97.79) (end 163.83 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.16 97.79) (end 143.51 97.79) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.89 123.19) (end 135.89 99.06) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.83 124.46) (end 137.16 124.46) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.1 99.06) (end 165.1 123.19) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.575 97.663) (xy 156.1465 98.1075) (xy 163.8935 98.1075) (xy 164.7825 98.933) (xy 164.7825 123.2535)
        (xy 163.8935 124.206) (xy 137.0965 124.206) (xy 136.144 123.2535) (xy 136.144 98.933) (xy 137.0965 98.044)
        (xy 144.145 98.044) (xy 144.145 85.471) (xy 155.575 85.471)
      )
    )
  )
  (zone (net 1) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.575 97.663) (xy 156.1465 98.1075) (xy 163.8935 98.1075) (xy 164.7825 98.933) (xy 164.7825 123.2535)
        (xy 163.8935 124.206) (xy 137.0965 124.206) (xy 136.144 123.2535) (xy 136.144 98.933) (xy 137.0965 98.044)
        (xy 144.145 98.044) (xy 144.145 85.471) (xy 155.575 85.471)
      )
    )
  )
)
