<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36.302" y2="0" width="0" layer="20"/>
<wire x1="36.302" y1="0" x2="36.302" y2="16.688" width="0" layer="20"/>
<wire x1="36.302" y1="16.688" x2="0" y2="16.688" width="0" layer="20"/>
<wire x1="0" y1="16.688" x2="0" y2="0" width="0" layer="20"/>
<text>ACME</text>
<text>CM4148</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CM4148" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="ACME" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="ACME" pad="4"/>
<contactref element="CM4148" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="ACME" pad="3"/>
<contactref element="CM4148" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="ACME" pad="6"/>
<contactref element="CM4148" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
