(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 0.3)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" mixed)
    (31 "B.Cu" mixed)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.21) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 58 77)
    (pcbplotparams
      (layerselection 0x00030d0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plot/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+12V")
  (net 3 "+6V")
  (net 4 "unconnected-(J1-Pad1)")
  (net 5 "unconnected-(J1-Pad3)")
  (net 6 "/1PPS")
  (net 7 "unconnected-(J1-Pad6)")
  (net 8 "/CTRL_TX_CLK")
  (net 9 "/CTRL_RX_DATA_NFE")
  (net 10 "/CTRL_TX_DATA")
  (net 11 "/DATA_MISO")
  (net 12 "/CTRL_RX_CLK_NFE")
  (net 13 "unconnected-(J1-Pad12)")
  (net 14 "/DATA_NFE_FS")
  (net 15 "unconnected-(J1-Pad14)")
  (net 16 "/NFPGA_DATA")
  (net 17 "/DATA_CLK_BUF")
  (net 18 "/PSOC_XRES_N")
  (net 19 "/DATA_MOSI")
  (net 20 "unconnected-(J1-Pad20)")
  (net 21 "/NFPGA_CLK")
  (net 22 "/NFPGA_LE")
  (net 23 "unconnected-(J1-Pad26)")
  (net 24 "+1V5")
  (net 25 "unconnected-(J1-Pad30)")
  (net 26 "unconnected-(J1-Pad31)")
  (net 27 "unconnected-(J2-Pad20)")
  (net 28 "Net-(R13-Pad2)")
  (net 29 "unconnected-(U3-Pad4)")
  (net 30 "+3.3V")
  (net 31 "unconnected-(U4-Pad4)")
  (footprint "b_all:R603" (layer "F.Cu")
    (tedit 61F05179)
    (at 104.3 115.1 -90)
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R13" (at 0 -2.2 -270) (layer "F.SilkS") hide)
    (fp_text value "575k" (at 0 1.9 -270) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd rect (at -0.7 0 270) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.7 0 270) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(R13-Pad2)") (pintype "passive"))
  )
  (footprint "b_all:C603" (layer "F.Cu")
    (tedit 61F315EC)
    (at 112.9 115.2 90)
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 0 -2.2 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.9 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.7 0 90) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "+3.3V") (pintype "passive"))
    (pad "2" smd rect locked (at 0.7 0 90) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
  )
  (footprint "b_all:SOT-23-5" (layer "F.Cu")
    (tedit 61F314F0)
    (at 111.7 118.4)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -2.9) (layer "F.SilkS") hide)
    (fp_text value "TPS7A20xx" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+6V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.1 0) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect locked (at -1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+6V") (pinfunction "EN") (pintype "input"))
    (pad "4" smd rect locked (at 1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(U3-Pad4)") (pinfunction "NU") (pintype "no_connect"))
    (pad "5" smd rect locked (at 1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "+3.3V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "b_all:C603" (layer "F.Cu")
    (tedit 61F315EC)
    (at 111.6 120.9)
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 0 -2.2) (layer "F.SilkS") hide)
    (fp_text value "10uF_25506-001" (at 0 1.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.7 0) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+6V") (pintype "passive"))
    (pad "2" smd rect locked (at 0.7 0) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
  )
  (footprint "b_all:SamRib_2x10_P1.27mm_Vertical_SMD" (layer "F.Cu")
    (tedit 59FED6E3)
    (at 108.7 107.7 180)
    (descr "surface-mounted straight pin header, 2x10, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x10 1.27mm double row")
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at -1.35 7.2) (layer "F.SilkS") hide)
    (fp_text value "SamRib" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.1 -5.74 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect (at 2.1 -5.715 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "/DATA_MOSI") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect (at -2.1 -4.47 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect (at 2.1 -4.445 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "/DATA_CLK_BUF") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect (at -2.1 -3.2 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect (at 2.1 -3.175 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/DATA_NFE_FS") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect (at -2.1 -1.93 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect (at 2.1 -1.905 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/CTRL_RX_CLK_NFE") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect (at -2.1 -0.66 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect (at 2.1 -0.635 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/DATA_MISO") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect (at -2.1 0.61 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect (at 2.1 0.635 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/CTRL_TX_DATA") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect (at -2.1 1.88 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect (at 2.1 1.905 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/CTRL_RX_DATA_NFE") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect (at -2.1 3.15 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect (at 2.1 3.175 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/CTRL_TX_CLK") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect (at -2.1 4.42 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect (at 2.1 4.445 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/1PPS") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect (at -2.1 5.69 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect (at 2.1 5.715 180) (size 2.8 0.74) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(J2-Pad20)") (pinfunction "Pin_20") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x10_P1.27mm_Vertical_SMD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "b_all:SOT-23-5" (layer "F.Cu")
    (tedit 61F314F0)
    (at 101.9 114.5 90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -2.9 90) (layer "F.SilkS") hide)
    (fp_text value "TPS7A20xx" (at 0 2.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+6V") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd rect (at -1.1 0 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+6V") (pinfunction "EN") (pintype "input"))
    (pad "4" smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "unconnected-(U4-Pad4)") (pinfunction "NU") (pintype "no_connect"))
    (pad "5" smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "+1V5") (pinfunction "OUT") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 104.8 120)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -4.5) (layer "F.SilkS") hide)
    (fp_text value "LT3080xST" (at 0 4.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "Net-(R13-Pad2)") (pinfunction "SET") (pintype "input"))
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+6V") (pinfunction "OUT") (pintype "power_out"))
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+12V") (pinfunction "IN") (pintype "power_in"))
    (pad "4" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+6V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "b_all:C603" (layer "F.Cu")
    (tedit 61F315EC)
    (at 102.8 111.9)
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 0 -2.2) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.9) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.7 0) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "+1V5") (pintype "passive"))
    (pad "2" smd rect locked (at 0.7 0) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
  )
  (footprint "b_all:C603" (layer "F.Cu")
    (tedit 61F315EC)
    (at 112.25 122.65 90)
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 0 -2.2 90) (layer "F.SilkS") hide)
    (fp_text value "1uF" (at 0 1.9 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.7 0 90) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+12V") (pintype "passive"))
    (pad "2" smd rect locked (at 0.7 0 90) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
  )
  (footprint "b_all:HIROSE_40P_NFE" (layer "B.Cu")
    (tedit 5B78AD86)
    (at 105 111 -90)
    (descr "Hirose  series connector, DF52-15S-0.8H (https://www.hirose.com/product/en/products/DF52/DF52-3S-0.8H%2821%29/), generated with kicad-footprint-generator")
    (tags "connector Hirose  top entry")
    (property "Sheetfile" "NFE40.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 0 2.81 90) (layer "B.SilkS") hide)
    (fp_text value "Conn_02x20_Odd_Even" (at 0.1 -4.9 90) (layer "B.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.2 8.8 90) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at -9.6 1.45 270) (size 0 0) (drill 1.4) (layers *.Mask))
    (pad "" np_thru_hole circle (at 9.6 1.45 270) (size 0 0) (drill 1.2) (layers *.Mask))
    (pad "1" smd roundrect (at -7.6 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "unconnected-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (pad "2" smd roundrect (at -7.7 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -6.8 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "unconnected-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at -6.9 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "/1PPS") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at -6 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at -6.1 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "unconnected-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive+no_connect"))
    (pad "7" smd roundrect (at -5.2 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/CTRL_TX_CLK") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd roundrect (at -5.3 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/CTRL_RX_DATA_NFE") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd roundrect (at -4.4 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "/CTRL_TX_DATA") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd roundrect (at -4.5 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "/DATA_MISO") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd roundrect (at -3.6 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "/CTRL_RX_CLK_NFE") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd roundrect (at -3.7 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "unconnected-(J1-Pad12)") (pinfunction "Pin_12") (pintype "passive+no_connect"))
    (pad "13" smd roundrect (at -2.8 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "/DATA_NFE_FS") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd roundrect (at -2.9 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "unconnected-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive+no_connect"))
    (pad "15" smd roundrect (at -2 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "/NFPGA_DATA") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd roundrect (at -2.1 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "/DATA_CLK_BUF") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd roundrect (at -1.2 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "/PSOC_XRES_N") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd roundrect (at -1.2 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "/DATA_MOSI") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd roundrect (at -0.4 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd roundrect (at -0.4 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "unconnected-(J1-Pad20)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd roundrect (at 0.4 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/NFPGA_CLK") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd roundrect (at 0.4 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd roundrect (at 1.2 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/NFPGA_LE") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd roundrect (at 1.2 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd roundrect (at 2 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd roundrect (at 2 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "unconnected-(J1-Pad26)") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" smd roundrect (at 2.8 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "+1V5") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" smd roundrect (at 2.8 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "+1V5") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" smd roundrect (at 3.6 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" smd roundrect (at 3.6 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "unconnected-(J1-Pad30)") (pinfunction "Pin_30") (pintype "passive+no_connect"))
    (pad "31" smd roundrect (at 4.4 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "unconnected-(J1-Pad31)") (pinfunction "Pin_31") (pintype "passive+no_connect"))
    (pad "32" smd roundrect (at 4.4 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "+3.3V") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" smd roundrect (at 5.2 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "+6V") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" smd roundrect (at 5.2 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "+6V") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" smd roundrect (at 6 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "+12V") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" smd roundrect (at 6 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "+12V") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" smd roundrect (at 6.8 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "+12V") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" smd roundrect (at 6.8 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "+12V") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" smd roundrect (at 7.6 2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "+12V") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" smd roundrect (at 7.6 -2.4 270) (size 0.5 3.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "+12V") (pinfunction "Pin_40") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Hirose.3dshapes/Hirose_DF52-15S-0.8H_1x15-1MP_P0.80mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 99.6 129.9) (end 99.5 129.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.5 100) (end 99.5 101.7) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.5 101.7) (end 99.5 129.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.6 100) (end 99.5 100) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.6 100) (end 114 100) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 114 129.9) (end 99.6 129.9) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 114 100) (end 114 129.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 114 129.8) (end 114 129.9) (layer "Edge.Cuts") (width 0.1))
  (gr_text "NFE40" (at 110.8 101.3) (layer "B.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.6 129.5)
        (xy 107.4 129.5)
        (xy 107.4 123.8)
        (xy 113.6 123.8)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.6 117.6)
        (xy 99.8 117.6)
        (xy 99.8 100.4)
        (xy 113.6 100.4)
      )
    )
  )
  (zone (net 3) (net_name "+6V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 109.5 121.7)
        (xy 104.5 121.7)
        (xy 104.5 119.9)
        (xy 102.5 119.9)
        (xy 102.5 119.3)
        (xy 103.8 119.3)
        (xy 103.8 118.2)
        (xy 109.5 118.2)
      )
    )
  )
  (zone (net 2) (net_name "+12V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.7 123.5)
        (xy 106.9 123.5)
        (xy 106.9 129.4)
        (xy 100.6 129.4)
        (xy 100.6 121.6)
        (xy 102.7 121.6)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.8 129.7)
        (xy 99.8 129.7)
        (xy 99.8 123.2)
        (xy 109.4 123.2)
        (xy 109.4 114.9)
        (xy 99.7 114.9)
        (xy 99.7 100.2)
        (xy 113.8 100.2)
      )
    )
  )
  (zone (net 2) (net_name "+12V") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.8 122.7)
        (xy 100.1 122.7)
        (xy 100.1 117)
        (xy 108.8 117)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.4 129.3)
        (xy 100.3 129.3)
        (xy 100.3 123.5)
        (xy 113.4 123.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.5 129.4)
        (xy 107.5 129.4)
        (xy 107.5 123.9)
        (xy 113.5 123.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.8 129.4)
        (xy 100.8 129.4)
        (xy 100.8 123.8)
        (xy 106.8 123.8)
      )
    )
  )
)
