(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 8)
    (no_connects 0)
    (area 140.924999 95.324999 167.575001 119.075001)
    (thickness 1.6)
    (drawings 8)
    (tracks 15)
    (zones 0)
    (modules 2)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 3.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad3)")
  (net 2 "Net-(J1-Pad4)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 3.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
  )
  (module MyConnectors:222D00M12LH-0004-430045 (layer F.Cu) (tedit 598C8426)
    (at 148.2 116.1)
    (fp_text reference J2 (at 0 -6.8) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -8) (layer F.Fab))
    (pad "" np_thru_hole circle (at 16.5 0) (size 2.8 2.8) (drill 2.2) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 4 0) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 8 0) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 12 0) (size 2 2) (drill 1.6) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad "" np_thru_hole circle (at -4.5 0) (size 2.8 2.8) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module MyConnectors:Phoenix_1777561 (layer B.Cu) (tedit 598DEF5E)
    (at 144.8 111.4)
    (fp_text reference J1 (at 0 3) (layer B.SilkS))
    (fp_text value Screw_Terminal_1x04 (at 0 4.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 6.35 0) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 12.7 0) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 19.05 0) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 1 thru_hole circle (at 0 -9) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 6.35 -9) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 12.7 -9) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 19.05 -9) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
  )
  (gr_line (start 167.5 95.4) (end 141 95.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 167.5 119) (end 167.5 95.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141 119) (end 141 95.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 4 (at 163.8 114.2) (layer B.SilkS))
  (gr_text 3 (at 157.2 114.2) (layer B.SilkS))
  (gr_text 2 (at 151 114.2) (layer B.SilkS))
  (gr_text 1 (at 145 114.2) (layer B.SilkS))
  (gr_line (start 141 119) (end 167.5 119) (angle 90) (layer Edge.Cuts) (width 0.15))
)
