(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.606)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "TOP")
		(2 "B.Cu" signal "BOTTOM")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user "Top Paste")
		(15 "B.Paste" user "Bottom Paste")
		(5 "F.SilkS" user "Top Overlay")
		(7 "B.SilkS" user "Bottom Overlay")
		(1 "F.Mask" user "Top Solder")
		(3 "B.Mask" user "Bottom Solder")
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user "Mechanical 12")
		(33 "B.Fab" user "Top Assembly")
		(39 "User.1" user "Top 3D Body")
		(41 "User.2" user "Top Designator")
		(43 "User.3" user "Route Tool Path")
		(45 "User.4" user "Board")
		(47 "User.5" user "Mechanical 5")
		(49 "User.6" user "Bottom Courtyard")
		(51 "User.7" user "Mechanical 7")
		(53 "User.8" user "Bottom 3D Body")
		(55 "User.9" user "Mechanical 9")
		(57 "User.10" user "Bottom Assembly")
		(59 "User.11" user "Mechanical 11")
		(61 "User.12" user "Mechanical 14")
		(63 "User.13" user "Top Courtyard")
		(65 "User.14" user "Mechanical 16")
	)
	(setup
		(pad_to_mask_clearance 0.05)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 127.20111 115.16359)
		(grid_origin 127.20111 115.16359)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/Power Subsystem/USB_CC1")
	(net 3 "/Power Subsystem/USB_CC2")
	(net 4 "Net-(C4-Pad1)")
	(net 5 "VBUS")
	(net 6 "/Power Subsystem/D+")
	(net 7 "/Power Subsystem/D-")
	(net 8 "Net-(C6-Pad1)")
	(net 9 "Net-(R5-Pad1)")
	(net 10 "unconnected-(J2-RX1+-PadB2)")
	(net 11 "/Power Subsystem/SDA")
	(net 12 "/Power Subsystem/SCL")
	(net 13 "/Power Subsystem/2V7")
	(net 14 "unconnected-(J2-RX2--PadA10)")
	(net 15 "unconnected-(J2-TX2+-PadB11)")
	(net 16 "unconnected-(J2-RX1--PadB3)")
	(net 17 "unconnected-(J2-SBU1-PadA8)")
	(net 18 "/Power Subsystem/VBUS_VS_DISCH")
	(net 19 "Net-(J2-CC1)")
	(net 20 "unconnected-(J2-TX1--PadA3)")
	(net 21 "unconnected-(J2-TX1+-PadA2)")
	(net 22 "unconnected-(J2-RX2+-PadA11)")
	(net 23 "unconnected-(J2-SBU2-PadB5)")
	(net 24 "unconnected-(J2-TX2--PadB10)")
	(net 25 "unconnected-(J3-SBU1-Pad10)")
	(net 26 "unconnected-(J3-SBU2-Pad4)")
	(net 27 "Net-(Q1-Pad1)")
	(net 28 "Net-(Q1-Pad4)")
	(net 29 "Net-(U1-ADDR0)")
	(net 30 "Net-(U1-ADDR1)")
	(net 31 "Net-(U1-RESET)")
	(net 32 "Net-(U1-VBUS_EN_SNK)")
	(net 33 "Net-(U1-DISCH)")
	(net 34 "unconnected-(U1-A_B_SIDE-Pad17)")
	(net 35 "unconnected-(U1-GPIO-Pad15)")
	(net 36 "unconnected-(U1-POWER_OK3-Pad14)")
	(net 37 "unconnected-(U1-ALERT-Pad19)")
	(net 38 "unconnected-(U1-POWER_OK2-Pad20)")
	(net 39 "unconnected-(U1-ATTACH-Pad11)")
	(net 40 "VDC")
	(footprint ""
		(layer "F.Cu")
		(at 103.88891 94.6064)
		(property "Reference" ""
			(at -47.125 39.285 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at -47.125 39.285 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.3)
			(solder_paste_margin 0)
			(thermal_bridge_angle 90)
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:CONN_USB4155_GCT"
		(layer "F.Cu")
		(at 142.253001 86.875001 90)
		(tags "USB4155-03-C ")
		(property "Reference" "J2"
			(at 0 -3.213001 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "USB4155-03-C"
			(at 5.895001 -5.313001 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "USB4155-03-C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_USB4155_GCT")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "25" smd oval
			(at -3.7 -7.253023 90)
			(size 0.9906 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "26" smd oval
			(at 3.7 -7.253023 90)
			(size 0.9906 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "A1" smd rect
			(at 2.875001 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "A2" smd rect
			(at 2.374999 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(J2-TX1+-PadA2)")
			(pinfunction "TX1+")
			(pintype "unspecified+no_connect")
		)
		(pad "A3" smd rect
			(at 1.875 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(J2-TX1--PadA3)")
			(pinfunction "TX1-")
			(pintype "unspecified+no_connect")
		)
		(pad "A4" smd rect
			(at 1.375001 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "VBUS")
			(pinfunction "VDD")
			(pintype "unspecified")
		)
		(pad "A5" smd rect
			(at 0.875 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(J2-CC1)")
			(pinfunction "CC1")
			(pintype "unspecified")
		)
		(pad "A6" smd rect
			(at 0.375001 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/Power Subsystem/D+")
			(pinfunction "D+")
			(pintype "unspecified")
		)
		(pad "A7" smd rect
			(at -0.125001 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/Power Subsystem/D-")
			(pinfunction "D-")
			(pintype "unspecified")
		)
		(pad "A8" smd rect
			(at -0.625 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(J2-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "unspecified+no_connect")
		)
		(pad "A9" smd rect
			(at -1.124999 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "VBUS")
			(pinfunction "VDD")
			(pintype "unspecified")
		)
		(pad "A10" smd rect
			(at -1.625001 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(J2-RX2--PadA10)")
			(pinfunction "RX2-")
			(pintype "unspecified+no_connect")
		)
		(pad "A11" smd rect
			(at -2.125 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(J2-RX2+-PadA11)")
			(pinfunction "RX2+")
			(pintype "unspecified+no_connect")
		)
		(pad "A12" smd rect
			(at -2.625001 -7.053001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "B1" smd rect
			(at -2.875001 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "B2" smd rect
			(at -2.374999 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(J2-RX1+-PadB2)")
			(pinfunction "RX1+")
			(pintype "unspecified+no_connect")
		)
		(pad "B3" smd rect
			(at -1.875 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(J2-RX1--PadB3)")
			(pinfunction "RX1-")
			(pintype "unspecified+no_connect")
		)
		(pad "B4" smd rect
			(at -1.375001 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "VBUS")
			(pinfunction "VDD")
			(pintype "unspecified")
		)
		(pad "B5" smd rect
			(at -0.875 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(J2-SBU2-PadB5)")
			(pinfunction "SBU2")
			(pintype "unspecified+no_connect")
		)
		(pad "B6" smd rect
			(at -0.375001 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/Power Subsystem/D-")
			(pinfunction "D-")
			(pintype "unspecified")
		)
		(pad "B7" smd rect
			(at 0.125001 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/Power Subsystem/D+")
			(pinfunction "D+")
			(pintype "unspecified")
		)
		(pad "B8" smd rect
			(at 0.625 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(J2-CC1)")
			(pinfunction "CC2")
			(pintype "unspecified")
		)
		(pad "B9" smd rect
			(at 1.124999 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "VBUS")
			(pinfunction "VDD")
			(pintype "unspecified")
		)
		(pad "B10" smd rect
			(at 1.625001 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(J2-TX2--PadB10)")
			(pinfunction "TX2-")
			(pintype "unspecified+no_connect")
		)
		(pad "B11" smd rect
			(at 2.125 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(J2-TX2+-PadB11)")
			(pinfunction "TX2+")
			(pintype "unspecified+no_connect")
		)
		(pad "B12" smd rect
			(at 2.625001 -5.553001 90)
			(size 0.3048 0.8128)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_USB4155-03-C/USB4155-03-C/3D/USB4155-03-C.stp"
			(offset
				(xyz 0 -7.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 180 180)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 131.675 84.23)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -0.237258 1.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(J2-CC1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:JAE_DX07S016JA1R1500"
		(layer "F.Cu")
		(at 105.55 86.61 -90)
		(property "Reference" "J3"
			(at 6.02 -1.09 90)
			(layer "F.SilkS")
		)
		(property "Value" "DX07S016JA1R1500"
			(at -0.68 1.13 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "JAE Industry Ltd."
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.31 mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_line
			(start 3.125 0.315)
			(end 2.875 0.315)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 2.875 -0.315)
			(end 3.125 -0.315)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 2.875 0.315)
			(mid 2.652261 0.222739)
			(end 2.56 0)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 2.56 0)
			(mid 2.652261 -0.222739)
			(end 2.875 -0.315)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 3.44 0)
			(mid 3.347739 0.222739)
			(end 3.125 0.315)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 3.125 -0.315)
			(mid 3.347739 -0.222739)
			(end 3.44 0)
			(layer "Edge.Cuts")
		)
		(fp_text user "PCB EDGE"
			(at 3.9385 4.6515 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -3 0 270)
			(size 0.63 0.63)
			(drill 0.63)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 3 0 270)
			(size 0.6 0.6)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 3 0 270)
			(size 0.63 0.63)
			(drill 0.63)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -3.1 -1.1 270)
			(size 0.52 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -2.35 -1.1 270)
			(size 0.52 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "VBUS")
			(pinfunction "VBUS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -1.75 -1.1 270)
			(size 0.27 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/Power Subsystem/USB_CC1")
			(pinfunction "CC1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -1.25 -1.1 270)
			(size 0.27 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(J3-SBU2-Pad4)")
			(pinfunction "SBU2")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -0.75 -1.1 270)
			(size 0.27 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/Power Subsystem/D-")
			(pinfunction "D-")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -0.25 -1.1 270)
			(size 0.27 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/Power Subsystem/D+")
			(pinfunction "D+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at 0.25 -1.1 270)
			(size 0.27 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/Power Subsystem/D+")
			(pinfunction "D+__1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at 0.75 -1.1 270)
			(size 0.27 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/Power Subsystem/D-")
			(pinfunction "D-__1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at 1.25 -1.1 270)
			(size 0.27 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/Power Subsystem/USB_CC2")
			(pinfunction "CC2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 1.75 -1.1 270)
			(size 0.27 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(J3-SBU1-Pad10)")
			(pinfunction "SBU1")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 2.35 -1.1 270)
			(size 0.52 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "VBUS")
			(pinfunction "VBUS__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 3.1 -1.1 270)
			(size 0.52 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "S1" smd rect
			(at -1.4 3.1 270)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "S2" smd rect
			(at 1.4 3.1 270)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHIELD__1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "S3" thru_hole oval
			(at -4.32 -0.725 270)
			(size 1.158 2.316)
			(drill oval 0.65 1.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD__2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "S4" thru_hole oval
			(at 4.32 -0.725 270)
			(size 1.158 2.316)
			(drill oval 0.65 1.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD__3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "S5" thru_hole oval
			(at -4.32 3.1 270)
			(size 1.2 2.4)
			(drill oval 0.65 1.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD__4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "S6" thru_hole oval
			(at 4.32 3.1 270)
			(size 1.2 2.4)
			(drill oval 0.65 1.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD__5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_DX07S016JA1R1500/DX07S016JA1R1500/3D/DX07S016JA1R1500.stp"
			(offset
				(xyz 0 0 1.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 -0 -0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 116.95 80.5 -90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "BUS"
			(at 2.05 -0.45 180)
			(layer "F.SilkS")
		)
		(property "Value" "SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "VBUS")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "VBUS")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:TVS_ESDA25P35-1U1M"
		(layer "F.Cu")
		(at 110.66 81.8 180)
		(property "Reference" "D3"
			(at 1.62 0.04 90)
			(layer "F.SilkS")
		)
		(property "Value" "ESDA25P35-1U1M"
			(at 1.87 0.86 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.6 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "STMicroelectronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "A" smd rect
			(at 0.625 0 180)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "C" smd rect
			(at -0.625 0 180)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask")
			(net 5 "VBUS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_ESDA25P35-1U1M/ESDA25P35-1U1M/3D/ESDA25P35-1U1M.stp"
			(offset
				(xyz 0 0 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 180)
			)
		)
	)
	(footprint "capstone-project:TRANS_STL6P3LLH6"
		(layer "F.Cu")
		(at 125.255 79.805)
		(property "Reference" "Q2"
			(at 0.025 -2.815 0)
			(layer "F.SilkS")
		)
		(property "Value" "STL6P3LLH6"
			(at 2.620001 2.6885 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "STMicroelectronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.9 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.525 -0.975)
			(size 0.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(Q1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -1.525 -0.325)
			(size 0.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(Q1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -1.525 0.325)
			(size 0.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(Q1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -1.525 0.975)
			(size 0.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q1-Pad4)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5_8" smd custom
			(at 0.7 0)
			(size 2.4 2.45)
			(layers "F.Cu")
			(net 5 "VBUS")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -1.2 -1.225) (xy -1.2 1.225) (xy -0.9 1.225) (xy -0.9 1.755) (xy -0.5 1.755) (xy -0.5 1.225)
						(xy 1.2 1.225) (xy 1.2 -1.225) (xy -0.5 -1.225) (xy -0.5 -1.755) (xy -0.9 -1.755) (xy -0.9 -1.225)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_STL6P3LLH6/STL6P3LLH6/3D/STL6P3LLH6.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 115.04 85.31 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at -1.99 -0.06 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VBUS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 136.86001 94.6)
		(property "Reference" ""
			(at -47.125 39.285 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at -47.125 39.285 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.3)
			(solder_paste_margin 0)
			(thermal_bridge_angle 90)
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 129.8399 95.425612)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 114.9865 83.4115)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 1.9635 -0.0115 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.0u"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.0135 -0.0215 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 110.74 85.71)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 1.94 0.26 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.06 0.06 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/Power Subsystem/USB_CC1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 117.1448 96.33 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at -1.97 -0.0448 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0.03 0.1552 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(R5-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/Power Subsystem/SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 104.39 78.61)
		(property "Reference" ""
			(at -47.125 39.285 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at -47.125 39.285 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.3)
			(solder_paste_margin 0)
			(thermal_bridge_angle 90)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 122.6715 85.5835 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -1.8835 0.3715 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0835 -0.0285 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U1-ADDR1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/Power Subsystem/2V7")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 117.54 89.525 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -0.185 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.237258 -0.05 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U1-RESET)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 120.8615 85.5835 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -1.8835 -0.0385 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.1835 -0.0085 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U1-ADDR0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/Power Subsystem/2V7")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_1.0x1.0mm"
		(layer "F.Cu")
		(at 121.1326 97.4852)
		(descr "SMD rectangular pad as test Point, square 1.0mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "TP1"
			(at 2.4384 0.0254 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 9 "Net-(R5-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 121.62 76.125 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 1.125 1.37 180)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.005 0.02 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(Q1-Pad4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(Q1-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 110.78 83.75)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 1.91 -0.02 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7u"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.07 0.09 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:CONN_PRT-14417_SPK"
		(layer "F.Cu")
		(at 112.369999 96.0715)
		(tags "PRT-14417 ")
		(property "Reference" "J1"
			(at 0.230001 -3.7615 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PRT-14417"
			(at -4.769999 0.1685 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "PRT-14417"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_PRT-14417_SPK")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -6.139999 0.5885 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 -2.1015)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -0.499999 -2.1015)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "VDC")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0.499999 -2.1015)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/Power Subsystem/SDA")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.5 -2.1015)
			(size 0.6096 1.5494)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/Power Subsystem/SCL")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -2.799999 1.773501)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 2.799999 1.773501)
			(size 1.1938 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_PRT-14417/PRT-14417/3D/PRT-14417.stp"
			(offset
				(xyz 0 1.5 -0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 121.48 94.53)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0.45 1.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U1-DISCH)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 126.1715 85.6035 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -1.9135 -0.0385 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.0u"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.0565 0.0215 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/Power Subsystem/2V7")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 115.045 87.05)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 1.955 0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.03 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/Power Subsystem/VBUS_VS_DISCH")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:TVS_ESDA25P35-1U1M"
		(layer "F.Cu")
		(at 114.525 81.75 180)
		(property "Reference" "D2"
			(at -0.51 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "ESDA25P35-1U1M"
			(at 5.9152 1.3064 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.6 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "STMicroelectronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "A" smd rect
			(at 0.625 0 180)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask")
			(net 5 "VBUS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "C" smd rect
			(at -0.625 0 180)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(C4-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_ESDA25P35-1U1M/ESDA25P35-1U1M/3D/ESDA25P35-1U1M.stp"
			(offset
				(xyz 0 0 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 180 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 118.9736 96.33 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0.035 1.41 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at -1.9172 0.0762 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(R5-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/Power Subsystem/SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:SOT65P210X110-3N"
		(layer "F.Cu")
		(at 110.77 90.31 180)
		(property "Reference" "D1"
			(at 2.26 0.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "ESDA25W"
			(at 4.6224 1.8164 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.1 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "STMicroelectronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.94 -0.65 180)
			(size 1.23 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 3 "/Power Subsystem/USB_CC2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -0.94 0.65 180)
			(size 1.23 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 2 "/Power Subsystem/USB_CC1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at 0.94 0 180)
			(size 1.23 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_ESDA25W/ESDA25W/3D/ESDA25W.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 121.45 81.53)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.15 -1.13 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(Q1-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 127.9215 85.6235 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -1.9235 0.0215 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.0u"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/Power Subsystem/2V7")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 124.4715 85.5835 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -1.8835 -0.0285 180)
			(layer "F.SilkS")
		)
		(property "Value" "1.0u"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/Power Subsystem/2V7")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 124.3076 94.9452 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0.0452 1.1924 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U1-ADDR0)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:TRANS_STL6P3LLH6"
		(layer "F.Cu")
		(at 116.235 76.83 180)
		(property "Reference" "Q1"
			(at 2.635 1.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "STL6P3LLH6"
			(at 7.66 3.135 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "STMicroelectronics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.9 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.525 -0.975 180)
			(size 0.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(Q1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -1.525 -0.325 180)
			(size 0.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(Q1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -1.525 0.325 180)
			(size 0.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(Q1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -1.525 0.975 180)
			(size 0.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q1-Pad4)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5_8" smd custom
			(at 0.7 0 180)
			(size 2.4 2.45)
			(layers "F.Cu")
			(net 5 "VBUS")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -1.2 -1.225) (xy -1.2 1.225) (xy -0.9 1.225) (xy -0.9 1.755) (xy -0.5 1.755) (xy -0.5 1.225)
						(xy 1.2 1.225) (xy 1.2 -1.225) (xy -0.5 -1.225) (xy -0.5 -1.755) (xy -0.9 -1.755) (xy -0.9 -1.225)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_STL6P3LLH6/STL6P3LLH6/3D/STL6P3LLH6.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 110.68 87.54)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 1.9 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.05 -0.08 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/Power Subsystem/USB_CC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 119.0415 85.5765 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -1.8765 -0.0585 180)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U1-ADDR0)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 119 80.475 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VBUS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:STUSB4500QTR"
		(layer "F.Cu")
		(at 122.62 90.3415)
		(tags "STUSB4500QTR ")
		(property "Reference" "U1"
			(at 3.61 1.9185 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "STUSB4500QTR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stusb4500.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN24EP_4X4_STM QFN24EP_4X4_STM-M QFN24EP_4X4_STM-L")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -3.32 -1.5715 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.5113 -1.5 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.5113 -1.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.9685 -1.25 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/Power Subsystem/USB_CC1")
			(pinfunction "CC1DB")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -1.9685 -0.750001 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/Power Subsystem/USB_CC1")
			(pinfunction "CC1")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at -1.9685 -0.25 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "4" smd rect
			(at -1.9685 0.25 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/Power Subsystem/USB_CC2")
			(pinfunction "CC2")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -1.9685 0.750001 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/Power Subsystem/USB_CC2")
			(pinfunction "CC2DB")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -1.9685 1.25 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(U1-RESET)")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -1.25 1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/Power Subsystem/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -0.750001 1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/Power Subsystem/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -0.25 1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "Net-(U1-DISCH)")
			(pinfunction "DISCH")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 0.25 1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "free")
		)
		(pad "11" smd rect
			(at 0.750001 1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "unconnected-(U1-ATTACH-Pad11)")
			(pinfunction "ATTACH")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at 1.25 1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(U1-ADDR0)")
			(pinfunction "ADDR0")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 1.9685 1.25 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(U1-ADDR1)")
			(pinfunction "ADDR1")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 1.9685 0.750001 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "unconnected-(U1-POWER_OK3-Pad14)")
			(pinfunction "POWER_OK3")
			(pintype "output+no_connect")
		)
		(pad "15" smd rect
			(at 1.9685 0.25 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(U1-GPIO-Pad15)")
			(pinfunction "GPIO")
			(pintype "output+no_connect")
		)
		(pad "16" smd rect
			(at 1.9685 -0.25 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "Net-(U1-VBUS_EN_SNK)")
			(pinfunction "VBUS_EN_SNK")
			(pintype "input")
		)
		(pad "17" smd rect
			(at 1.9685 -0.750001 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(U1-A_B_SIDE-Pad17)")
			(pinfunction "A_B_SIDE")
			(pintype "output+no_connect")
		)
		(pad "18" smd rect
			(at 1.9685 -1.25 90)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/Power Subsystem/VBUS_VS_DISCH")
			(pinfunction "VBUS_VS_DISCH")
			(pintype "input")
		)
		(pad "19" smd rect
			(at 1.25 -1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(U1-ALERT-Pad19)")
			(pinfunction "ALERT")
			(pintype "output+no_connect")
		)
		(pad "20" smd rect
			(at 0.750001 -1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(U1-POWER_OK2-Pad20)")
			(pinfunction "POWER_OK2")
			(pintype "output+no_connect")
		)
		(pad "21" smd rect
			(at 0.25 -1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/Power Subsystem/2V7")
			(pinfunction "VREG_1V2")
			(pintype "power_in")
		)
		(pad "22" smd rect
			(at -0.25 -1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "23" smd rect
			(at -0.750001 -1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/Power Subsystem/2V7")
			(pinfunction "VREG_2V7")
			(pintype "power_in")
		)
		(pad "24" smd rect
			(at -1.25 -1.9685)
			(size 0.254 0.9144)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/Power Subsystem/2V7")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "25" smd rect
			(at 0 0)
			(size 2.794 2.794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_STUSB4500QTR/STUSB4500QTR/3D/STUSB4500QTR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 119.7 76.365 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -1.905 0.66 180)
			(layer "F.SilkS")
		)
		(property "Value" "22k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.06 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U1-VBUS_EN_SNK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(Q1-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:TVS_ESDA25P35-1U1M"
		(layer "F.Cu")
		(at 130.32 76.815 90)
		(property "Reference" "D4"
			(at 0.425 1.48 90)
			(layer "F.SilkS")
		)
		(property "Value" "ESDA25P35-1U1M"
			(at 5.9152 1.3064 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.6 mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "STMicroelectronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(pad "A" smd rect
			(at 0.625 0 90)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "C" smd rect
			(at -0.625 0 90)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask")
			(net 5 "VBUS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/Jairo Thiongo/Downloads/LIB_ESDA25P35-1U1M/ESDA25P35-1U1M/3D/ESDA25P35-1U1M.stp"
			(offset
				(xyz 0 0 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 180)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded"
		(layer "F.Cu")
		(at 131.62 80.87)
		(descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
		(tags "test point wire loop bead")
		(property "Reference" "TP2"
			(at 0.67 -2.39 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "VBUS")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 136.39 78.58)
		(property "Reference" ""
			(at -47.125 39.285 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at -47.125 39.285 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.3)
			(solder_paste_margin 0)
			(thermal_bridge_angle 90)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 99.89001 78.42999)
		(end 99.89001 94.803076)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 104.39 99.29001)
		(mid 101.208026 97.971991)
		(end 99.89001 94.803076)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 136.39 73.92999)
		(mid 139.57199 75.248005)
		(end 140.89001 78.430003)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.39 99.29001)
		(end 136.38995 99.29001)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.38999 73.92999)
		(end 104.389969 73.93)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 140.89 94.789963)
		(mid 139.571962 97.971979)
		(end 136.38995 99.29001)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 99.890001 78.429995)
		(mid 101.208014 75.248007)
		(end 104.389969 73.93)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 140.89001 78.430003)
		(end 140.89 94.789963)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 140.89001 73.92999) (xy 140.89001 99.29) (xy 137.68999 99.29) (xy 137.68999 73.92999)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(arc
					(start 99.89001 94.79001)
					(mid 101.208029 97.971991)
					(end 104.39001 99.29001)
				)
				(arc
					(start 136.389995 99.29001)
					(mid 139.571977 97.971994)
					(end 140.89 94.790015)
				)
				(xy 140.89 94.79001)
				(arc
					(start 140.89001 78.429994)
					(mid 139.571983 75.248008)
					(end 136.389994 73.92999)
				)
				(xy 136.38999 73.92999)
				(arc
					(start 104.390005 73.93)
					(mid 101.208023 75.248016)
					(end 99.89 78.429995)
				)
				(xy 99.89001 78.42999)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(arc
					(start 99.89001 94.79001)
					(mid 101.208029 97.971991)
					(end 104.39001 99.29001)
				)
				(arc
					(start 136.389995 99.29001)
					(mid 139.571977 97.971994)
					(end 140.89 94.790015)
				)
				(xy 140.89 94.79001)
				(arc
					(start 140.89001 78.429994)
					(mid 139.571983 75.248008)
					(end 136.389994 73.92999)
				)
				(xy 136.38999 73.92999)
				(arc
					(start 104.390005 73.93)
					(mid 101.208023 75.248016)
					(end 99.89 78.429995)
				)
				(xy 99.89001 78.42999)
			)
		)
	)
	(embedded_fonts no)
)
