(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 35)
    (no_connects 0)
    (area 80.924999 91.924999 117.075001 151.075001)
    (thickness 1.6)
    (drawings 6)
    (tracks 251)
    (zones 0)
    (modules 19)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 97.155 80.4545)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 /i)
  (net 3 /o)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad1)")
  (net 6 "Net-(D5-Pad2)")
  (net 7 "Net-(D10-Pad1)")
  (net 8 "Net-(D10-Pad2)")
  (net 9 /h)
  (net 10 /p)
  (net 11 /z)
  (net 12 /k)
  (net 13 /a)
  (net 14 /e)
  (net_class Default "Esta es la clase de red por defecto."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /a)
    (add_net /e)
    (add_net /h)
    (add_net /i)
    (add_net /k)
    (add_net /o)
    (add_net /p)
    (add_net /z)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D5-Pad2)")
  )
  (module Battery_Holders:Keystone_3000_1x12mm-CoinCell (layer F.Cu) (tedit 5A896E14)
    (at 99.187 102.87 180)
    (descr http://www.keyelco.com/product-pdf.cfm?p=777)
    (tags "Keystone type 3000 coin cell retainer")
    (attr smd)
    (fp_text reference BT1 (at 0 -8 180) (layer B.SilkS))
    (fp_text value Battery_Cell (at 0 7.5 180) (layer B.SilkS))
    (pad 1 smd rect (at -7.9 0 180) (size 3.5 3.3) (layers B.Cu B.Paste B.Mask)
      (net 2 /i))
    (pad 1 smd rect (at 7.9 0 180) (size 3.5 3.3) (layers B.Cu B.Paste B.Mask)
      (net 2 /i))
    (pad 2 smd rect (at 0 0 180) (size 4 4) (layers B.Cu B.Mask)
      (net 3 /o))
    (model Battery_Holders.3dshapes/Keystone_3000_1x12mm-CoinCell.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch1.27mm (layer F.Cu) (tedit 5A895E4E)
    (at 89.027 138.176 180)
    (descr "Through hole straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 1.27mm double row")
    (fp_text reference J1 (at 0.635 -1.695 180) (layer F.SilkS))
    (fp_text value "" (at 0.635 4.235 180) (layer F.Fab))
    (fp_text user %R (at 0.635 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /h))
    (pad 2 smd oval (at 1.27 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /p))
    (pad 3 smd oval (at 0 1.27 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /z))
    (pad 4 smd oval (at 1.27 1.27 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /o))
    (pad 5 smd oval (at 0 2.54 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /k))
    (pad 6 smd oval (at 1.27 2.54 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /i))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 95.6945 101.4095)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D1 (at 0 -1.85) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 95.631 108.0135 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 95.758 114.6175)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D3 (at 0 -1.85) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 108.966 103.4415 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 12 /k))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 89.281 103.4415 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /a))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A895385)
    (at 108.839 114.6175 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /h))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 95.631 121.0945 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D4 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 95.631 127.6985)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D5 (at 0 -1.85) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 102.2985 101.4095 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 102.235 108.0135)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D7 (at 0 -1.85) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 102.1715 114.554 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D8 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 102.235 121.0945)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D9 (at 0 -1.85) (layer F.SilkS))
    (fp_text value D (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206_HandSoldering (layer F.Cu) (tedit 595FC724)
    (at 102.235 127.6985 90)
    (descr "LED SMD 1206, hand soldering")
    (tags "LED 1206")
    (attr smd)
    (fp_text reference D10 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value D (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5A8952D8)
    (at 89.281 114.2365 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 /p))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 108.712 125.5395 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 /e))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 89.408 125.7935 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /z))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:SMDIP-8_W9.53mm (layer F.Cu) (tedit 59C75EE7)
    (at 99.187 139.827)
    (descr "8-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)")
    (tags "SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil")
    (attr smd)
    (fp_text reference U1 (at 0 -6.14) (layer F.SilkS))
    (fp_text value ATTINY85-20SU (at 0 6.14) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.765 -3.81) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 11 /z))
    (pad 5 smd rect (at 4.765 3.81) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 12 /k))
    (pad 2 smd rect (at -4.765 -1.27) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 13 /a))
    (pad 6 smd rect (at 4.765 1.27) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 9 /h))
    (pad 3 smd rect (at -4.765 1.27) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 14 /e))
    (pad 7 smd rect (at 4.765 -1.27) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 10 /p))
    (pad 4 smd rect (at -4.765 3.81) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 3 /o))
    (pad 8 smd rect (at 4.765 -3.81) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 2 /i))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/SMDIP-8_W9.53mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 81 133) (end 81 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117 133) (end 117 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99 133) (end 117 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99 133) (end 99 151) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99 110) (end 99 92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99 110) (end 81 110) (angle 90) (layer Edge.Cuts) (width 0.15))
)
