<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>eSwitch</text>
<text>Aux LED</text>
<text>Ground</text>
<text>VCC</text>
<text>N/C</text>
<text>PWM: FET</text>
<text>PWM: 1x7135</text>
<wire x1="-0.1" y1="7.4" x2="4.45" y2="7.4" width="0.001" layer="46"/>
<wire x1="-0.1" y1="-0.3" x2="-0.1" y2="7.4" width="0.1" layer="46"/>
<wire x1="7.1" y1="6.3" x2="7.1" y2="-0.3" width="0.1" layer="46"/>
<text>+</text>
<text>R</text>
<wire x1="7.1" y1="6.3" x2="4.45" y2="6.3" width="0.001" layer="46"/>
<wire x1="4.45" y1="6.3" x2="4.45" y2="7.4" width="0.001" layer="46"/>
<wire x1="-0.1" y1="-0.3" x2="1" y2="-0.3" width="0.001" layer="46"/>
<wire x1="1" y1="-0.3" x2="1" y2="0" width="0.001" layer="46"/>
<wire x1="1" y1="0" x2="6" y2="0" width="0.001" layer="46"/>
<wire x1="7.1" y1="-0.3" x2="6" y2="-0.3" width="0.001" layer="46"/>
<wire x1="6" y1="-0.3" x2="6" y2="0" width="0.001" layer="46"/>
<text>FW3A
T85  to
T1616
Adapter</text>
</plain>
<libraries>
<library name="gch_VQFN_20_3x3">
<packages>
<package name="VQFN_20_3X3">
<description>GCH VQFN 20 pin 3x3x0.9mm</description>
</package>
</packages>
</library>
<library name="gch_UPDI_Pads">
<packages>
<package name="UPDI_PADS_3">
<description>UPDI Programming Key pads
Linear layout
UPDATED LAYOUT with GND in center</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP09R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$2" library="gch_VQFN_20_3x3" package="VQFN_20_3X3" value="">
<attribute name="VALUE"/>
</element>
<element name="E$3" library="gch_UPDI_Pads" package="UPDI_PADS_3" value=""/>
<element name="R" library="testpad" package="TP09R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G" library="testpad" package="TP09R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="B" library="testpad" package="TP09R" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="E$2" pad="4-VDD"/>
<contactref element="E$3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="E$2" pad="3-GND"/>
<contactref element="E$3" pad="2"/>
<contactref element="E$2" pad="21"/>
</signal>
<signal name="RESET">
<contactref element="E$2" pad="19-PA0/RST"/>
<contactref element="E$3" pad="3"/>
</signal>
<signal name="FET">
<contactref element="E$2" pad="14-PB0"/>
</signal>
<signal name="SW">
<contactref element="E$2" pad="6-PA5"/>
</signal>
<signal name="AUX">
<contactref element="E$2" pad="9-PB5"/>
</signal>
<signal name="S$5">
</signal>
<signal name="7135">
<contactref element="E$2" pad="13-PB1"/>
</signal>
<signal name="S$11">
</signal>
<signal name="BLUE">
<contactref element="E$2" pad="18-PC3"/>
<contactref element="B" pad="TP"/>
</signal>
<signal name="RED">
<contactref element="R" pad="TP"/>
<contactref element="E$2" pad="16-PC1"/>
</signal>
<signal name="GREEN">
<contactref element="G" pad="TP"/>
<contactref element="E$2" pad="17-PC2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
