(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 54)
    (tracks 2472)
    (zones 0)
    (modules 188)
    (nets 139)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.127)
    (trace_clearance 0.16)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.3)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3 2)
    (pad_drill 2.7)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FF5F7FF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C6-Pad2)")
  (net 4 "Net-(C7-Pad2)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 ROW0)
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D3-Pad2)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(D5-Pad2)")
  (net 11 "Net-(D6-Pad2)")
  (net 12 "Net-(D7-Pad2)")
  (net 13 "Net-(D8-Pad2)")
  (net 14 "Net-(D9-Pad2)")
  (net 15 "Net-(D10-Pad2)")
  (net 16 "Net-(D11-Pad2)")
  (net 17 "Net-(D12-Pad2)")
  (net 18 "Net-(D13-Pad2)")
  (net 19 ROW1)
  (net 20 "Net-(D14-Pad2)")
  (net 21 "Net-(D15-Pad2)")
  (net 22 "Net-(D16-Pad2)")
  (net 23 "Net-(D17-Pad2)")
  (net 24 "Net-(D18-Pad2)")
  (net 25 "Net-(D19-Pad2)")
  (net 26 "Net-(D20-Pad2)")
  (net 27 "Net-(D21-Pad2)")
  (net 28 "Net-(D22-Pad2)")
  (net 29 "Net-(D23-Pad2)")
  (net 30 "Net-(D24-Pad2)")
  (net 31 ROW2)
  (net 32 "Net-(D25-Pad2)")
  (net 33 "Net-(D26-Pad2)")
  (net 34 "Net-(D27-Pad2)")
  (net 35 "Net-(D28-Pad2)")
  (net 36 "Net-(D29-Pad2)")
  (net 37 "Net-(D30-Pad2)")
  (net 38 "Net-(D31-Pad2)")
  (net 39 "Net-(D32-Pad2)")
  (net 40 "Net-(D33-Pad2)")
  (net 41 "Net-(D34-Pad2)")
  (net 42 ROW3)
  (net 43 "Net-(D35-Pad2)")
  (net 44 "Net-(D36-Pad2)")
  (net 45 "Net-(D37-Pad2)")
  (net 46 "Net-(D38-Pad2)")
  (net 47 "Net-(D39-Pad2)")
  (net 48 "Net-(D40-Pad2)")
  (net 49 "Net-(D41-Pad2)")
  (net 50 "Net-(D42-Pad2)")
  (net 51 "Net-(D43-Pad2)")
  (net 52 VCC)
  (net 53 "Net-(LED1-Pad2)")
  (net 54 "Net-(LED1-Pad4)")
  (net 55 "Net-(LED2-Pad2)")
  (net 56 "Net-(LED3-Pad2)")
  (net 57 "Net-(LED4-Pad2)")
  (net 58 "Net-(LED5-Pad2)")
  (net 59 "Net-(LED6-Pad2)")
  (net 60 "Net-(LED7-Pad2)")
  (net 61 "Net-(LED8-Pad2)")
  (net 62 "Net-(LED10-Pad4)")
  (net 63 "Net-(LED10-Pad2)")
  (net 64 "Net-(LED11-Pad2)")
  (net 65 "Net-(LED12-Pad2)")
  (net 66 "Net-(LED13-Pad2)")
  (net 67 "Net-(MX1-Pad4)")
  (net 68 COL0)
  (net 69 COL1)
  (net 70 "Net-(MX2-Pad4)")
  (net 71 COL2)
  (net 72 "Net-(MX3-Pad4)")
  (net 73 "Net-(MX4-Pad4)")
  (net 74 COL3)
  (net 75 "Net-(MX5-Pad4)")
  (net 76 COL4)
  (net 77 "Net-(MX6-Pad4)")
  (net 78 COL5)
  (net 79 "Net-(MX7-Pad4)")
  (net 80 COL6)
  (net 81 COL7)
  (net 82 "Net-(MX8-Pad4)")
  (net 83 "Net-(MX9-Pad4)")
  (net 84 COL8)
  (net 85 COL9)
  (net 86 "Net-(MX10-Pad4)")
  (net 87 "Net-(MX11-Pad4)")
  (net 88 COL10)
  (net 89 COL11)
  (net 90 "Net-(MX12-Pad4)")
  (net 91 "Net-(MX13-Pad4)")
  (net 92 "Net-(MX14-Pad4)")
  (net 93 "Net-(MX15-Pad4)")
  (net 94 "Net-(MX16-Pad4)")
  (net 95 "Net-(MX17-Pad4)")
  (net 96 "Net-(MX18-Pad4)")
  (net 97 "Net-(MX19-Pad4)")
  (net 98 "Net-(MX20-Pad4)")
  (net 99 "Net-(MX21-Pad4)")
  (net 100 "Net-(MX22-Pad4)")
  (net 101 "Net-(MX23-Pad4)")
  (net 102 "Net-(MX24-Pad4)")
  (net 103 "Net-(MX25-Pad4)")
  (net 104 "Net-(MX26-Pad4)")
  (net 105 "Net-(MX27-Pad4)")
  (net 106 "Net-(MX28-Pad4)")
  (net 107 "Net-(MX29-Pad4)")
  (net 108 "Net-(MX30-Pad4)")
  (net 109 "Net-(MX31-Pad4)")
  (net 110 "Net-(MX32-Pad4)")
  (net 111 "Net-(MX33-Pad4)")
  (net 112 "Net-(MX34-Pad4)")
  (net 113 "Net-(MX35-Pad4)")
  (net 114 "Net-(MX36-Pad4)")
  (net 115 "Net-(MX37-Pad4)")
  (net 116 "Net-(MX38-Pad4)")
  (net 117 "Net-(MX39-Pad4)")
  (net 118 "Net-(MX40-Pad4)")
  (net 119 "Net-(MX41-Pad4)")
  (net 120 "Net-(MX42-Pad4)")
  (net 121 "Net-(MX43-Pad4)")
  (net 122 "Net-(NPNR1-Pad2)")
  (net 123 LEDPWM)
  (net 124 LEDGND)
  (net 125 RST)
  (net 126 "Net-(R2-Pad1)")
  (net 127 RGBIN)
  (net 128 MOSI)
  (net 129 SCK)
  (net 130 MISO)
  (net 131 "Net-(U1-Pad17)")
  (net 132 "Net-(U1-Pad16)")
  (net 133 D+)
  (net 134 D-)
  (net 135 "Net-(UR3-Pad2)")
  (net 136 "Net-(UR4-Pad1)")
  (net 137 "Net-(J1-Pad3)")
  (net 138 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net COL0)
    (add_net COL1)
    (add_net COL10)
    (add_net COL11)
    (add_net COL2)
    (add_net COL3)
    (add_net COL4)
    (add_net COL5)
    (add_net COL6)
    (add_net COL7)
    (add_net COL8)
    (add_net COL9)
    (add_net D+)
    (add_net D-)
    (add_net GND)
    (add_net LEDGND)
    (add_net LEDPWM)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D21-Pad2)")
    (add_net "Net-(D22-Pad2)")
    (add_net "Net-(D23-Pad2)")
    (add_net "Net-(D24-Pad2)")
    (add_net "Net-(D25-Pad2)")
    (add_net "Net-(D26-Pad2)")
    (add_net "Net-(D27-Pad2)")
    (add_net "Net-(D28-Pad2)")
    (add_net "Net-(D29-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D30-Pad2)")
    (add_net "Net-(D31-Pad2)")
    (add_net "Net-(D32-Pad2)")
    (add_net "Net-(D33-Pad2)")
    (add_net "Net-(D34-Pad2)")
    (add_net "Net-(D35-Pad2)")
    (add_net "Net-(D36-Pad2)")
    (add_net "Net-(D37-Pad2)")
    (add_net "Net-(D38-Pad2)")
    (add_net "Net-(D39-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D40-Pad2)")
    (add_net "Net-(D41-Pad2)")
    (add_net "Net-(D42-Pad2)")
    (add_net "Net-(D43-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED1-Pad4)")
    (add_net "Net-(LED10-Pad2)")
    (add_net "Net-(LED10-Pad4)")
    (add_net "Net-(LED11-Pad2)")
    (add_net "Net-(LED12-Pad2)")
    (add_net "Net-(LED13-Pad2)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(LED3-Pad2)")
    (add_net "Net-(LED4-Pad2)")
    (add_net "Net-(LED5-Pad2)")
    (add_net "Net-(LED6-Pad2)")
    (add_net "Net-(LED7-Pad2)")
    (add_net "Net-(LED8-Pad2)")
    (add_net "Net-(MX1-Pad4)")
    (add_net "Net-(MX10-Pad4)")
    (add_net "Net-(MX11-Pad4)")
    (add_net "Net-(MX12-Pad4)")
    (add_net "Net-(MX13-Pad4)")
    (add_net "Net-(MX14-Pad4)")
    (add_net "Net-(MX15-Pad4)")
    (add_net "Net-(MX16-Pad4)")
    (add_net "Net-(MX17-Pad4)")
    (add_net "Net-(MX18-Pad4)")
    (add_net "Net-(MX19-Pad4)")
    (add_net "Net-(MX2-Pad4)")
    (add_net "Net-(MX20-Pad4)")
    (add_net "Net-(MX21-Pad4)")
    (add_net "Net-(MX22-Pad4)")
    (add_net "Net-(MX23-Pad4)")
    (add_net "Net-(MX24-Pad4)")
    (add_net "Net-(MX25-Pad4)")
    (add_net "Net-(MX26-Pad4)")
    (add_net "Net-(MX27-Pad4)")
    (add_net "Net-(MX28-Pad4)")
    (add_net "Net-(MX29-Pad4)")
    (add_net "Net-(MX3-Pad4)")
    (add_net "Net-(MX30-Pad4)")
    (add_net "Net-(MX31-Pad4)")
    (add_net "Net-(MX32-Pad4)")
    (add_net "Net-(MX33-Pad4)")
    (add_net "Net-(MX34-Pad4)")
    (add_net "Net-(MX35-Pad4)")
    (add_net "Net-(MX36-Pad4)")
    (add_net "Net-(MX37-Pad4)")
    (add_net "Net-(MX38-Pad4)")
    (add_net "Net-(MX39-Pad4)")
    (add_net "Net-(MX4-Pad4)")
    (add_net "Net-(MX40-Pad4)")
    (add_net "Net-(MX41-Pad4)")
    (add_net "Net-(MX42-Pad4)")
    (add_net "Net-(MX43-Pad4)")
    (add_net "Net-(MX5-Pad4)")
    (add_net "Net-(MX6-Pad4)")
    (add_net "Net-(MX7-Pad4)")
    (add_net "Net-(MX8-Pad4)")
    (add_net "Net-(MX9-Pad4)")
    (add_net "Net-(NPNR1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(UR3-Pad2)")
    (add_net "Net-(UR4-Pad1)")
    (add_net RGBIN)
    (add_net ROW0)
    (add_net ROW1)
    (add_net ROW2)
    (add_net ROW3)
    (add_net RST)
    (add_net SCK)
  )
  (net_class VCC ""
    (clearance 0.16)
    (trace_width 0.2032)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net VCC)
  )
  (module keyboard_parts:PIN_1 (layer F.Cu) (tedit 5B88180D)
    (at 68.707 62.484 90)
    (tags "CONN pin 1 circle")
    (fp_text reference P? (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -1.45 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 3 2) (drill oval 2.7 1.7) (layers *.Cu *.Mask))
  )
  (module Buttons_Switches_SMD:SW_SPST_TL3342 (layer B.Cu) (tedit 58724C2D)
    (at 233.3244 85.852 270)
    (descr "Low-profile SMD Tactile Switch, https://www.e-switch.com/system/asset/product_line/data_sheet/165/TL3342.pdf")
    (tags "SPST Tactile Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 3.75 270) (layer B.SilkS))
    (fp_text value SW_PUSH (at 0 -3.75 270) (layer B.Fab))
    (fp_text user %R (at 0 3.75 270) (layer B.Fab))
    (pad 1 smd rect (at -3.15 1.9 270) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 3.15 1.9 270) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.15 -1.9 270) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 125 RST))
    (pad 2 smd rect (at 3.15 -1.9 270) (size 1.7 1) (layers B.Cu B.Paste B.Mask)
      (net 125 RST))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_TL3342.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module keyboard_parts:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B6E110B)
    (at 128.1176 118.7958 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference SPI1 (at 1.32588 6.8707 90) (layer B.SilkS))
    (fp_text value "2x3 SPI" (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 125 RST))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 MOSI))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 SCK))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 130 MISO))
  )
  (module keyboard_parts:Crystal_SMD_3225-4pin_3.2x2.5mm (layer B.Cu) (tedit 5B7ABDC0)
    (at 120.015 127.254 90)
    (descr "crystal Epson Toyocom FA-238 and TSX-3225 series")
    (fp_text reference X1 (at 0 2.45 90) (layer B.Fab))
    (fp_text value Crystal_GND24 (at 0 -2.45 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.15 -0.85 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 131 "Net-(U1-Pad17)"))
    (pad 2 smd rect (at 1.15 -0.85 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.15 0.85 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.15 0.85 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 132 "Net-(U1-Pad16)"))
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02D0)
    (at 167.386 75.946)
    (fp_text reference LED7 (at 0 4.191) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(LED7-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(LED6-Pad2)"))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3_TabPin2 (layer B.Cu) (tedit 58CE4E7E)
    (at 157.19552 130.83032)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 0 4.5) (layer B.SilkS))
    (fp_text value Q_NPN_BCE (at 0 -4.5) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -3.15 2.3) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(NPNR1-Pad2)"))
    (pad 3 smd rect (at -3.15 -2.3) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at 3.15 0) (size 2 3.8) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 100.203 123.571 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 0.1uf (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 116.38534 118.80596 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -1.54432 -1.55702 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 115.0493 132.9944 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.20828 -1.8923 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 101.6 120.015 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.524 180) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 103.44404 133.18744 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -1.4478 1.27 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 111.125 117.475 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -0.0762 1.4224 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 38.735 99.568 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 3.0988 0.3302 90) (layer B.SilkS))
    (fp_text value 4.7uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 78.0796 112.5982 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0.127 -1.905 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 62.1792 120.0404 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 59.69 93.853)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.524) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 57.404 74.422 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 95.6945 74.6125 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 1.778 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 133.477 74.422 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at -0.0254 1.7272 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 172.085 74.6125 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at -0.1016 1.651 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 210.058 74.6125 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at -0.1016 1.8034 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 248.158 74.6125 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at -0.0762 1.651 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 241.554 99.822 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 242.2652 112.4712 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C19 (at 0 -1.778 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 201.168 117.114 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at -1.016 -1.6764 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5B940296)
    (at 181.61 115.443)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at -0.635 -1.651) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 149.098 124.46)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C22 (at 0 1.778) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 51.562 66.5226 90)
    (attr smd)
    (fp_text reference D1 (at -0.0254 -1.397 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 71.501 66.548 90)
    (attr smd)
    (fp_text reference D2 (at 0.1016 -1.4478 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 7 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 89.6874 66.548 90)
    (attr smd)
    (fp_text reference D3 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 8 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 108.7628 66.7004 90)
    (attr smd)
    (fp_text reference D4 (at 0.1524 -1.3208 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 9 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 127.8128 66.7258 90)
    (attr smd)
    (fp_text reference D5 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 10 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 146.8374 66.5226 90)
    (attr smd)
    (fp_text reference D6 (at 0.1016 -1.2954 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 11 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D6-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 165.8874 66.5226 90)
    (attr smd)
    (fp_text reference D7 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 12 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D7-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 184.9374 66.4972 90)
    (attr smd)
    (fp_text reference D8 (at -0.0254 -1.2954 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 13 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D8-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 204.0128 66.4972 90)
    (attr smd)
    (fp_text reference D9 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 14 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D9-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 223.0882 66.5226 90)
    (attr smd)
    (fp_text reference D10 (at -0.0254 -1.3462 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 15 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D10-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 242.1128 66.4972 90)
    (attr smd)
    (fp_text reference D11 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 16 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D11-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 261.1755 66.4845 90)
    (attr smd)
    (fp_text reference D12 (at 0.0635 -1.3335 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 17 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 6 ROW0))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D12-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 ROW0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 35.306 74.168 270)
    (attr smd)
    (fp_text reference D13 (at -0.254 -1.524 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 18 "Net-(D13-Pad2)"))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D13-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B881257)
    (at 75.311 84.455 90)
    (attr smd)
    (fp_text reference D14 (at 0.381 -1.397 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 20 "Net-(D14-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D14-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D14-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 94.996 84.709 90)
    (attr smd)
    (fp_text reference D15 (at 0.254 -1.397 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 21 "Net-(D15-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D15-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 113.919 84.836 90)
    (attr smd)
    (fp_text reference D16 (at 0.127 -1.397 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 22 "Net-(D16-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D16-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 132.842 84.963 90)
    (attr smd)
    (fp_text reference D17 (at 0 -1.397 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 23 "Net-(D17-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D17-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D17-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 151.511 85.09 90)
    (attr smd)
    (fp_text reference D18 (at 0.254 -1.27 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 24 "Net-(D18-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D18-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D18-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 170.942 85.1535 90)
    (attr smd)
    (fp_text reference D19 (at 0.1905 -1.27 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D19-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D19-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 25 "Net-(D19-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 189.992 85.09 90)
    (attr smd)
    (fp_text reference D20 (at 0.127 -1.27 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 26 "Net-(D20-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(D20-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(D20-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 208.9785 85.09 90)
    (attr smd)
    (fp_text reference D21 (at 0 -1.4605 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 27 "Net-(D21-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(D21-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(D21-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 227.9015 84.7725 90)
    (attr smd)
    (fp_text reference D22 (at -0.0254 -1.5875 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 28 "Net-(D22-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(D22-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(D22-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 254.635 85.1535 90)
    (attr smd)
    (fp_text reference D23 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 29 "Net-(D23-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(D23-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 19 ROW1))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(D23-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 19 ROW1))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 39.878 106.934 90)
    (attr smd)
    (fp_text reference D24 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 30 "Net-(D24-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(D24-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(D24-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 63.9826 104.7369 90)
    (attr smd)
    (fp_text reference D25 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(D25-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(D25-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 32 "Net-(D25-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 99.314 104.775 90)
    (attr smd)
    (fp_text reference D26 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(D26-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(D26-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 33 "Net-(D26-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 118.237 104.775 90)
    (attr smd)
    (fp_text reference D27 (at 0.127 -1.397 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(D27-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(D27-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 34 "Net-(D27-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 137.287 104.775 90)
    (attr smd)
    (fp_text reference D28 (at 0.254 -1.397 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(D28-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(D28-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 35 "Net-(D28-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 156.337 104.775 90)
    (attr smd)
    (fp_text reference D29 (at 0.254 -1.651 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(D29-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(D29-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 36 "Net-(D29-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 175.387 104.775 90)
    (attr smd)
    (fp_text reference D30 (at -2.159 4.064 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 37 "Net-(D30-Pad2)"))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(D30-Pad2)"))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(D30-Pad2)"))
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 194.437 104.775 90)
    (attr smd)
    (fp_text reference D31 (at 0.127 -1.397 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(D31-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(D31-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 38 "Net-(D31-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 213.614 104.775 90)
    (attr smd)
    (fp_text reference D32 (at -0.0254 -1.524 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(D32-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(D32-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 39 "Net-(D32-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 232.537 103.378 90)
    (attr smd)
    (fp_text reference D33 (at -0.0254 1.4 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(D33-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(D33-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 40 "Net-(D33-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 256.54 104.14 90)
    (attr smd)
    (fp_text reference D34 (at 0.03556 -1.33604 90) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 31 ROW2))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(D34-Pad2)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 31 ROW2))
    (pad 1 smd rect (at 1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 2 smd rect (at -1.4 0 90) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(D34-Pad2)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 41 "Net-(D34-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 53.975 129.159 270)
    (attr smd)
    (fp_text reference D35 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(D35-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(D35-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 43 "Net-(D35-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 77.851 129.159 270)
    (attr smd)
    (fp_text reference D36 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(D36-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(D36-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 44 "Net-(D36-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 85.471 129.286 270)
    (attr smd)
    (fp_text reference D37 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(D37-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(D37-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 45 "Net-(D37-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 139.827 128.9685 270)
    (attr smd)
    (fp_text reference D38 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(D38-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(D38-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 46 "Net-(D38-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 178.562 130.3655 270)
    (attr smd)
    (fp_text reference D39 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(D39-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(D39-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 47 "Net-(D39-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 202.057 130.4925 270)
    (attr smd)
    (fp_text reference D40 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(D40-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(D40-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 48 "Net-(D40-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 223.012 130.2258 270)
    (attr smd)
    (fp_text reference D41 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(D41-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(D41-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 49 "Net-(D41-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 242.189 130.4925 270)
    (attr smd)
    (fp_text reference D42 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(D42-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(D42-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 50 "Net-(D42-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Diode-Hybrid-Back (layer F.Cu) (tedit 5B1AAB68)
    (at 261.3025 130.2385 270)
    (attr smd)
    (fp_text reference D43 (at -0.0254 1.4 270) (layer B.SilkS))
    (fp_text value D (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 42 ROW3))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(D43-Pad2)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 42 ROW3))
    (pad 1 smd rect (at 1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 2 smd rect (at -1.4 0 270) (size 1.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(D43-Pad2)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 51 "Net-(D43-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.step
      (offset (xyz 0 0 -1.8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02A2)
    (at 81.8515 120.904 180)
    (fp_text reference LED1 (at 0.127 -4.572 180) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(LED1-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(LED1-Pad4)"))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D029E)
    (at 57.9755 120.9675)
    (fp_text reference LED2 (at 0 4.7) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8) (layer B.SilkS) hide)
    (pad 4 smd rect (at 1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(LED1-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(LED2-Pad2)"))
    (pad 1 smd rect (at 1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D0297)
    (at 59.6265 98.552 180)
    (fp_text reference LED3 (at 0 -4.445 180) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(LED3-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(LED2-Pad2)"))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D0292)
    (at 53.086 75.946)
    (fp_text reference LED4 (at 0 4.445) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8) (layer B.SilkS) hide)
    (pad 4 smd rect (at 1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(LED3-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(LED4-Pad2)"))
    (pad 1 smd rect (at 1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D028A)
    (at 91.186 75.946)
    (fp_text reference LED5 (at 0 4.191) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(LED5-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(LED4-Pad2)"))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D0280)
    (at 129.286 75.946)
    (fp_text reference LED6 (at -0.0635 4.191) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8) (layer B.SilkS) hide)
    (pad 4 smd rect (at 1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(LED5-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(LED6-Pad2)"))
    (pad 1 smd rect (at 1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02CC)
    (at 205.486 75.946)
    (fp_text reference LED8 (at 0 4.191) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8) (layer B.SilkS) hide)
    (pad 4 smd rect (at 1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(LED7-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(LED8-Pad2)"))
    (pad 1 smd rect (at 1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02C7)
    (at 243.586 75.946)
    (fp_text reference LED9 (at 0 4.191 180) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(LED10-Pad4)"))
    (pad 3 smd rect (at -1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(LED8-Pad2)"))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02C2)
    (at 236.982 98.552)
    (fp_text reference LED10 (at 0.0635 -4.3815) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8) (layer B.SilkS) hide)
    (pad 4 smd rect (at 1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(LED10-Pad4)"))
    (pad 3 smd rect (at -1.65 -2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(LED10-Pad2)"))
    (pad 1 smd rect (at 1.65 2.4) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02BF)
    (at 243.5225 120.904 180)
    (fp_text reference LED11 (at 0 4.3815 180) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(LED11-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(LED10-Pad2)"))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02B9)
    (at 205.4225 120.904 180)
    (fp_text reference LED12 (at -0.0254 -4.2926) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8 180) (layer B.SilkS) hide)
    (pad 4 smd rect (at 1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(LED11-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(LED12-Pad2)"))
    (pad 1 smd rect (at 1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02B3)
    (at 181.991 120.904 180)
    (fp_text reference LED13 (at -0.0254 -4.3434 180) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8 180) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.65 2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(LED13-Pad2)"))
    (pad 3 smd rect (at -1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.65 -2.4 180) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(LED12-Pad2)"))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module WS2812B:WS2812B (layer B.Cu) (tedit 5B4D02AF)
    (at 150.29434 119.9642 270)
    (fp_text reference LED14 (at -3.429 0) (layer B.SilkS))
    (fp_text value WS2812B (at 0 -4.8 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at 1.65 2.4 270) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.65 2.4 270) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -1.65 -2.4 270) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.65 -2.4 270) (size 1.4 1.8) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(LED13-Pad2)"))
    (model ${KIPRJMOD}/3D/WS2812_RGB_LED_updated.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 43.51996 69.85648)
    (fp_text reference MX1 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 67 "Net-(MX1-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 68 COL0))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 68 COL0))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 62.56996 69.85648)
    (fp_text reference MX2 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 69 COL1))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 69 COL1))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 70 "Net-(MX2-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 81.61996 69.85648)
    (fp_text reference MX3 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 8 "Net-(D3-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 71 COL2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 71 COL2))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 72 "Net-(MX3-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 100.66996 69.85648)
    (fp_text reference MX4 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 73 "Net-(MX4-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 74 COL3))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 74 COL3))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 119.71996 69.85648)
    (fp_text reference MX5 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 75 "Net-(MX5-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 76 COL4))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 76 COL4))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 10 "Net-(D5-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 138.76996 69.85648)
    (fp_text reference MX6 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 77 "Net-(MX6-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 78 COL5))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 78 COL5))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 11 "Net-(D6-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 11 "Net-(D6-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 157.81996 69.85648)
    (fp_text reference MX7 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 79 "Net-(MX7-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 80 COL6))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 80 COL6))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 12 "Net-(D7-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 12 "Net-(D7-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 176.86996 69.85648)
    (fp_text reference MX8 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 13 "Net-(D8-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 13 "Net-(D8-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 81 COL7))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 81 COL7))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 82 "Net-(MX8-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 195.91996 69.85648)
    (fp_text reference MX9 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 83 "Net-(MX9-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 84 COL8))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 84 COL8))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 14 "Net-(D9-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 14 "Net-(D9-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 214.96996 69.85648)
    (fp_text reference MX10 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 15 "Net-(D10-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 15 "Net-(D10-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 85 COL9))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 85 COL9))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 86 "Net-(MX10-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 234.01996 69.85648)
    (fp_text reference MX11 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 87 "Net-(MX11-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 88 COL10))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 88 COL10))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 16 "Net-(D11-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 16 "Net-(D11-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 253.06996 69.85648)
    (fp_text reference MX12 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 17 "Net-(D12-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 17 "Net-(D12-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 89 COL11))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 89 COL11))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 90 "Net-(MX12-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 67.33052 88.90648)
    (fp_text reference MX14 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 20 "Net-(D14-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 20 "Net-(D14-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 69 COL1))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 69 COL1))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 92 "Net-(MX14-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 86.38052 88.90648)
    (fp_text reference MX15 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 93 "Net-(MX15-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 71 COL2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 71 COL2))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 21 "Net-(D15-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 21 "Net-(D15-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 105.43052 88.90648)
    (fp_text reference MX16 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 22 "Net-(D16-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 22 "Net-(D16-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 74 COL3))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 74 COL3))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 94 "Net-(MX16-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 124.48052 88.90648)
    (fp_text reference MX17 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 95 "Net-(MX17-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 76 COL4))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 76 COL4))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 23 "Net-(D17-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 23 "Net-(D17-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 143.53052 88.90648)
    (fp_text reference MX18 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 96 "Net-(MX18-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 78 COL5))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 78 COL5))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 24 "Net-(D18-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 24 "Net-(D18-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 162.58052 88.90648)
    (fp_text reference MX19 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 97 "Net-(MX19-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 80 COL6))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 80 COL6))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 25 "Net-(D19-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 25 "Net-(D19-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 181.63052 88.90648)
    (fp_text reference MX20 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 98 "Net-(MX20-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 81 COL7))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 81 COL7))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 26 "Net-(D20-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 26 "Net-(D20-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 200.68052 88.90648)
    (fp_text reference MX21 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 99 "Net-(MX21-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 84 COL8))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 84 COL8))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 27 "Net-(D21-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 27 "Net-(D21-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 219.73052 88.90648)
    (fp_text reference MX22 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 28 "Net-(D22-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 28 "Net-(D22-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 85 COL9))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 85 COL9))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 100 "Net-(MX22-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.75U locked (layer F.Cu) (tedit 5A9F3CCD)
    (at 245.92496 88.9022)
    (fp_text reference MX23 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.75U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 29 "Net-(D23-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 29 "Net-(D23-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 88 COL10))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 88 COL10))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 101 "Net-(MX23-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.5U locked (layer F.Cu) (tedit 5A9F3C23)
    (at 48.28032 107.95508)
    (fp_text reference MX24 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.5U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 30 "Net-(D24-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 30 "Net-(D24-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 68 COL0))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 68 COL0))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 102 "Net-(MX24-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 72.08792 107.95568)
    (fp_text reference MX25 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 32 "Net-(D25-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 32 "Net-(D25-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 69 COL1))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 69 COL1))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 103 "Net-(MX25-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 91.13792 107.95568)
    (fp_text reference MX26 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 33 "Net-(D26-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 33 "Net-(D26-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 71 COL2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 71 COL2))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 104 "Net-(MX26-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 110.18792 107.95568)
    (fp_text reference MX27 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 105 "Net-(MX27-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 74 COL3))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 74 COL3))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 34 "Net-(D27-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 34 "Net-(D27-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 129.23792 107.95568)
    (fp_text reference MX28 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 35 "Net-(D28-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 35 "Net-(D28-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 76 COL4))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 76 COL4))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 106 "Net-(MX28-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 148.28792 107.95568)
    (fp_text reference MX29 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 36 "Net-(D29-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 36 "Net-(D29-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 78 COL5))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 78 COL5))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 107 "Net-(MX29-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 167.33792 107.95568)
    (fp_text reference MX30 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 37 "Net-(D30-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 37 "Net-(D30-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 80 COL6))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 80 COL6))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 108 "Net-(MX30-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 186.38792 107.95568)
    (fp_text reference MX31 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 38 "Net-(D31-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 38 "Net-(D31-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 81 COL7))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 81 COL7))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 109 "Net-(MX31-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 205.43792 107.95568)
    (fp_text reference MX32 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 110 "Net-(MX32-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 84 COL8))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 84 COL8))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 39 "Net-(D32-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 39 "Net-(D32-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 224.48792 107.95568)
    (fp_text reference MX33 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 111 "Net-(MX33-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 85 COL9))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 85 COL9))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 40 "Net-(D33-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 40 "Net-(D33-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.25U locked (layer F.Cu) (tedit 5A9F3BE7)
    (at 45.90034 127.00254)
    (fp_text reference MX35 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.25U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 43 "Net-(D35-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 43 "Net-(D35-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 68 COL0))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 68 COL0))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 113 "Net-(MX35-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.25U locked (layer F.Cu) (tedit 5A9F3BE7)
    (at 69.71224 127.00254)
    (fp_text reference MX36 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.25U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 114 "Net-(MX36-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 69 COL1))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 69 COL1))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 44 "Net-(D36-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 44 "Net-(D36-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.25U locked (layer F.Cu) (tedit 5A9F3BE7)
    (at 93.5228 127.00254)
    (fp_text reference MX37 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.25U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 115 "Net-(MX37-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 71 COL2))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 71 COL2))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 45 "Net-(D37-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 45 "Net-(D37-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-2.75U locked (layer F.Cu) (tedit 5A9F41B2)
    (at 131.60756 126.99492 180)
    (fp_text reference MX38 (at 0 3.175 180) (layer Dwgs.User))
    (fp_text value MX-2.75U (at 0 -7.9375 180) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 266.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 46 "Net-(D38-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 46 "Net-(D38-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 228.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 76 COL4))
    (pad "" np_thru_hole circle (at 0 0 180) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4 180) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 76 COL4))
    (pad 3 thru_hole circle (at -1.27 5.08 180) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08 180) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 116 "Net-(MX38-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 228.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 228.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.938 -6.985 180) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.938 -6.985 180) (size 3.048 3.048) (drill 3.048) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.938 8.255 180) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.938 8.255 180) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.25U locked (layer F.Cu) (tedit 5A9F3BE7)
    (at 169.7222 127.00254)
    (fp_text reference MX39 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.25U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 47 "Net-(D39-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 47 "Net-(D39-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 80 COL6))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 80 COL6))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 117 "Net-(MX39-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.25U locked (layer F.Cu) (tedit 5A9F3BE7)
    (at 193.5353 127.00254)
    (fp_text reference MX40 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.25U (at 0 -7.9375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 118 "Net-(MX40-Pad4)"))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 81 COL7))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 81 COL7))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 48 "Net-(D40-Pad2)"))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 48 "Net-(D40-Pad2)"))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 214.96722 127.00254)
    (fp_text reference MX41 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 49 "Net-(D41-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 49 "Net-(D41-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 84 COL8))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 84 COL8))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 119 "Net-(MX41-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 234.01722 127.00254)
    (fp_text reference MX42 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 50 "Net-(D42-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 50 "Net-(D42-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 85 COL9))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 85 COL9))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 120 "Net-(MX42-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1U locked (layer F.Cu) (tedit 5A9F3A9A)
    (at 253.06722 127.00254)
    (fp_text reference MX43 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 51 "Net-(D43-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 51 "Net-(D43-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 89 COL11))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 89 COL11))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 121 "Net-(MX43-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 156.5148 122.0724 90)
    (attr smd)
    (fp_text reference NPNR1 (at -0.0254 1.5 90) (layer B.SilkS))
    (fp_text value 1.5k (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 122 "Net-(NPNR1-Pad2)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 122 "Net-(NPNR1-Pad2)"))
    (pad 1 smd rect (at 1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 123 LEDPWM))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 123 LEDPWM) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(NPNR1-Pad2)"))
    (pad 1 thru_hole circle (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 123 LEDPWM))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 238.506 85.344 90)
    (attr smd)
    (fp_text reference R1 (at -0.0254 1.5 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 125 RST))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 1 +5V) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 125 RST))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 125 RST) (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 100.711 130.7084 270)
    (attr smd)
    (fp_text reference R2 (at -0.0635 1.3335 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 126 "Net-(R2-Pad1)"))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 126 "Net-(R2-Pad1)") (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 126 "Net-(R2-Pad1)"))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 2 GND) (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 54.3306 67.437 270)
    (attr smd)
    (fp_text reference R3 (at -0.0254 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(MX1-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(MX1-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 67 "Net-(MX1-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 73.533 69.215 270)
    (attr smd)
    (fp_text reference R4 (at 0.127 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(MX2-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(MX2-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 70 "Net-(MX2-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 78.994 78.232 180)
    (attr smd)
    (fp_text reference R5 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 72 "Net-(MX3-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(MX3-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(MX3-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 111.633 69.215 270)
    (attr smd)
    (fp_text reference R6 (at -0.127 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(MX4-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(MX4-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 73 "Net-(MX4-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 119.507 78.105 180)
    (attr smd)
    (fp_text reference R7 (at 0.127 -1.524 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 75 "Net-(MX5-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(MX5-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(MX5-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 139.446 78.105 180)
    (attr smd)
    (fp_text reference R8 (at 0 -1.524 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 77 "Net-(MX6-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(MX6-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(MX6-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 149.733 69.215 270)
    (attr smd)
    (fp_text reference R9 (at -0.127 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(MX7-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(MX7-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 79 "Net-(MX7-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 177.038 78.232 180)
    (attr smd)
    (fp_text reference R10 (at -0.0254 -1.778 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 82 "Net-(MX8-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 82 "Net-(MX8-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(MX8-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 187.833 69.215 270)
    (attr smd)
    (fp_text reference R11 (at -0.127 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(MX9-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 83 "Net-(MX9-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 83 "Net-(MX9-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 214.884 78.105 180)
    (attr smd)
    (fp_text reference R12 (at -0.0254 -1.524 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 86 "Net-(MX10-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 86 "Net-(MX10-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(MX10-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 225.933 69.215 270)
    (attr smd)
    (fp_text reference R13 (at -0.127 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(MX11-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 87 "Net-(MX11-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 87 "Net-(MX11-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 253.492 78.105 180)
    (attr smd)
    (fp_text reference R14 (at -0.0254 1.397 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 90 "Net-(MX12-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 90 "Net-(MX12-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 90 "Net-(MX12-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 57.023 86.741 270)
    (attr smd)
    (fp_text reference R15 (at 0 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 91 "Net-(MX13-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 91 "Net-(MX13-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 91 "Net-(MX13-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 78.232 88.5444 270)
    (attr smd)
    (fp_text reference R16 (at -0.1016 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 92 "Net-(MX14-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 92 "Net-(MX14-Pad4)"))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 92 "Net-(MX14-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 97.4344 88.4428 270)
    (attr smd)
    (fp_text reference R17 (at -0.1778 -1.3716 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(MX15-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(MX15-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 93 "Net-(MX15-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 116.4336 88.4428 270)
    (attr smd)
    (fp_text reference R18 (at 0.0762 -1.4224 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 94 "Net-(MX16-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 94 "Net-(MX16-Pad4)"))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 94 "Net-(MX16-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 135.5344 88.392 270)
    (attr smd)
    (fp_text reference R19 (at 0.127 -1.3716 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 95 "Net-(MX17-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 95 "Net-(MX17-Pad4)"))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 95 "Net-(MX17-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 154.4828 88.392 270)
    (attr smd)
    (fp_text reference R20 (at 0 -1.3462 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 96 "Net-(MX18-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 96 "Net-(MX18-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 96 "Net-(MX18-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 173.5455 88.392 270)
    (attr smd)
    (fp_text reference R21 (at -0.127 -1.4605 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 97 "Net-(MX19-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(MX19-Pad4)"))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 97 "Net-(MX19-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 192.6082 90.2208 270)
    (attr smd)
    (fp_text reference R22 (at -0.0254 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(MX20-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(MX20-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 98 "Net-(MX20-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 197.739 80.899 180)
    (attr smd)
    (fp_text reference R23 (at 0.127 -1.397 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 99 "Net-(MX21-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 99 "Net-(MX21-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(MX21-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 211.582 88.392 270)
    (attr smd)
    (fp_text reference R24 (at 0 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 100 "Net-(MX22-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 100 "Net-(MX22-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 100 "Net-(MX22-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 258.191 88.138 270)
    (attr smd)
    (fp_text reference R25 (at -0.127 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(MX23-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 101 "Net-(MX23-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 101 "Net-(MX23-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B6E0860)
    (at 36.449 107.823 90)
    (attr smd)
    (fp_text reference R26 (at -1.10744 1.45288 90) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 90) (layer B.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 102 "Net-(MX24-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 102 "Net-(MX24-Pad4)"))
    (pad 1 smd rect (at 1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(MX24-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 70.612 97.282 180)
    (attr smd)
    (fp_text reference R27 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(MX25-Pad4)"))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 103 "Net-(MX25-Pad4)"))
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 103 "Net-(MX25-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 91.567 97.1296 180)
    (attr smd)
    (fp_text reference R28 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 104 "Net-(MX26-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 104 "Net-(MX26-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(MX26-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 120.523 105.918 270)
    (attr smd)
    (fp_text reference R29 (at -0.0254 -1.524 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 105 "Net-(MX27-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 105 "Net-(MX27-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 105 "Net-(MX27-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 140.208 105.918 270)
    (attr smd)
    (fp_text reference R30 (at -0.254 -1.524 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 106 "Net-(MX28-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 106 "Net-(MX28-Pad4)"))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(MX28-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 159.258 105.918 270)
    (attr smd)
    (fp_text reference R31 (at -0.127 -1.397 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 107 "Net-(MX29-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 107 "Net-(MX29-Pad4)"))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 107 "Net-(MX29-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 177.99558 105.88752 270)
    (attr smd)
    (fp_text reference R32 (at -2.159 4.064 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 108 "Net-(MX30-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 108 "Net-(MX30-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 108 "Net-(MX30-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 197.231 105.918 270)
    (attr smd)
    (fp_text reference R33 (at 0 -1.524 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 109 "Net-(MX31-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 109 "Net-(MX31-Pad4)"))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 109 "Net-(MX31-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 216.281 105.918 270)
    (attr smd)
    (fp_text reference R34 (at 0 -1.524 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(MX32-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 110 "Net-(MX32-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 110 "Net-(MX32-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 235.204 110.236 270)
    (attr smd)
    (fp_text reference R35 (at -0.0254 1.5 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 111 "Net-(MX33-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 111 "Net-(MX33-Pad4)"))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(MX33-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 259.842 104.013 90)
    (attr smd)
    (fp_text reference R36 (at 6.08076 0.03556 90) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 112 "Net-(MX34-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 112 "Net-(MX34-Pad4)"))
    (pad 1 smd rect (at 1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(MX34-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 37.719 122.381 90)
    (attr smd)
    (fp_text reference R37 (at -0.0254 1.5 90) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(MX35-Pad4)"))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 113 "Net-(MX35-Pad4)"))
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 113 "Net-(MX35-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 69.596 118.491 180)
    (attr smd)
    (fp_text reference R38 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 114 "Net-(MX36-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 114 "Net-(MX36-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(MX36-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 92.837 118.364 180)
    (attr smd)
    (fp_text reference R39 (at 0 -1.905 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(MX37-Pad4)"))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 115 "Net-(MX37-Pad4)"))
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 115 "Net-(MX37-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 138.9634 118.1354 90)
    (attr smd)
    (fp_text reference R40 (at -0.0254 1.5 90) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 116 "Net-(MX38-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 116 "Net-(MX38-Pad4)"))
    (pad 1 smd rect (at 1.35 0 90) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 90) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(MX38-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 169.037 118.3005 180)
    (attr smd)
    (fp_text reference R41 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(MX39-Pad4)"))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 117 "Net-(MX39-Pad4)"))
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 117 "Net-(MX39-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 192.9765 118.491 180)
    (attr smd)
    (fp_text reference R42 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(MX40-Pad4)"))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 118 "Net-(MX40-Pad4)"))
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 118 "Net-(MX40-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 214.757 118.6815 180)
    (attr smd)
    (fp_text reference R43 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 119 "Net-(MX41-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 119 "Net-(MX41-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(MX41-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 233.4895 118.6815 180)
    (attr smd)
    (fp_text reference R44 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(MX42-Pad4)"))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 120 "Net-(MX42-Pad4)"))
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 120 "Net-(MX42-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 253.5682 117.2718 180)
    (attr smd)
    (fp_text reference R45 (at -0.0254 1.5 180) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 121 "Net-(MX43-Pad4)") (solder_mask_margin -999))
    (pad 2 smd rect (at -1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 121 "Net-(MX43-Pad4)"))
    (pad 1 smd rect (at 1.35 0 180) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 124 LEDGND))
    (pad 1 smd rect (at 2.5 0 180) (size 2.9 0.5) (layers B.Cu)
      (net 124 LEDGND) (solder_mask_margin -999))
    (pad 2 thru_hole circle (at -3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(MX43-Pad4)"))
    (pad 1 thru_hole circle (at 3.9 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 124 LEDGND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Keebio-Parts:Resistor-Hybrid-Back (layer F.Cu) (tedit 5B0F073E)
    (at 81.788 130.048 270)
    (attr smd)
    (fp_text reference RGBR1 (at -0.0254 1.5 270) (layer B.SilkS))
    (fp_text value 470 (at 0 -1.925 270) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 127 RGBIN))
    (pad 2 thru_hole circle (at -3.9 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(LED1-Pad4)"))
    (pad 1 smd rect (at 2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 127 RGBIN) (solder_mask_margin -999))
    (pad 1 smd rect (at 1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 127 RGBIN))
    (pad 2 smd rect (at -1.35 0 270) (size 1.5 1.2) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(LED1-Pad4)"))
    (pad 2 smd rect (at -2.5 0 270) (size 2.9 0.5) (layers B.Cu)
      (net 54 "Net-(LED1-Pad4)") (solder_mask_margin -999))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.step
      (offset (xyz 0 0 -1.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module keyboard_parts:QFP44 locked (layer B.Cu) (tedit 5485B3DD)
    (at 109.093 126.238 270)
    (attr smd)
    (fp_text reference U1 (at 0 1.905 270) (layer B.SilkS))
    (fp_text value ATmega32U4 (at 0 -1.905 270) (layer B.SilkS))
    (pad 39 smd rect (at 0 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 71 COL2))
    (pad 40 smd rect (at -0.8001 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 69 COL1))
    (pad 41 smd rect (at -1.6002 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 68 COL0))
    (pad 42 smd rect (at -2.4003 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask))
    (pad 43 smd rect (at -3.2004 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 44 smd rect (at -4.0005 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 38 smd rect (at 0.8001 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 89 COL11))
    (pad 37 smd rect (at 1.6002 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask))
    (pad 36 smd rect (at 2.4003 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask))
    (pad 35 smd rect (at 3.2004 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 34 smd rect (at 4.0005 5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 17 smd rect (at 0 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 131 "Net-(U1-Pad17)"))
    (pad 16 smd rect (at -0.8001 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 132 "Net-(U1-Pad16)"))
    (pad 15 smd rect (at -1.6002 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -2.4003 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 13 smd rect (at -3.2004 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 125 RST))
    (pad 12 smd rect (at -4.0005 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 6 ROW0))
    (pad 18 smd rect (at 0.8001 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 42 ROW3))
    (pad 19 smd rect (at 1.6002 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 76 COL4))
    (pad 20 smd rect (at 2.4003 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 78 COL5))
    (pad 21 smd rect (at 3.2004 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 80 COL6))
    (pad 22 smd rect (at 4.0005 -5.715 270) (size 0.4064 1.524) (layers B.Cu B.Paste B.Mask)
      (net 81 COL7))
    (pad 6 smd rect (at -5.715 0 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C6-Pad2)"))
    (pad 28 smd rect (at 5.715 0 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -5.715 -0.8001 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 27 smd rect (at 5.715 -0.8001 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 88 COL10))
    (pad 26 smd rect (at 5.715 -1.6002 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 85 COL9))
    (pad 8 smd rect (at -5.715 -1.6002 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -5.715 -2.4003 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 129 SCK))
    (pad 25 smd rect (at 5.715 -2.4003 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 84 COL8))
    (pad 24 smd rect (at 5.715 -3.2004 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 10 smd rect (at -5.715 -3.2004 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 128 MOSI))
    (pad 11 smd rect (at -5.715 -4.0005 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 130 MISO))
    (pad 23 smd rect (at 5.715 -4.0005 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 29 smd rect (at 5.715 0.8001 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 123 LEDPWM))
    (pad 5 smd rect (at -5.715 0.8001 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -5.715 1.6002 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 133 D+))
    (pad 30 smd rect (at 5.715 1.6002 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 127 RGBIN))
    (pad 31 smd rect (at 5.715 2.4003 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 19 ROW1))
    (pad 3 smd rect (at -5.715 2.4003 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 134 D-))
    (pad 2 smd rect (at -5.715 3.2004 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 32 smd rect (at 5.715 3.2004 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 31 ROW2))
    (pad 33 smd rect (at 5.715 4.0005 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 126 "Net-(R2-Pad1)"))
    (pad 1 smd rect (at -5.715 4.0005 270) (size 1.524 0.4064) (layers B.Cu B.Paste B.Mask)
      (net 74 COL3))
    (model "${KIPRJMOD}/3D/qfp80p-10mmx10mm-44 v1.step"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Nexperia:SOT143B (layer B.Cu) (tedit 5B4BBDCA)
    (at 41.91 98.7425)
    (descr SOT143B)
    (solder_mask_margin 0.05)
    (attr smd)
    (fp_text reference U2 (at 0 2.3495) (layer B.SilkS))
    (fp_text value PRTR5V0U2X (at 0 -0.25) (layer B.Fab) hide)
    (fp_text user %R (at 0 0.254) (layer B.Fab))
    (pad 1 smd rect (at -0.75 -1) (size 1 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 -1) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 137 "Net-(J1-Pad3)"))
    (pad 3 smd rect (at 0.95 1) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 138 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at -0.95 1) (size 0.6 1.2) (layers B.Cu B.Paste B.Mask)
      (net 52 VCC))
    (model ${KIPRJMOD}/3D/TO-253AA.stp
      (offset (xyz -0.76 -1.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 120.015 130.429)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference XC1 (at 3.7465 0.1905) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 131 "Net-(U1-Pad17)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 120.015 123.8758 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference XC2 (at -3.8735 0.0635 180) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.249999 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 132 "Net-(U1-Pad16)"))
    (pad 2 smd rect (at 1.249999 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.5U locked (layer F.Cu) (tedit 5A9F3C23)
    (at 248.30532 107.95254)
    (fp_text reference MX34 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.25U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 41 "Net-(D34-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 41 "Net-(D34-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 88 COL10))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 88 COL10))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 112 "Net-(MX34-Pad4)"))
    (pad "" np_thru_hole circle (at -5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MX_Alps_Hybrid:MX-1.25U-FLIPPED locked (layer F.Cu) (tedit 5B4CD45B)
    (at 45.89996 88.90648)
    (fp_text reference MX13 (at 0 3.175) (layer Dwgs.User))
    (fp_text value MX-1.25U (at 0 -7.9375) (layer Dwgs.User))
    (pad 2 thru_hole oval (at 2.5 -4.5 86.0548) (size 2.831378 2.25) (drill 1.47 (offset 0.290689 0)) (layers *.Cu B.Mask)
      (net 18 "Net-(D13-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -5.08) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 18 "Net-(D13-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 48.0996) (size 4.211556 2.25) (drill 1.47 (offset 0.980778 0)) (layers *.Cu B.Mask)
      (net 68 COL0))
    (pad "" np_thru_hole circle (at 0 0) (size 3.9878 3.9878) (drill 3.9878) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.5 -4) (size 2.25 2.25) (drill 1.47) (layers *.Cu B.Mask)
      (net 68 COL0))
    (pad 3 thru_hole circle (at -1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 1 +5V))
    (pad 4 thru_hole rect (at 1.27 5.08) (size 1.905 1.905) (drill 1.04) (layers *.Cu B.Mask)
      (net 91 "Net-(MX13-Pad4)"))
    (pad "" np_thru_hole circle (at 5.08 0 48.0996) (size 1.75 1.75) (drill 1.75) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/MX_Alps_Hybrid.pretty-master/cherrymx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Type-C:HRO-TYPE-C-31-M-12-HandSoldering locked (layer B.Cu) (tedit 5ACED934)
    (at 30.4165 91.5035 90)
    (fp_text reference USB1 (at 0 10.2 90) (layer B.SilkS))
    (fp_text value HRO-TYPE-C-31-M-12 (at 0 -1.15 90) (layer Dwgs.User))
    (pad 13 thru_hole oval (at 4.32 2.6 90) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu F.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 13 thru_hole oval (at -4.32 2.6 90) (size 1 1.6) (drill oval 0.6 1.2) (layers *.Cu F.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 13 thru_hole oval (at 4.32 6.78 90) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu F.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 13 thru_hole oval (at -4.32 6.78 90) (size 1 2.1) (drill oval 0.6 1.7) (layers *.Cu F.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad "" np_thru_hole circle (at -2.89 6.25 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.89 6.25 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 smd rect (at -0.25 8.195 90) (size 0.3 2.45) (layers B.Cu B.Paste B.Mask)
      (net 137 "Net-(J1-Pad3)"))
    (pad 7 smd rect (at 0.25 8.195 90) (size 0.3 2.45) (layers B.Cu B.Paste B.Mask)
      (net 138 "Net-(J1-Pad2)"))
    (pad 8 smd rect (at 0.75 8.195 90) (size 0.3 2.45) (layers B.Cu B.Paste B.Mask)
      (net 137 "Net-(J1-Pad3)"))
    (pad 5 smd rect (at -0.75 8.195 90) (size 0.3 2.45) (layers B.Cu B.Paste B.Mask)
      (net 138 "Net-(J1-Pad2)"))
    (pad 9 smd rect (at 1.25 8.195 90) (size 0.3 2.45) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -1.25 8.195 90) (size 0.3 2.45) (layers B.Cu B.Paste B.Mask)
      (net 136 "Net-(UR4-Pad1)"))
    (pad 10 smd rect (at 1.75 8.195 90) (size 0.3 2.45) (layers B.Cu B.Paste B.Mask)
      (net 135 "Net-(UR3-Pad2)"))
    (pad 3 smd rect (at -1.75 8.195 90) (size 0.3 2.45) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -2.45 8.195 90) (size 0.6 2.45) (layers B.Cu B.Paste B.Mask)
      (net 52 VCC))
    (pad 11 smd rect (at 2.45 8.195 90) (size 0.6 2.45) (layers B.Cu B.Paste B.Mask)
      (net 52 VCC))
    (pad 1 smd rect (at -3.225 8.195 90) (size 0.6 2.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 3.225 8.195 90) (size 0.6 2.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KIPRJMOD}/3D/K3D-DX07B024JJ1-V1_JAE_Proprietary.STEP
      (offset (xyz 0 6.5 1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_HandSoldering (layer B.Cu) (tedit 0)
    (at 37.973 82.169)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann 433 Series, Hand Soldering,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann 433 Series Hand Soldering ")
    (attr smd)
    (fp_text reference F1 (at -0.05 2.2) (layer B.SilkS))
    (fp_text value "500mA Hold" (at -0.15 -2.5) (layer B.Fab))
    (pad 2 smd rect (at 2.09 0 270) (size 2.03 2.65) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -2.09 0 270) (size 2.03 2.65) (layers B.Cu B.Paste B.Mask)
      (net 52 VCC))
    (model ${KIPRJMOD}/3D/res1206r.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 46.99 99.80676)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference UR1 (at 0 1.66624) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 138 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 134 D-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 46.99 97.663 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference UR2 (at 0 1.524 180) (layer B.SilkS))
    (fp_text value 22 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 137 "Net-(J1-Pad3)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 133 D+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 51.34864 84.66582 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference UR3 (at 0 1.61036 90) (layer B.SilkS))
    (fp_text value 5.1k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 135 "Net-(UR3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 53.721 88.9 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference UR4 (at 0 1.651 90) (layer B.SilkS))
    (fp_text value 5.1k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 136 "Net-(UR4-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 35.179 99.187 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference UR5 (at -3.06832 0.04572 180) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C7-Pad2)"))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Mixed Lib:CPM12deg" (layer F.Cu) (tedit 0)
    (at 74.549 97.79)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module "Mixed Lib:CPMtitle4" (layer F.Cu) (tedit 5B5269E7)
    (at 158.623 122.3645)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 61.8236 79.9338 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at -2.0828 -4.064) (layer B.SilkS))
    (fp_text value Conn_01x04 (at 0 -9.95 270) (layer B.Fab))
    (fp_text user %R (at 0 -3.81 180) (layer B.Fab))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 VCC))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 137 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module keyboard_parts:PIN_1 (layer F.Cu) (tedit 5B8815F5)
    (at 62.103 62.484 90)
    (tags "CONN pin 1 circle")
    (fp_text reference P? (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 -1.45 90) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 3 2) (drill oval 2.7 1.7) (layers *.Cu *.Mask))
  )
  (gr_text JLCJLCJLCJLC (at 50.87112 134.86892) (layer B.SilkS))
  (gr_text GND (at 59.8678 79.8322 90) (layer B.SilkS))
  (gr_text VCC (at 71.4248 80.0608 90) (layer B.SilkS))
  (gr_text D+ (at 66.9798 82.1436 270) (layer B.SilkS))
  (gr_text "D-\n" (at 64.4144 82.169 270) (layer B.SilkS))
  (gr_text "22pF\n" (at 122.61088 121.93016) (layer B.SilkS))
  (gr_text "22pF\n" (at 123.2662 132.6007) (layer B.SilkS))
  (gr_text "1.5K\n\n" (at 155.64104 121.91492 90) (layer B.SilkS))
  (gr_text "10K\n" (at 237.07344 85.36432 90) (layer B.SilkS))
  (gr_text 0.1uF (at 172.27804 71.76516) (layer B.SilkS))
  (gr_text 0.1uF (at 133.71576 71.5772) (layer B.SilkS))
  (gr_text 0.1uF (at 210.44408 71.80072) (layer B.SilkS))
  (gr_text 0.1uF (at 96.8248 77.74432) (layer B.SilkS))
  (gr_text 4.7uF (at 101.78796 123.54814 270) (layer B.SilkS))
  (gr_text 0.1uF (at 115.2398 135.91032) (layer B.SilkS))
  (gr_text 1uF (at 111.3282 114.8334) (layer B.SilkS))
  (gr_text 0.1uF (at 241.56416 95.33636 90) (layer B.SilkS))
  (gr_text 0.1uF (at 101.69906 117.06606) (layer B.SilkS))
  (gr_text "10K\n" (at 98.1456 130.6322 90) (layer B.SilkS))
  (gr_text "4.7uF\n" (at 37.2364 99.4918 90) (layer B.SilkS))
  (gr_text 0.1uF (at 103.74884 136.05764) (layer B.SilkS))
  (gr_text 0.1uF (at 201.13752 114.2492) (layer B.SilkS))
  (gr_text 0.1uF (at 244.08384 112.44072 90) (layer B.SilkS))
  (gr_text 0.1uF (at 114.85372 116.84508 90) (layer B.SilkS))
  (gr_text 0.1uF (at 146.1262 124.50572 90) (layer B.SilkS))
  (gr_text 0.1uF (at 177.22088 115.5192) (layer B.SilkS))
  (gr_text 0.1uF (at 248.24436 71.74992) (layer B.SilkS))
  (gr_text 0.1uF (at 62.23508 115.74272 90) (layer B.SilkS))
  (gr_text 0.1uF (at 55.245 93.8022) (layer B.SilkS))
  (gr_text 0.1uF (at 58.58256 77.60716) (layer B.SilkS))
  (gr_line (start 33.274 97.282) (end 32.766 97.282) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32.766 85.852) (end 33.274 85.852) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 33.274 62.992) (end 33.274 85.852) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 33.274 97.282) (end 33.274 134.112) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 30.988 87.63) (end 30.988 95.504) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 32.766 87.63) (end 32.766 85.852) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 32.766 95.504) (end 30.988 95.504) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 36.068 60.198) (end 260.35 60.198) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 260.35 136.906) (end 36.068 136.906) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 263.144 62.992) (end 263.144 134.112) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 260.35 62.992) (end 263.144 62.992) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 260.35 134.112) (end 260.35 136.906) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 36.068 134.112) (end 33.274 134.112) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 36.068 62.992) (end 36.068 60.198) (angle -90) (layer Edge.Cuts) (width 0.2))
  (gr_text "Rev 2.0\n" (at 39.243 134.747) (layer B.SilkS))
  (gr_text "Pcb designed by Gtrx in collaboration with croa. Github repo: https://github.com/Gtrx0/cpm43" (at 157.099 97.917) (layer B.SilkS))
  (gr_text "5V\n" (at 126.4285 115.062 -45) (layer B.SilkS))
  (gr_text MOSI (at 132.7531 114.046 45) (layer B.SilkS))
  (gr_text GND (at 135.2677 114.3762 45) (layer B.SilkS))
  (gr_text "RST\n" (at 134.9502 120.5992 -45) (layer B.SilkS))
  (gr_text SCK (at 130.77952 120.30456) (layer B.SilkS))
  (gr_text MISO (at 125.3236 117.8179 -45) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.956 58.42) (xy 28.956 138.176) (xy 264.16 138.176) (xy 263.652 58.42)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.956 58.42) (xy 28.956 138.176) (xy 264.16 138.176) (xy 263.652 58.42)
      )
    )
  )
)
