(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad5)")
  (net 3 "Net-(J1-Pad7)")
  (net 4 "Net-(J1-Pad11)")
  (net 5 "Net-(J10-Pad1)")
  (net 6 "Net-(J10-Pad2)")
  (net 7 "Net-(J10-Pad3)")
  (net 8 "Net-(J10-Pad4)")
  (net 9 "Net-(J10-Pad5)")
  (net 10 "Net-(J10-Pad6)")
  (net 11 "Net-(J10-Pad7)")
  (net 12 "Net-(J10-Pad8)")
  (net 13 "Net-(J10-Pad9)")
  (net 14 "Net-(J1-Pad1)")
  (net 15 "Net-(J1-Pad3)")
  (net 16 "Net-(J1-Pad4)")
  (net 17 "Net-(J1-Pad6)")
  (net 18 "Net-(J1-Pad8)")
  (net 19 "Net-(J1-Pad9)")
  (net 20 "Net-(J1-Pad10)")
  (net 21 "Net-(J1-Pad13)")
  (net 22 "Net-(J1-Pad14)")
  (net 23 "Net-(J1-Pad15)")
  (footprint "Connector_Dsub:DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 137.605331 129.921 -90)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at 6.477 -2.602669 -90) (layer "F.SilkS"))
    (fp_text value "DB15_Female" (at -9.695 18.61 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -9.695 14.025 -90) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -26.345 1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "0" thru_hole circle (at 6.955 1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -13.85 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -16.62 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -19.39 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -1.385 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad9)") (pinfunction "P9") (pintype "passive"))
    (pad "10" thru_hole circle (at -4.155 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad10)") (pinfunction "P10") (pintype "passive"))
    (pad "11" thru_hole circle (at -6.925 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad11)") (pinfunction "P111") (pintype "passive"))
    (pad "12" thru_hole circle (at -9.695 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad11)") (pinfunction "P12") (pintype "passive"))
    (pad "13" thru_hole circle (at -12.465 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad13)") (pinfunction "P13") (pintype "passive"))
    (pad "14" thru_hole circle (at -15.235 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -18.005 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad15)") (pinfunction "P15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_Horizontal" (layer "F.Cu")
    (tedit 5A1DBF6A)
    (at 157.576 96.8425 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 2.89 0.0685 90) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack" (at -6.2 -5.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 -2.95) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 7 "Net-(J10-Pad3)") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -6 0 180) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(J10-Pad4)") (pintype "passive"))
    (pad "3" thru_hole roundrect (at -3 4.7 180) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 148.59 82.296 -90)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.905 1.27 180) (layer "F.SilkS"))
    (fp_text value "DB9_Female" (at -5.08 7.62 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.54 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J10-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J10-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J10-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J10-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J10-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -1.385 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J10-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -4.155 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -6.925 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J10-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -9.695 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J10-Pad9)") (pinfunction "9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 152.654 105.918 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP2" (at 0 -2.794 180) (layer "F.SilkS"))
    (fp_text value "Jumper_2_Open" (at -2.54 1.91 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad5)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J10-Pad4)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 165.5 106.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.Fab"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED1)
    (at 165.1 69.723 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Vertical || order number: 1803426 8A 160V")
    (tags "phoenix_contact connector MCV_01x02_G_3.81mm")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 1.9 -5.45 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 1.9 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.9 -3.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 9 "Net-(J10-Pad5)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.81 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(J10-Pad8)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_3-G-3.81_1x03_P3.81mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED1)
    (at 150.5425 64.516 180)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-3.81; number of pins: 03; pin pitch: 3.81mm; Vertical || order number: 1803439 8A 160V")
    (tags "phoenix_contact connector MCV_01x03_G_3.81mm")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at -3.5735 -2.54 90) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x03" (at 3.81 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -3.55) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 10 "Net-(J10-Pad6)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.81 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(J10-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.62 0 180) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(J10-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_3-G-3.81_1x03_P3.81mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 147.574 105.918 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP1" (at 0 -2.54 180) (layer "F.SilkS"))
    (fp_text value "Jumper_2_Open" (at 2.54 1.275 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad7)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J10-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 137.31 82.296 -90)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at -5.54 -2.8 90) (layer "F.SilkS"))
    (fp_text value "DB9_Female" (at -5.54 18.61 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -5.54 14.025 90) (layer "F.Fab"))
    (pad "0" thru_hole circle (at -18.04 1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "0" thru_hole circle (at 6.96 1.42 270) (size 4 4) (drill 3.2) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J10-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J10-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J10-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J10-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J10-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -1.385 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J10-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -4.155 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -6.925 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J10-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -9.695 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J10-Pad9)") (pinfunction "9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 130.25 96.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.Fab"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 146.75 136.25)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.2) (layer "F.Fab"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_3-G-3.81_1x03_P3.81mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED1)
    (at 165.1 122.174 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-3.81; number of pins: 03; pin pitch: 3.81mm; Vertical || order number: 1803439 8A 160V")
    (tags "phoenix_contact connector MCV_01x03_G_3.81mm")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 11.43 -0.508 180) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x02" (at 3.81 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -3.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 4 "Net-(J1-Pad11)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.81 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.62 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad15)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_3-G-3.81_1x03_P3.81mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_3-G-3.81_1x03_P3.81mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED1)
    (at 165.1 84.709 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/3-G-3.81; number of pins: 03; pin pitch: 3.81mm; Vertical || order number: 1803439 8A 160V")
    (tags "phoenix_contact connector MCV_01x03_G_3.81mm")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -3.937 0.254 180) (layer "F.SilkS"))
    (fp_text value "Screw_Terminal_01x03" (at 3.81 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 -3.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 13 "Net-(J10-Pad9)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.81 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(J10-Pad4)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.62 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J10-Pad7)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_3-G-3.81_1x03_P3.81mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 151.13 95.25)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at -2.54 1.275 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J10-Pad3)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J10-Pad4)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Dsub:DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm" (layer "F.Cu")
    (tedit 59FEDEE2)
    (at 146.685 129.921 -90)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.77x2.84mm, pin-PCB-offset 7.699999999999999mm, distance of mounting holes 33.3mm, distance of mounting holes to PCB edge 9.12mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.77x2.84mm pin-PCB-offset 7.699999999999999mm mounting-holes-distance 33.3mm mounting-hole-offset 33.3mm")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 1.905 1.27) (layer "F.SilkS"))
    (fp_text value "DB15_Female" (at -9.695 5.08 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.77 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.54 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -8.31 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -11.08 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad5)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -13.85 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad6)") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at -16.62 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad7)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at -19.39 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad8)") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at -1.385 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad9)") (pinfunction "P9") (pintype "passive"))
    (pad "10" thru_hole circle (at -4.155 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad10)") (pinfunction "P10") (pintype "passive"))
    (pad "11" thru_hole circle (at -6.925 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad11)") (pinfunction "P111") (pintype "passive"))
    (pad "12" thru_hole circle (at -9.695 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad11)") (pinfunction "P12") (pintype "passive"))
    (pad "13" thru_hole circle (at -12.465 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J1-Pad13)") (pinfunction "P13") (pintype "passive"))
    (pad "14" thru_hole circle (at -15.235 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad14)") (pinfunction "P14") (pintype "passive"))
    (pad "15" thru_hole circle (at -18.005 2.84 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad15)") (pinfunction "P15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-15_Female_Horizontal_P2.77x2.84mm_EdgePinOffset7.70mm_Housed_MountingHolesOffset9.12mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_Horizontal" (layer "F.Cu")
    (tedit 5A1DBF6A)
    (at 157.576 134.8155 180)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at -7.016 5.588) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack" (at -6.2 -5.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 -2.95) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad7)") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -6 0 180) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad5)") (pintype "passive"))
    (pad "3" thru_hole roundrect (at -3 4.7 180) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 156.75 64.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "MKS902B_breakout.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.Fab"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_rect (start 126.365 60.96) (end 168.91 140.208) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "0-10V" (at 157.226 69.85 90) (layer "F.SilkS"))
  (gr_text "-" (at 148.082 97.79) (layer "F.SilkS"))
  (gr_text "Tx" (at 159.004 75.946) (layer "F.SilkS"))
  (gr_text "Rx" (at 158.75 84.836) (layer "F.SilkS"))
  (gr_text "CHS GND" (at 156.972 114.554) (layer "F.SilkS"))
  (gr_text "NO    NC    COM" (at 147.32 69.596) (layer "F.SilkS"))
  (gr_text "9 10 11 12 13 14 15" (at 141.986 120.142 90) (layer "F.SilkS"))
  (gr_text "24V DC" (at 154.432 132.842 90) (layer "F.SilkS"))
  (gr_text "24V DC" (at 162.052 102.616) (layer "F.SilkS"))
  (gr_text "+" (at 148.082 95.25) (layer "F.SilkS"))
  (gr_text "SIG CMN" (at 156.972 122.428) (layer "F.SilkS"))
  (gr_text "CMN" (at 157.734 81.026) (layer "F.SilkS"))
  (gr_text " 6 7 8 9" (at 143.51 77.216 90) (layer "F.SilkS"))
  (gr_text "0-5V SIG" (at 156.718 118.872) (layer "F.SilkS"))
  (gr_text "+  -" (at 159.512 68.072 90) (layer "F.SilkS"))
  (gr_text "1 2 3 4 5" (at 151.13 76.581 90) (layer "F.SilkS"))
  (gr_text "1 2 3 4 5 6 7 8" (at 149.098 120.142 90) (layer "F.SilkS"))
  (gr_text "15-24VDC\nMKS GM50A" (at 141.478 104.648 90) (layer "F.SilkS"))
  (gr_text "9-30VDC\nMKS 902B" (at 141.478 88.138 90) (layer "F.SilkS"))
)
