(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 105)
    (no_connects 2)
    (area 121.674999 88.174999 177.075001 138.075001)
    (thickness 1.6)
    (drawings 39)
    (tracks 286)
    (zones 0)
    (modules 36)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.0762)
    (uvia_drill 0.0508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEEE9)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VIN)
  (net 3 VOUT)
  (net 4 SGND)
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(C6-Pad2)")
  (net 7 ITH)
  (net 8 "Net-(C8-Pad2)")
  (net 9 BOOST1)
  (net 10 SW1)
  (net 11 BOOST2)
  (net 12 SW2)
  (net 13 INTVCC)
  (net 14 "Net-(D3-Pad2)")
  (net 15 GATE_A)
  (net 16 GATE_B)
  (net 17 GATE_C)
  (net 18 GATE_D)
  (net 19 "Net-(R1-Pad2)")
  (net 20 "Net-(R2-Pad2)")
  (net 21 "Net-(R3-Pad1)")
  (net 22 VFB)
  (net 23 "Net-(U1-Pad9)")
  (net 24 "Net-(U1-Pad20)")
  (net 25 "Net-(U1-Pad28)")
  (net 26 GNDIN)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.0762)
    (uvia_drill 0.0508)
    (add_net BOOST1)
    (add_net BOOST2)
    (add_net GNDIN)
    (add_net INTVCC)
    (add_net ITH)
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad9)")
    (add_net SW1)
    (add_net SW2)
    (add_net VFB)
  )
  (net_class MED ""
    (clearance 0.1524)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.0762)
    (uvia_drill 0.0508)
    (add_net GATE_A)
    (add_net GATE_B)
    (add_net GATE_C)
    (add_net GATE_D)
  )
  (net_class WIDE ""
    (clearance 0.1524)
    (trace_width 0.3)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.0762)
    (uvia_drill 0.0508)
    (add_net GND)
    (add_net SGND)
    (add_net VIN)
    (add_net VOUT)
  )
  (module sensor_lib:SOIC8-INFINEON (layer F.Cu) (tedit 57A7DEF8)
    (at 123.25 110.5 270)
    (fp_text reference Q5 (at 2 -0.25 270) (layer F.SilkS))
    (fp_text value BSC009NE2LS (at 0 -0.5 270) (layer F.Fab))
    (pad 5 smd rect (at -6 -3.81 270) (size 0.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 GNDIN))
    (pad 4 smd rect (at 0 -3.81 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 3 smd rect (at 0 -2.54 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 -1.27 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -3.5 -1.905 270) (size 4.5 4.46) (layers F.Cu F.Paste F.Mask)
      (net 26 GNDIN))
    (pad 5 smd rect (at -6 -2.54 270) (size 0.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 GNDIN))
    (pad 5 smd rect (at -6 -1.27 270) (size 0.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 GNDIN))
    (pad 5 smd rect (at -6 0 270) (size 0.5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 GNDIN))
  )
  (module Oddities:NetTie-I_Connected_SMD (layer F.Cu) (tedit 57A7DB49)
    (at 149.25 127.25)
    (descr "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
    (tags "Just a \"Net tie\" as an more or less elegant way to connect two different nets without disturbing ERC and DRC.")
    (fp_text reference R0 (at -12 2) (layer F.SilkS) hide)
    (fp_text value 0 (at 0 -3.048) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 SGND))
  )
  (module sensor_lib:BHAVPAD (layer F.Cu) (tedit 57A7A317)
    (at 173.2 101)
    (fp_text reference - (at -3 0) (layer F.SilkS))
    (fp_text value BHAVPAD (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module sensor_lib:BHAVPAD (layer F.Cu) (tedit 57A7A30C)
    (at 173.2 94.6)
    (fp_text reference + (at -3 0) (layer F.SilkS))
    (fp_text value BHAVPAD (at 0 -0.4) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
  )
  (module sensor_lib:hxf_sensorworks_logo_20_17_pos (layer F.Cu) (tedit 0)
    (at 132.25 128.5)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module sensor_lib:BHAVPAD (layer F.Cu) (tedit 57A7A31E)
    (at 125.8 94.6)
    (fp_text reference + (at 3 0) (layer F.SilkS))
    (fp_text value BHAVPAD (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
  )
  (module sensor_lib:LIN-SSOP28 (layer F.Cu) (tedit 57A679AF)
    (at 144.25 130 90)
    (fp_text reference U1 (at 3.1 -1.15 90) (layer F.SilkS))
    (fp_text value LTC3789 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 22 VFB) (solder_mask_margin 0.05))
    (pad 2 smd rect (at 0 0.635 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)") (solder_mask_margin 0.05))
    (pad 3 smd rect (at 0 1.27 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R1-Pad2)") (solder_mask_margin 0.05))
    (pad 4 smd rect (at 0 1.905 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R2-Pad2)") (solder_mask_margin 0.05))
    (pad 5 smd rect (at 0 2.54 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 7 ITH) (solder_mask_margin 0.05))
    (pad 6 smd rect (at 0 3.175 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 4 SGND) (solder_mask_margin 0.05))
    (pad 7 smd rect (at 0 3.81 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 4 SGND) (solder_mask_margin 0.05))
    (pad 8 smd rect (at 0 4.445 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R3-Pad1)") (solder_mask_margin 0.05))
    (pad 9 smd rect (at 0 5.08 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad9)") (solder_mask_margin 0.05))
    (pad 10 smd rect (at 0 5.715 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN) (solder_mask_margin 0.05))
    (pad 11 smd rect (at 0 6.35 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT) (solder_mask_margin 0.05))
    (pad 12 smd rect (at 0 6.985 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 4 SGND) (solder_mask_margin 0.05))
    (pad 13 smd rect (at 0 7.62 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT) (solder_mask_margin 0.05))
    (pad 14 smd rect (at 0 8.255 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT) (solder_mask_margin 0.05))
    (pad 15 smd rect (at 5.1435 8.255 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad 16 smd rect (at 5.1435 7.62 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2) (solder_mask_margin 0.05))
    (pad 17 smd rect (at 5.1435 6.985 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 18 GATE_D) (solder_mask_margin 0.05))
    (pad 18 smd rect (at 5.1435 6.35 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 11 BOOST2) (solder_mask_margin 0.05))
    (pad 19 smd rect (at 5.1435 5.715 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 17 GATE_C) (solder_mask_margin 0.05))
    (pad 20 smd rect (at 5.1435 5.08 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad20)") (solder_mask_margin 0.05))
    (pad 21 smd rect (at 5.1435 4.445 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 13 INTVCC) (solder_mask_margin 0.05))
    (pad 22 smd rect (at 5.1435 3.81 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C6-Pad2)") (solder_mask_margin 0.05))
    (pad 23 smd rect (at 5.1435 3.175 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 16 GATE_B) (solder_mask_margin 0.05))
    (pad 24 smd rect (at 5.1435 2.54 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.05))
    (pad 25 smd rect (at 5.1435 1.905 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 9 BOOST1) (solder_mask_margin 0.05))
    (pad 26 smd rect (at 5.1435 1.27 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 15 GATE_A) (solder_mask_margin 0.05))
    (pad 27 smd rect (at 5.1435 0.635 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1) (solder_mask_margin 0.05))
    (pad 28 smd rect (at 5.1435 0 90) (size 1.27 0.4191) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad28)") (solder_mask_margin 0.05))
  )
  (module Resistors_SMD:R_2512_HandSoldering (layer F.Cu) (tedit 57A67A10)
    (at 148.25 113.5 270)
    (descr "Resistor SMD 2512, hand soldering")
    (tags "resistor 2512")
    (attr smd)
    (fp_text reference RS1 (at 0 -3.1 270) (layer F.SilkS))
    (fp_text value 8m (at 0 3.1 270) (layer F.Fab))
    (pad 2 smd rect (at 3.95 1.2 270) (size 2.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.01))
    (pad 2 smd rect (at 3.95 -1.2 270) (size 2.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.01))
    (pad 1 smd rect (at -3.95 0 270) (size 2.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)") (solder_mask_margin 0.01))
    (pad 1 smd rect (at -3.95 1.2 270) (size 2.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)") (solder_mask_margin 0.01))
    (pad 1 smd rect (at -3.95 -1.2 270) (size 2.7 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)") (solder_mask_margin 0.01))
    (pad 2 smd rect (at 3.95 0 270) (size 2.7 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.01))
    (model Resistors_SMD.3dshapes/R_2512_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L11.5_P3.5 (layer F.Cu) (tedit 57A7D7BA)
    (at 130.75 112.5 270)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 11.5mm, Pitch 3.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 7 0 270) (layer F.SilkS))
    (fp_text value 270uF (at 1.75 5.3 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 VIN))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L11.5_P3.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_10x10.5 (layer F.Cu) (tedit 57A69452)
    (at 169.75 110.25 180)
    (descr "SMT capacitor, aluminium electrolytic, 10x10.5")
    (attr smd)
    (fp_text reference C3 (at -0.05 6.075 360) (layer F.SilkS))
    (fp_text value 330uF (at 0 6.35 180) (layer F.Fab))
    (pad 1 smd rect (at 4.0005 0 180) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
    (pad 2 smd rect (at -4.0005 0 180) (size 4.0005 2.4003) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_10x10.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57A67DB2)
    (at 161.725 113.525 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -4.025 -0.025 360) (layer F.SilkS))
    (fp_text value 22uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A66F43)
    (at 142.24 134.62 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -0.254 -1.524 90) (layer F.SilkS))
    (fp_text value 6.8nF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 SGND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 144.018 120.904)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 2.1) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A67116)
    (at 151.13 133.858 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 3.302 0 180) (layer F.SilkS))
    (fp_text value 1nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 SGND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 ITH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A67118)
    (at 154.94 132.842 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 3.302 0 270) (layer F.SilkS))
    (fp_text value 3.3nF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 SGND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 57A66DA1)
    (at 141.75 122.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -0.5 1.75 270) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 BOOST1))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 154.75 122.5 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 0.22uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 BOOST2))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sensor_lib:XAL1010-COILCRAFT (layer F.Cu) (tedit 57A523CD)
    (at 145 93.75)
    (fp_text reference L1 (at 3.35 5.3) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2.38 9) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 2 smd rect (at 6.65 0) (size 2.38 9) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
  )
  (module sensor_lib:SOIC8-INFINEON (layer F.Cu) (tedit 57A67A54)
    (at 138.5 97.75)
    (fp_text reference Q1 (at -3 -5) (layer F.SilkS))
    (fp_text value BSC009NE2LS (at 0 -0.5) (layer F.Fab))
    (pad 5 smd rect (at -3.75 0) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 5 smd rect (at -3.75 -1.27) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 5 smd rect (at -3.75 -2.54) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 5 smd rect (at -3.75 -3.81) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 4 smd rect (at 0 -3.81) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 GATE_A))
    (pad 3 smd rect (at 0 -2.54) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 2 smd rect (at 0 -1.27) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 1 smd rect (at 0 0) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 5 smd rect (at -3.5 -1.905) (size 4.5 4.46) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
  )
  (module sensor_lib:SOIC8-INFINEON (layer F.Cu) (tedit 57A65826)
    (at 142.25 106.5 270)
    (fp_text reference Q2 (at -3 -5.25 270) (layer F.SilkS))
    (fp_text value BSC011N03LSI (at 0 -0.5 270) (layer F.Fab))
    (pad 5 smd rect (at -3.75 0 270) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 5 smd rect (at -3.75 -1.27 270) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 5 smd rect (at -3.75 -2.54 270) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 5 smd rect (at -3.75 -3.81 270) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 4 smd rect (at 0 -3.81 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 GATE_B))
    (pad 3 smd rect (at 0 -2.54 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0 -1.27 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at 0 0 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 5 smd rect (at -3.5 -1.905 270) (size 4.5 4.46) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
  )
  (module sensor_lib:SOIC8-INFINEON (layer F.Cu) (tedit 57A508AB)
    (at 150.5 106.5 270)
    (fp_text reference Q3 (at -2.95 1.2 270) (layer F.SilkS))
    (fp_text value BSC011N03LSI (at 0 -0.5 270) (layer F.Fab))
    (pad 5 smd rect (at -3.75 0 270) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (pad 5 smd rect (at -3.75 -1.27 270) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (pad 5 smd rect (at -3.75 -2.54 270) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (pad 5 smd rect (at -3.75 -3.81 270) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (pad 4 smd rect (at 0 -3.81 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 GATE_C))
    (pad 3 smd rect (at 0 -2.54 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0 -1.27 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at 0 0 270) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 5 smd rect (at -3.5 -1.905 270) (size 4.5 4.46) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
  )
  (module sensor_lib:SOIC8-INFINEON (layer F.Cu) (tedit 57A508AB)
    (at 158 94 180)
    (fp_text reference Q4 (at -2.95 1.2 180) (layer F.SilkS))
    (fp_text value BSC009NE2LS (at 0 -0.5 180) (layer F.Fab))
    (pad 5 smd rect (at -3.75 0 180) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
    (pad 5 smd rect (at -3.75 -1.27 180) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
    (pad 5 smd rect (at -3.75 -2.54 180) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
    (pad 5 smd rect (at -3.75 -3.81 180) (size 5 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
    (pad 4 smd rect (at 0 -3.81 180) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 GATE_D))
    (pad 3 smd rect (at 0 -2.54 180) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (pad 2 smd rect (at 0 -1.27 180) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (pad 1 smd rect (at 0 0 180) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (pad 5 smd rect (at -3.5 -1.905 180) (size 4.5 4.46) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57A7D1C8)
    (at 144.75 134.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -1.5 -2.25 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57A7D1CB)
    (at 146.75 134.5 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -1.5 2 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 57A6710E)
    (at 151.13 131.826)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.302 0) (layer F.SilkS))
    (fp_text value 162k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 SGND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57A67112)
    (at 154.75 132.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.302 0 270) (layer B.SilkS))
    (fp_text value 68K (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 ITH))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 54189DEE)
    (at 142.5 117 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 10 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 VIN))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57AA16EF)
    (at 166.25 116.5 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.75 270) (layer B.SilkS))
    (fp_text value 113k (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 VOUT))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 VFB))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 57A693A7)
    (at 167.6 120.4)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.4 0.1) (layer B.SilkS))
    (fp_text value 4.22k (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 VFB))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sensor_lib:PowerDI-123 (layer F.Cu) (tedit 57AA16CB)
    (at 145.5 121.75 180)
    (descr http://www.diodes.com/_files/datasheets/ds30497.pdf)
    (tags "PowerDI diode vishay")
    (attr smd)
    (fp_text reference D1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value DFLS160 (at 0 -3 180) (layer F.Fab))
    (pad 1 smd rect (at 0.85 0 180) (size 2.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 BOOST1))
    (pad 2 smd rect (at -1.525 0 180) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 INTVCC))
    (model Diodes_SMD.3dshapes/POWERDI-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sensor_lib:PowerDI-123 (layer F.Cu) (tedit 57AA16C7)
    (at 151 121.75)
    (descr http://www.diodes.com/_files/datasheets/ds30497.pdf)
    (tags "PowerDI diode vishay")
    (attr smd)
    (fp_text reference D2 (at 0 1.75) (layer F.SilkS))
    (fp_text value DFLS160 (at 0 -3) (layer F.Fab))
    (pad 1 smd rect (at 0.85 0) (size 2.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 BOOST2))
    (pad 2 smd rect (at -1.525 0) (size 1.05 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 INTVCC))
    (model Diodes_SMD.3dshapes/POWERDI-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SMA_Standard (layer F.Cu) (tedit 57A69465)
    (at 139.5 105.5 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D3 (at -0.1 2.85 270) (layer F.SilkS))
    (fp_text value B240A (at 0 4.3 270) (layer F.Fab))
    (fp_text user K (at -2.9 2.95 270) (layer F.SilkS) hide)
    (fp_text user A (at 2.9 2.9 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 10 SW1))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SMA_Standard (layer F.Cu) (tedit 57A69458)
    (at 159 100.75 180)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D4 (at 0 -2.75 180) (layer F.SilkS))
    (fp_text value B240A (at 0 4.3 180) (layer F.Fab))
    (fp_text user K (at -2.9 2.95 180) (layer F.SilkS) hide)
    (fp_text user A (at 3 -0.15 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.99898 0 180) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 VOUT))
    (pad 2 smd rect (at 1.99898 0 180) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 12 SW2))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 57A68979)
    (at 144.75 117.25 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -0.15 -1.75 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 13 INTVCC))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sensor_lib:BHAVPAD (layer F.Cu) (tedit 57A7D566)
    (at 125.8 101)
    (fp_text reference - (at 3 0) (layer F.SilkS))
    (fp_text value BHAVPAD (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 26 GNDIN))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 57A7D7B7)
    (at 136.25 114 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.5 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 121.75 135.5) (end 121.75 88.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.25 138) (end 121.75 135.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.5 138) (end 124.25 138) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177 135.5) (end 174.5 138) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177 88.25) (end 177 135.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.75 88.25) (end 177 88.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text OUTPUT (at 170 90.25) (layer F.SilkS))
  (gr_text INPUT (at 129 91) (layer F.SilkS))
  (gr_text "22V BOOST CONVERTER\nDESIGN INPUT 7.5-10V\nMAX CURRENT 3.5A\nREVISION 0.1" (at 165.5 128) (layer F.SilkS))
  (gr_text SW2 (at 157 90.25) (layer Eco1.User))
  (gr_text SW1 (at 139.5 90.25) (layer Eco1.User))
  (gr_text "BC COMMON SOURCE" (at 147.5 111) (layer Eco1.User))
  (gr_text "GND POUR" (at 159.725 125.225) (layer Eco1.User))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.108))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.75 119.45) (xy 148.4 119.8) (xy 148.1 119.8) (xy 147.75 119.45) (xy 147.75 115.95)
        (xy 148.75 115.95) (xy 148.75 119.45)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.108))
    (min_thickness 0.2)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.75 107.55) (xy 148.75 111.05) (xy 147.75 111.05) (xy 147.75 107.55) (xy 148.1 107.2)
        (xy 148.4 107.2) (xy 148.75 107.55)
      )
    )
  )
  (zone (net 3) (net_name VOUT) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.354)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 176.5 97.25) (xy 169 97.25) (xy 169 113.25) (xy 159.25 113.25) (xy 159.25 88.5)
        (xy 176.5 88.5) (xy 176.5 97.25)
      )
    )
  )
  (zone (net 12) (net_name SW2) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.354)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 158.75 105.25) (xy 148.75 105.25) (xy 148.75 88.5) (xy 158.75 88.5) (xy 158.75 105.25)
      )
    )
  )
  (zone (net 10) (net_name SW1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.354)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 147.75 105.25) (xy 137.75 105.25) (xy 137.75 88.5) (xy 147.75 88.5) (xy 147.75 105.25)
      )
    )
  )
  (zone (net 2) (net_name VIN) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.354)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 137.5 113.75) (xy 130.25 113.75) (xy 129.5 113.75) (xy 129.5 109.75) (xy 130.25 109.75)
        (xy 130.25 97.25) (xy 122.25 97.25) (xy 122.25 88.5) (xy 137.25 88.5) (xy 137.25 113.25)
      )
    )
  )
  (zone (net 14) (net_name "Net-(D3-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.354)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 158.5 113.5) (xy 138 113.5) (xy 138 105.75) (xy 158.5 105.75) (xy 158.5 113.5)
      )
    )
  )
  (zone (net 4) (net_name SGND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.354)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 176.5 135.25) (xy 174.25 137.5) (xy 124.5 137.5) (xy 122.25 135.25) (xy 122.25 128.25)
        (xy 149.25 128.25) (xy 149.25 126.5) (xy 176.5 126.5) (xy 176.5 135.25)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1))
    (min_thickness 0.354)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 176.5 126.25) (xy 148.75 126.25) (xy 148.75 128) (xy 122.25 128) (xy 122.25 109.75)
        (xy 128.75 109.75) (xy 128.75 114.25) (xy 170 114.25) (xy 170 98.25) (xy 176.5 98.25)
        (xy 176.5 126.25)
      )
    )
  )
  (zone (net 26) (net_name GNDIN) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.354)
    (fill yes (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.8))
    (polygon
      (pts
        (xy 129.25 109.25) (xy 122.25 109.25) (xy 122.25 98.25) (xy 129.25 98.25) (xy 129.25 109.25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.354)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.2) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 128.75 111.5) (xy 126.25 111.5) (xy 126.25 109.75) (xy 128.75 109.75) (xy 128.75 111.5)
      )
    )
  )
)
