(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 31)
    (no_connects 1)
    (area 136.830999 101.270999 158.063001 112.597001)
    (thickness 1.6)
    (drawings 4)
    (tracks 116)
    (zones 0)
    (modules 17)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 0.3048)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad3)")
  (net 7 "Net-(P1-Pad2)")
  (net 8 "Net-(P1-Pad3)")
  (net 9 "Net-(Q1-Pad1)")
  (net 10 "Net-(D2-Pad1)")
  (net 11 "Net-(D2-Pad2)")
  (net 12 3V3)
  (net 13 24V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 24V)
    (add_net 3V3)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D1-Pad3)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(Q1-Pad1)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 142.24 111.252 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5980B7BB)
    (at 141.986 104.394 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.524 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 12 3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5980CE77)
    (at 153.162 107.188 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 1.27 270) (layer F.SilkS))
    (fp_text value C (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23 (layer F.Cu) (tedit 5980B4A9)
    (at 145.542 106.426)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value BAT54S (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad3)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-323 (layer F.Cu) (tedit 5980CE74)
    (at 155.702 108.966 270)
    (tags "SMD SOT")
    (attr smd)
    (fp_text reference Q1 (at 2.032 -1.016 270) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at -0.65024 -0.94996 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0.65024 -0.94996 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (pad 3 smd rect (at 0 0.94996 270) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-323.wrl
      (at (xyz 0 0 0.001))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5980B7CF)
    (at 142.24 109.728)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 3.048 0) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 24V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5980CE87)
    (at 146.304 110.236 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.524 270) (layer F.SilkS))
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5980B7BE)
    (at 142.24 111.506)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 3.048 0) (layer F.SilkS))
    (fp_text value R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 24V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5980CE84)
    (at 149.606 108.458 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference RV1 (at -0.254 0 180) (layer F.SilkS))
    (fp_text value POT (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 1.2 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 1.2 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 3 smd rect (at 0 -1.50114 180) (size 1.2 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5980B5DD)
    (at 155.956 103.124)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference TP1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value INV_OUT (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(Q1-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5980B5D8)
    (at 145.796 103.124)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference TP2 (at 0 -5.1) (layer F.SilkS))
    (fp_text value RCV_OUT (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D1-Pad3)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 5980B5E5)
    (at 150.876 103.124)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference TP3 (at 0 -5.1) (layer F.SilkS))
    (fp_text value INV_IN (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C3-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5980B7C9)
    (at 141.732 104.394 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0.508 0 270) (layer F.SilkS))
    (fp_text value DS90LV (at -0.05 2.35 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 3V3))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P1-Pad2)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-353 (layer F.Cu) (tedit 5980CE80)
    (at 155.956 106.426)
    (descr SOT353)
    (attr smd)
    (fp_text reference U3 (at 0 0 90) (layer F.SilkS))
    (fp_text value 17SZ14 (at 0.09906 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.016 -0.635) (size 1 0.3048) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.016 0.635) (size 1 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.016 -0.635) (size 1 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 12 3V3))
    (pad 2 smd rect (at -1.016 0) (size 1 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at 1.016 0.635) (size 1 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(Q1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 138.176 103.124)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CANBUS (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 24V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer B.Cu) (tedit 0)
    (at 143.002 107.696 270)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U1 (at -0.09906 4.24942 270) (layer B.SilkS))
    (fp_text value LM7805 (at -0.20066 -4.59994 270) (layer B.Fab))
    (pad 1 smd rect (at -1.50114 -1.85166 270) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 12 3V3))
    (pad 2 smd rect (at 0 -1.85166 270) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.50114 -1.85166 270) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0 1.09982 270) (size 1.99898 2.99974) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd trapezoid (at 0 -0.7493 90) (size 1.50114 0.7493) (rect_delta 0 -0.50038 ) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT89-3_Housing.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5980CE70)
    (at 153.67 111.252 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D2 (at 1.524 1.524 180) (layer F.SilkS))
    (fp_text value LED (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 157.988 112.522) (end 157.988 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.906 101.346) (end 157.988 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.906 112.522) (end 136.906 101.346) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157.988 112.522) (end 136.906 112.522) (angle 90) (layer Edge.Cuts) (width 0.15))
)
