(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x0001330_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "meta/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "unconnected-(U1-Pad1)")
  (net 3 "unconnected-(U1-Pad2)")
  (net 4 "unconnected-(U1-Pad5)")
  (net 5 "/SDA")
  (net 6 "/SCL")
  (net 7 "unconnected-(J2-Pad4)")
  (net 8 "unconnected-(J2-Pad8)")
  (net 9 "unconnected-(J2-Pad10)")
  (net 10 "unconnected-(J2-Pad12)")
  (net 11 "unconnected-(J2-Pad13)")
  (net 12 "unconnected-(J2-Pad15)")
  (net 13 "unconnected-(J2-Pad16)")
  (net 14 "unconnected-(J2-Pad18)")
  (net 15 "unconnected-(J2-Pad19)")
  (net 16 "unconnected-(J2-Pad21)")
  (net 17 "unconnected-(J2-Pad22)")
  (net 18 "unconnected-(J2-Pad23)")
  (net 19 "unconnected-(J2-Pad24)")
  (net 20 "unconnected-(J2-Pad26)")
  (net 21 "unconnected-(J2-Pad27)")
  (net 22 "unconnected-(J2-Pad28)")
  (net 23 "unconnected-(J2-Pad32)")
  (net 24 "unconnected-(J2-Pad33)")
  (net 25 "unconnected-(J2-Pad35)")
  (net 26 "unconnected-(J2-Pad36)")
  (net 27 "unconnected-(J2-Pad37)")
  (net 28 "unconnected-(J2-Pad38)")
  (net 29 "unconnected-(J2-Pad40)")
  (net 30 "Net-(228EJVAYFR1-Pad1)")
  (net 31 "Net-(3.7V1-Pad1)")
  (net 32 "Net-(228EJVAYFR1-Pad5)")
  (net 33 "Net-(J2-Pad11)")
  (net 34 "unconnected-(J2-Pad17)")
  (net 35 "unconnected-(J2-Pad1)")
  (net 36 "unconnected-(U2-Pad1)")
  (net 37 "unconnected-(U2-Pad2)")
  (net 38 "unconnected-(U2-Pad4)")
  (net 39 "unconnected-(U2-Pad5)")
  (net 40 "unconnected-(U2-Pad6)")
  (net 41 "Net-(J2-Pad31)")
  (net 42 "unconnected-(228EJVAYFR1-Pad2)")
  (net 43 "Net-(228EJVAYFR1-Pad7)")
  (net 44 "Net-(J2-Pad29)")
  (net 45 "/5V_USB")
  (net 46 "/UPS_TRIGGER")
  (net 47 "Net-(12V_Batt1-Pad1)")
  (net 48 "Net-(R1-Pad2)")
  (footprint "RPi_Hat:RPi_Hat_Mounting_Hole" locked (layer "F.Cu")
    (tedit 55217C7B)
    (at 74 170.24)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (attr through_hole)
    (fp_text reference "" (at 0 -4.0005) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.09906 3.59918) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (footprint "RPi_Hat:RPi_Hat_Mounting_Hole" locked (layer "F.Cu")
    (tedit 55217CA2)
    (at 16 170.24)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (attr through_hole)
    (fp_text reference "" (at 0 -4.0005) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.09906 3.59918) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (footprint "RPi_Hat:RPi_Hat_Mounting_Hole" locked (layer "F.Cu")
    (tedit 55217CCB)
    (at 74 193.24)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (attr through_hole)
    (fp_text reference "" (at 0 -4.0005) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.09906 3.59918) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (footprint "RPi_Hat:RPi_Hat_Mounting_Hole" locked (layer "F.Cu")
    (tedit 55217CCB)
    (at 16 193.24)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (attr through_hole)
    (fp_text reference "" (at 0 -4.0005) (layer "F.SilkS") hide)
    (fp_text value "" (at 0.09906 3.59918) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 53.34 177.8 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 0 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad29)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 46.99 175.26)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(3.7V1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/UPS_TRIGGER") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 58.42 193.04 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "3.7V1" (at 2.194644 1.108246) (layer "F.SilkS"))
    (fp_text value "3.7V Battery" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(3.7V1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 33.02 185.42)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 0) (layer "F.SilkS"))
    (fp_text value "22K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(R1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(12V_Batt1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 43.18 187.96 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 0) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 66.04 193.04 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "From Pi" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/UPS_TRIGGER") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/5V_USB") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "New FootPrint Library:228EJVAYFR" (layer "F.Cu")
    (tedit 0)
    (at 20.36 182.88 -90)
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "228EJVAYFR1" (at 0 5.08 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Switch_w/_LED" (at 0 -5.08 -90 unlocked) (layer "F.Fab"))
    (fp_circle (center -1.75 -1.7) (end -1.25 -1.7) (layer "Edge.Cuts") (width 0.12) (fill none))
    (fp_circle (center 1.75 -1.7) (end 2.25 -1.7) (layer "Edge.Cuts") (width 0.12) (fill none))
    (pad "1" smd roundrect (at -3.175 -2.5 270) (size 1.65 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 30 "Net-(228EJVAYFR1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at 3.175 -2.5 270) (size 1.65 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 42 "unconnected-(228EJVAYFR1-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "3" smd roundrect (at -3.175 -0.9 270) (size 1.65 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1))
    (pad "4" smd roundrect (at 3.175 -0.9 270) (size 1.65 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "GND") (pinfunction "A") (pintype "input"))
    (pad "5" smd roundrect (at 3.175 0.9 270) (size 1.65 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 32 "Net-(228EJVAYFR1-Pad5)") (pinfunction "L2") (pintype "input"))
    (pad "6" smd roundrect (at -3.175 2.5 270) (size 1.65 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1))
    (pad "7" smd roundrect (at 3.175 2.5 270) (size 1.65 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 43 "Net-(228EJVAYFR1-Pad7)") (pinfunction "L1") (pintype "input"))
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 50.8 187.96 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 5.08 0 90) (layer "F.SilkS"))
    (fp_text value "4.7K" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "/5V_USB") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad29)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED5CC)
    (at 20.87 171.51 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -2.33 90) (layer "F.SilkS"))
    (fp_text value "RPi_GPIO" (at 1.27 50.59 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 24.13) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "unconnected-(J2-Pad1)") (pinfunction "3.3V") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(228EJVAYFR1-Pad7)") (pinfunction "5V") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/SDA") (pinfunction "GPIO02_SDA1_I2C") (pintype "bidirectional"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J2-Pad4)") (pinfunction "5V") (pintype "power_in"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/SCL") (pinfunction "GPIO03_SCL1_I2C") (pintype "bidirectional"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(228EJVAYFR1-Pad1)") (pinfunction "GPIO04_GCLK") (pintype "bidirectional"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J2-Pad8)") (pinfunction "GPIO14_TXD0") (pintype "bidirectional"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "10" thru_hole oval locked (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "unconnected-(J2-Pad10)") (pinfunction "GPIO15_RXD0") (pintype "bidirectional"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad11)") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "12" thru_hole oval locked (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J2-Pad12)") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "unconnected-(J2-Pad13)") (pinfunction "GPIO27") (pintype "bidirectional"))
    (pad "14" thru_hole oval locked (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "unconnected-(J2-Pad15)") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "16" thru_hole oval locked (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "unconnected-(J2-Pad16)") (pinfunction "GPIO23") (pintype "bidirectional"))
    (pad "17" thru_hole oval locked (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J2-Pad17)") (pinfunction "3.3V") (pintype "power_in"))
    (pad "18" thru_hole oval locked (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "unconnected-(J2-Pad18)") (pinfunction "GPIO24") (pintype "bidirectional"))
    (pad "19" thru_hole oval locked (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "unconnected-(J2-Pad19)") (pinfunction "GPIO10_SPI_MOSI") (pintype "bidirectional"))
    (pad "20" thru_hole oval locked (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "21" thru_hole oval locked (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "unconnected-(J2-Pad21)") (pinfunction "GPIO09_SPI_MISO") (pintype "bidirectional"))
    (pad "22" thru_hole oval locked (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J2-Pad22)") (pinfunction "GPIO25") (pintype "bidirectional"))
    (pad "23" thru_hole oval locked (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "unconnected-(J2-Pad23)") (pinfunction "GPIO11_SPI_CLK") (pintype "bidirectional"))
    (pad "24" thru_hole oval locked (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "unconnected-(J2-Pad24)") (pinfunction "GPIO08_SPI_CE0_N") (pintype "bidirectional"))
    (pad "25" thru_hole oval locked (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "26" thru_hole oval locked (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "unconnected-(J2-Pad26)") (pinfunction "GPIO07_SPI_CE1_N") (pintype "bidirectional"))
    (pad "27" thru_hole oval locked (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "unconnected-(J2-Pad27)") (pinfunction "ID_SD") (pintype "bidirectional"))
    (pad "28" thru_hole oval locked (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J2-Pad28)") (pinfunction "ID_SC") (pintype "bidirectional"))
    (pad "29" thru_hole oval locked (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad29)") (pinfunction "GPIO05") (pintype "bidirectional"))
    (pad "30" thru_hole oval locked (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "31" thru_hole oval locked (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad31)") (pinfunction "GPIO06") (pintype "bidirectional"))
    (pad "32" thru_hole oval locked (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J2-Pad32)") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "33" thru_hole oval locked (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "unconnected-(J2-Pad33)") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "34" thru_hole oval locked (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole oval locked (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J2-Pad35)") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "36" thru_hole oval locked (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J2-Pad36)") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "37" thru_hole oval locked (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "unconnected-(J2-Pad37)") (pinfunction "GPIO26") (pintype "bidirectional"))
    (pad "38" thru_hole oval locked (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "unconnected-(J2-Pad38)") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "39" thru_hole oval locked (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "40" thru_hole oval locked (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "unconnected-(J2-Pad40)") (pinfunction "GPIO21") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 27.94 190.5 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 5.08 -2.37 90) (layer "F.SilkS"))
    (fp_text value "250" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(228EJVAYFR1-Pad5)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(J2-Pad11)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 72.217099 175.055939 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 5.08 -2.37) (layer "F.SilkS"))
    (fp_text value "10K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad31)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "New FootPrint Library:Adafruit ADS1115" (layer "F.Cu")
    (tedit 0)
    (at 38.1 185.42 90)
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 7.62 90 unlocked) (layer "F.SilkS"))
    (fp_text value "Adafruit_ADS1115_Breakout" (at 0 12.7 90 unlocked) (layer "F.Fab"))
    (fp_text user "VIN" (at 6.705274 8.918212 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -10.16 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -7.62 5.08 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 36 "unconnected-(U2-Pad1)") (pinfunction "AIN3") (pintype "input"))
    (pad "2" thru_hole circle (at -7.62 2.54 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 37 "unconnected-(U2-Pad2)") (pinfunction "AIN2") (pintype "input"))
    (pad "3" thru_hole circle (at -7.62 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(R1-Pad2)") (pinfunction "AIN1") (pintype "input"))
    (pad "4" thru_hole circle (at -7.62 -2.54 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 38 "unconnected-(U2-Pad4)") (pinfunction "AIN0") (pintype "input"))
    (pad "5" thru_hole circle (at 5.08 -5.08 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 39 "unconnected-(U2-Pad5)") (pinfunction "ALERT") (pintype "input"))
    (pad "6" thru_hole circle (at 5.08 -2.54 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 40 "unconnected-(U2-Pad6)") (pinfunction "ADDR") (pintype "input"))
    (pad "7" thru_hole circle (at 5.08 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 "/SDA") (pinfunction "SDA") (pintype "input"))
    (pad "8" thru_hole circle (at 5.08 2.54 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "9" thru_hole circle (at 5.08 5.08 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "10" thru_hole circle (at 5.08 7.62 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(228EJVAYFR1-Pad7)") (pinfunction "VIN") (pintype "input"))
    (pad "11" thru_hole circle (at -7.62 7.62 90) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad "12" thru_hole circle (at -7.62 -5.08 90) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  )
  (footprint "New FootPrint Library:DF robot lipo connection" (layer "F.Cu")
    (tedit 0)
    (at 25.4 194.25)
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -0.5 unlocked) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 0 5.08 unlocked) (layer "F.Fab"))
    (fp_text user "3.7V" (at 0 -2.54 unlocked) (layer "F.SilkS"))
    (fp_text user "+" (at 3.81 0 unlocked) (layer "F.SilkS"))
    (fp_text user "-" (at -3.81 0 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.6 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.6 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(3.7V1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 66.116797 186.360878 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "ATtiny85-20P" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "unconnected-(U1-Pad1)") (pinfunction "~{RESET}/PB5") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "unconnected-(U1-Pad2)") (pinfunction "XTAL1/PB3") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "/UPS_TRIGGER") (pinfunction "XTAL2/PB4") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "unconnected-(U1-Pad5)") (pinfunction "AREF/PB0") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad31)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad29)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(3.7V1-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 73.66 180.34)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "AEROLINUX UPS HAT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "12V_Batt1" (at 2.54 1.27 90) (layer "F.SilkS"))
    (fp_text value "12V Battery" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(12V_Batt1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 15.5 196.74) (mid 13.37868 195.86132) (end 12.5 193.74) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 77.5 193.74) (mid 76.62132 195.86132) (end 74.5 196.74) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 74.5 166.74) (mid 76.62132 167.61868) (end 77.5 169.74) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 15.5 166.74) (end 74.5 166.74) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 12.5 169.74) (mid 13.37868 167.61868) (end 15.5 166.74) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 12.5 169.74) (end 12.5 193.74) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 77.5 169.74) (end 77.5 193.74) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 15.5 196.74) (end 74.5 196.74) (layer "Edge.Cuts") (width 0.1))
  (gr_text "R.Pi Zero AEROLINUX UPS HAT V1.2\nZ. McBride NASA GSFC 03/2023" (at 30.48 175.26) (layer "B.SilkS"))
  (gr_text "5V" (at 63.47 195.58) (layer "F.SilkS"))
  (gr_text "SHUTDOWN" (at 15.24 182.88 270) (layer "F.SilkS"))
  (gr_text "Select one of these board edges depending \nupon the type of socket that is used." (at 20.5 9.5) (layer "Cmts.User"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 20 54.5) (xy 20 51))
    (height 2.5)
    (gr_text "3.5000 mm" (at 20.85 52.75 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 78.5 54.5) (xy 78.5 24.5))
    (height 3.5)
    (gr_text "30.0000 mm" (at 80.35 39.5 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 78.5 54.5) (xy 78.5 24))
    (height 8.5)
    (gr_text "30.5000 mm" (at 85.35 39.25 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 16.068883 55.2811) (xy 12.568883 55.2811))
    (height -3)
    (gr_text "3.5000 mm" (at 14.318883 56.6311) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 45 32) (xy 16 32))
    (height -2.499999)
    (gr_text "29.0000 mm" (at 30.5 32.849999) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 77.5 23) (xy 12.5 23))
    (height 7)
    (gr_text "65.0000 mm" (at 45 14.35) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 11.5 28) (xy 11.5 51))
    (height 2.5)
    (gr_text "23.0000 mm" (at 7.35 39.5 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 74 23) (xy 16 23))
    (height 2.5)
    (gr_text "58.0000 mm" (at 45 18.85) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 81.28 200.66)
        (xy 10.16 200.66)
        (xy 10.16 165.1)
        (xy 81.28 165.1)
      )
    )
  )
)
