(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A")
	(title_block
		(title "ZX81 Issue ONE D")
		(date "2024")
		(company "Sinclair")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Test/")
		)
	)
	(net 0 "")
	(net 1 "D0")
	(net 2 "D1")
	(net 3 "D2")
	(net 4 "D3")
	(net 5 "D4")
	(net 6 "D5")
	(net 7 "D6")
	(net 8 "D7")
	(net 9 "D'0")
	(net 10 "D'1")
	(net 11 "D'2")
	(net 12 "D'3")
	(net 13 "D'4")
	(net 14 "D'5")
	(net 15 "D'6")
	(net 16 "D'7")
	(net 17 "+5V")
	(net 18 "GND")
	(net 19 "A0")
	(net 20 "A1")
	(net 21 "A2")
	(net 22 "A3")
	(net 23 "A4")
	(net 24 "A5")
	(net 25 "A7")
	(net 26 "A8")
	(net 27 "A9")
	(net 28 "A10")
	(net 29 "A11")
	(net 30 "A12")
	(net 31 "A13")
	(net 32 "A14")
	(net 33 "A15")
	(net 34 "A'0")
	(net 35 "A'1")
	(net 36 "A'2")
	(net 37 "A'3")
	(net 38 "A'4")
	(net 39 "A'5")
	(net 40 "A'6")
	(net 41 "A'7")
	(net 42 "A'8")
	(net 43 "/M1")
	(net 44 "/MREQ")
	(net 45 "/IORQ")
	(net 46 "/RD")
	(net 47 "/WR")
	(net 48 "/RFSH")
	(net 49 "/HALT")
	(net 50 "/WAIT")
	(net 51 "A6/INT")
	(net 52 "/NMI")
	(net 53 "/RESET")
	(net 54 "/BUSRQ")
	(net 55 "/BUSAK")
	(net 56 "CLK")
	(net 57 "/RAMCS")
	(net 58 "/ROMCS")
	(net 59 "N$1")
	(net 60 "N$2")
	(net 61 "KBD0")
	(net 62 "KBD1")
	(net 63 "KBD2")
	(net 64 "KBD3")
	(net 65 "KBD4")
	(net 66 "USA/UK")
	(net 67 "N$17")
	(net 68 "TAPE_IN")
	(net 69 "TAPEIN")
	(net 70 "VIDEO")
	(net 71 "N$21")
	(net 72 "TAPE_OUT")
	(net 73 "N$23")
	(net 74 "N$25")
	(net 75 "CHNSW")
	(net 76 "N$3")
	(net 77 "N$4")
	(net 78 "N$5")
	(net 79 "N$6")
	(net 80 "PHI")
	(net 81 "+9V")
	(net 82 "N$8")
	(net 83 "N$9")
	(net 84 "N$10")
	(net 85 "N$11")
	(net 86 "N$12")
	(net 87 "N$13")
	(net 88 "N$14")
	(net 89 "N$15")
	(net 90 "N$152")
	(net 91 "N$153")
	(net 92 "N$155")
	(net 93 "N$18")
	(net 94 "N$19")
	(net 95 "N$16")
	(net 96 "N$20")
	(footprint "ZXKLINKE4POL"
		(layer "F.Cu")
		(at 82.64485 141.35485)
		(property "Reference" "K4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DCIN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 2.1 4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "+9V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "1'" thru_hole circle
			(at 2.1 -4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "+9V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -2.1 4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2'" thru_hole circle
			(at -2.1 -4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "DIL18"
		(layer "F.Cu")
		(at 202.02485 108.96985)
		(property "Reference" "IC4a"
			(at 2.46515 -9.60985 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2114"
			(at -3.175 13.716 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -3.81 -10.16)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -3.81 -7.62)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -3.81 -5.08)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -3.81 -2.54)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -3.81 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -3.81 2.54)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "A2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at -3.81 5.08)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "A0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at -3.81 7.62)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/RAMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at -3.81 10.16)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at 3.81 10.16 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/WR")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at 3.81 7.62 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "D'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at 3.81 5.08 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "D'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "D'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at 3.81 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "D'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "A1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at 3.81 -5.08 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at 3.81 -7.62 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at 3.81 -10.16 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "JUMPER"
		(layer "F.Cu")
		(at 145.187218 89.76296 -90)
		(property "Reference" "JP3"
			(at 2.93704 -1.422782 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at -2.84296 2.567218 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -1.27 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "N$5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 1.27 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "A13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 154.641006 146.359082)
		(property "Reference" "R81"
			(at -2.131006 0.870918 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -2.286 0.5588 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "N$19")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "SIL8P"
		(layer "F.Cu")
		(at 140.27745 106.897932 -90)
		(property "Reference" "RP5"
			(at -10.16 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "470"
			(at -2.54 -1.27 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -8.89 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "D'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "D5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -3.81 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "D6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -1.27 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "D'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 1.27 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "D'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 3.81 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "D7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "D0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 8.89 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "D'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 92.37235 118.2186 -90)
		(property "Reference" "C10"
			(at 1.7114 -0.84765 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at -2.286 2.794 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "TAPE_IN")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "N$17")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "SIL10"
		(layer "F.Cu")
		(at 169.63985 101.1911 -90)
		(property "Reference" "RP2"
			(at 1.6689 1.28985 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "not used"
			(at -2.54 -1.27 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "1"
			(at -13.1011 -0.46015 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -11.43 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -8.89 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -3.81 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -1.27 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 1.27 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 3.81 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "A2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at 8.89 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "A1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at 11.43 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "A0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "ZX81CON"
		(layer "F.Cu")
		(at 189.9561 56.6596)
		(property "Reference" "K1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ZX81CONN"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A1" smd rect
			(at -27.94 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 16 "D'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A2" smd rect
			(at -25.4 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 57 "/RAMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A4" smd rect
			(at -20.32 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 9 "D'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A5" smd rect
			(at -17.78 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 10 "D'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A6" smd rect
			(at -15.24 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 11 "D'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A7" smd rect
			(at -12.7 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 15 "D'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A8" smd rect
			(at -10.16 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 14 "D'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A9" smd rect
			(at -7.62 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 12 "D'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A10" smd rect
			(at -5.08 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 13 "D'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A11" smd rect
			(at -2.54 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A12" smd rect
			(at 0 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 52 "/NMI")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A13" smd rect
			(at 2.54 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 49 "/HALT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A14" smd rect
			(at 5.08 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 44 "/MREQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A15" smd rect
			(at 7.62 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 45 "/IORQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A16" smd rect
			(at 10.16 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 46 "/RD")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A17" smd rect
			(at 12.7 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 47 "/WR")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A18" smd rect
			(at 15.24 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 55 "/BUSAK")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A19" smd rect
			(at 17.78 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 50 "/WAIT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A20" smd rect
			(at 20.32 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 54 "/BUSRQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A21" smd rect
			(at 22.86 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 53 "/RESET")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A22" smd rect
			(at 25.4 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 43 "/M1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "A23" smd rect
			(at 27.94 2.54 180)
			(size 1.524 6.477)
			(layers "F.Cu" "F.Mask")
			(net 48 "/RFSH")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B1" smd rect
			(at -27.94 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B2" smd rect
			(at -25.4 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 81 "+9V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B4" smd rect
			(at -20.32 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B5" smd rect
			(at -17.78 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B6" smd rect
			(at -15.24 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 80 "PHI")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B7" smd rect
			(at -12.7 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 19 "A0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B8" smd rect
			(at -10.16 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 20 "A1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B9" smd rect
			(at -7.62 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 21 "A2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B10" smd rect
			(at -5.08 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 22 "A3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B11" smd rect
			(at -2.54 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 33 "A15")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B12" smd rect
			(at 0 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 32 "A14")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B13" smd rect
			(at 2.54 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 31 "A13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B14" smd rect
			(at 5.08 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 30 "A12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B15" smd rect
			(at 7.62 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 29 "A11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B16" smd rect
			(at 10.16 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 28 "A10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B17" smd rect
			(at 12.7 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 27 "A9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B18" smd rect
			(at 15.24 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 26 "A8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B19" smd rect
			(at 17.78 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 25 "A7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B20" smd rect
			(at 20.32 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B21" smd rect
			(at 22.86 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 24 "A5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B22" smd rect
			(at 25.4 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 23 "A4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "B23" smd rect
			(at 27.94 2.54 180)
			(size 1.524 6.477)
			(layers "B.Cu" "B.Mask")
			(net 58 "/ROMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 138.7211 88.3661)
		(property "Reference" "C7"
			(at -1.5611 0.8239 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2n2"
			(at -2.286 2.794 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "PHI")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "N$6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 110.29485 58.06985)
		(property "Reference" "R1"
			(at -1.59485 0.89015 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -2.91485 -1.26985 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/HALT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "N$3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "JUMPER"
		(layer "F.Cu")
		(at 152.4311 141.6686 90)
		(property "Reference" "JP1"
			(at 0.3486 1.5789 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at -2.54 3.175 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -1.27 0 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "N$18")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "E3,8-5"
		(layer "F.Cu")
		(at 136.5561 73.8436 180)
		(property "Reference" "C5"
			(at 0.7561 1.3836 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1µF"
			(at -1.4139 4.1236 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "+" thru_hole circle
			(at -1.905 0 180)
			(size 1.6002 1.6002)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/RESET")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "-" thru_hole circle
			(at 1.905 0 180)
			(size 1.6002 1.6002)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 109.63235 133.41735 180)
		(property "Reference" "R30"
			(at 2.21235 -0.88265 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "USA only"
			(at -2.286 0.5588 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "USA/UK")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "DIL28"
		(layer "F.Cu")
		(at 202.8186 105.15985)
		(property "Reference" "IC4"
			(at -1.8286 -11.07985 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "62256"
			(at -5.08 -7.62 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A14")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "A12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "A1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at -7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at -7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at -7.62 6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "A2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at -7.62 8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "A0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at -7.62 11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "D'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at -7.62 13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "D'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at -7.62 16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "D'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at -7.62 19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at 7.62 19.05 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "D'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at 7.62 16.51 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "D'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at 7.62 13.97 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "D'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at 7.62 11.43 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "D'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "19" thru_hole circle
			(at 7.62 8.89 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "D'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "20" thru_hole circle
			(at 7.62 6.35 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/RAMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "21" thru_hole circle
			(at 7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "A10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "22" thru_hole circle
			(at 7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/RAMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "23" thru_hole circle
			(at 7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "A11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at 7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "25" thru_hole circle
			(at 7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "26" thru_hole circle
			(at 7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "A13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "27" thru_hole circle
			(at 7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/WR")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "28" thru_hole circle
			(at 7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "78XXL"
		(layer "F.Cu")
		(at 90.8745 149.3 -90)
		(property "Reference" "REG"
			(at -6.9511 -6.79015 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "7805"
			(at 2.77 -10.81 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "GND" thru_hole oval
			(at 0 0)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "IN" thru_hole oval
			(at -2.54 0)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "+9V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "OUT" thru_hole oval
			(at 2.54 0)
			(size 3.048 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 212.81985 144.52985 -90)
		(property "Reference" "D7"
			(at -3.175 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4148"
			(at -3.175 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "N$14")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A14")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 214.2486 82.61735)
		(property "Reference" "@HOLE4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 149.7961 72.2986)
		(property "Reference" "@HOLE2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 125.878287 82.52931 -90)
		(property "Reference" "C6"
			(at 1.50069 -0.841713 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100p"
			(at -2.286 2.794 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "N$5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "N$4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 110.3011 60.9161)
		(property "Reference" "C1"
			(at -1.5 0.8439 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47p"
			(at -1.4011 2.7039 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/HALT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "N$3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "ZXKLINKE4POL"
		(layer "F.Cu")
		(at 82.64485 112.14485)
		(property "Reference" "K3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "EAR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 2.1 4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "TAPE_IN")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "1'" thru_hole circle
			(at 2.1 -4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "TAPE_IN")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -2.1 4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2'" thru_hole circle
			(at -2.1 -4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 197.57985 144.52985 -90)
		(property "Reference" "D1"
			(at -3.175 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4148"
			(at -3.175 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "N$8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "A11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 125.480125 64.137991 90)
		(property "Reference" "R2"
			(at -1.642009 0.859875 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "680"
			(at -1.632009 -1.140125 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "N$1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/RAMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "ZXKBD8"
		(layer "F.Cu")
		(at 206.46985 150.87985)
		(property "Reference" "KB2"
			(at 0.02015 2.36015 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ZXKBD8CON"
			(at 1.27 -1.905 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "P$1" thru_hole circle
			(at -8.89 0)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "N$8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" thru_hole circle
			(at -6.35 0)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "N$9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$3" thru_hole circle
			(at -3.81 0)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "N$10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$4" thru_hole circle
			(at -1.27 0)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "N$11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$5" thru_hole circle
			(at 1.27 0)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "N$12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$6" thru_hole circle
			(at 3.81 0)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "N$13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$7" thru_hole circle
			(at 6.35 0)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "N$14")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$8" thru_hole circle
			(at 8.89 0)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "N$15")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 140.562159 64.213391 90)
		(property "Reference" "R35"
			(at -2.326609 0.867841 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -3.826609 -1.232159 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "N$16")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 132.51985 90.92985)
		(property "Reference" "R3"
			(at -1.59985 0.87015 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "not used"
			(at -3.32985 2.45015 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "N$6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "JUMPER"
		(layer "F.Cu")
		(at 128.033806 59.05405 -90)
		(property "Reference" "JP4"
			(at 4.04595 1.273806 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at -3.87405 -2.736194 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -1.27 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "N$3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 1.27 0)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "N$20")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "SIL8P"
		(layer "F.Cu")
		(at 128.6261 104.2536 -90)
		(property "Reference" "RP4"
			(at -10.16 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "470"
			(at -2.54 -1.27 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -8.89 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "D'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "D4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -3.81 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "D3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -1.27 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "D'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 1.27 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "D2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 3.81 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "D'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "D1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 8.89 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "D'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 128.630212 73.273979 -90)
		(property "Reference" "C4"
			(at 1.576021 -0.819788 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at -2.286 2.794 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 141.5686 85.80485)
		(property "Reference" "R6"
			(at -1.5586 0.86515 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2k2"
			(at -2.286 0.5588 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "PHI")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "N$6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "B3F-31XX"
		(layer "F.Cu")
		(at 81.9461 66.4536 -90)
		(descr "OMRON SWITCH")
		(property "Reference" "S1"
			(at -4.0036 3.2061 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Reset"
			(at -3.683 5.969 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole roundrect
			(at -2.2606 1.2446 270)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole roundrect
			(at 2.2606 1.2446 270)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(chamfer_ratio 0.2928932188)
			(chamfer top_left top_right bottom_left bottom_right)
			(net 53 "/RESET")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -3.5052 -1.2446 270)
			(size 2.159 2.159)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 3.5052 -1.2446 270)
			(size 2.159 2.159)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 133.260621 82.58275 -90)
		(property "Reference" "R4"
			(at 1.17725 -0.889379 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "18k"
			(at -2.286 0.5588 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "N$5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 138.64 79.33)
		(property "Reference" "T2"
			(at 1.27 -2.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "NPN"
			(at 1.5 1.09 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "C"
			(at 0.72 0.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B"
			(at -1.42 0.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "E"
			(at -3.43 0.44 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "B" thru_hole circle
			(at 0 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "N$6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at 2.11 -0.01)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "CLK")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "E" thru_hole circle
			(at -2.07 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 205.24485 128.6361 180)
		(property "Reference" "C9"
			(at -1.50515 0.7861 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at -2.286 2.794 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "SIL8P"
		(layer "F.Cu")
		(at 186.1261 138.7536)
		(property "Reference" "RP6"
			(at -10.16 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at -2.54 -1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -8.89 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "A'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -3.81 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "A'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -1.27 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 1.27 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "A'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 3.81 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "A'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 8.89 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "A0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "DIL28"
		(layer "F.Cu")
		(at 134.387 132.788344)
		(property "Reference" "IC2"
			(at -1.927 -11.588344 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "27C512"
			(at -5.08 -7.62 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "N$19")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "A12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "A'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "A'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "A'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "A'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at -7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "A'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at -7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "A'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at -7.62 6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "A'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at -7.62 8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "A'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at -7.62 11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "D'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at -7.62 13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "D'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at -7.62 16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "D'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at -7.62 19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at 7.62 19.05 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "D'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at 7.62 16.51 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "D'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at 7.62 13.97 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "D'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at 7.62 11.43 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "D'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "19" thru_hole circle
			(at 7.62 8.89 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "D'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "20" thru_hole circle
			(at 7.62 6.35 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/ROMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "21" thru_hole circle
			(at 7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "A10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "22" thru_hole circle
			(at 7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/ROMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "23" thru_hole circle
			(at 7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "A11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at 7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "25" thru_hole circle
			(at 7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "A'8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "26" thru_hole circle
			(at 7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "A13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "27" thru_hole circle
			(at 7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "N$18")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "28" thru_hole circle
			(at 7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "ZXKLINKE4POL"
		(layer "F.Cu")
		(at 82.64485 126.74985)
		(property "Reference" "K2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MIC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 2.1 4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "TAPE_OUT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "1'" thru_hole circle
			(at 2.1 -4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "TAPE_OUT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -2.1 4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2'" thru_hole circle
			(at -2.1 -4.7)
			(size 3.816 3.816)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "E5-5"
		(layer "F.Cu")
		(at 144.486218 60.730438 -90)
		(property "Reference" "C3"
			(at 0.939562 1.596218 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22µF"
			(at -4.980438 -1.843782 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "+" thru_hole circle
			(at -2.54 0 270)
			(size 1.6002 1.6002)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "+9V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "-" thru_hole circle
			(at 2.54 0 270)
			(size 1.6002 1.6002)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 149.95485 59.12235)
		(property "Reference" "@HOLE1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "DIL40"
		(layer "F.Cu")
		(at 114.8711 91.50735)
		(property "Reference" "IC1"
			(at -1.5911 -20.87735 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ZX81ULA"
			(at -5.08 -17.78 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -7.62 -24.13)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "A'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -7.62 -21.59)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "A'8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -7.62 -19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "A'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -7.62 -16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "A'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "A'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/RD")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at -7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/IORQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at -7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/WR")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at -7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/MREQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at -7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/M1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at -7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A14")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at -7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "N$1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at -7.62 6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "N$2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at -7.62 8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "PHI")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at -7.62 11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/NMI")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at -7.62 13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "VIDEO")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at -7.62 16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/HALT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at -7.62 19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "A15")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "19" thru_hole circle
			(at -7.62 21.59)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "D7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "20" thru_hole circle
			(at -7.62 24.13)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "TAPEIN")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "21" thru_hole circle
			(at 7.62 24.13)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "D6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "22" thru_hole circle
			(at 7.62 21.59)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "USA/UK")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "23" thru_hole circle
			(at 7.62 19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "D5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at 7.62 16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "D4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "25" thru_hole circle
			(at 7.62 13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "KBD4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "26" thru_hole circle
			(at 7.62 11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "D3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "27" thru_hole circle
			(at 7.62 8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "KBD3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "28" thru_hole circle
			(at 7.62 6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "D2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "29" thru_hole circle
			(at 7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "KBD2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "30" thru_hole circle
			(at 7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "D1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "31" thru_hole circle
			(at 7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "KBD1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "32" thru_hole circle
			(at 7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "D0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "33" thru_hole circle
			(at 7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "KBD0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "34" thru_hole circle
			(at 7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "35" thru_hole circle
			(at 7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "N$5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "36" thru_hole circle
			(at 7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "A'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "37" thru_hole circle
			(at 7.62 -16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "A'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "38" thru_hole circle
			(at 7.62 -19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "A'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "39" thru_hole circle
			(at 7.62 -21.59)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "A'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "40" thru_hole circle
			(at 7.62 -24.13)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "ZXKDB5"
		(layer "F.Cu")
		(at 184.87985 152.78485 180)
		(property "Reference" "KB1"
			(at -0.07015 0.95485 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ZXKBD5CON"
			(at 0 -1.905 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "P$1" thru_hole circle
			(at -5.08 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "KBD0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$2" thru_hole circle
			(at -2.54 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "KBD1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$3" thru_hole circle
			(at 0 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "KBD2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$4" thru_hole circle
			(at 2.54 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "KBD3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$5" thru_hole circle
			(at 5.08 0 180)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "KBD4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 210.27985 144.52985 -90)
		(property "Reference" "D6"
			(at -3.175 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4148"
			(at -3.175 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "N$13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 189.92735 84.23235 -90)
		(property "Reference" "R17"
			(at 2.30765 -0.87265 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.286 0.5588 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/WAIT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "SIL6"
		(layer "F.Cu")
		(at 186.14985 146.43485 180)
		(property "Reference" "RP3"
			(at -1.83015 2.57485 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "1"
			(at -7.86015 -0.47515 180)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "KBD0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -1.27 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "KBD1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 1.27 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "KBD2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "KBD3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "KBD4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 205.19985 144.52985 -90)
		(property "Reference" "D4"
			(at -3.175 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4148"
			(at -3.175 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "N$11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "HC49"
		(layer "F.Cu")
		(at 129.623181 82.659794 -90)
		(property "Reference" "X1"
			(at 1.670206 -0.866819 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "6,5MHz"
			(at -5.08 3.937 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.413 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.413 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "N$4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 215.373175 144.53985 -90)
		(property "Reference" "D8"
			(at -3.175 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4148"
			(at -3.175 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "N$15")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "A15")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 91.3761 111.19235)
		(property "Reference" "@HOLE0"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 176.51985 84.0736 -90)
		(property "Reference" "R15"
			(at 2.2864 -0.86015 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "220k"
			(at -2.286 0.5588 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/RESET")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "SIL10P"
		(layer "F.Cu")
		(at 186.1261 131.7536)
		(property "Reference" "RP7"
			(at -12.7 -1.27 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at -2.54 -1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "1"
			(at -13.7461 0.508 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -11.43 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "A1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -8.89 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "A'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "A'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -3.81 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "A2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -1.27 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "A'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 1.27 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 3.81 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "A'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at 8.89 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "A'8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at 11.43 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 141.581593 83.171444 180)
		(property "Reference" "R5"
			(at 1.591593 -0.888556 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at -1.698407 2.451444 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "CLK")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "PINHEAD2X4"
		(layer "F.Cu")
		(at 98.3611 88.1736 90)
		(property "Reference" "K5"
			(at -11.110622 -2.616425 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PINHEAD-2X4"
			(at -9.1464 3.1489 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -7.62 0 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "CHNSW")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -7.62 -2.54 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -5.08 0 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "TAPE_IN")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -5.08 -2.54 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "VIDEO")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -2.54 0 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "USA/UK")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -2.54 -2.54 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/RESET")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 0 0 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 0 -2.54 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 95.5036 141.03735 180)
		(property "Reference" "R27"
			(at 2.2936 -0.87265 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.286 0.5588 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "TAPE_OUT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 200.11985 144.52985 -90)
		(property "Reference" "D2"
			(at -3.175 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4148"
			(at -3.175 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "N$9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "A10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 166.267721 137.563435)
		(property "Reference" "C8"
			(at -1.577721 0.886565 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at -2.286 2.794 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "SIL9"
		(layer "F.Cu")
		(at 146.6211 111.3511 90)
		(property "Reference" "RP1"
			(at -1.9189 -1.2711 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -1.27 -1.27 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "1"
			(at -12.5089 0.5089 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -10.16 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -7.62 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "D1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -5.08 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "D0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -2.54 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "D7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 0 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "D2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 2.54 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "D6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 5.08 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "D5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 7.62 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "D3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at 10.16 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "D4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 114.8711 144.6886)
		(property "Reference" "@HOLE5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "JUMPER"
		(layer "F.Cu")
		(at 149.8911 141.6686 90)
		(property "Reference" "JP2"
			(at 0.3186 -5.7011 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "JUMPER"
			(at -2.54 3.175 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -1.27 0 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 1.27 0 180)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "N$19")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 154.64479 137.566891)
		(property "Reference" "R80"
			(at -2.27479 0.903109 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -2.286 0.5588 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "N$18")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 132.98 60.31)
		(property "Reference" "T3"
			(at 1.2 -2.69 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 1.48 1.14 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "C"
			(at -3.43 0.44 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "E"
			(at 0.72 0.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B"
			(at -1.42 0.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "B" thru_hole circle
			(at 0 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/WAIT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at 2.11 -0.01)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "N$16")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "E" thru_hole circle
			(at -2.07 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "N$20")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 97.5361 131.2711)
		(property "Reference" "R32"
			(at -2.2461 0.8889 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "not used"
			(at -9.8161 1.7189 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "N$25")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "N$23")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D15"
		(layer "F.Cu")
		(at 96.2411 128.2111 180)
		(property "Reference" "D9"
			(at 1.397 -0.635 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 2.0411 -0.7589 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 5.08 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "VIDEO")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -5.08 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "N$23")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 101.8536 121.35235)
		(property "Reference" "R33"
			(at -2.2836 0.88765 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at -1.6836 -1.20235 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "N$17")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "TAPEIN")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 184.8861 84.17735 90)
		(property "Reference" "R16"
			(at -2.28265 0.8739 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.286 0.5588 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 90)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/BUSRQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 202.65985 144.52985 -90)
		(property "Reference" "D3"
			(at -3.175 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4148"
			(at -3.175 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "N$10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "A12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 121.14 58.6)
		(property "Reference" "T1"
			(at 1.48 -2.69 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "NPN"
			(at 1.53 1.14 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at -1.27 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "C"
			(at 0.72 0.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "E"
			(at -3.43 0.44 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B"
			(at -1.42 0.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "B" thru_hole circle
			(at 0 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "N$3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at 2.11 -0.01)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/WAIT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "E" thru_hole circle
			(at -2.07 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/NMI")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 137.788506 60.372979 -90)
		(property "Reference" "C2"
			(at 1.567021 -0.861494 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at -5.092979 -1.861494 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 96.93235 137.7036)
		(property "Reference" "R29"
			(at -2.21235 0.8964 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at -2.286 0.5588 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "N$21")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "VIDEO")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "DIL18"
		(layer "F.Cu")
		(at 178.52985 106.2711)
		(property "Reference" "IC4b"
			(at 2.53015 -9.4311 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2114"
			(at -3.175 13.716 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -3.81 -10.16)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -3.81 -7.62)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -3.81 -5.08)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -3.81 -2.54)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -3.81 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -3.81 2.54)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "A2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at -3.81 5.08)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "A0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at -3.81 7.62)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/RAMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at -3.81 10.16)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at 3.81 10.16 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/WR")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at 3.81 7.62 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "D'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at 3.81 5.08 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "D'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "D'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at 3.81 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "D'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "A1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at 3.81 -5.08 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at 3.81 -7.62 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at 3.81 -10.16 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 93.43985 125.79735)
		(property "Reference" "C11"
			(at -1.63985 0.98265 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47n"
			(at -3.92985 1.77265 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "TAPE_OUT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 98.858846 109.939744 -90)
		(property "Reference" "R34"
			(at 2.240256 -0.901154 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at -0.609744 2.318846 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "TAPE_IN")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 98.0436 134.68735 180)
		(property "Reference" "R31"
			(at 2.1536 -0.88265 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "not used"
			(at 3.5536 -0.42265 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "N$25")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 191.22985 72.2986)
		(property "Reference" "@HOLE3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 2.8)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "C025-025X050"
		(layer "F.Cu")
		(at 93.43985 123.4161)
		(property "Reference" "C12"
			(at -1.69985 0.8339 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47pF"
			(at -4.02985 0.8839 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "TAPE_OUT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "N$21")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "DIL24"
		(layer "F.Cu")
		(at 131.847 137.868344)
		(property "Reference" "IC2B0"
			(at -3.047 -11.238344 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ZXROM-SMALL"
			(at -5.08 -7.62 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "A'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "A'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "A'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "A'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "A'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "A'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at -7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "A'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at -7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "A'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at -7.62 6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "D'0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at -7.62 8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "D'1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at -7.62 11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "D'2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at -7.62 13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at 7.62 13.97 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "D'3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at 7.62 11.43 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "D'4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at 7.62 8.89 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "D'5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at 7.62 6.35 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "D'6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at 7.62 3.81 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "D'7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at 7.62 1.27 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "A11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "19" thru_hole circle
			(at 7.62 -1.27 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "A10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "20" thru_hole circle
			(at 7.62 -3.81 180)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/ROMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "21" thru_hole circle
			(at 7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "A12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "22" thru_hole circle
			(at 7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "23" thru_hole circle
			(at 7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "A'8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at 7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "R207_12"
		(layer "F.Cu")
		(at 112.80735 137.7036)
		(property "Reference" "R28"
			(at -2.27735 0.8764 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "680"
			(at -2.286 0.5588 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "N$2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/ROMCS")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "DIL40"
		(layer "F.Cu")
		(at 157.89235 110.0811)
		(property "Reference" "IC3"
			(at -2.05235 -21.0411 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Z80CPU"
			(at -5.08 -17.78 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at -7.62 -24.13)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "A11")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -7.62 -21.59)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "A12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -7.62 -19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "A13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -7.62 -16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "A14")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "A15")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "CLK")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at -7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "D4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at -7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "D3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at -7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "D5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10" thru_hole circle
			(at -7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "D6")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11" thru_hole circle
			(at -7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "+5V")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12" thru_hole circle
			(at -7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "D2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13" thru_hole circle
			(at -7.62 6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "D7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14" thru_hole circle
			(at -7.62 8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "D0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15" thru_hole circle
			(at -7.62 11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "D1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16" thru_hole circle
			(at -7.62 13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "17" thru_hole circle
			(at -7.62 16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/NMI")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "18" thru_hole circle
			(at -7.62 19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/HALT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "19" thru_hole circle
			(at -7.62 21.59)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/MREQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "20" thru_hole circle
			(at -7.62 24.13)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/IORQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "21" thru_hole circle
			(at 7.62 24.13)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/RD")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "22" thru_hole circle
			(at 7.62 21.59)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/WR")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "23" thru_hole circle
			(at 7.62 19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/BUSAK")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at 7.62 16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/WAIT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "25" thru_hole circle
			(at 7.62 13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/BUSRQ")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "26" thru_hole circle
			(at 7.62 11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/RESET")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "27" thru_hole circle
			(at 7.62 8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/M1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "28" thru_hole circle
			(at 7.62 6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/RFSH")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "29" thru_hole circle
			(at 7.62 3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "GND")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "30" thru_hole circle
			(at 7.62 1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "A0")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "31" thru_hole circle
			(at 7.62 -1.27)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "A1")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "32" thru_hole circle
			(at 7.62 -3.81)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "A2")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "33" thru_hole circle
			(at 7.62 -6.35)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A3")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "34" thru_hole circle
			(at 7.62 -8.89)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A4")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "35" thru_hole circle
			(at 7.62 -11.43)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A5")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "36" thru_hole circle
			(at 7.62 -13.97)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "A6/INT")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "37" thru_hole circle
			(at 7.62 -16.51)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A7")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "38" thru_hole circle
			(at 7.62 -19.05)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A8")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "39" thru_hole circle
			(at 7.62 -21.59)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A9")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "40" thru_hole circle
			(at 7.62 -24.13)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "A10")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(footprint "D-TR-10"
		(layer "F.Cu")
		(at 207.73985 144.52985 -90)
		(property "Reference" "D5"
			(at -3.175 -1.27 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N4148"
			(at -3.175 2.54 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "A" thru_hole circle
			(at 3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "N$12")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "C" thru_hole circle
			(at -3.81 0 270)
			(size 1.3208 1.3208)
			(drill 0.8128)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "A13")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
	)
	(gr_line
		(start 166.2011 63.0036)
		(end 168.0011 63.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.5661 55.0036)
		(end 166.2011 55.6386)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.0011 55.6386)
		(end 168.6361 55.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 77.5011 155.0036)
		(end 77.5011 55.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.0011 63.0036)
		(end 168.0011 55.6386)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 77.5011 55.0036)
		(end 165.5661 55.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.6361 55.0036)
		(end 219.5011 55.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 77.5011 155.0036)
		(end 219.5011 155.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.5011 55.0036)
		(end 219.5011 155.0036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.2011 55.6386)
		(end 166.2011 63.0036)
		(layer "Edge.Cuts")
	)
	(gr_text "c"
		(at 90.39 89.57 90)
		(layer "B.Cu")
	)
	(gr_text "ISSUE ONE D"
		(at 91.283475 65.371807 90)
		(layer "B.Cu")
	)
	(gr_text "1980"
		(at 86.961018 87.96921 -270)
		(layer "B.Cu")
	)
	(gr_text "ZX81"
		(at 88.05 68.46 90)
		(layer "B.Cu")
	)
	(gr_text "MIC"
		(at 79.81 127.86 0)
		(layer "F.SilkS")
	)
	(gr_text "W"
		(at 126.87 64.52 0)
		(layer "F.SilkS")
	)
	(gr_text "Reset"
		(at 87.02 89.87 0)
		(layer "F.SilkS")
	)
	(gr_text "9VDC"
		(at 78.91 142.64 0)
		(layer "F.SilkS")
	)
	(gr_text "RESET"
		(at 83.65 67.42 0)
		(layer "F.SilkS")
	)
	(gr_text "RP4"
		(at 127.4 105.88 90)
		(layer "F.SilkS")
	)
	(gr_text "D1-D8"
		(at 203.57 139.82 0)
		(layer "F.SilkS")
	)
	(gr_text "SINCLAIR  ZX81"
		(at 157.67 70.84 0)
		(layer "F.SilkS")
	)
	(gr_text "+5VDC"
		(at 87.05 94.96 0)
		(layer "F.SilkS")
	)
	(gr_text "vLA81"
		(at 146.97 87.53 90)
		(layer "F.SilkS")
	)
	(gr_text "AIT"
		(at 127.67 64.52 0)
		(layer "F.SilkS")
	)
	(gr_text "EAR"
		(at 79.87 113.29 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 88.59 89.09 0)
		(layer "F.SilkS")
	)
	(gr_text "RP6"
		(at 184.64 137.54 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 86.56 87.36 0)
		(layer "F.SilkS")
	)
	(gr_text "ChSw"
		(at 88.14 96.68 0)
		(layer "F.SilkS")
	)
	(gr_text "RP5"
		(at 139 108.68 90)
		(layer "F.SilkS")
	)
	(gr_text "RP7"
		(at 184.41 130.53 0)
		(layer "F.SilkS")
	)
	(gr_text "A15"
		(at 154.18 143.62 0)
		(layer "F.SilkS")
	)
	(gr_text "A14"
		(at 145.35 143.62 0)
		(layer "F.SilkS")
	)
	(gr_text "Ear"
		(at 88.85 94.14 0)
		(layer "F.SilkS")
	)
	(gr_text "Video"
		(at 87.26 92.4 0)
		(layer "F.SilkS")
	)
	(gr_text "NTSC"
		(at 88.3 91.6 0)
		(layer "F.SilkS")
	)
	(gr_text "ISSUE ONE D"
		(at 160.41 73.93 0)
		(layer "F.SilkS")
	)
	(zone
		(net 17)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.4064)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3548)
			(thermal_bridge_width 0.3548)
		)
		(polygon
			(pts
				(xy 195.909585 88.962972) (xy 197.292412 88.969105) (xy 198.46992 89.007025) (xy 199.474391 89.023323)
				(xy 200.902414 89.081961) (xy 202.66818 89.229679) (xy 203.752865 89.381759) (xy 204.110081 89.684757)
				(xy 204.185786 90.174072) (xy 203.999366 90.594438) (xy 203.691657 90.799791) (xy 203.299935 90.805817)
				(xy 202.473581 90.66763) (xy 200.70461 90.538008) (xy 199.025816 90.495119) (xy 196.271572 90.278703)
				(xy 195.122319 90.153696) (xy 193.362656 90.397865) (xy 192.228417 90.935714) (xy 190.955189 91.848797)
				(xy 183.122476 91.818458) (xy 182.011521 91.65975) (xy 181.09458 91.65975) (xy 180.175199 91.966211)
				(xy 178.841802 92.618816) (xy 178.526191 92.947649) (xy 178.198529 93.039883) (xy 177.679458 93.154527)
				(xy 177.062397 93.069332) (xy 176.568249 92.919438) (xy 175.289223 92.279925) (xy 171.806562 90.696898)
				(xy 171.349704 90.544612) (xy 170.1643 90.354595) (xy 169.605175 90.096022) (xy 169.451122 89.610725)
				(xy 169.693971 89.405141) (xy 170.132522 89.226414) (xy 170.559113 89.142678) (xy 171.507284 88.957915)
				(xy 189.847398 89.259202) (xy 191.963696 89.128032) (xy 193.617024 88.904284)
			)
		)
	)
	(zone
		(net 18)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3548)
			(thermal_bridge_width 0.3548)
		)
		(polygon
			(pts
				(xy 109.32 154.74) (xy 93.33 154.77) (xy 93.33 144.13) (xy 109.32 144.08)
			)
		)
	)
	(zone
		(net 18)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.563059 128.998744) (xy 190.3067 129.2962) (xy 198.194441 129.2962) (xy 201.578107 128.373382)
				(xy 201.731824 127.667703) (xy 202.499954 127.173306) (xy 203.313994 127.299077) (xy 203.73481 127.661643)
				(xy 203.943946 128.550149) (xy 203.755186 129.512152) (xy 203.212963 130.235117) (xy 189.455105 130.395092)
				(xy 188.615145 130.059108) (xy 185.597374 127.835489) (xy 184.521508 127.374404) (xy 182.170986 127.061)
				(xy 178.536194 127.061) (xy 174.737783 127.377535) (xy 172.702886 127.690596) (xy 171.810108 128.136985)
				(xy 171.034944 129.377247) (xy 169.92231 130.807776) (xy 169.257722 131.80466) (xy 168.500158 131.994051)
				(xy 167.89995 131.593912) (xy 167.89995 131.170119) (xy 168.075116 130.644621) (xy 169.998048 128.240957)
				(xy 170.806923 127.270306) (xy 171.779678 126.621803) (xy 173.081017 125.808466) (xy 174.545344 125.645763)
				(xy 184.452816 124.686975)
			)
		)
	)
	(zone
		(net 18)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.3048)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3548)
			(thermal_bridge_width 0.3548)
		)
		(polygon
			(pts
				(xy 102.611 100.2385) (xy 78.4187 100.2185) (xy 78.3387 55.8562) (xy 102.531 55.8762)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 94.523968 67.206519) (xy 94.923968 67.206519) (xy 94.923968 64.456519) (xy 95.398968 64.456519)
				(xy 95.398968 67.681519) (xy 94.048968 67.681519) (xy 94.048968 64.931519) (xy 93.648968 64.931519)
				(xy 93.648968 67.681519) (xy 93.173968 67.681519) (xy 93.173968 64.456519) (xy 94.523968 64.456519)
			)
		)
	)
	(zone
		(net 17)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 108.075597 118.147879) (xy 108.39759 118.577279) (xy 108.39759 119.034471) (xy 108.121219 119.587313)
				(xy 107.571772 119.583729) (xy 106.804609 119.583729) (xy 99.483925 126.43123) (xy 97.93786 130.017896)
				(xy 96.212597 151.227275) (xy 91.932111 153.895059) (xy 88.15625 153.908644) (xy 86.089915 153.960167)
				(xy 85.503092 153.603741) (xy 85.365676 152.894879) (xy 85.586627 152.182795) (xy 86.252721 151.635546)
				(xy 87.106572 151.33549) (xy 90.795134 151.227617) (xy 90.817473 151.205274) (xy 91.913073 151.182914)
				(xy 94.288789 150.036525) (xy 96.09147 129.638617) (xy 97.921533 125.250066) (xy 105.632769 118.108718)
				(xy 107.566013 117.994976)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 93.023968 68.431519) (xy 92.548968 68.431519) (xy 92.548968 67.956519) (xy 93.023968 67.956519)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 95.398968 69.181519) (xy 93.648968 69.181519) (xy 93.648968 71.456519) (xy 95.398968 71.456519)
				(xy 95.398968 71.931519) (xy 93.173968 71.931519) (xy 93.173968 68.706519) (xy 95.398968 68.706519)
			)
		)
	)
	(zone
		(net 18)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 198.543455 118.308398) (xy 198.997087 118.875388) (xy 198.983462 124.579128) (xy 203.24358 126.916279)
				(xy 203.804963 127.476577) (xy 203.854843 127.938464) (xy 203.854846 128.74754) (xy 203.75087 129.049834)
				(xy 203.278904 129.610358) (xy 202.61026 129.731941) (xy 201.914234 129.489819) (xy 201.604426 128.901122)
				(xy 201.661173 128.134941) (xy 201.782595 127.73016) (xy 195.059335 125.076624) (xy 194.624017 124.641257)
				(xy 194.432762 124.194944) (xy 194.571875 123.777563) (xy 195.147961 123.383354) (xy 196.075593 123.357583)
				(xy 197.205667 122.282658) (xy 197.318688 118.982405) (xy 197.77603 118.409848) (xy 198.08021 118.274644)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 95.398968 76.181519) (xy 92.423968 76.181519) (xy 92.423968 75.706519) (xy 95.398968 75.706519)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 93.648968 79.206519) (xy 95.398968 79.206519) (xy 95.398968 79.681519) (xy 93.173968 79.681519)
				(xy 93.173968 76.456519) (xy 93.648968 76.456519)
			)
		)
	)
	(zone
		(net 81)
		(net_name "+9V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.684429 57.201276) (xy 158.488399 57.506264) (xy 159.045221 57.979617) (xy 159.696235 58.874861)
				(xy 160.071458 59.92024) (xy 160.774183 62.419108) (xy 161.221896 63.240005) (xy 161.553899 63.505635)
				(xy 162.12641 63.553352) (xy 162.908948 63.528894) (xy 163.374168 63.203203) (xy 163.704091 62.755404)
				(xy 163.824931 62.06048) (xy 165.419306 62.092373) (xy 165.38418 62.865201) (xy 165.011435 63.438715)
				(xy 164.256227 64.140059) (xy 163.242526 64.807044) (xy 162.177045 65.298859) (xy 161.343793 65.241387)
				(xy 160.573577 64.784911) (xy 160.154676 64.086667) (xy 157.959931 58.347886) (xy 154.343956 58.285895)
				(xy 152.042633 62.684197) (xy 150.637687 62.64578) (xy 148.631866 62.523491) (xy 146.907913 62.041117)
				(xy 146.432448 61.908095) (xy 145.041438 61.463475) (xy 142.207059 61.487954) (xy 139.83838 61.440693)
				(xy 137.764094 61.464436) (xy 135.904265 62.078749) (xy 134.747864 62.71965) (xy 133.377613 63.088535)
				(xy 131.442209 63.134237) (xy 129.868004 63.099589) (xy 128.403842 63.059585) (xy 126.353154 63.035205)
				(xy 124.265483 63.152444) (xy 122.038545 63.094285) (xy 120.341842 63.088547) (xy 118.854551 63.10318)
				(xy 114.614447 63.260514) (xy 103.789579 63.341539) (xy 101.548269 64.072014) (xy 100.308083 65.319614)
				(xy 99.453798 66.834525) (xy 98.811732 68.65433) (xy 98.668576 70.25802) (xy 98.700843 82.459593)
				(xy 98.611114 84.002114) (xy 98.068978 85.01427) (xy 96.57447 86.000106) (xy 95.698117 86.430863)
				(xy 94.977849 86.944598) (xy 94.451364 87.711576) (xy 94.077991 88.415079) (xy 93.972008 89.240287)
				(xy 93.844316 94.256003) (xy 93.135846 95.548333) (xy 91.844657 96.423292) (xy 89.2331 96.624249)
				(xy 87.368547 96.818534) (xy 86.244678 97.493072) (xy 85.652954 98.55181) (xy 85.277389 100.094703)
				(xy 85.257699 101.41672) (xy 85.804824 102.714277) (xy 86.42321 103.566145) (xy 87.459932 104.56142)
				(xy 88.317513 105.491977) (xy 88.776077 106.484523) (xy 88.86532 107.27746) (xy 88.782835 130.642054)
				(xy 88.786845 131.407407) (xy 88.823931 133.384883) (xy 88.623127 134.66894) (xy 88.395475 135.422626)
				(xy 87.946246 136.086623) (xy 87.598147 136.729339) (xy 86.833928 137.444973) (xy 86.643009 138.402031)
				(xy 86.643009 146.121506) (xy 86.424964 146.912386) (xy 85.953598 147.45849) (xy 85.468639 147.830849)
				(xy 84.604322 148.087481) (xy 83.980128 147.891177) (xy 83.597802 147.670264) (xy 82.861624 146.555035)
				(xy 82.878718 146.227644) (xy 82.878718 137.019641) (xy 82.987686 135.92985) (xy 83.450452 135.206695)
				(xy 84.396112 134.789446) (xy 85.512094 134.555841) (xy 86.296786 134.101595) (xy 86.963062 133.0781)
				(xy 87.208179 132.172402) (xy 87.25315 131.701556) (xy 87.096554 106.617611) (xy 86.691106 105.842278)
				(xy 85.250062 104.601717) (xy 84.41999 103.588199) (xy 83.889917 102.465542) (xy 83.628348 101.188743)
				(xy 83.565708 99.678892) (xy 84.057276 98.062018) (xy 84.835557 96.621406) (xy 86.000491 95.562412)
				(xy 86.9559 95.05089) (xy 90.264718 94.770822) (xy 91.437919 94.219782) (xy 91.975262 92.769448)
				(xy 92.013354 88.662479) (xy 92.289808 87.165678) (xy 92.864231 86.423068) (xy 93.603933 85.63306)
				(xy 94.852344 84.927317) (xy 96.276727 84.244701) (xy 96.781023 83.670574) (xy 96.964527 82.696975)
				(xy 96.740737 69.098263) (xy 97.046704 67.223155) (xy 97.524966 66.125796) (xy 98.413685 64.401103)
				(xy 99.657665 63.089654) (xy 100.338082 62.634952) (xy 101.927788 62.108882) (xy 103.693032 62.063675)
				(xy 114.824647 62.012441) (xy 117.091735 61.817538) (xy 121.504729 61.75388) (xy 123.63506 61.743917)
				(xy 125.118293 61.750987) (xy 126.834599 61.582323) (xy 127.629812 61.605532) (xy 128.2216 61.566278)
				(xy 128.944434 61.528764) (xy 130.087891 61.527708) (xy 131.189266 61.511845) (xy 132.284191 61.487338)
				(xy 133.563807 61.470961) (xy 135.203692 60.991054) (xy 136.672509 60.37454) (xy 137.932117 60.192761)
				(xy 139.473045 60.189994) (xy 140.877455 60.159255) (xy 141.611606 59.798606) (xy 142.308113 59.606267)
				(xy 142.792994 59.198574) (xy 143.390162 58.32242) (xy 143.673581 57.578652) (xy 144.306006 57.175825)
				(xy 145.098833 57.350249) (xy 145.395704 57.778695) (xy 146.065713 59.161842) (xy 147.19781 60.702716)
				(xy 147.4544 61.073451) (xy 148.833734 61.571583) (xy 149.390253 61.666924) (xy 150.469937 61.721273)
				(xy 151.537685 61.807036) (xy 153.790149 57.184157) (xy 156.504503 57.12082)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 95.398968 79.306519) (xy 94.923968 79.306519) (xy 94.923968 76.931519) (xy 94.523968 76.931519)
				(xy 94.523968 79.306519) (xy 94.048968 79.306519) (xy 94.048968 76.456519) (xy 95.398968 76.456519)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 95.398968 80.431519) (xy 93.173968 80.431519) (xy 93.173968 79.956519) (xy 95.398968 79.956519)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 95.398968 68.431519) (xy 93.173968 68.431519) (xy 93.173968 67.956519) (xy 95.398968 67.956519)
			)
		)
	)
	(zone
		(net 17)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 117.410272 66.041154) (xy 119.835382 65.935807) (xy 125.241241 66.083534) (xy 131.929848 69.132557)
				(xy 132.383307 69.627309) (xy 132.668693 70.320484) (xy 132.668693 72.906668) (xy 132.307356 73.493925)
				(xy 131.640093 73.589258) (xy 131.255885 73.25303) (xy 130.67029 71.573864) (xy 129.242341 71.557653)
				(xy 128.740364 71.578855) (xy 128.634041 71.574887) (xy 128.318092 71.55182) (xy 128.064925 71.560351)
				(xy 127.794662 71.3163) (xy 125.751636 69.224394) (xy 125.030728 68.719687) (xy 124.163108 68.466598)
				(xy 123.24686 68.356633) (xy 121.75776 68.42928) (xy 121.12863 68.848761) (xy 120.093842 69.920653)
				(xy 119.127276 71.29634) (xy 118.271167 72.934346) (xy 117.712015 74.574751) (xy 117.513557 75.354939)
				(xy 117.333081 76.334446) (xy 117.190456 77.015795) (xy 117.140537 78.208476) (xy 117.214429 114.332359)
				(xy 117.258422 117.395202) (xy 117.263463 119.2194) (xy 116.937436 119.783443) (xy 116.33115 119.82061)
				(xy 115.957352 119.591481) (xy 115.672749 119.162616) (xy 115.555924 118.869381) (xy 115.490011 118.410032)
				(xy 115.368534 117.432132) (xy 115.316597 114.904198) (xy 115.375969 80.862917) (xy 115.344234 77.39109)
				(xy 114.896836 75.218201) (xy 113.715401 72.613433) (xy 109.972253 67.324154) (xy 109.689773 66.587007)
				(xy 110.072845 65.766383) (xy 110.850772 65.675147)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 95.398968 75.431519) (xy 94.923968 75.431519) (xy 94.923968 72.681519) (xy 93.648968 72.681519)
				(xy 93.648968 75.431519) (xy 93.173968 75.431519) (xy 93.173968 72.206519) (xy 95.398968 72.206519)
			)
		)
	)
	(zone
		(net 18)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.254)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 157.391959 58.94962) (xy 159.508269 64.572098) (xy 159.892772 64.976913) (xy 160.709073 65.604951)
				(xy 161.659062 65.862063) (xy 162.606731 65.832553) (xy 163.819401 65.236746) (xy 165.812525 64.272859)
				(xy 167.503327 63.745758) (xy 168.534082 63.462755) (xy 168.956006 61.974654) (xy 173.099926 61.974654)
				(xy 173.009169 62.700826) (xy 172.71186 63.196436) (xy 172.169859 63.526408) (xy 170.953859 64.057124)
				(xy 169.134567 64.605205) (xy 167.092365 65.148443) (xy 165.758508 65.664869) (xy 164.479474 66.358711)
				(xy 163.229769 66.983679) (xy 162.538473 67.029772) (xy 161.716501 67.007551) (xy 160.923452 66.89424)
				(xy 159.838961 66.397089) (xy 159.137865 65.808967) (xy 158.396354 64.932473) (xy 157.884985 63.776123)
				(xy 157.315423 62.308136) (xy 156.989785 61.265907) (xy 156.634568 60.471745) (xy 156.177958 60.01505)
				(xy 155.811542 59.886782) (xy 155.218869 59.982393) (xy 154.812315 60.350295) (xy 154.538787 60.819289)
				(xy 154.518893 61.515627) (xy 154.854107 62.500493) (xy 156.542482 65.509817) (xy 157.510695 66.865562)
				(xy 158.324537 67.679556) (xy 160.584182 69.54845) (xy 165.552855 73.580791) (xy 166.906081 74.759622)
				(xy 167.870779 75.614854) (xy 168.433702 76.222924) (xy 168.908242 77.104378) (xy 169.171311 78.028522)
				(xy 169.267513 79.297823) (xy 169.289428 80.7079) (xy 169.238115 82.186892) (xy 168.829904 85.115255)
				(xy 168.590693 86.724768) (xy 168.4611 88.020966) (xy 168.4611 113.017175) (xy 168.637218 113.408624)
				(xy 169.033982 113.951662) (xy 169.660584 114.555996) (xy 169.833585 115.050376) (xy 169.855405 141.699538)
				(xy 169.737936 142.193001) (xy 169.456937 142.73168) (xy 168.995322 143.193382) (xy 160.178845 145.188849)
				(xy 159.452973 145.956648) (xy 159.145934 146.90617) (xy 159.305553 147.535574) (xy 159.471356 147.774389)
				(xy 160.813556 148.008226) (xy 164.055218 148.022681) (xy 171.624125 148.044556) (xy 172.139232 148.265357)
				(xy 172.562781 148.713906) (xy 172.660031 149.273209) (xy 172.660031 154.99266) (xy 98.942743 154.99266)
				(xy 98.942743 143.403741) (xy 112.251344 143.359444) (xy 112.45046 143.558592) (xy 112.407809 147.376452)
				(xy 119.354842 147.721706) (xy 121.442239 150.983867) (xy 127.125094 150.833157) (xy 135.891399 152.621638)
				(xy 143.283333 153.252241) (xy 170.417333 153.273974) (xy 171.177944 152.493716) (xy 171.137313 149.526897)
				(xy 162.082845 149.585578) (xy 160.465005 149.435832) (xy 159.517734 149.351878) (xy 158.970964 149.239677)
				(xy 158.186253 149.089322) (xy 157.615344 148.655359) (xy 157.1806 148.043113) (xy 157.062733 147.690467)
				(xy 156.833461 146.787126) (xy 157.07152 145.673783) (xy 157.633055 144.743838) (xy 158.22514 144.095212)
				(xy 167.299735 141.880259) (xy 167.743463 140.926572) (xy 167.807725 138.955501) (xy 167.807725 116.074977)
				(xy 165.456313 114.572411) (xy 165.431663 113.167054) (xy 167.197792 111.945804) (xy 167.219515 87.549266)
				(xy 167.402418 85.391841) (xy 167.721127 82.230454) (xy 167.764686 79.419416) (xy 167.693658 78.633751)
				(xy 167.526272 77.998872) (xy 167.182944 77.277333) (xy 166.607669 76.505926) (xy 160.651119 71.70067)
				(xy 158.468473 69.801417) (xy 156.895024 68.336968) (xy 155.689223 67.08709) (xy 155.049533 66.292842)
				(xy 154.552076 65.569138) (xy 154.325669 64.719944) (xy 145.307914 64.154204) (xy 145.09366 64.280529)
				(xy 144.456762 64.456762) (xy 143.818041 64.17023) (xy 143.494028 63.875449) (xy 137.224715 63.77284)
				(xy 136.918898 63.916318) (xy 136.481303 64.26642) (xy 136.175327 64.584655) (xy 135.870019 65.174585)
				(xy 135.93162 75.014728) (xy 137.106302 78.633994) (xy 137.25531 79.326011) (xy 136.132247 79.700915)
				(xy 135.099192 80.321008) (xy 129.788785 83.59124) (xy 129.263351 83.575042) (xy 128.810511 83.575044)
				(xy 122.482542 83.472665) (xy 122.060232 83.296946) (xy 121.772495 82.799855) (xy 121.799308 82.183075)
				(xy 122.267431 81.825032) (xy 129.644733 81.846864) (xy 130.966869 81.145603) (xy 130.946676 79.348237)
				(xy 129.516214 77.404506) (xy 128.979662 76.618862) (xy 128.299193 76.56347) (xy 127.831072 76.11646)
				(xy 127.839251 75.450833) (xy 128.377 74.999012) (xy 129.183383 74.969454) (xy 131.104129 74.973718)
				(xy 131.653546 74.768448) (xy 132.121054 74.300904) (xy 132.930831 73.472235) (xy 133.612799 72.706472)
				(xy 133.625464 68.589213) (xy 126.076601 65.285979) (xy 119.310414 65.185876) (xy 115.158034 65.153552)
				(xy 113.791904 65.146272) (xy 112.807247 65.174681) (xy 106.322011 65.32637) (xy 105.908036 65.409171)
				(xy 105.320993 65.581327) (xy 104.917235 65.860694) (xy 104.252231 66.289023) (xy 103.641363 67.167428)
				(xy 102.907336 68.558669) (xy 102.733275 70.262427) (xy 102.733275 93.662144) (xy 102.623486 95.265361)
				(xy 102.403351 96.586408) (xy 102.13786 97.626444) (xy 101.866628 98.304647) (xy 101.394946 99.001074)
				(xy 100.832716 99.653376) (xy 100.108163 100.174243) (xy 99.301507 100.532823) (xy 98.237869 100.865271)
				(xy 97.218314 101.042618) (xy 96.290418 101.108907) (xy 88.200939 101.130776) (xy 87.465737 100.900793)
				(xy 86.766094 100.320605) (xy 86.429038 99.715375) (xy 86.408894 98.98541) (xy 86.845956 98.228541)
				(xy 87.476906 97.878809) (xy 88.499903 97.791141) (xy 96.089179 97.791141) (xy 97.168894 97.809405)
				(xy 98.07518 97.711121) (xy 98.516309 97.574452) (xy 99.107573 97.219678) (xy 99.52081 96.740748)
				(xy 99.794528 96.098713) (xy 99.840892 95.174795) (xy 99.793592 70.674117) (xy 99.836215 70.223007)
				(xy 99.852735 69.755036) (xy 100.27968 68.142779) (xy 101.121936 66.457717) (xy 101.727042 65.529593)
				(xy 102.39293 64.791395) (xy 103.107168 64.239221) (xy 103.704682 63.973639) (xy 104.400344 63.868053)
				(xy 114.913222 63.851984) (xy 116.33876 63.863455) (xy 118.301622 63.837126) (xy 120.777682 63.777486)
				(xy 123.065875 63.755691) (xy 125.784271 63.712189) (xy 127.215146 63.608891) (xy 129.223914 63.608891)
				(xy 131.262313 63.581372) (xy 133.003744 63.640832) (xy 134.054759 63.471879) (xy 135.204971 63.136181)
				(xy 136.95489 62.155923) (xy 143.975117 62.198759) (xy 144.645926 62.064574) (xy 145.114669 62.174699)
				(xy 145.483875 62.52225) (xy 146.993861 62.846308) (xy 152.490563 63.146234) (xy 154.77715 58.855375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 95.398968 81.181519) (xy 93.648968 81.181519) (xy 93.648968 83.931519) (xy 93.173968 83.931519)
				(xy 93.173968 80.706519) (xy 95.398968 80.706519)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.000001)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.15)
			(thermal_bridge_width 0.15)
		)
		(polygon
			(pts
				(xy 93.023968 80.431519) (xy 92.548968 80.431519) (xy 92.548968 79.956519) (xy 93.023968 79.956519)
			)
		)
	)
	(zone
		(net 17)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.000001)
		)
		(min_thickness 0.1524)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 210.321395 90.018216) (xy 210.856014 90.247382) (xy 211.159168 90.803263) (xy 211.184138 91.252839)
				(xy 211.079219 91.67259) (xy 210.631337 92.041507) (xy 209.813403 92.084563) (xy 209.32991 92.586744)
				(xy 209.287739 94.442588) (xy 209.309512 97.709278) (xy 209.331319 127.806591) (xy 208.96513 128.813803)
				(xy 208.505167 129.394913) (xy 207.873959 129.571683) (xy 207.257482 129.417533) (xy 206.978631 129.027073)
				(xy 206.978631 128.428892) (xy 207.199998 127.808953) (xy 207.305418 127.028697) (xy 207.305418 125.602682)
				(xy 207.292859 125.087292) (xy 207.117225 124.45295) (xy 207.044339 123.452885) (xy 207.03466 100.366266)
				(xy 204.891176 99.762274) (xy 204.601564 99.446274) (xy 204.386118 98.847714) (xy 204.386118 97.935463)
				(xy 204.257714 96.672571) (xy 202.668789 91.513059) (xy 202.573254 90.939745) (xy 202.726835 90.530123)
				(xy 203.025262 90.157018) (xy 203.34235 90.005726)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 88.29 77.425) (xy 87.815 77.425) (xy 87.815 75.675) (xy 85.54 75.675) (xy 85.54 77.425) (xy 85.065 77.425)
				(xy 85.065 75.2) (xy 88.29 75.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 84.04 75.675) (xy 81.29 75.675) (xy 81.29 76.075) (xy 84.04 76.075) (xy 84.04 77.425) (xy 80.815 77.425)
				(xy 80.815 76.95) (xy 83.565 76.95) (xy 83.565 76.55) (xy 80.815 76.55) (xy 80.815 75.2) (xy 84.04 75.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.79 75.05) (xy 96.315 75.05) (xy 96.315 74.575) (xy 96.79 74.575)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.04 77.425) (xy 95.565 77.425) (xy 95.565 75.675) (xy 92.815 75.675) (xy 92.815 75.2) (xy 96.04 75.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.79 75.675) (xy 89.04 75.675) (xy 89.04 76.95) (xy 91.79 76.95) (xy 91.79 77.425) (xy 88.565 77.425)
				(xy 88.565 75.2) (xy 91.79 75.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 84.79 75.05) (xy 84.315 75.05) (xy 84.315 74.575) (xy 84.79 74.575)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 84.79 77.425) (xy 84.315 77.425) (xy 84.315 75.2) (xy 84.79 75.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.54 77.425) (xy 92.065 77.425) (xy 92.065 74.45) (xy 92.54 74.45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 95.565 76.55) (xy 93.29 76.55) (xy 93.29 76.95) (xy 95.565 76.95) (xy 95.565 77.425) (xy 92.815 77.425)
				(xy 92.815 76.075) (xy 95.565 76.075)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100.29 75.675) (xy 97.54 75.675) (xy 97.54 77.425) (xy 97.065 77.425) (xy 97.065 75.2) (xy 100.29 75.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.SilkS")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.79 77.425) (xy 96.315 77.425) (xy 96.315 75.2) (xy 96.79 75.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 93.56 154.36) (xy 109.14 154.35) (xy 109.14 144.25) (xy 93.56 144.24)
			)
		)
	)
)