<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0.06858125" y1="-0.010159375" x2="47.99858125" y2="-0.010159375" width="0" layer="20"/>
<wire x1="47.99858125" y1="-0.010159375" x2="48.021440625" y2="56.388159375" width="0" layer="20"/>
<wire x1="48.021440625" y1="56.388159375" x2="0.091440625" y2="56.388159375" width="0" layer="20"/>
<wire x1="0.091440625" y1="56.388159375" x2="0.06858125" y2="-0.010159375" width="0" layer="20"/>
<text>LT</text>
<text>RT</text>
<text>BU</text>
<text>TM</text>
<text>GD</text>
<text>Mount LEDs This Side</text>
<text>RT-B</text>
<text>LT-B</text>
<text>BU</text>
<text>BU</text>
<text>TM</text>
<text>TM</text>
<text>TM</text>
<text>TM</text>
<text>TM</text>
<text>TM</text>
<text>TM</text>
<text>RV-Project.Com Trailer Display Board V1.2</text>
<text>7/27/2021</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>GD</text>
<text>LT</text>
<text>BU</text>
<text>RT</text>
<text>TM</text>
<text>EB</text>
<text>AX</text>
<text>EB</text>
<text>AX</text>
<text>Meter-Switch</text>
<text>White</text>
<text>White</text>
<text>Input</text>
<text>Keystone 24424 standoffs (M2.5x12MM)</text>
<text>OptoComponents SSI-LXMP059ID Rectangular LED (LT-TM-RT)</text>
<text>Keystone 8659 Round LED Bezel (TM)</text>
<text>Keystone 8677 Square LED Bezel (BU)</text>
<text>ALARM</text>
<text>AX</text>
<text>INPUT</text>
<text>EB LED</text>
<text>AX LED</text>
<text>ALARM LED</text>
</plain>
<libraries>
<library name="a-lib">
<description>Archive Library (for old designs) - do not use for new components.</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="RECTANGLELED">
<description>&lt;h3&gt;LED 3MM - No Silk&lt;/h3&gt;
3 mm, round</description>
</package>
<package name="1/4W_AXIAL_RESISTOR_3.5MIL(V2)">
<description>Axial 1/4Watt Resistor&lt;p&gt;Pitch: 0.35"</description>
</package>
<package name="MO1-22AWG-SMALL">
</package>
<package name="WAFER3PINVERTICAL2.54">
<description>Pitch: 0.1" (2.54mm)</description>
</package>
<package name="KEYSTONE2442X">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="MO1-20AWG-SMALL">
</package>
<package name="WAFER2PINVERTICAL2.54">
<description>Pitch: 0.1" (2.54mm)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="a-lib" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="a-lib" package="RECTANGLELED" value="">
<attribute name="VALUE"/>
</element>
<element name="LED9" library="a-lib" package="RECTANGLELED" value="">
<attribute name="VALUE"/>
</element>
<element name="LED10" library="a-lib" package="RECTANGLELED" value="">
<attribute name="VALUE"/>
</element>
<element name="LED11" library="a-lib" package="RECTANGLELED" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value=""/>
<element name="JP1" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="JP2" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="JP3" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="JP4" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="JP5" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="J2" library="a-lib" package="WAFER3PINVERTICAL2.54" value="WAFER3PVERTICAL_2.54"/>
<element name="J3" library="a-lib" package="WAFER3PINVERTICAL2.54" value="WAFER3PVERTICAL_2.54"/>
<element name="J4" library="a-lib" package="WAFER3PINVERTICAL2.54" value="WAFER3PVERTICAL_2.54"/>
<element name="JP7" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="JP8" library="a-lib" package="MO1-22AWG-SMALL" value=""/>
<element name="U$1" library="a-lib" package="KEYSTONE2442X" value="M2.5"/>
<element name="U$3" library="a-lib" package="KEYSTONE2442X" value="M2.5">
<attribute name="VALUE"/>
</element>
<element name="TB2" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB1" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB3" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB4" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB5" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB6" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB7" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB8" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="TB9" library="a-lib_Connectors" package="MO1-20AWG-SMALL" value=""/>
<element name="R12" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="a-lib" package="1/4W_AXIAL_RESISTOR_3.5MIL(V2)" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="a-lib_Connectors" package="WAFER2PINVERTICAL2.54" value="M2VERTICAL2.54"/>
<element name="J5" library="a-lib_Connectors" package="WAFER2PINVERTICAL2.54" value="M2VERTICAL2.54"/>
<element name="J6" library="a-lib_Connectors" package="WAFER2PINVERTICAL2.54" value="M2VERTICAL2.54"/>
</elements>
<signals>
<signal name="N$7">
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED4" pad="A"/>
<contactref element="LED11" pad="A"/>
<contactref element="LED9" pad="A"/>
<contactref element="JP3" pad="P$1"/>
<contactref element="J2" pad="P$2"/>
<contactref element="TB6" pad="P$1"/>
</signal>
<signal name="N$18">
<contactref element="LED7" pad="A"/>
<contactref element="LED6" pad="A"/>
<contactref element="JP2" pad="P$1"/>
<contactref element="J2" pad="P$1"/>
<contactref element="TB5" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="LED10" pad="A"/>
<contactref element="JP1" pad="P$1"/>
<contactref element="J4" pad="P$3"/>
<contactref element="TB4" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="LED8" pad="A"/>
<contactref element="JP4" pad="P$1"/>
<contactref element="J2" pad="P$3"/>
<contactref element="TB7" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="K"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="K"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="LED4" pad="K"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="LED5" pad="K"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R10" pad="2"/>
<contactref element="LED10" pad="K"/>
</signal>
<signal name="N$11">
<contactref element="LED7" pad="K"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R11" pad="2"/>
<contactref element="LED11" pad="K"/>
</signal>
<signal name="N$14">
<contactref element="R6" pad="2"/>
<contactref element="LED6" pad="K"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R8" pad="2"/>
<contactref element="LED8" pad="K"/>
</signal>
<signal name="N$13">
<contactref element="R9" pad="2"/>
<contactref element="LED9" pad="K"/>
</signal>
<signal name="GND">
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R11" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="JP5" pad="P$1"/>
<contactref element="J4" pad="P$1"/>
<contactref element="J4" pad="P$2"/>
<contactref element="TB2" pad="P$1"/>
<contactref element="R14" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="J3" pad="P$1"/>
<contactref element="JP7" pad="P$1"/>
<contactref element="TB1" pad="P$1"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="N$16">
<contactref element="J3" pad="P$2"/>
<contactref element="JP8" pad="P$1"/>
<contactref element="J3" pad="P$3"/>
<contactref element="TB3" pad="P$1"/>
</signal>
<signal name="N$17">
<contactref element="J1" pad="P$1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="J5" pad="P$1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="J6" pad="P$1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="J5" pad="P$2"/>
<contactref element="TB8" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="J6" pad="P$2"/>
<contactref element="TB9" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
