(kicad_pcb (version 20171130) (host pcbnew 5.1.2)
  (general
    (thickness 1.6)
    (drawings 16)
    (tracks 61)
    (zones 0)
    (modules 13)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 3)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.0254)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J0-Pad1)")
  (net 2 "Net-(J0-Pad2)")
  (net 3 "Net-(J0-Pad3)")
  (net 4 "Net-(J0-Pad4)")
  (net 5 "Net-(J0-Pad5)")
  (net 6 "Net-(J0-Pad6)")
  (net 7 "Net-(J0-Pad7)")
  (net 8 "Net-(J0-Pad8)")
  (net 9 "Net-(J0-Pad9)")
  (net 10 "Net-(J0-Pad10)")
  (net 11 "Net-(J0-Pad11)")
  (net 12 "Net-(J0-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net "Net-(J0-Pad1)")
    (add_net "Net-(J0-Pad10)")
    (add_net "Net-(J0-Pad11)")
    (add_net "Net-(J0-Pad12)")
    (add_net "Net-(J0-Pad2)")
    (add_net "Net-(J0-Pad3)")
    (add_net "Net-(J0-Pad4)")
    (add_net "Net-(J0-Pad5)")
    (add_net "Net-(J0-Pad6)")
    (add_net "Net-(J0-Pad7)")
    (add_net "Net-(J0-Pad8)")
    (add_net "Net-(J0-Pad9)")
  )
  (module mpms-transport-pcb:samtec-fte-106-xx-x-dh-x-xx (layer F.Cu) (tedit 5CF6B070)
    (at 100 100)
    (fp_text reference J0 (at 0 3.5) (layer F.SilkS) hide)
    (fp_text value Conn_02x06_Counter_Clockwise (at 0 5) (layer F.Fab) hide)
    (fp_text user 1 (at -3.25 -1.27) (layer F.SilkS) hide)
    (fp_text user 7 (at 3.25 1.27) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2 -1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J0-Pad1)"))
    (pad 2 smd rect (at -1.2 -1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J0-Pad2)"))
    (pad 3 smd rect (at -0.4 -1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J0-Pad3)"))
    (pad 4 smd rect (at 0.4 -1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J0-Pad4)"))
    (pad 5 smd rect (at 1.2 -1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J0-Pad5)"))
    (pad 6 smd rect (at 2 -1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J0-Pad6)"))
    (pad 7 smd rect (at 2 1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J0-Pad7)"))
    (pad 8 smd rect (at 1.2 1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J0-Pad8)"))
    (pad 9 smd rect (at 0.4 1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J0-Pad9)"))
    (pad 10 smd rect (at -0.4 1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J0-Pad10)"))
    (pad 11 smd rect (at -1.2 1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J0-Pad11)"))
    (pad 12 smd rect (at -2 1.27) (size 0.508 2.032) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J0-Pad12)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 98 104.5 270)
    (fp_text reference 12 (at -1.4 -0.4) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 12 "Net-(J0-Pad12)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 98.25 107 315)
    (fp_text reference 11 (at 0 0.707107 315) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 45) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 11 "Net-(J0-Pad11)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 98.25 109 315)
    (fp_text reference 10 (at 0 0.707107 135) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 45) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 10 "Net-(J0-Pad10)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 101.75 109 45)
    (fp_text reference 9 (at 0.035355 0.883883 45) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 135) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 9 "Net-(J0-Pad9)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 101.75 107 45)
    (fp_text reference 8 (at 0.035355 0.883883 45) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 135) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 8 "Net-(J0-Pad8)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 102 104.5 90)
    (fp_text reference 7 (at 1.4 -0.4) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 90) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 180) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 7 "Net-(J0-Pad7)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 101.75 115 45)
    (fp_text reference 6 (at 0.035355 0.883883 225) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 135) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 6 "Net-(J0-Pad6)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 101.75 113 45)
    (fp_text reference 5 (at 0.035355 0.883883 45) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 135) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 5 "Net-(J0-Pad5)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 101.75 111 45)
    (fp_text reference 4 (at 0.035355 0.883883 45) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 45) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 135) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 4 "Net-(J0-Pad4)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 98.25 111 315)
    (fp_text reference 3 (at -0.035355 0.883883 135) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 45) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 3 "Net-(J0-Pad3)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 98.25 113 315)
    (fp_text reference 2 (at -0.035355 0.883883 135) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 45) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 2 "Net-(J0-Pad2)"))
  )
  (module mpms-transport-pcb:mpms-transport-stick-wire-pad (layer F.Cu) (tedit 5CF6D674)
    (at 98.25 115 315)
    (fp_text reference 1 (at -0.035355 0.883883 315) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 2.5 135) (layer F.Fab) hide)
    (pad 1 smd roundrect (at 0 0 45) (size 0.5 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.5)
      (net 1 "Net-(J0-Pad1)"))
  )
  (gr_line (start 96.5 96.5) (end 97.5 93.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.5 93.25) (end 103.5 96.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.5 93.25) (end 102.5 93.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 98 123.5) (end 102 123.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 96.5 118.5) (end 98 123.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102 123.5) (end 103.5 118.5) (layer Edge.Cuts) (width 0.05))
  (gr_text "FTE-106-01-G-DH\nCLE-106-01-G-DV" (at 101.75 109 90) (layer B.SilkS))
  (gr_text "Samtec\nconnectors" (at 101.5 100.584 90) (layer B.SilkS))
  (gr_text "MPMS transport stick v1" (at 98.552 107.188 90) (layer B.SilkS))
  (gr_circle (center 100 120) (end 101.4732 120) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 96.5 96.5) (end 96.5 118.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 103.5 96.5) (end 103.5 118.5) (layer Edge.Cuts) (width 0.05))
)
