(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 21)
    (tracks 128)
    (zones 0)
    (modules 7)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CIA_gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(R2-Pad1)")
  (net 5 /14A)
  (net 6 /13A)
  (net 7 /14B)
  (net 8 /13B)
  (net 9 /c)
  (net 10 /s)
  (net 11 /tick)
  (net 12 /rs0)
  (net 13 /_pc)
  (net 14 /rs1)
  (net 15 /pb7)
  (net 16 /rs2)
  (net 17 /pb6)
  (net 18 /rs3)
  (net 19 /pb5)
  (net 20 /_reset)
  (net 21 /d0)
  (net 22 /d1)
  (net 23 /pb2)
  (net 24 /d2)
  (net 25 /pb1)
  (net 26 /d3)
  (net 27 /pb0)
  (net 28 /d4)
  (net 29 /pa7)
  (net 30 /d5)
  (net 31 /pa6)
  (net 32 /d6)
  (net 33 /pa5)
  (net 34 /d7)
  (net 35 /pa4)
  (net 36 /e)
  (net 37 /pa3)
  (net 38 /_f)
  (net 39 /pa2)
  (net 40 /_cs)
  (net 41 /pa1)
  (net 42 /_w)
  (net 43 /pa0)
  (net 44 /_int)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /13A)
    (add_net /13B)
    (add_net /14A)
    (add_net /14B)
    (add_net /_cs)
    (add_net /_f)
    (add_net /_int)
    (add_net /_pc)
    (add_net /_reset)
    (add_net /_w)
    (add_net /c)
    (add_net /d0)
    (add_net /d1)
    (add_net /d2)
    (add_net /d3)
    (add_net /d4)
    (add_net /d5)
    (add_net /d6)
    (add_net /d7)
    (add_net /e)
    (add_net /pa0)
    (add_net /pa1)
    (add_net /pa2)
    (add_net /pa3)
    (add_net /pa4)
    (add_net /pa5)
    (add_net /pa6)
    (add_net /pa7)
    (add_net /pb0)
    (add_net /pb1)
    (add_net /pb2)
    (add_net /pb5)
    (add_net /pb6)
    (add_net /pb7)
    (add_net /rs0)
    (add_net /rs1)
    (add_net /rs2)
    (add_net /rs3)
    (add_net /s)
    (add_net /tick)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(R2-Pad1)")
    (add_net VCC)
  )
  (module KiCad/kicad-footprints/Connector_PinHeader_2.54mm.pretty:PinHeader_1x02_P2.54mm_Horizontal (layer B.Cu) (tedit 601CA9EC)
    (at 33.625 123.2 270)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 0 2.33 270) (layer F.Fab) hide)
    (fp_text value Conn_01x02 (at 0 -4.87 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 -1.27) (layer B.Fab) hide)
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/kicad-footprints/Package_DIP.pretty:DIP-40_W15.24mm (layer F.Cu) (tedit 601CA73A)
    (at 25.895 72.07)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U1 (at 7.62 -2.33) (layer F.Fab) hide)
    (fp_text value "CIA8520 socket" (at 7.62 50.59) (layer F.Fab) hide)
    (fp_text user %R (at 7.62 24.13) (layer F.Fab) hide)
    (pad 40 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /c))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /s))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /tick))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /rs0))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /_pc))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /rs1))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /pb7))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /rs2))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /pb6))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /rs3))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /pb5))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /_reset))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 /14A))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /d0))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /13A))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /d1))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /pb2))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /d2))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /pb1))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /d3))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /pb0))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /d4))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /pa7))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /d5))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /pa6))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /d6))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /pa5))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /d7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /pa4))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /e))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /pa3))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /_f))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /pa2))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /_cs))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /pa1))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /_w))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /pa0))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /_int))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/kicad-footprints/Package_DIP.pretty:DIP-40_W15.24mm (layer F.Cu) (tedit 601CA701)
    (at 28.525 72.075)
    (descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
    (fp_text reference U3 (at 7.62 -2.33) (layer F.Fab) hide)
    (fp_text value "CIA8520 pin header" (at 7.62 50.59) (layer F.Fab) hide)
    (fp_text user %R (at 7.62 24.13) (layer F.Fab) hide)
    (pad 40 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /c))
    (pad 20 thru_hole oval (at 0 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /s))
    (pad 19 thru_hole oval (at 0 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /tick))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 /rs0))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /_pc))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 /rs1))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 /pb7))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /rs2))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /pb6))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /rs3))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /pb5))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 /_reset))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /14B))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /d0))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /13B))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /d1))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /pb2))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /d2))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /pb1))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /d3))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /pb0))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /d4))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /pa7))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 /d5))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 /pa6))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 /d6))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 /pa5))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /d7))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /pa4))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /e))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /pa3))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /_f))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 /pa2))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 /_cs))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /pa1))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /_w))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /pa0))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /_int))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/kicad-footprints/Package_SO.pretty:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 34.9 113.2 180)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 0 -6.2) (layer F.Fab) hide)
    (fp_text value 74LS153 (at 0 6.2) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd roundrect (at 2.475 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VCC))
    (pad 15 smd roundrect (at 2.475 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 14 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(R2-Pad1)"))
    (pad 13 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 12 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /14A))
    (pad 10 smd roundrect (at 2.475 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /13A))
    (pad 9 smd roundrect (at 2.475 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /14B))
    (pad 8 smd roundrect (at -2.475 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at -2.475 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /13B))
    (pad 6 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /14A))
    (pad 5 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /13A))
    (pad 4 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at -2.475 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -2.475 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adamgreig/agg-kicad/agg.pretty:0805 (layer F.Cu) (tedit 57654490)
    (at 33.325 120.225)
    (fp_text reference C1 (at -2.225 0 90) (layer F.Fab) hide)
    (fp_text value 0.1UF (at 2.225 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.9 0) (size 1.15 1.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9 0) (size 1.15 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module sparkfun/SparkFun-KiCad-Libraries/Footprints/Resistors.pretty:0805 (layer F.Cu) (tedit 200000)
    (at 37.15 100.85)
    (descr "GENERIC 2012 (0805) PACKAGE")
    (tags "GENERIC 2012 (0805) PACKAGE")
    (attr smd)
    (fp_text reference R2 (at 0 -1.27) (layer F.Fab) hide)
    (fp_text value 330R (at 0 1.27) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.89916 0) (size 0.79756 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.89916 0) (size 0.79756 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(R2-Pad1)") (solder_mask_margin 0.1016))
  )
  (module sparkfun/SparkFun-KiCad-Libraries/Footprints/Resistors.pretty:0805 (layer F.Cu) (tedit 200000)
    (at 37.15 103.475)
    (descr "GENERIC 2012 (0805) PACKAGE")
    (tags "GENERIC 2012 (0805) PACKAGE")
    (attr smd)
    (fp_text reference R1 (at 0 -1.27) (layer F.Fab) hide)
    (fp_text value 10K (at 0 1.27) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.89916 0) (size 0.79756 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -0.89916 0) (size 0.79756 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC) (solder_mask_margin 0.1016))
  )
  (gr_line (start 35.675 70.325) (end 44.775 70.325) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 24.825 70.325) (end 33.925 70.325) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 44.775 70.65) (end 45.1 70.65) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 44.775 121.975) (end 44.775 122.3) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 38.425 122.625) (end 38.425 122.3) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 37.775 127.425) (end 37.775 127.75) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 31.975 127.425) (end 31.65 127.425) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 31.325 122.625) (end 31.65 122.625) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 24.825 121.975) (end 24.5 121.975) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 24.5 70.65) (end 24.5 121.975) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 34.8 70.325) (end 35.675 70.325) (angle 180) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 24.825 70.65) (end 24.825 70.325) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 38.1 127.425) (end 38.1 122.625) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 31.975 127.75) (end 37.775 127.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 31.65 122.625) (end 31.65 127.425) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 31.325 122.3) (end 24.825 122.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 44.775 122.3) (end 38.425 122.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 45.1 70.65) (end 45.1 121.975) (layer Edge.Cuts) (width 0.05))
  (gr_text "Based on work by Jussi Kilpeläinen\nCopyright 2021 Stefan Reinauer\nhttps://amiga.technology/" (at 35.125 95.875 90) (layer B.SilkS))
  (gr_text "Amiga Boot Selector\n" (at 31.4 87.125 90) (layer F.SilkS))
  (gr_text "OPEN   = DF0\nCLOSED = DF1" (at 37.425 90.4 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 44.9 70.5) (xy 45.275 123.825) (xy 24.175 123.6) (xy 24.825 70.45)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 45.375 123.275) (xy 24 123.5) (xy 24.425 70.275) (xy 45.15 70.275)
      )
    )
  )
)
