<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="-12.7" y1="-12.7" x2="12.7" y2="-12.7" width="0" layer="20"/>
<wire x1="12.7" y1="-12.7" x2="12.7" y2="12.7" width="0" layer="20"/>
<wire x1="12.7" y1="12.7" x2="-12.7" y2="12.7" width="0" layer="20"/>
<wire x1="-12.7" y1="12.7" x2="-12.7" y2="-12.7" width="0" layer="20"/>
<hole x="0" y="0" drill="2.4384"/>
<text>12</text>
<text>14</text>
<text>2</text>
<text>1</text>
<text>3/3/20 SAW proj</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
<package name="SMD2,54-5,08">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="A-CCS_028-Z-T">
<description>&lt;ASSMANN WSW 1.27mm Pitch Female PLCC Socket, 28 Way, Through Hole, Tin over Nickel Plated Contacts 1A&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="ACCS028ZT">
<description>&lt;b&gt;A-CCS 028-Z-T-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun RF, WiFi, Cellular, and Bluetooth&lt;/h3&gt;
In this library you'll find things that send or receive RF-- cellular modules, Bluetooth, WiFi, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARF3078-ND">
<description>mmcx connector</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="11" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="16" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="18" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="19" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="21" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="23" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="25" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="26" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="28" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="5" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="7" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="9" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="15"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="21"/>
<attribute name="VALUE"/>
</element>
<element name="GND2" library="wirepad" package="SMD2,54-5,08" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="21"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="A-CCS_028-Z-T" package="ACCS028ZT" value="A-CCS_028-Z-T">
<attribute name="DESCRIPTION" value="ASSMANN WSW 1.27mm Pitch Female PLCC Socket, 28 Way, Through Hole, Tin over Nickel Plated Contacts 1A"/>
<attribute name="HEIGHT" value="8.3mm"/>
<attribute name="MANUFACTURER_NAME" value="ASSMANN WSW components GmbH"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="A-CCS 028-Z-T"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value="6742533"/>
<attribute name="RS_PRICE-STOCK" value="https://uk.rs-online.com/web/p/products/6742533"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-RF" package="ARF3078-ND" value="ARF3078-ND"/>
<element name="U$2" library="SparkFun-RF" package="ARF3078-ND" value="ARF3078-ND"/>
</elements>
<signals>
<signal name="N$4">
<contactref element="5" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="J1" pad="7"/>
<contactref element="7" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="J1" pad="9"/>
<contactref element="9" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="J1" pad="11"/>
<contactref element="11" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="16"/>
<contactref element="16" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="18"/>
<contactref element="18" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="19"/>
<contactref element="19" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J1" pad="21"/>
<contactref element="21" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="J1" pad="23"/>
<contactref element="23" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="25"/>
<contactref element="25" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="13"/>
<contactref element="GND2" pad="1"/>
<contactref element="J1" pad="27"/>
<contactref element="GND" pad="1"/>
<contactref element="J1" pad="24"/>
<contactref element="J1" pad="22"/>
<contactref element="J1" pad="17"/>
<contactref element="J1" pad="15"/>
<contactref element="J1" pad="20"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="P$2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="4"/>
<contactref element="U$2" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="J1" pad="28"/>
<contactref element="28" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="J1" pad="26"/>
<contactref element="26" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="14"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="J1" pad="12"/>
<contactref element="U$1" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
