(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 0)
    (no_connects 0)
    (area 55.169999 51.994999 245.820001 132.155001)
    (thickness 1.6)
    (drawings 57)
    (tracks 2773)
    (zones 0)
    (modules 264)
    (nets 158)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.6 0.6)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 +5V-A)
  (net 4 +5V-B)
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad2)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D3-Pad2)")
  (net 10 "Net-(D3-Pad1)")
  (net 11 "Net-(D4-Pad2)")
  (net 12 "Net-(D4-Pad1)")
  (net 13 "Net-(D5-Pad2)")
  (net 14 "Net-(D5-Pad1)")
  (net 15 "Net-(D6-Pad2)")
  (net 16 "Net-(D6-Pad1)")
  (net 17 "Net-(D7-Pad2)")
  (net 18 "Net-(D7-Pad1)")
  (net 19 "Net-(D8-Pad2)")
  (net 20 "Net-(D8-Pad1)")
  (net 21 "Net-(D9-Pad2)")
  (net 22 "Net-(D9-Pad1)")
  (net 23 "Net-(D10-Pad2)")
  (net 24 "Net-(D10-Pad1)")
  (net 25 "Net-(D11-Pad2)")
  (net 26 "Net-(D11-Pad1)")
  (net 27 "Net-(D12-Pad2)")
  (net 28 "Net-(D12-Pad1)")
  (net 29 "Net-(D13-Pad2)")
  (net 30 "Net-(D13-Pad1)")
  (net 31 "Net-(D14-Pad2)")
  (net 32 "Net-(D14-Pad1)")
  (net 33 "Net-(D15-Pad2)")
  (net 34 "Net-(D15-Pad1)")
  (net 35 "Net-(D16-Pad2)")
  (net 36 "Net-(D16-Pad1)")
  (net 37 "Net-(JP1-Pad1)")
  (net 38 "Net-(JP2-Pad1)")
  (net 39 "Net-(JP3-Pad1)")
  (net 40 "Net-(JP4-Pad1)")
  (net 41 "Net-(JP5-Pad1)")
  (net 42 "Net-(JP6-Pad1)")
  (net 43 "Net-(JP7-Pad1)")
  (net 44 "Net-(JP8-Pad1)")
  (net 45 "Net-(JP9-Pad1)")
  (net 46 "Net-(JP10-Pad1)")
  (net 47 "Net-(JP11-Pad1)")
  (net 48 "Net-(JP12-Pad1)")
  (net 49 "Net-(JP13-Pad1)")
  (net 50 "Net-(JP14-Pad1)")
  (net 51 "Net-(P1-Pad1)")
  (net 52 SDA)
  (net 53 SCL)
  (net 54 "Net-(P6-Pad2)")
  (net 55 "Net-(P6-Pad4)")
  (net 56 "Net-(P6-Pad6)")
  (net 57 "Net-(P6-Pad8)")
  (net 58 "Net-(P7-Pad2)")
  (net 59 "Net-(P7-Pad4)")
  (net 60 "Net-(P7-Pad6)")
  (net 61 "Net-(P7-Pad8)")
  (net 62 "Net-(P8-Pad2)")
  (net 63 "Net-(P8-Pad4)")
  (net 64 "Net-(P8-Pad6)")
  (net 65 "Net-(P8-Pad8)")
  (net 66 "Net-(P9-Pad2)")
  (net 67 "Net-(P9-Pad4)")
  (net 68 "Net-(P9-Pad6)")
  (net 69 "Net-(P9-Pad8)")
  (net 70 +3V3)
  (net 71 "Net-(Q1-Pad1)")
  (net 72 OE-Disable)
  (net 73 "/Power Driver A/LED Driver A/LED1")
  (net 74 "/Power Driver A/LED Driver A/LED2")
  (net 75 "Net-(Q4-Pad1)")
  (net 76 "Net-(Q4-Pad2)")
  (net 77 "Net-(Q5-Pad3)")
  (net 78 "Net-(Q6-Pad1)")
  (net 79 "Net-(Q6-Pad2)")
  (net 80 "Net-(Q7-Pad3)")
  (net 81 "/Power Driver A/LED Driver A/LED3")
  (net 82 "/Power Driver A/LED Driver A/LED4")
  (net 83 "Net-(Q10-Pad1)")
  (net 84 "Net-(Q10-Pad2)")
  (net 85 "Net-(Q11-Pad3)")
  (net 86 "Net-(Q12-Pad1)")
  (net 87 "Net-(Q12-Pad2)")
  (net 88 "Net-(Q13-Pad3)")
  (net 89 "/Power Driver B/LED Driver A/LED1")
  (net 90 "/Power Driver B/LED Driver A/LED2")
  (net 91 "Net-(Q16-Pad1)")
  (net 92 "Net-(Q16-Pad2)")
  (net 93 "Net-(Q17-Pad3)")
  (net 94 "/Power Driver A/LED Driver B/LED1")
  (net 95 "/Power Driver A/LED Driver B/LED2")
  (net 96 "Net-(Q20-Pad1)")
  (net 97 "Net-(Q20-Pad2)")
  (net 98 "Net-(Q21-Pad3)")
  (net 99 "Net-(Q22-Pad1)")
  (net 100 "Net-(Q22-Pad2)")
  (net 101 "Net-(Q23-Pad3)")
  (net 102 "Net-(Q24-Pad1)")
  (net 103 "Net-(Q24-Pad2)")
  (net 104 "Net-(Q25-Pad3)")
  (net 105 "/Power Driver A/LED Driver B/LED3")
  (net 106 "/Power Driver A/LED Driver B/LED4")
  (net 107 "/Power Driver B/LED Driver A/LED3")
  (net 108 "/Power Driver B/LED Driver A/LED4")
  (net 109 "Net-(Q30-Pad1)")
  (net 110 "Net-(Q30-Pad2)")
  (net 111 "Net-(Q31-Pad3)")
  (net 112 "Net-(Q32-Pad1)")
  (net 113 "Net-(Q32-Pad2)")
  (net 114 "Net-(Q33-Pad3)")
  (net 115 "Net-(Q34-Pad1)")
  (net 116 "Net-(Q35-Pad1)")
  (net 117 "Net-(Q35-Pad2)")
  (net 118 "Net-(Q36-Pad3)")
  (net 119 "Net-(Q37-Pad1)")
  (net 120 "Net-(Q37-Pad2)")
  (net 121 "Net-(Q38-Pad3)")
  (net 122 "/Power Driver B/LED Driver B/LED1")
  (net 123 "/Power Driver B/LED Driver B/LED2")
  (net 124 "Net-(Q55-Pad1)")
  (net 125 "Net-(Q55-Pad2)")
  (net 126 "Net-(Q56-Pad3)")
  (net 127 "Net-(Q57-Pad1)")
  (net 128 "Net-(Q57-Pad2)")
  (net 129 "Net-(Q58-Pad3)")
  (net 130 "/Power Driver B/LED Driver B/LED3")
  (net 131 "/Power Driver B/LED Driver B/LED4")
  (net 132 "Net-(Q63-Pad1)")
  (net 133 "Net-(Q63-Pad2)")
  (net 134 "Net-(Q64-Pad3)")
  (net 135 "Net-(Q65-Pad1)")
  (net 136 "Net-(Q65-Pad2)")
  (net 137 "Net-(Q66-Pad3)")
  (net 138 "Net-(R13-Pad1)")
  (net 139 "Net-(R14-Pad1)")
  (net 140 "Net-(R19-Pad1)")
  (net 141 "Net-(R20-Pad1)")
  (net 142 "Net-(R25-Pad1)")
  (net 143 "Net-(R26-Pad1)")
  (net 144 "Net-(R31-Pad1)")
  (net 145 "Net-(R32-Pad1)")
  (net 146 "Net-(R45-Pad1)")
  (net 147 "Net-(R46-Pad1)")
  (net 148 "Net-(R51-Pad1)")
  (net 149 "Net-(R52-Pad1)")
  (net 150 "Net-(R57-Pad1)")
  (net 151 "Net-(R58-Pad1)")
  (net 152 "Net-(R63-Pad1)")
  (net 153 "Net-(R64-Pad1)")
  (net 154 "Net-(U1-Pad4)")
  (net 155 "Net-(U2-Pad4)")
  (net 156 /+12V-A)
  (net 157 /+12V-B)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V-A)
    (add_net +5V-B)
    (add_net /+12V-A)
    (add_net /+12V-B)
    (add_net "/Power Driver A/LED Driver A/LED1")
    (add_net "/Power Driver A/LED Driver A/LED2")
    (add_net "/Power Driver A/LED Driver A/LED3")
    (add_net "/Power Driver A/LED Driver A/LED4")
    (add_net "/Power Driver A/LED Driver B/LED1")
    (add_net "/Power Driver A/LED Driver B/LED2")
    (add_net "/Power Driver A/LED Driver B/LED3")
    (add_net "/Power Driver A/LED Driver B/LED4")
    (add_net "/Power Driver B/LED Driver A/LED1")
    (add_net "/Power Driver B/LED Driver A/LED2")
    (add_net "/Power Driver B/LED Driver A/LED3")
    (add_net "/Power Driver B/LED Driver A/LED4")
    (add_net "/Power Driver B/LED Driver B/LED1")
    (add_net "/Power Driver B/LED Driver B/LED2")
    (add_net "/Power Driver B/LED Driver B/LED3")
    (add_net "/Power Driver B/LED Driver B/LED4")
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad1)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP10-Pad1)")
    (add_net "Net-(JP11-Pad1)")
    (add_net "Net-(JP12-Pad1)")
    (add_net "Net-(JP13-Pad1)")
    (add_net "Net-(JP14-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(JP4-Pad1)")
    (add_net "Net-(JP5-Pad1)")
    (add_net "Net-(JP6-Pad1)")
    (add_net "Net-(JP7-Pad1)")
    (add_net "Net-(JP8-Pad1)")
    (add_net "Net-(JP9-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad4)")
    (add_net "Net-(P6-Pad6)")
    (add_net "Net-(P6-Pad8)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad4)")
    (add_net "Net-(P7-Pad6)")
    (add_net "Net-(P7-Pad8)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P8-Pad4)")
    (add_net "Net-(P8-Pad6)")
    (add_net "Net-(P8-Pad8)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(P9-Pad4)")
    (add_net "Net-(P9-Pad6)")
    (add_net "Net-(P9-Pad8)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q10-Pad1)")
    (add_net "Net-(Q10-Pad2)")
    (add_net "Net-(Q11-Pad3)")
    (add_net "Net-(Q12-Pad1)")
    (add_net "Net-(Q12-Pad2)")
    (add_net "Net-(Q13-Pad3)")
    (add_net "Net-(Q16-Pad1)")
    (add_net "Net-(Q16-Pad2)")
    (add_net "Net-(Q17-Pad3)")
    (add_net "Net-(Q20-Pad1)")
    (add_net "Net-(Q20-Pad2)")
    (add_net "Net-(Q21-Pad3)")
    (add_net "Net-(Q22-Pad1)")
    (add_net "Net-(Q22-Pad2)")
    (add_net "Net-(Q23-Pad3)")
    (add_net "Net-(Q24-Pad1)")
    (add_net "Net-(Q24-Pad2)")
    (add_net "Net-(Q25-Pad3)")
    (add_net "Net-(Q30-Pad1)")
    (add_net "Net-(Q30-Pad2)")
    (add_net "Net-(Q31-Pad3)")
    (add_net "Net-(Q32-Pad1)")
    (add_net "Net-(Q32-Pad2)")
    (add_net "Net-(Q33-Pad3)")
    (add_net "Net-(Q34-Pad1)")
    (add_net "Net-(Q35-Pad1)")
    (add_net "Net-(Q35-Pad2)")
    (add_net "Net-(Q36-Pad3)")
    (add_net "Net-(Q37-Pad1)")
    (add_net "Net-(Q37-Pad2)")
    (add_net "Net-(Q38-Pad3)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q5-Pad3)")
    (add_net "Net-(Q55-Pad1)")
    (add_net "Net-(Q55-Pad2)")
    (add_net "Net-(Q56-Pad3)")
    (add_net "Net-(Q57-Pad1)")
    (add_net "Net-(Q57-Pad2)")
    (add_net "Net-(Q58-Pad3)")
    (add_net "Net-(Q6-Pad1)")
    (add_net "Net-(Q6-Pad2)")
    (add_net "Net-(Q63-Pad1)")
    (add_net "Net-(Q63-Pad2)")
    (add_net "Net-(Q64-Pad3)")
    (add_net "Net-(Q65-Pad1)")
    (add_net "Net-(Q65-Pad2)")
    (add_net "Net-(Q66-Pad3)")
    (add_net "Net-(Q7-Pad3)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R25-Pad1)")
    (add_net "Net-(R26-Pad1)")
    (add_net "Net-(R31-Pad1)")
    (add_net "Net-(R32-Pad1)")
    (add_net "Net-(R45-Pad1)")
    (add_net "Net-(R46-Pad1)")
    (add_net "Net-(R51-Pad1)")
    (add_net "Net-(R52-Pad1)")
    (add_net "Net-(R57-Pad1)")
    (add_net "Net-(R58-Pad1)")
    (add_net "Net-(R63-Pad1)")
    (add_net "Net-(R64-Pad1)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad4)")
    (add_net OE-Disable)
    (add_net SCL)
    (add_net SDA)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 63.5 125.73)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 63.5 58.42)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 237.49 125.73)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 139.922 107.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 138.922 107.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 137.922 107.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 139.922 106.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 138.922 106.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 137.922 106.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 139.922 105.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 138.922 105.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 162.671 76.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 162.671 74.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 162.671 75.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 161.639 75.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 161.639 76.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 160.639 76.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 160.639 75.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 158.718 75.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 158.718 76.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 159.639 76.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 158.718 74.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 159.639 75.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 159.639 74.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 161.639 74.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 160.639 74.93)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 126.349 74.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 127.349 75.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 127.349 74.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 126.349 75.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 126.349 73.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 127.349 73.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 130.27 75.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 129.27 75.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 128.27 75.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 130.27 74.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 129.27 74.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 128.27 74.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 130.27 73.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 129.27 73.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 86.614 66.802 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q6 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(Q6-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 102.362 64.262 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q7 (at 0 -4.318 270) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 55 "Net-(P6-Pad4)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 80 "Net-(Q7-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 78 "Net-(Q6-Pad1)"))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 102.362 77.47 90)
    (fp_text reference Rsense2 (at -0.1 2.4 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(Q7-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 110.49 64.262 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q11 (at 0 -4.318 270) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 56 "Net-(P6-Pad6)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 85 "Net-(Q11-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 83 "Net-(Q10-Pad1)"))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 94.234 64.262 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q5 (at 0 -4.318 270) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 54 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 77 "Net-(Q5-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 75 "Net-(Q4-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 71.882 78.994)
    (fp_text reference RV1 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(Q4-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(Q4-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R13-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 87.122 72.898 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R20-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 82.042 78.994)
    (fp_text reference RV3 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(Q10-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(Q10-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R19-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 71.882 72.898 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R13-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 87.122 78.994)
    (fp_text reference RV4 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(Q12-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(Q12-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R20-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 76.962 72.898 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R14-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 82.042 72.898 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 76.962 78.994)
    (fp_text reference RV2 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(Q6-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(Q6-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R14-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 86.614 61.722 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(Q4-Pad2)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 75.438 64.262 270)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value LM324AN (at 0 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(Q4-Pad2)"))
    (pad 2 smd rect (at -2.54 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(R13-Pad1)"))
    (pad 3 smd rect (at -1.27 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(Q5-Pad3)"))
    (pad 4 smd rect (at 0 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (pad 5 smd rect (at 1.27 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(Q7-Pad3)"))
    (pad 6 smd rect (at 2.54 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(R14-Pad1)"))
    (pad 7 smd rect (at 3.81 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(Q6-Pad2)"))
    (pad 8 smd rect (at 3.81 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(Q10-Pad2)"))
    (pad 9 smd rect (at 2.54 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(R19-Pad1)"))
    (pad 11 smd rect (at 0 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -1.27 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(Q13-Pad3)"))
    (pad 13 smd rect (at -2.54 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(R20-Pad1)"))
    (pad 14 smd rect (at -3.81 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(Q12-Pad2)"))
    (pad 10 smd rect (at 1.27 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(Q11-Pad3)"))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 82.55 66.802)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q10 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(Q10-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 82.55 61.722)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q12 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(Q12-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(Q12-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 115.57 79.502 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 118.618 77.47 90)
    (fp_text reference Rsense4 (at -0.1 2.4 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(Q13-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 113.03 79.522 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 114.554 74.93)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q8 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 81 "/Power Driver A/LED Driver A/LED3"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 118.618 64.262 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q13 (at 0 -4.318 270) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 57 "Net-(P6-Pad8)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 88 "Net-(Q13-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 86 "Net-(Q12-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 99.822 80.01 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 110.49 77.47 90)
    (fp_text reference Rsense3 (at -0.1 2.4 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(Q11-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 98.298 75.438)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Power Driver A/LED Driver A/LED1"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 97.282 80.01 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 123.19 75.438)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q9 (at 0 -2.54) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 82 "/Power Driver A/LED Driver A/LED4"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 124.206 80.01 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D4-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 121.666 80.01 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 105.41 79.522 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 107.95 79.522 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 94.234 77.597 90)
    (fp_text reference Rsense1 (at -0.1 2.4 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(Q5-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 106.426 75.438)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 74 "/Power Driver A/LED Driver A/LED2"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 91.948 101.981 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 100.711 102.362 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D6-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 109.347 102.743 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D7-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 117.602 102.87 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D8-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 176.276 80.01 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D9-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 184.912 79.502 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D10 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D10-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 193.04 80.01 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D11 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D11-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 201.168 80.01 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D12 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D12-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 175.768 102.87 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D13 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D13-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 184.404 102.87 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D14 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D14-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D14-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 192.532 102.87 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D15 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D15-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 57FE93EC)
    (at 200.66 102.87 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D16 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D16-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 131.826 89.662)
    (fp_text reference JP1 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A0 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 127.762 89.662)
    (fp_text reference JP2 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A1 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(JP2-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 123.698 89.662)
    (fp_text reference JP3 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A2 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(JP3-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 119.634 89.662)
    (fp_text reference JP4 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A3 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(JP4-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 115.57 89.662)
    (fp_text reference JP5 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A4 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(JP5-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 111.506 89.662)
    (fp_text reference JP6 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A5 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(JP6-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 107.442 89.662)
    (fp_text reference JP7 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A6 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(JP7-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 173.354996 89.724)
    (fp_text reference JP8 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A0 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(JP8-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 169.20633 89.724)
    (fp_text reference JP9 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A1 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(JP9-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 165.057664 89.724)
    (fp_text reference JP10 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A2 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(JP10-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 160.908998 89.724)
    (fp_text reference JP11 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A3 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(JP11-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 156.760332 89.724)
    (fp_text reference JP12 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A4 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(JP12-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 152.611666 89.724)
    (fp_text reference JP13 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A5 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(JP13-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
  )
  (module Custom_Footprints:Jumper_SMD (layer F.Cu) (tedit 588BE8C1)
    (at 148.463 89.724)
    (fp_text reference JP14 (at 2.3 0 90) (layer F.SilkS))
    (fp_text value A6 (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(JP14-Pad1)"))
    (pad 2 smd rect (at 0 0.7) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 132.461 78.105)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 51 "Net-(P1-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Custom_Footprints:Screw_Connector_M5 (layer F.Cu) (tedit 58700478)
    (at 148.336 76.2 90)
    (fp_text reference P2 (at 0 8 90) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -9.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.5 -5.5 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 2 thru_hole circle (at 5.3 -5.5 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 3 thru_hole circle (at -5.5 -0.29 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 4 thru_hole circle (at 5.3 -0.29 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 5 thru_hole circle (at -5.5 4.92 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 6 thru_hole circle (at 5.3 4.92 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 128.778 107.188 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 1.016 -2.667 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 SDA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 SCL))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 128.778 99.822 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 1.143 -2.54 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0.454667 -3.4 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 52 SDA))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 53 SCL))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Custom_Footprints:Screw_Connector_M5 (layer F.Cu) (tedit 58700478)
    (at 148.844 106.172 90)
    (fp_text reference P5 (at 0 8 90) (layer F.SilkS))
    (fp_text value CONN_01X06 (at 0 -9.5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.5 -5.5 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5.3 -5.5 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at -5.5 -0.29 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole circle (at 5.3 -0.29 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole circle (at -5.5 4.92 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole circle (at 5.3 4.92 90) (size 4 4) (drill 2.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 127.762 59.182)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P6 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 54 "Net-(P6-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 55 "Net-(P6-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 56 "Net-(P6-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 57 "Net-(P6-Pad8)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 127.762 123.698)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 58 "Net-(P7-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 59 "Net-(P7-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 60 "Net-(P7-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 61 "Net-(P7-Pad8)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 152.4 59.182)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P8 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 62 "Net-(P8-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 63 "Net-(P8-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 64 "Net-(P8-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 65 "Net-(P8-Pad8)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 152.4 123.698)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P9 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 66 "Net-(P9-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 67 "Net-(P9-Pad4)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 68 "Net-(P9-Pad6)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +12V))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 69 "Net-(P9-Pad8)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 168.275 74.93 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P10 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 70 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 92.44 90.236)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 72 OE-Disable))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 175.768 75.438 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q14 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D9-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 89 "/Power Driver B/LED Driver A/LED1"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 183.896 75.438 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q15 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 90 "/Power Driver B/LED Driver A/LED2"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 217.424 63.754)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q16 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(Q16-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(Q16-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 179.324 64.389 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q17 (at 0 -4.318 270) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 62 "Net-(P8-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 93 "Net-(Q17-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 91 "Net-(Q16-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 93.726 107.569)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q18 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 94 "/Power Driver A/LED Driver B/LED1"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 102.108 107.569)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q19 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 95 "/Power Driver A/LED Driver B/LED2"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 213.36 63.754)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q20 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(Q20-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(Q20-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 187.536666 64.389 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q21 (at 0 -4.318 270) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 63 "Net-(P8-Pad4)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 98 "Net-(Q21-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 96 "Net-(Q20-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 73.726 117.332 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q22 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(Q22-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(Q22-Pad2)"))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 97.79 118.364 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q23 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 58 "Net-(P7-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 101 "Net-(Q23-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 99 "Net-(Q22-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 78.486 117.348 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q24 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(Q24-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(Q24-Pad2)"))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 106.172 118.364 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q25 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 59 "Net-(P7-Pad4)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 104 "Net-(Q25-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 102 "Net-(Q24-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 110.617 107.823)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q26 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 105 "/Power Driver A/LED Driver B/LED3"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 118.618 107.823)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q27 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 106 "/Power Driver A/LED Driver B/LED4"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 192.024 75.438 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q28 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 107 "/Power Driver B/LED Driver A/LED3"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 200.152 75.438 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q29 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Power Driver B/LED Driver A/LED4"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 87.884 117.348 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q30 (at 0 2.54 270) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(Q30-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(Q30-Pad2)"))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 114.3 118.364 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q31 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 60 "Net-(P7-Pad6)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 111 "Net-(Q31-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 109 "Net-(Q30-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 83.312 117.348 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q32 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(Q32-Pad1)"))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(Q32-Pad2)"))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 122.428 118.364 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q33 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 61 "Net-(P7-Pad8)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 114 "Net-(Q33-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 112 "Net-(Q32-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 144.542 91.948)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q34 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(Q34-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 72 OE-Disable))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 225.552 63.754)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q35 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(Q35-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(Q35-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 195.749332 64.389 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q36 (at 0 -4.318 270) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 64 "Net-(P8-Pad6)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 118 "Net-(Q36-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 116 "Net-(Q35-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 221.488 63.754)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q37 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(Q37-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(Q37-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 203.961998 64.389 270)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q38 (at 0 -4.318 270) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 65 "Net-(P8-Pad8)"))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 121 "Net-(Q38-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 270) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 119 "Net-(Q37-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 175.26 107.442)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q51 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 122 "/Power Driver B/LED Driver B/LED1"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 182.88 107.95)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q52 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 123 "/Power Driver B/LED Driver B/LED2"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 223.52 111.506)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q55 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(Q55-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(Q55-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 178.990855 119.054938 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q56 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 66 "Net-(P9-Pad2)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 126 "Net-(Q56-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 124 "Net-(Q55-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 218.948 111.506)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q57 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(Q57-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(Q57-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 187.118854 119.054938 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q58 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 67 "Net-(P9-Pad4)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 129 "Net-(Q58-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 127 "Net-(Q57-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 191.516 107.95)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q59 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 130 "/Power Driver B/LED Driver B/LED3"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 199.644 107.442)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q60 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 131 "/Power Driver B/LED Driver B/LED4"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 214.376 111.506)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q63 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(Q63-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(Q63-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 195.246853 119.054938 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q64 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 68 "Net-(P9-Pad6)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 134 "Net-(Q64-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 132 "Net-(Q63-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 583F39EB)
    (at 209.804 111.506)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q65 (at 0 -2.5) (layer F.SilkS))
    (fp_text value BC413 (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(Q65-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(Q65-Pad2)"))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 203.374852 119.054938 90)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference Q66 (at 0 -4.318 90) (layer F.SilkS))
    (fp_text value BUT11 (at 0 -4.318 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 69 "Net-(P9-Pad8)"))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 137 "Net-(Q66-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 135 "Net-(Q65-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 131.826 93.98 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(JP1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 127.762 93.98 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(JP2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 123.698 93.98 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(JP3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 119.888 93.9 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(JP4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 115.57 93.98 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(JP5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 111.506 93.98 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(JP6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 107.442 93.9 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(JP7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 91.266 94.234)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 91.186 68.072 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Power Driver A/LED Driver A/LED1"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 99.314 68.072 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(Q6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 74 "/Power Driver A/LED Driver A/LED2"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 107.442 68.072 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(Q10-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 81 "/Power Driver A/LED Driver A/LED3"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 115.316 67.564 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(Q12-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 82 "/Power Driver A/LED Driver A/LED4"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 94.869 101.854 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 103.378 101.981 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 93.599 118.237 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(Q22-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 94 "/Power Driver A/LED Driver B/LED1"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 102.489 117.856 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(Q24-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 95 "/Power Driver A/LED Driver B/LED2"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 82.042 106.426 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R25-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 85.09 106.426 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(R26-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 112.014 102.489 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 120.142 102.489 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R28 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D8-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 111.125 118.11 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R29 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 109 "Net-(Q30-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 105 "/Power Driver A/LED Driver B/LED3"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 119.126 118.11 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R30 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 112 "Net-(Q32-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 106 "/Power Driver A/LED Driver B/LED4"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 82.042 112.014 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R31 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R31-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 88.138 106.426 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R32 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R32-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 173.228 95.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R33 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(JP8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 169.672 95.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R34 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(JP9-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 166.116 95.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R35 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(JP10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 162.56 95.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R36 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(JP11-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 159.004 95.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R37 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(JP12-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 155.448 95.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R38 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(JP13-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 151.892 95.25 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R39 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(JP14-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 148.336 95.25 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R40 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(Q34-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 173.228 80.01 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R41 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D9-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 182.372 80.01 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R42 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D10-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 175.768 68.326 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R43 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(Q16-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 89 "/Power Driver B/LED Driver A/LED1"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 183.896 68.326 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R44 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(Q20-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 90 "/Power Driver B/LED Driver A/LED2"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 212.344 74.041 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R45 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(R45-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 214.884 68.326 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R46 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 2K (at 0 2.159 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R46-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 190.5 80.01 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R47 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D11-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 198.628 80.01 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R48 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(D12-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 192.532 68.326 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R49 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 116 "Net-(Q35-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 107 "/Power Driver B/LED Driver A/LED3"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 200.66 68.326 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R50 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 119 "Net-(Q37-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Power Driver B/LED Driver A/LED4"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 212.344 68.326 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R51 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R51-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 214.884 74.041 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R52 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R52-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 172.72 102.87 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R53 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D13-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 181.864 103.378 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R54 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(D14-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 182.372 117.094 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R55 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 124 "Net-(Q55-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 122 "/Power Driver B/LED Driver B/LED1"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 190.5 117.094 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R56 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 127 "Net-(Q57-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 123 "/Power Driver B/LED Driver B/LED2"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 221.488 120.142)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R57 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R57-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 221.488 115.062)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R58 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R58-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 189.992 102.87 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R59 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(D15-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 198.12 102.87 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R60 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 330 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D16-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 198.628 117.094 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R61 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(Q63-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 130 "/Power Driver B/LED Driver B/LED3"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 206.756 117.094 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R62 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(Q65-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 131 "/Power Driver B/LED Driver B/LED4"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 221.488 117.602)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R63 (at 0 -2.032) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R63-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 221.488 122.682)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R64 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 2K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R64-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 140.462 92.202 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R65 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 72 OE-Disable))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(P1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 167.212 80.391)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R66 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 4.7K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 52 SDA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 167.132 83.312)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R67 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 4.7K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 53 SCL))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 70 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 97.79 105.156 270)
    (fp_text reference Rsense5 (at -0.1 2.4 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(Q23-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 106.172 104.902 270)
    (fp_text reference Rsense6 (at -0.1 2.4 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 104 "Net-(Q25-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 114.3 104.902 270)
    (fp_text reference Rsense7 (at -0.1 2.4 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(Q31-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 122.428 104.902 270)
    (fp_text reference Rsense8 (at -0.1 2.4 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(Q33-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 179.324 77.978 90)
    (fp_text reference Rsense9 (at 0.124 2.4 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 93 "Net-(Q17-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 187.452 77.978 90)
    (fp_text reference Rsense10 (at -0.1 2.4 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0 -2.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 98 "Net-(Q21-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 195.58 77.978 90)
    (fp_text reference Rsense11 (at -0.1 2.4 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(Q36-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 203.708 77.978 90)
    (fp_text reference Rsense12 (at -0.1 2.4 90) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(Q38-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 178.990852 105.338938 270)
    (fp_text reference Rsense13 (at 0.124 1.953 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(Q56-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 187.267852 105.338938 270)
    (fp_text reference Rsense14 (at -0.1 2.4 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 129 "Net-(Q58-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 195.321352 105.338938 270)
    (fp_text reference Rsense15 (at -0.1 2.4 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(Q64-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Current_Sense_Resistor (layer F.Cu) (tedit 57DE1991)
    (at 203.374852 105.338938 270)
    (fp_text reference Rsense16 (at -0.1 2.4 270) (layer F.SilkS))
    (fp_text value 0.1 (at 0.3 -2.9 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 137 "Net-(Q66-Pad3)"))
    (pad 2 thru_hole circle (at -5.715 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 72.136 99.822)
    (fp_text reference RV5 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(Q22-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(Q22-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R25-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 77.25 99.785)
    (fp_text reference RV6 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(Q24-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(Q24-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(R26-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 82.296 99.785)
    (fp_text reference RV7 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(Q30-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(Q30-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R31-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 87.376 99.775)
    (fp_text reference RV8 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(Q32-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(Q32-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R32-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 211.836 80.01)
    (fp_text reference RV9 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(Q16-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(Q16-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(R45-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 217.424 80.01)
    (fp_text reference RV10 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(Q20-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(Q20-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R46-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 223.012 80.01)
    (fp_text reference RV11 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(Q35-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(Q35-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R51-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 228.6 80.01)
    (fp_text reference RV12 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(Q37-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(Q37-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R52-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 210.312 105.41)
    (fp_text reference RV13 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(Q55-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(Q55-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R57-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 215.392 105.41)
    (fp_text reference RV14 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(Q57-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(Q57-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R58-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 220.472 105.41)
    (fp_text reference RV15 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(Q63-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(Q63-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R63-Pad1)"))
  )
  (module Custom_Footprints:Bourns-TC33 (layer F.Cu) (tedit 588BE463)
    (at 225.552 105.41)
    (fp_text reference RV16 (at 0 4) (layer F.SilkS))
    (fp_text value 10K (at 0 -4.5) (layer F.Fab))
    (pad 1 smd rect (at -1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(Q65-Pad2)"))
    (pad 2 smd rect (at 0 -1.45) (size 1.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(Q65-Pad2)"))
    (pad 3 smd rect (at 1.4 1.8) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R64-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 583F3A3F)
    (at 84.836 89.662 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at 0 -2.9 180) (layer F.SilkS))
    (fp_text value LD3985G (at 0 2.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 156 /+12V-A))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 156 /+12V-A))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 154 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 583F3A3F)
    (at 188.194524 93.916)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 -2.9) (layer F.SilkS))
    (fp_text value LD3985G (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 157 /+12V-B))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 157 /+12V-B))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 155 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SSOP-20 (layer F.Cu) (tedit 0)
    (at 100.33 89.662 180)
    (descr "SSOP 20 pins")
    (tags "CMS SSOP SMD")
    (attr smd)
    (fp_text reference U3 (at -0.021001 -0.635 180) (layer F.SilkS))
    (fp_text value PCA9634 (at 0 0.635 180) (layer F.Fab))
    (pad 1 smd rect (at -2.921 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(JP1-Pad1)"))
    (pad 2 smd rect (at -2.286 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(JP2-Pad1)"))
    (pad 3 smd rect (at -1.6256 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(JP3-Pad1)"))
    (pad 4 smd rect (at -0.9652 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(JP4-Pad1)"))
    (pad 5 smd rect (at -0.3302 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(JP5-Pad1)"))
    (pad 6 smd rect (at 0.3302 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 73 "/Power Driver A/LED Driver A/LED1"))
    (pad 7 smd rect (at 0.9906 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 74 "/Power Driver A/LED Driver A/LED2"))
    (pad 8 smd rect (at 1.6256 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 81 "/Power Driver A/LED Driver A/LED3"))
    (pad 9 smd rect (at 2.286 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 82 "/Power Driver A/LED Driver A/LED4"))
    (pad 10 smd rect (at 2.921 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.921 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 94 "/Power Driver A/LED Driver B/LED1"))
    (pad 12 smd rect (at 2.286 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 95 "/Power Driver A/LED Driver B/LED2"))
    (pad 13 smd rect (at 1.6256 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 105 "/Power Driver A/LED Driver B/LED3"))
    (pad 14 smd rect (at 0.9906 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 106 "/Power Driver A/LED Driver B/LED4"))
    (pad 15 smd rect (at 0.3302 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(Q1-Pad1)"))
    (pad 16 smd rect (at -0.3302 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(JP6-Pad1)"))
    (pad 17 smd rect (at -0.9652 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(JP7-Pad1)"))
    (pad 18 smd rect (at -1.6256 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 53 SCL))
    (pad 19 smd rect (at -2.286 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 52 SDA))
    (pad 20 smd rect (at -2.921 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (model SMD_Packages.3dshapes/SSOP-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.255 0.33 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SSOP-20 (layer F.Cu) (tedit 0)
    (at 180.086 89.916 180)
    (descr "SSOP 20 pins")
    (tags "CMS SSOP SMD")
    (attr smd)
    (fp_text reference U6 (at 0 -0.635 180) (layer F.SilkS))
    (fp_text value PCA9634 (at 0 0.635 180) (layer F.Fab))
    (pad 1 smd rect (at -2.921 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(JP8-Pad1)"))
    (pad 2 smd rect (at -2.286 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(JP9-Pad1)"))
    (pad 3 smd rect (at -1.6256 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(JP10-Pad1)"))
    (pad 4 smd rect (at -0.9652 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(JP11-Pad1)"))
    (pad 5 smd rect (at -0.3302 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(JP12-Pad1)"))
    (pad 6 smd rect (at 0.3302 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 89 "/Power Driver B/LED Driver A/LED1"))
    (pad 7 smd rect (at 0.9906 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 90 "/Power Driver B/LED Driver A/LED2"))
    (pad 8 smd rect (at 1.6256 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 107 "/Power Driver B/LED Driver A/LED3"))
    (pad 9 smd rect (at 2.286 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 108 "/Power Driver B/LED Driver A/LED4"))
    (pad 10 smd rect (at 2.921 2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 2.921 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 122 "/Power Driver B/LED Driver B/LED1"))
    (pad 12 smd rect (at 2.286 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 123 "/Power Driver B/LED Driver B/LED2"))
    (pad 13 smd rect (at 1.6256 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 130 "/Power Driver B/LED Driver B/LED3"))
    (pad 14 smd rect (at 0.9906 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 131 "/Power Driver B/LED Driver B/LED4"))
    (pad 15 smd rect (at 0.3302 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 115 "Net-(Q34-Pad1)"))
    (pad 16 smd rect (at -0.3302 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(JP13-Pad1)"))
    (pad 17 smd rect (at -0.9652 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(JP14-Pad1)"))
    (pad 18 smd rect (at -1.6256 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 53 SCL))
    (pad 19 smd rect (at -2.286 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 52 SDA))
    (pad 20 smd rect (at -2.921 -2.667 180) (size 0.4064 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (model SMD_Packages.3dshapes/SSOP-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.255 0.33 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 75.184 109.22 270)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U5 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value LM324AN (at 0 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(Q22-Pad2)"))
    (pad 2 smd rect (at -2.54 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 142 "Net-(R25-Pad1)"))
    (pad 3 smd rect (at -1.27 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(Q23-Pad3)"))
    (pad 4 smd rect (at 0 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (pad 5 smd rect (at 1.27 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(Q25-Pad3)"))
    (pad 6 smd rect (at 2.54 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 143 "Net-(R26-Pad1)"))
    (pad 7 smd rect (at 3.81 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(Q24-Pad2)"))
    (pad 8 smd rect (at 3.81 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 110 "Net-(Q30-Pad2)"))
    (pad 9 smd rect (at 2.54 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 144 "Net-(R31-Pad1)"))
    (pad 11 smd rect (at 0 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -1.27 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 114 "Net-(Q33-Pad3)"))
    (pad 13 smd rect (at -2.54 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 145 "Net-(R32-Pad1)"))
    (pad 14 smd rect (at -3.81 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 113 "Net-(Q32-Pad2)"))
    (pad 10 smd rect (at 1.27 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 111 "Net-(Q31-Pad3)"))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 223.393 70.993 270)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U7 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value LM324AN (at 0 1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(Q16-Pad2)"))
    (pad 2 smd rect (at -2.54 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(R45-Pad1)"))
    (pad 3 smd rect (at -1.27 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(Q17-Pad3)"))
    (pad 4 smd rect (at 0 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (pad 5 smd rect (at 1.27 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 98 "Net-(Q21-Pad3)"))
    (pad 6 smd rect (at 2.54 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 147 "Net-(R46-Pad1)"))
    (pad 7 smd rect (at 3.81 3.302 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(Q20-Pad2)"))
    (pad 8 smd rect (at 3.81 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(Q35-Pad2)"))
    (pad 9 smd rect (at 2.54 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(R51-Pad1)"))
    (pad 11 smd rect (at 0 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -1.27 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 121 "Net-(Q38-Pad3)"))
    (pad 13 smd rect (at -2.54 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(R52-Pad1)"))
    (pad 14 smd rect (at -3.81 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 120 "Net-(Q37-Pad2)"))
    (pad 10 smd rect (at 1.27 -3.048 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(Q36-Pad3)"))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-14_N (layer F.Cu) (tedit 0)
    (at 213.36 119.126 90)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U8 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value LM324AN (at 0 1.27 90) (layer F.Fab))
    (pad 1 smd rect (at -3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 125 "Net-(Q55-Pad2)"))
    (pad 2 smd rect (at -2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 150 "Net-(R57-Pad1)"))
    (pad 3 smd rect (at -1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 126 "Net-(Q56-Pad3)"))
    (pad 4 smd rect (at 0 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (pad 5 smd rect (at 1.27 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 129 "Net-(Q58-Pad3)"))
    (pad 6 smd rect (at 2.54 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 151 "Net-(R58-Pad1)"))
    (pad 7 smd rect (at 3.81 3.302 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 128 "Net-(Q57-Pad2)"))
    (pad 8 smd rect (at 3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(Q63-Pad2)"))
    (pad 9 smd rect (at 2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 152 "Net-(R63-Pad1)"))
    (pad 11 smd rect (at 0 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(Q66-Pad3)"))
    (pad 13 smd rect (at -2.54 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(R64-Pad1)"))
    (pad 14 smd rect (at -3.81 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(Q65-Pad2)"))
    (pad 10 smd rect (at 1.27 -3.048 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(Q64-Pad3)"))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 98.298 71.882)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 77 "Net-(Q5-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 106.426 71.882)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP2 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 80 "Net-(Q7-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 114.554 71.882)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP3 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 85 "Net-(Q11-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 123.19 71.882)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP4 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 88 "Net-(Q13-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 94.107 110.871)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP5 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 101 "Net-(Q23-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 102.489 110.617)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP6 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 104 "Net-(Q25-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 110.617 110.744)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP7 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 111 "Net-(Q31-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 118.618 110.871)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP8 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 114 "Net-(Q33-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 183.388 72.39)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP9 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 93 "Net-(Q17-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 190.5 72.39)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP10 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 98 "Net-(Q21-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 199.136 72.39)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP11 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 118 "Net-(Q36-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 208.28 72.39)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP12 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 121 "Net-(Q38-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 175.26 110.998)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP13 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 126 "Net-(Q56-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 183.388 110.998)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP14 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 129 "Net-(Q58-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 191.516 110.998)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP15 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 134 "Net-(Q64-Pad3)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 199.136 110.998)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP16 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 137 "Net-(Q66-Pad3)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 79.248 87.63 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 156 /+12V-A))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 195.072 95.25)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 157 /+12V-B))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 79.248 91.694 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V-A))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58307B90)
    (at 195.072 92.329)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V-B))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 69.215 88.265 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P11 (at 1.143 -2.413 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 156 /+12V-A))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 228.346 91.567 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P12 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 157 /+12V-B))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 83.82 84.074)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P13 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 +5V-A))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 54E9F75E)
    (at 187.452 88.138)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P14 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 +5V-B))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 589928CA)
    (at 128.27 73.787)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Custom_Footprints:VIA-0.6mm (layer F.Cu) (tedit 58992966)
    (at 137.922 105.41)
    (fp_text reference REF** (at 0 1.5) (layer F.SilkS) hide)
    (fp_text value VIA-0.6mm (at 0 -1.1) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
      (net 1 +12V) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 237.49 58.42)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text 12V (at 220.98 93.98) (layer F.SilkS))
  (gr_text GND (at 220.98 91.44) (layer F.SilkS))
  (gr_text "Rev A" (at 237.49 117.475) (layer F.SilkS))
  (gr_text "David Lenfesty" (at 243.205 61.595 90) (layer F.SilkS))
  (gr_text "16 Channel PWM LED Driver" (at 209.55 128.27 360) (layer F.SilkS))
  (gr_text 12V (at 167.64 118.11 90) (layer F.SilkS))
  (gr_text 12V (at 162.56 118.11 90) (layer F.SilkS))
  (gr_text 12V (at 157.48 118.11 90) (layer F.SilkS))
  (gr_text 12V (at 152.4 118.11 90) (layer F.SilkS))
  (gr_text 12V (at 142.875 118.11 90) (layer F.SilkS))
  (gr_text 12V (at 137.795 118.11 90) (layer F.SilkS))
  (gr_text 12V (at 132.715 118.11 90) (layer F.SilkS))
  (gr_text 12V (at 127.635 118.11 90) (layer F.SilkS))
  (gr_text B8 (at 170.18 118.745 90) (layer F.SilkS))
  (gr_text B7 (at 165.1 118.745 90) (layer F.SilkS))
  (gr_text B6 (at 160.02 118.745 90) (layer F.SilkS))
  (gr_text B5 (at 154.94 118.745 90) (layer F.SilkS))
  (gr_text A8 (at 145.415 118.745 90) (layer F.SilkS))
  (gr_text A7 (at 140.335 118.745 90) (layer F.SilkS))
  (gr_text A6 (at 135.255 118.745 90) (layer F.SilkS))
  (gr_text A5 (at 130.175 118.745 90) (layer F.SilkS))
  (gr_text B4 (at 170.18 64.135 90) (layer F.SilkS))
  (gr_text B3 (at 165.1 64.135 90) (layer F.SilkS))
  (gr_text B2 (at 160.02 64.135 90) (layer F.SilkS))
  (gr_text B1 (at 154.94 64.135 90) (layer F.SilkS))
  (gr_text A4 (at 145.415 64.135 90) (layer F.SilkS))
  (gr_text A3 (at 140.335 64.135 90) (layer F.SilkS))
  (gr_text A2 (at 135.255 64.135 90) (layer F.SilkS))
  (gr_text A1 (at 130.175 64.135 90) (layer F.SilkS))
  (gr_text 12V (at 162.56 64.77 90) (layer F.SilkS))
  (gr_text 12V (at 157.48 64.77 90) (layer F.SilkS))
  (gr_text 12V (at 137.795 64.77 90) (layer F.SilkS))
  (gr_text 12V (at 132.715 64.77 90) (layer F.SilkS))
  (gr_text 12V (at 167.64 64.77 90) (layer F.SilkS))
  (gr_text 12V (at 152.4 64.77 90) (layer F.SilkS))
  (gr_text 12V (at 142.875 64.77 90) (layer F.SilkS))
  (gr_text 12V (at 127.635 64.77 90) (layer F.SilkS))
  (gr_line (start 55.245 132.08) (end 55.245 52.07) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 245.745 132.08) (end 55.245 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 245.745 52.07) (end 245.745 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55.245 52.07) (end 245.745 52.07) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 3v3 (at 167.005 71.755) (layer F.SilkS))
  (gr_text SCL (at 134.747 109.855) (layer F.SilkS))
  (gr_text SDA (at 134.62 106.934 360) (layer F.SilkS))
  (gr_text SCL (at 134.747 102.87) (layer F.SilkS))
  (gr_text SDA (at 134.62 99.822 360) (layer F.SilkS))
  (gr_text 12V (at 147.955 76.2) (layer F.SilkS))
  (gr_text GND (at 148.59 106.172) (layer F.SilkS))
  (gr_text OE (at 133.731 82.677) (layer F.SilkS))
  (gr_text GND (at 185.547 85.725) (layer F.SilkS))
  (gr_text 5V (at 193.675 88.646) (layer F.SilkS))
  (gr_text 5V (at 89.662 85.09) (layer F.SilkS))
  (gr_text GND (at 79.629 84.709) (layer F.SilkS))
  (gr_text 12V (at 199.644 95.377) (layer F.SilkS))
  (gr_text GND (at 199.644 92.583) (layer F.SilkS))
  (gr_text 12V (at 74.549 91.44) (layer F.SilkS))
  (gr_text GND (at 74.549 88.265) (layer F.SilkS))
  (zone (net 1) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 140.97 105.41) (xy 140.335 112.395) (xy 140.97 113.665) (xy 142.875 114.3) (xy 146.685 114.3)
        (xy 151.13 117.475) (xy 153.67 121.285) (xy 153.67 125.095) (xy 156.21 125.095) (xy 156.21 122.555)
        (xy 158.75 122.555) (xy 158.75 125.095) (xy 161.29 125.095) (xy 161.29 122.555) (xy 163.195 121.285)
        (xy 165.735 120.65) (xy 167.64 121.285) (xy 168.91 122.555) (xy 168.91 124.46) (xy 168.275 125.73)
        (xy 166.37 125.095) (xy 166.37 123.19) (xy 165.735 122.555) (xy 163.83 122.555) (xy 163.83 125.095)
        (xy 162.56 127) (xy 137.795 127) (xy 136.525 125.095) (xy 136.525 121.92) (xy 133.985 121.92)
        (xy 133.985 125.095) (xy 131.445 125.095) (xy 132.08 121.92) (xy 129.54 121.92) (xy 128.905 123.19)
        (xy 128.905 124.46) (xy 126.365 124.46) (xy 126.365 120.65) (xy 127 120.015) (xy 138.43 120.015)
        (xy 139.065 121.285) (xy 139.065 125.095) (xy 141.605 125.095) (xy 142.24 121.285) (xy 143.51 121.285)
        (xy 144.145 122.555) (xy 144.145 125.095) (xy 147.32 125.095) (xy 147.32 120.65) (xy 144.78 117.475)
        (xy 137.795 115.57) (xy 137.16 110.49) (xy 137.16 104.775) (xy 140.97 104.775)
      )
    )
  )
  (zone (net 1) (net_name +12V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 168.91 59.69) (xy 166.37 59.69) (xy 166.37 57.785) (xy 163.83 57.785) (xy 163.83 60.96)
        (xy 161.29 60.96) (xy 161.29 57.785) (xy 158.75 57.785) (xy 158.75 60.96) (xy 156.21 60.96)
        (xy 156.21 57.785) (xy 153.67 57.785) (xy 153.67 67.31) (xy 156.845 67.31) (xy 156.845 85.09)
        (xy 144.62125 85.09) (xy 143.51 93.98) (xy 143.51 97.155) (xy 140.97 99.06) (xy 140.97 107.95)
        (xy 136.525 107.95) (xy 137.16 97.79) (xy 139.065 94.615) (xy 139.7 85.725) (xy 139.911667 85.09)
        (xy 139.7 85.09) (xy 139.7 67.31) (xy 142.24 67.31) (xy 142.24 57.785) (xy 139.065 57.785)
        (xy 139.065 60.325) (xy 137.16 60.325) (xy 137.16 57.785) (xy 133.985 57.785) (xy 133.985 60.325)
        (xy 131.445 60.325) (xy 131.445 57.785) (xy 128.27 57.785) (xy 128.27 60.325) (xy 126.365 60.325)
        (xy 126.365 56.515) (xy 144.145 56.515) (xy 144.145 62.23) (xy 151.13 62.23) (xy 151.13 55.88)
        (xy 168.91 55.88)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 90.805 73.66) (xy 125.476 73.66) (xy 125.476 71.501) (xy 131.699 71.501) (xy 131.826 75.311)
        (xy 130.683 77.343) (xy 126.365 77.66685) (xy 126.365 86.995) (xy 128.905 86.995) (xy 128.905 82.55)
        (xy 137.795 82.55) (xy 138.43 92.075) (xy 135.255 100.965) (xy 135.255 109.22) (xy 142.24 109.22)
        (xy 142.24 99.06) (xy 145.415 99.06) (xy 145.415 97.79) (xy 144.78 97.79) (xy 144.78 91.44)
        (xy 146.05 86.995) (xy 158.115 86.995) (xy 158.115 71.12) (xy 163.195 71.12) (xy 163.195 80.645)
        (xy 177.165 80.645) (xy 177.165 78.105) (xy 205.74 78.105) (xy 205.74 86.36) (xy 198.755 86.204778)
        (xy 198.755 86.995) (xy 199.39 86.995) (xy 199.39 90.805) (xy 209.55 90.805) (xy 209.55 76.835)
        (xy 172.085 76.835) (xy 172.085 74.295) (xy 209.55 74.295) (xy 209.55 61.595) (xy 227.965 61.595)
        (xy 228.095735 66.04) (xy 230.759 66.04) (xy 233.807 76.962) (xy 233.807 89.662) (xy 231.775 89.662)
        (xy 231.775 96.52) (xy 225.425 96.52) (xy 225.425 93.98) (xy 212.09 93.98) (xy 212.09 102.87)
        (xy 227.965 102.87) (xy 228.6 125.095) (xy 205.105 125.095) (xy 205.105 113.03) (xy 209.55 109.22)
        (xy 209.55 104.14) (xy 207.01 104.14) (xy 207.01 109.22) (xy 173.355 109.22) (xy 173.355 106.68)
        (xy 204.47 106.68) (xy 204.47 102.235) (xy 209.55 102.235) (xy 209.55 93.98) (xy 199.39 93.98)
        (xy 199.39 98.425) (xy 205.74 98.425) (xy 205.74 101.6) (xy 203.2 101.6) (xy 203.2 104.775)
        (xy 155.575 104.775) (xy 155.575 113.665) (xy 144.145 113.665) (xy 143.51 114.935) (xy 136.525 114.935)
        (xy 131.445 115.57) (xy 128.27 114.935) (xy 126.365 114.3) (xy 125.095 112.395) (xy 124.46 111.125)
        (xy 124.46 109.22) (xy 123.825 109.22) (xy 123.825 108.585) (xy 121.285 108.712) (xy 107.188 108.839)
        (xy 90.805 109.22) (xy 90.805 120.65) (xy 70.485 120.65) (xy 70.485 113.422545) (xy 67.818 110.998)
        (xy 67.818 104.394) (xy 70.485 104.291423) (xy 70.485 93.98) (xy 67.31 93.98) (xy 67.31 85.09)
        (xy 70.485 85.09) (xy 70.485 58.42) (xy 90.805 58.42)
      )
    )
    (polygon
      (pts        (xy 68.58 105.918) (xy 68.58 109.982) (xy 70.485 112.447294) (xy 70.485 105.82275)
      )
    )
    (polygon
      (pts        (xy 126.365 97.155) (xy 126.365 111.76) (xy 130.81 111.76) (xy 130.81 97.155)
      )
    )
    (polygon
      (pts        (xy 228.129353 67.183) (xy 228.6 83.185) (xy 212.09 83.185) (xy 212.09 90.805) (xy 225.425 90.805)
        (xy 225.425 88.9) (xy 230.81615 88.9) (xy 231.521 79.502) (xy 231.267 75.692) (xy 229.235 67.183)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 134.493 73.406) (xy 153.543 73.787) (xy 163.195 73.279) (xy 162.941 78.613) (xy 155.702 78.486)
        (xy 139.827 78.74) (xy 137.795 76.581) (xy 135.122267 76.212347) (xy 129.926477 76.695677) (xy 129.921 76.708)
        (xy 125.222 76.708) (xy 125.476 72.898)
      )
    )
  )
)
