(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 52)
    (no_connects 0)
    (area 146.540929 89.898928 166.145772 105.85)
    (thickness 1.6)
    (drawings 18)
    (tracks 232)
    (zones 0)
    (modules 31)
    (nets 22)
  )
  (page A4)
  (title_block
    (title pam8404)
    (date 2016-12-02)
    (rev 0.01)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.127)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory OUT/gerbers/))
  )
  (net 0 "")
  (net 1 INL+)
  (net 2 "Net-(C1-Pad2)")
  (net 3 INL-)
  (net 4 "Net-(C2-Pad2)")
  (net 5 INR+)
  (net 6 "Net-(C3-Pad2)")
  (net 7 INR-)
  (net 8 "Net-(C4-Pad2)")
  (net 9 VDD)
  (net 10 GND)
  (net 11 G1)
  (net 12 G0)
  (net 13 OUTL+)
  (net 14 OUTL-)
  (net 15 OUTR+)
  (net 16 OUTR-)
  (net 17 "Net-(C10-Pad1)")
  (net 18 "Net-(C11-Pad1)")
  (net 19 "Net-(C12-Pad1)")
  (net 20 "Net-(C13-Pad1)")
  (net 21 ~SDL)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net G0)
    (add_net G1)
    (add_net INL+)
    (add_net INL-)
    (add_net INR+)
    (add_net INR-)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net OUTL+)
    (add_net OUTL-)
    (add_net OUTR+)
    (add_net OUTR-)
    (add_net ~SDL)
  )
  (net_class PWR ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VDD)
  )
  (module w_smd_qfn:qfn-20 (layer F.Cu) (tedit 58415CD7)
    (at 155.3845 97.0915)
    (descr "Plastic QFP, Microchip QFN-20")
    (fp_text reference U1 (at 1.73482 -2.51714) (layer F.SilkS))
    (fp_text value PAM8404 (at 0 3.0988) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.00076 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 11 G1) (solder_mask_margin 0.07112))
    (pad 2 smd rect (at -0.50038 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 13 OUTL+) (solder_mask_margin 0.07112))
    (pad 3 smd rect (at 0 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD) (solder_mask_margin 0.07112))
    (pad 4 smd rect (at 0.50038 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 10 GND) (solder_mask_margin 0.07112))
    (pad 6 smd rect (at 1.96596 1.00076) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07112))
    (pad 7 smd rect (at 1.96596 0.50038) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 21 ~SDL) (solder_mask_margin 0.07112))
    (pad 8 smd rect (at 1.96596 0) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 21 ~SDL) (solder_mask_margin 0.07112))
    (pad 9 smd rect (at 1.96596 -0.50038) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD) (solder_mask_margin 0.07112))
    (pad 10 smd rect (at 1.96596 -1.00076) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.07112))
    (pad 21 thru_hole rect (at 0.62484 0.62484) (size 1.24968 1.24968) (drill 0.3) (layers *.Cu F.Mask)
      (net 10 GND) (solder_mask_margin 0.07112) (solder_paste_margin -0.09906))
    (pad 21 thru_hole rect (at -0.62484 0.62484) (size 1.24968 1.24968) (drill 0.3) (layers *.Cu F.Mask)
      (net 10 GND) (solder_mask_margin 0.07112) (solder_paste_margin -0.09906))
    (pad 21 thru_hole rect (at -0.62484 -0.62484) (size 1.24968 1.24968) (drill 0.3) (layers *.Cu F.Mask)
      (net 10 GND) (solder_mask_margin 0.07112) (solder_paste_margin -0.09906))
    (pad 21 thru_hole rect (at 0.62484 -0.62484) (size 1.24968 1.24968) (drill 0.3) (layers *.Cu F.Mask)
      (net 10 GND) (solder_mask_margin 0.07112) (solder_paste_margin -0.09906))
    (pad 11 smd rect (at 1.00076 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 16 OUTR-) (solder_mask_margin 0.07112))
    (pad 12 smd rect (at 0.50038 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 10 GND) (solder_mask_margin 0.07112))
    (pad 13 smd rect (at 0 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD) (solder_mask_margin 0.07112))
    (pad 14 smd rect (at -0.50038 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 15 OUTR+) (solder_mask_margin 0.07112))
    (pad 15 smd rect (at -1.00076 -1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 12 G0) (solder_mask_margin 0.07112))
    (pad 16 smd rect (at -1.96596 -1.00076) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 5 INR+) (solder_mask_margin 0.07112))
    (pad 17 smd rect (at -1.96596 -0.50038) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 7 INR-) (solder_mask_margin 0.07112))
    (pad 18 smd rect (at -1.96596 0) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 10 GND) (solder_mask_margin 0.07112))
    (pad 19 smd rect (at -1.96596 0.50038) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 3 INL-) (solder_mask_margin 0.07112))
    (pad 20 smd rect (at -1.96596 1.00076) (size 0.72898 0.29972) (layers F.Cu F.Paste F.Mask)
      (net 1 INL+) (solder_mask_margin 0.07112))
    (pad 5 smd rect (at 1.00076 1.96596) (size 0.29972 0.72898) (layers F.Cu F.Paste F.Mask)
      (net 14 OUTL-) (solder_mask_margin 0.07112))
    (model walter/smd_qfn/qfn-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_2x1_1.27mm_pitch (layer F.Cu) (tedit 58412748)
    (at 149.6695 93.0275 270)
    (fp_text reference P1 (at -0.2185 1.64386 270) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0 1.905 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -0.635 0 270) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 10 GND))
    (pad 2 thru_hole circle (at 0.635 0 270) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 9 VDD))
  )
  (module w_smd_inductors:inductor_smd_0402 (layer F.Cu) (tedit 584129E5)
    (at 159.639 100.076)
    (descr "Inductor SMD, 0402")
    (fp_text reference L1 (at -1.27 0 90) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.47752 0) (size 0.4953 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 13 OUTL+))
    (pad 2 smd rect (at 0.47752 0) (size 0.4953 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C10-Pad1)"))
    (model walter/smd_inductors/inductor_smd_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0402 (layer F.Cu) (tedit 584129E0)
    (at 159.639 98.933)
    (descr "Inductor SMD, 0402")
    (fp_text reference L2 (at -1.27 0 90) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.47752 0) (size 0.4953 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 14 OUTL-))
    (pad 2 smd rect (at 0.47752 0) (size 0.4953 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C12-Pad1)"))
    (model walter/smd_inductors/inductor_smd_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0402 (layer F.Cu) (tedit 584129D9)
    (at 159.639 92.964)
    (descr "Inductor SMD, 0402")
    (fp_text reference L3 (at -1.27 0 90) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.47752 0) (size 0.4953 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 15 OUTR+))
    (pad 2 smd rect (at 0.47752 0) (size 0.4953 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C11-Pad1)"))
    (model walter/smd_inductors/inductor_smd_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_inductors:inductor_smd_0402 (layer F.Cu) (tedit 58412AFC)
    (at 159.639 94.107)
    (descr "Inductor SMD, 0402")
    (fp_text reference L4 (at -1.27 0 90) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.47752 0) (size 0.4953 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 16 OUTR-))
    (pad 2 smd rect (at 0.47752 0) (size 0.4953 0.65786) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C13-Pad1)"))
    (model walter/smd_inductors/inductor_smd_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 5841298C)
    (at 149.6695 100.965)
    (fp_text reference EN1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 21 ~SDL))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 5841272E)
    (at 149.6695 99.441)
    (fp_text reference PINL+1 (at 0.382 -1.166) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 5841273E)
    (at 149.6695 98.171)
    (fp_text reference PINL-1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C3-Pad2)"))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 58412721)
    (at 149.6695 96.774)
    (fp_text reference PINR-1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C4-Pad2)"))
  )
  (module mylib:jumper_0402 (layer F.Cu) (tedit 58415CE3)
    (at 152.4 94.6912)
    (descr "SMT resistor, 0402")
    (fp_text reference R1 (at 1.41732 -0.0508 90) (layer F.SilkS))
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.4445 0) (size 0.7 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 12 G0))
    (pad 2 smd rect (at -0.4445 0) (size 0.7 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:jumper_0402 (layer F.Cu) (tedit 58414BD9)
    (at 152.7302 101.0666)
    (descr "SMT resistor, 0402")
    (fp_text reference R2 (at 1.4605 -0.0127 90) (layer F.SilkS))
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.4445 0) (size 0.7 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 G1))
    (pad 2 smd rect (at -0.4445 0) (size 0.7 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:jumper_0402 (layer F.Cu) (tedit 58415CDA)
    (at 152.4 93.5736)
    (descr "SMT resistor, 0402")
    (fp_text reference R3 (at 1.41732 -0.02032 90) (layer F.SilkS))
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.4445 0) (size 0.7 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 12 G0))
    (pad 2 smd rect (at -0.4445 0) (size 0.7 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:jumper_0402 (layer F.Cu) (tedit 58414BD6)
    (at 152.7302 99.9617)
    (descr "SMT resistor, 0402")
    (fp_text reference R4 (at 1.4605 0 90) (layer F.SilkS))
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.4445 0) (size 0.7 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 11 G1))
    (pad 2 smd rect (at -0.4445 0) (size 0.7 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 584145F8)
    (at 149.6695 95.504)
    (fp_text reference PINR+1 (at 0 3.81) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58415DBE)
    (at 151.6634 98.8187)
    (descr "SMT capacitor, 0402")
    (fp_text reference C1 (at -0.4064 1.7272 90) (layer F.SilkS))
    (fp_text value 220n (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 INL+))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58415E1D)
    (at 151.6634 95.8596)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at -0.6223 -1.7018 90) (layer F.SilkS))
    (fp_text value 220n (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 INR+))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58415DBC)
    (at 151.6634 97.8916)
    (descr "SMT capacitor, 0402")
    (fp_text reference C3 (at -1.0414 2.0828 90) (layer F.SilkS))
    (fp_text value 220n (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 INL-))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58415E26)
    (at 151.6634 96.774)
    (descr "SMT capacitor, 0402")
    (fp_text reference C4 (at -1.1557 -1.8669 90) (layer F.SilkS))
    (fp_text value 220n (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 7 INR-))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C4-Pad2)"))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 58415E68)
    (at 152.2984 92.3036)
    (descr "SMT capacitor, 0603")
    (fp_text reference C6 (at -1.7272 -0.127 90) (layer F.SilkS))
    (fp_text value 1u (at 0 0.635) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 5841614E)
    (at 160.2232 96.7994 270)
    (descr "SMT capacitor, 0603")
    (fp_text reference C7 (at -1.778 -0.3048 360) (layer F.SilkS))
    (fp_text value 10u (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 58415CD5)
    (at 158.75 96.139 270)
    (descr "SMT capacitor, 0603")
    (fp_text reference C8 (at 1.74752 -0.26416 360) (layer F.SilkS))
    (fp_text value 1u (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0603_mod0 (layer F.Cu) (tedit 581B5904)
    (at 155.194 92.3036 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C9 (at -0.4445 -1.143 180) (layer F.SilkS))
    (fp_text value 10u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 5841603F)
    (at 161.798 100.53828 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C10 (at -0.4826 -0.8128 270) (layer F.SilkS))
    (fp_text value 220p (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58416047)
    (at 161.798 92.2274 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C11 (at -0.3302 0.8636 450) (layer F.SilkS))
    (fp_text value 220p (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58427129)
    (at 161.798 98.23704 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C12 (at -1.45796 0.34544 540) (layer F.SilkS))
    (fp_text value 220p (at 0 0.635 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:c_0402_mod0 (layer F.Cu) (tedit 58427125)
    (at 161.798 94.54388 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference C13 (at -1.4986 -0.10668 180) (layer F.SilkS))
    (fp_text value 220p (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at -0.54864 0 90) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 58426DD8)
    (at 163.0172 100.584)
    (fp_text reference P2 (at 0.127 -1.016) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C10-Pad1)"))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 58426DD4)
    (at 163.0172 98.044)
    (fp_text reference P3 (at 0.4572 -1.016) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C12-Pad1)"))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 58426DD6)
    (at 163.0172 92.1004)
    (fp_text reference P4 (at 0.0762 1.0668) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(C11-Pad1)"))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 58426DD1)
    (at 163.0172 94.6404)
    (fp_text reference P5 (at 0.4318 1.0668) (layer F.SilkS))
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C13-Pad1)"))
  )
  (gr_text EN (at 148.6916 101.0158 90) (layer F.SilkS))
  (gr_text - (at 148.6916 92.329 90) (layer F.SilkS))
  (gr_text + (at 148.6916 93.6752 90) (layer F.SilkS))
  (gr_text R (at 148.6916 96.1136 90) (layer F.SilkS))
  (gr_text L (at 148.6916 98.7298 90) (layer F.SilkS))
  (gr_text L (at 163.81476 99.01428 90) (layer F.SilkS))
  (gr_text R (at 163.79952 93.63456 90) (layer F.SilkS))
  (gr_line (start 148.209 102.362) (end 148.209 90.932) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.4015 102.362) (end 148.209 102.362) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.4015 90.932) (end 164.4015 102.362) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.209 90.932) (end 164.4015 90.932) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "pamamp8404\nrev0.01\nrel/2016-12" (at 159.7406 93.0402 90) (layer B.SilkS))
  (zone (net 10) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.4015 102.362) (xy 148.209 102.362) (xy 148.209 90.932) (xy 164.4015 90.932)
      )
    )
  )
  (zone (net 10) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.4015 102.362) (xy 148.209 102.362) (xy 148.209 90.932) (xy 164.4015 90.932)
      )
    )
  )
)
