<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="33.55195625" y1="50.8" x2="2.289525" y2="50.8" width="0" layer="20"/>
<wire x1="2.289525" y1="50.8" x2="0" y2="48.510475" width="0" layer="20" curve="90"/>
<wire x1="33.55195625" y1="0" x2="2.00804375" y2="0" width="0" layer="20"/>
<wire x1="2.00804375" y1="0" x2="0" y2="2.00804375" width="0" layer="20" curve="-90"/>
<wire x1="0" y1="2.00804375" x2="0" y2="48.510475" width="0" layer="20"/>
<wire x1="33.55195625" y1="50.8" x2="35.56" y2="48.79195625" width="0" layer="20" curve="-90"/>
<wire x1="35.56" y1="48.79195625" x2="35.56" y2="2.00804375" width="0" layer="20"/>
<wire x1="35.56" y1="2.00804375" x2="33.55195625" y2="0" width="0" layer="20" curve="-90"/>
<hole x="2.54" y="2.54" drill="3"/>
<hole x="2.54" y="48.26" drill="3"/>
<hole x="33.02" y="2.54" drill="3"/>
<hole x="33.02" y="48.26" drill="3"/>
<text>LED</text>
<text>+</text>
<text>-</text>
<text>POT</text>
<text>+</text>
<text>-</text>
<text>S</text>
<text>~</text>
<text>~</text>
<text>adnbr.co.uk</text>
</plain>
<libraries>
<library name="tidyeagle">
<description>&lt;h4&gt;A neat and tidy Eagle Library.&lt;/h4&gt;

&lt;p&gt;This is my personal Eagle library where I add parts that I need as and when I need them with the aim of keeping the look and feel consistent across the schematic and the board.&lt;/p&gt;

&lt;p&gt;&lt;a href="https://github.com/adnbr/TidyEagle"&gt;Pick up the latest version at GitHub.&lt;/a&gt;&lt;/p&gt;

&lt;p&gt;This library draws inspiration from the libraries included with Eagle, as well as those from companies such as &lt;a href="http://www.opencircuits.com/SFE_Footprint_Library_Eagle"&gt;SparkFun&lt;/a&gt; and &lt;a href="https://github.com/adafruit/Adafruit-Eagle-Library"&gt;Adafruit&lt;/a&gt;. Check out their libraries, they contain an eclectic mix of, well almost anything you could need.&lt;/p&gt;

&lt;p&gt;Take care to look in the description under the details for each part as to whether the package has been tested. This is very important, as I don't take any responsibility for any errors in production this library causes!&lt;/p&gt;</description>
<packages>
<package name="TO220-HORZ-DRILL">
</package>
<package name="RESISTOR-4MMX10MM/9">
<description>0.5 Watt</description>
</package>
<package name="CAPACITOR-5MM-GRID">
</package>
<package name="TO92-TRIANGLE">
</package>
<package name="J02-LONG">
</package>
<package name="DIL08-3">
</package>
<package name="J03-NOSILK">
</package>
<package name="J03-LONG">
</package>
<package name="CAPACITOR-RADIAL-5MM">
<description>&lt;strong&gt;Tested&lt;/strong&gt;</description>
</package>
<package name="DIL04-3-BRIDGE-RECTIFIER">
<description>DB101G</description>
</package>
<package name="CAPACITOR-RADIAL-10MM">
<description>Untested.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="tidyeagle" package="TO220-HORZ-DRILL" value="LM317">
<attribute name="NAME"/>
</element>
<element name="R1" library="tidyeagle" package="RESISTOR-4MMX10MM/9" value="3R3">
<attribute name="NAME"/>
</element>
<element name="C1" library="tidyeagle" package="CAPACITOR-5MM-GRID" value="10nF">
<attribute name="NAME"/>
</element>
<element name="T1" library="tidyeagle" package="TO92-TRIANGLE" value="2N7000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="tidyeagle" package="J02-LONG" value="LED">
<attribute name="NAME"/>
</element>
<element name="IC1" library="tidyeagle" package="DIL08-3" value="AVR-ATTINY13-DIP8">
<attribute name="NAME"/>
</element>
<element name="C2" library="tidyeagle" package="CAPACITOR-5MM-GRID" value="10nF">
<attribute name="NAME"/>
</element>
<element name="J2" library="tidyeagle" package="J03-LONG" value="POT">
<attribute name="NAME"/>
</element>
<element name="IC3" library="tidyeagle" package="TO220-HORZ-DRILL" value="7805">
<attribute name="NAME"/>
</element>
<element name="C3" library="tidyeagle" package="CAPACITOR-RADIAL-5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="tidyeagle" package="CAPACITOR-RADIAL-5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="tidyeagle" package="CAPACITOR-5MM-GRID" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="tidyeagle" package="DIL04-3-BRIDGE-RECTIFIER" value="DB101G">
<attribute name="NAME"/>
</element>
<element name="J3" library="tidyeagle" package="J02-LONG" value="SINE"/>
<element name="C6" library="tidyeagle" package="CAPACITOR-RADIAL-5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="tidyeagle" package="CAPACITOR-RADIAL-10MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="tidyeagle" package="J03-NOSILK" value="SPARES">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="+5V">
<contactref element="IC2" pad="3"/>
<contactref element="C1" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="C2" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="C4" pad="A"/>
<contactref element="C5" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="IC2" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="C4" pad="C"/>
<contactref element="C5" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="C3" pad="C"/>
<contactref element="D1" pad="-"/>
<contactref element="C6" pad="C"/>
<contactref element="C7" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="T1" pad="3"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="PWM">
<contactref element="T1" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="7"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IC3" pad="1"/>
<contactref element="C3" pad="A"/>
<contactref element="C6" pad="A"/>
<contactref element="D1" pad="+"/>
<contactref element="C7" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="D1" pad="SINE0"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="J3" pad="1"/>
<contactref element="D1" pad="SINE1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="3"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="5"/>
<contactref element="J4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
