(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 23)
    (no_connects 0)
    (area 121.57158 55.855799 173.82012 124.612401)
    (thickness 1.6)
    (drawings 28)
    (tracks 114)
    (zones 0)
    (modules 12)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2286)
    (trace_clearance 0.2286)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2286)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7874)
    (via_drill 0.5334)
    (via_min_size 0.762)
    (via_min_drill 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad0)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad6)")
  (net 6 "Net-(J1-Pad7)")
  (net 7 "Net-(J1-Pad8)")
  (net 8 "Net-(J1-PadPGM)")
  (net 9 "Net-(J1-PadDAC)")
  (net 10 "Net-(J1-Pad16)")
  (net 11 "Net-(J1-Pad22)")
  (net 12 "Net-(J1-PadVIN)")
  (net 13 "Net-(J1-Pad21)")
  (net 14 "Net-(J1-Pad20)")
  (net 15 "Net-(J1-Pad23)")
  (net 16 "Net-(J1-Pad14)")
  (net 17 /CS)
  (net 18 /RST)
  (net 19 /GND)
  (net 20 "Net-(J1-Pad9)")
  (net 21 "Net-(J1-Pad10)")
  (net 22 "Net-(J1-Pad11)")
  (net 23 "Net-(J1-Pad12)")
  (net 24 "Net-(J1-Pad13)")
  (net 25 /SDA)
  (net 26 /3.3V)
  (net 27 /VIN)
  (net 28 /SCK)
  (net 29 /3V0)
  (net 30 /SDO)
  (net 31 "Net-(GPIO0-Pad1)")
  (net 32 "Net-(GPIO2-Pad1)")
  (net 33 "Net-(J1-Pad4)")
  (net 34 "Net-(R1-Pad2)")
  (net 35 "Net-(RST1-Pad1)")
  (net 36 "Net-(CAP1-Pad1)")
  (net 37 "Net-(J1-Pad17)")
  (net_class Default "This is the default net class."
    (clearance 0.2286)
    (trace_width 0.2286)
    (via_dia 0.7874)
    (via_drill 0.5334)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3V)
    (add_net /3V0)
    (add_net /CS)
    (add_net /GND)
    (add_net /RST)
    (add_net /SCK)
    (add_net /SDA)
    (add_net /SDO)
    (add_net /VIN)
    (add_net "Net-(CAP1-Pad1)")
    (add_net "Net-(GPIO0-Pad1)")
    (add_net "Net-(GPIO2-Pad1)")
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(RST1-Pad1)")
  )
  (module Wickerlib:TEENSY-LC (layer F.Cu) (tedit 57999D63)
    (at 153.136601 71.094601)
    (fp_text reference J1 (at -10.16 25.4 180) (layer F.SilkS))
    (fp_text value TEENSY3.2-72MHz (at -5.410201 -0.635001 90) (layer B.SilkS))
    (fp_text user TEENSY (at -2.209801 8.712199) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /GND))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /RST))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad12)"))
    (pad 17A thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /GND))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J1-Pad13)"))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad16)"))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SDA))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(J1-Pad17)"))
    (pad G3 thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /SCK))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(CAP1-Pad1)"))
  )
  (module Wickerlib:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 0)
    (at 168.656 68.834)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 -5.1) (layer F.SilkS))
    (fp_text value OLED-I2C (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /SCK))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /RST))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /3.3V))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x07 (layer F.Cu) (tedit 0)
    (at 132.08 82.804 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value ADAFRUIT_BME280 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /3V0))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /SCK))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /SDO))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SDA))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /CS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 57999FF9)
    (at 129.286 93.0148 270)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 -4.38912 270) (layer F.Fab) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082 270) (layer F.Fab) hide)
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57999DF5)
    (at 168.5036 85.852 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference 3V3 (at 0.0508 2.5908 270) (layer F.SilkS))
    (fp_text value 3V3 (at 0.1016 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57999E23)
    (at 133.6548 61.2648)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference GND1 (at 0 2.1336 180) (layer F.SilkS))
    (fp_text value GND (at -2.54 0.254 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57999F8E)
    (at 137.0584 105.0544 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference GPIO0 (at -2.2352 -0.127 360) (layer F.SilkS))
    (fp_text value GPIO0 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(GPIO0-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57999F92)
    (at 132.8928 105.0036 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference GPIO2 (at -2.3114 0.1524 360) (layer F.SilkS))
    (fp_text value GPIO2 (at 0.0508 2.3368 450) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(GPIO2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 169.3164 91.948 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at 4.05892 -3.50012 270) (layer F.SilkS))
    (fp_text value R (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 /VIN))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 "Net-(R1-Pad2)"))
  )
  (module Wickerlib:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 57999F9E)
    (at 137.1092 100.2792 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference RST1 (at -2.3876 0.0254 360) (layer F.SilkS))
    (fp_text value RST (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(RST1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module ESP8266:ESP-01 (layer F.Cu) (tedit 553C10FF)
    (at 156.3624 101.4476 270)
    (descr "Module, ESP-8266, ESP-01, 8 pin")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U1 (at 0.254 -4.572 270) (layer F.SilkS))
    (fp_text value ESP-01v090 (at 12.192 3.556 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-Pad9)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /GND))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(R1-Pad2)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(GPIO2-Pad1)"))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(RST1-Pad1)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(GPIO0-Pad1)"))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /VIN))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-Pad10)"))
  )
  (module Wickerlib:CAPSENSE_CIRCLE_D10 (layer F.Cu) (tedit 56C12BC6)
    (at 129.286 93.1672)
    (fp_text reference CAP1 (at -0.025 -7.05) (layer F.SilkS))
    (fp_text value CAPSENSE_CIRCLE (at 0.025 7.325) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 10.16 10.16) (layers F.Cu)
      (net 36 "Net-(CAP1-Pad1)") (clearance 0.508))
  )
  (gr_text "commit: bf1d95b" (at 164.1856 90.297 270) (layer B.SilkS))
  (gr_text https://github.com/pdp7/teensy-weather-badge (at 161.4424 79.0448 270) (layer B.SilkS))
  (gr_text 2016-08-05 (at 152.2476 106.2736 180) (layer B.SilkS))
  (gr_circle (center 127 59.6392) (end 128.4224 60.706) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 127.7112 102.0064) (end 129.1336 103.0732) (layer Edge.Cuts) (width 0.15))
  (gr_text "drew@oshpark.com\n" (at 163.2712 75.9968 270) (layer F.SilkS))
  (gr_line (start 173.5836 59.9948) (end 173.5836 62.738) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 169.5196 55.9308) (end 173.5836 59.9948) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.7792 55.9308) (end 169.5196 55.9308) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.1364 55.9308) (end 163.7792 55.9308) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.73 56.3372) (end 126.1364 55.9308) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.968 57.0992) (end 125.73 56.3372) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.682 59.3852) (end 124.968 57.0992) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 165.608 59.2836) (end 167.0304 60.3504) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 165.0492 103.9368) (end 166.4716 105.0036) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.682 101.7524) (end 122.682 59.3344) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.524 107.5944) (end 122.682 101.7524) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.0144 107.5944) (end 128.524 107.5944) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.6344 99.9744) (end 166.0144 107.5944) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.6344 61.976) (end 173.6344 99.9744) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "drew@oshpark.com\n" (at 126.492 77.724 90) (layer B.SilkS))
  (gr_text "DREW FUSTINI\n" (at 137.3632 74.93 270) (layer F.SilkS))
  (gr_text "DREW FUSTINI\n" (at 153.924 69.85 270) (layer B.SilkS))
  (gr_text "drew@oshpark.com\n" (at 147.066 57.658 180) (layer F.SilkS))
  (gr_text "drew@oshpark.com\n" (at 146.9136 96.6724) (layer B.SilkS))
  (gr_text "DREW FUSTINI\n" (at 129.54 75.184 90) (layer B.SilkS))
  (gr_text "I2C OLED" (at 171.958 75.5904 90) (layer F.SilkS))
  (gr_text BME280 (at 128.8288 74.8284 270) (layer F.SilkS))
  (zone (net 19) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 127.762 56.5912) (xy 126.1872 56.5404) (xy 123.4948 59.3344) (xy 123.444 85.598) (xy 123.19 89.7128)
        (xy 123.2916 94.9452) (xy 123.444 100.2792) (xy 123.952 101.3968) (xy 126.0856 104.2416) (xy 127.6604 105.5624)
        (xy 129.1336 107.0356) (xy 165.0492 106.934) (xy 166.0144 106.68) (xy 166.6748 106.0196) (xy 172.6692 99.9744)
        (xy 172.6692 61.6204) (xy 169.5196 57.8104) (xy 167.7416 56.642) (xy 166.37 56.388) (xy 128.4732 56.4388)
      )
    )
  )
)
