<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="44.45" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="44.45" x2="1.27" y2="45.72" width="0" layer="20" curve="-90"/>
<wire x1="1.27" y1="45.72" x2="29.21" y2="45.72" width="0" layer="20"/>
<wire x1="29.21" y1="45.72" x2="30.48" y2="44.45" width="0" layer="20" curve="-90"/>
<wire x1="30.48" y1="44.45" x2="30.48" y2="1.27" width="0" layer="20"/>
<wire x1="30.48" y1="1.27" x2="29.21" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="29.21" y1="0" x2="1.27" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0" layer="20" curve="-90"/>
<text>CONDOR CABSIM PCB REV.2
THIS LAYOUT IS FOR DIY USE ONLY
LAYOUTED FOR FREESTOMPBOXES.ORG
BY GRRRUNGE / KNUCKLEHEAD.DK
ORG. CIRCUIT BY RUNOFFGROOVE.COM</text>
<text>G</text>
<text>D</text>
<text>S</text>
<text>KNUCKLEHEAD.DK
RUNOFFGROOVE.COM
CONDOR CABSIM</text>
<text>SOME CAP VALUES ARE DENOTED XX/YY
FOR ROG'S STANDARD VERSION: MOUNT XX
FOR GRRRUNGE'S MODERN MOD: MOUNT YY</text>
</plain>
<libraries>
<library name="integrated-circuits">
<description>Standard stomp box IC's</description>
<packages>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="trans-mosfet">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="TO92-">
</package>
</packages>
</library>
<library name="resistors">
<description>Standard 0703 resistor</description>
<packages>
<package name="0703">
<description>Standard 0703 resistor</description>
</package>
</packages>
</library>
<library name="potentiometers">
<description>16mm PCB mount Potentiometers</description>
<packages>
<package name="16MM-OCTA">
</package>
</packages>
</library>
<library name="caps-electro">
<description>Capacitors, Polar Electrolytic, Radial</description>
<packages>
<package name="050_020">
<description>5mm diameter, 2 mm lead spacing</description>
</package>
</packages>
</library>
<library name="caps-box">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B3">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 3 mm, grid 5.08 mm</description>
</package>
<package name="C2.5-3">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 3 mm, grid 2.54 mm</description>
</package>
<package name="C2.5-2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 2.5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="supply">
<description>Supply Symbols</description>
<packages>
<package name="OCTOGON">
<description>&lt;b&gt;Octogonal Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 1 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41">
<description>DO-41</description>
</package>
</packages>
</library>
<library name="trimmers">
<description>Trimmer Potentiometers</description>
<packages>
<package name="S64W">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
Spectrol</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="integrated-circuits" package="DIL14" value="4OPA"/>
<element name="Q1" library="trans-mosfet" package="TO92-" value="2N5457"/>
<element name="R1" library="resistors" package="0703" value="18K"/>
<element name="R2" library="resistors" package="0703" value="1M"/>
<element name="GAIN" library="potentiometers" package="16MM-OCTA" value="B1K"/>
<element name="VOLUME" library="potentiometers" package="16MM-OCTA" value="A10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="caps-electro" package="050_020" value="22µ"/>
<element name="C1" library="caps-box" package="C5B3" value="47n"/>
<element name="C4" library="caps-box" package="C5B3" value="1n"/>
<element name="R4" library="resistors" package="0703" value="100K"/>
<element name="R5" library="resistors" package="0703" value="100K"/>
<element name="R6" library="resistors" package="0703" value="100K"/>
<element name="C3" library="caps-box" package="C5B3" value="15n"/>
<element name="C5" library="caps-box" package="C5B3" value="47n/22n"/>
<element name="C6" library="caps-box" package="C5B3" value="47n/15n"/>
<element name="R7" library="resistors" package="0703" value="18K"/>
<element name="R8" library="resistors" package="0703" value="100K"/>
<element name="R9" library="resistors" package="0703" value="22K"/>
<element name="R11" library="resistors" package="0703" value="22K"/>
<element name="C7" library="caps-box" package="C5B3" value="3n9/2n2"/>
<element name="C9" library="caps-box" package="C5B3" value="1n"/>
<element name="R13" library="resistors" package="0703" value="22K"/>
<element name="R15" library="resistors" package="0703" value="22K"/>
<element name="C11" library="caps-box" package="C5B3" value="3n9/2n2"/>
<element name="C13" library="caps-box" package="C5B3" value="1n"/>
<element name="IN" library="supply" package="OCTOGON" value="IN"/>
<element name="OUT" library="supply" package="OCTOGON" value="OUT"/>
<element name="C15" library="caps-electro" package="050_020" value="22µ"/>
<element name="D1" library="diodes" package="DO41" value="4001"/>
<element name="9V" library="supply" package="OCTOGON" value="9V"/>
<element name="0V" library="supply" package="OCTOGON" value="0V"/>
<element name="R10" library="resistors" package="0703" value="100R"/>
<element name="C8" library="caps-electro" package="050_020" value="22µ"/>
<element name="R12" library="resistors" package="0703" value="22K"/>
<element name="R14" library="resistors" package="0703" value="22K"/>
<element name="C12" library="caps-electro" package="050_020" value="22µ"/>
<element name="C14" library="caps-box" package="C2.5-3" value="100n"/>
<element name="C10" library="caps-box" package="C2.5-2" value="100n"/>
<element name="TR1" library="trimmers" package="S64W" value="100K"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="Q1" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="TR1" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="2"/>
<contactref element="GAIN" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="GAIN" pad="2"/>
<contactref element="C2" pad="+"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="-"/>
<contactref element="GAIN" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="VOLUME" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="0V" pad="1"/>
<contactref element="C8" pad="-"/>
<contactref element="R14" pad="1"/>
<contactref element="C12" pad="-"/>
<contactref element="C14" pad="2"/>
<contactref element="IC1" pad="11"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VA">
<contactref element="R10" pad="2"/>
<contactref element="C8" pad="+"/>
<contactref element="R12" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="C10" pad="1"/>
<contactref element="TR1" pad="S"/>
<contactref element="TR1" pad="E"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="C4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="VB">
<contactref element="R6" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C12" pad="+"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="7"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C6" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="12"/>
<contactref element="R11" pad="2"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R11" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="C7" pad="1"/>
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="13"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C11" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R15" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="9"/>
<contactref element="C11" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="C15" pad="+"/>
</signal>
<signal name="N$19">
<contactref element="R1" pad="1"/>
<contactref element="IN" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="VOLUME" pad="2"/>
<contactref element="OUT" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="C15" pad="-"/>
<contactref element="VOLUME" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="D1" pad="C"/>
<contactref element="9V" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
