(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 52)
    (no_connects 1)
    (area 142.448724 78.87338 179.907001 92.150002)
    (thickness 1.6)
    (drawings 23)
    (tracks 267)
    (zones 0)
    (modules 15)
    (nets 28)
  )
  (page A4)
  (title_block
    (title rockbreak)
    (date 2016-12-01)
    (rev 0.01)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.45)
    (user_trace_width 0.5)
    (trace_clearance 0.1)
    (zone_clearance 0.3)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.127)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 BACKL_EN)
  (net 3 VCC_3V3)
  (net 4 V_LED+)
  (net 5 V_LED-)
  (net 6 R7)
  (net 7 R6)
  (net 8 R5)
  (net 9 R4)
  (net 10 R3)
  (net 11 G2)
  (net 12 G3)
  (net 13 G4)
  (net 14 G5)
  (net 15 G6)
  (net 16 G7)
  (net 17 B7)
  (net 18 B6)
  (net 19 B5)
  (net 20 B4)
  (net 21 B3)
  (net 22 DE)
  (net 23 VSYNC)
  (net 24 HSYNC)
  (net 25 DISP)
  (net 26 CLOCK)
  (net 27 "Net-(L2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net B3)
    (add_net B4)
    (add_net B5)
    (add_net B6)
    (add_net B7)
    (add_net CLOCK)
    (add_net DE)
    (add_net DISP)
    (add_net G2)
    (add_net G3)
    (add_net G4)
    (add_net G5)
    (add_net G6)
    (add_net G7)
    (add_net HSYNC)
    (add_net "Net-(L2-Pad2)")
    (add_net R3)
    (add_net R4)
    (add_net R5)
    (add_net R6)
    (add_net R7)
    (add_net VSYNC)
    (add_net V_LED+)
    (add_net V_LED-)
  )
  (net_class PWR ""
    (clearance 0.1)
    (trace_width 0.35)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC_3V3)
  )
  (net_class SIG ""
    (clearance 0.1)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BACKL_EN)
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 58417B9E)
    (at 146.00936 89.82456 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R9 (at 1.5 0 540) (layer F.SilkS))
    (fp_text value 2R43 (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 V_LED-))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 57F18C8C)
    (at 151.638 82.423)
    (fp_text reference P6 (at 0 1.2065) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 2 BACKL_EN))
  )
  (module w_smd_cap:c_0603 (layer F.Cu) (tedit 584275FB)
    (at 151.14524 88.48852 180)
    (descr "SMT capacitor, 0603")
    (fp_text reference C8 (at -1.68656 0.02032 450) (layer F.SilkS))
    (fp_text value 1u (at 0 0.635 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC_3V3))
    (pad 2 smd rect (at -0.75184 0 180) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 58427602)
    (at 152.21204 85.50656 270)
    (descr "SMT resistor, 0402")
    (fp_text reference R12 (at -0.01016 -0.79248 270) (layer F.SilkS))
    (fp_text value 10k (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 BACKL_EN))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:pin_header_5x1_1.27mm_pitch (layer F.Cu) (tedit 58411206)
    (at 155.448 82.423 180)
    (fp_text reference P1 (at -0.0635 -1.524 180) (layer F.SilkS) hide)
    (fp_text value CONN_5m (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 6 R7))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 7 R6))
    (pad 3 thru_hole circle (at 0 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 8 R5))
    (pad 4 thru_hole circle (at 1.27 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 9 R4))
    (pad 5 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 10 R3))
  )
  (module mylib:pin_header_6x1_1.27mm_pitch (layer F.Cu) (tedit 58411209)
    (at 162.433 82.423)
    (fp_text reference P2 (at -0.1905 1.651) (layer F.SilkS) hide)
    (fp_text value CONN_6 (at -0.09144 -2.67462) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.175 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 11 G2))
    (pad 2 thru_hole circle (at -1.905 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 12 G3))
    (pad 3 thru_hole circle (at -0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 13 G4))
    (pad 4 thru_hole circle (at 0.635 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 14 G5))
    (pad 5 thru_hole circle (at 1.905 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 15 G6))
    (pad 6 thru_hole circle (at 3.175 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 16 G7))
  )
  (module mylib:pin_header_5x1_1.27mm_pitch (layer F.Cu) (tedit 5841120B)
    (at 169.418 82.423 180)
    (fp_text reference P3 (at -0.0635 -1.8415 180) (layer F.SilkS) hide)
    (fp_text value CONN_5m (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 17 B7))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 18 B6))
    (pad 3 thru_hole circle (at 0 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 19 B5))
    (pad 4 thru_hole circle (at 1.27 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 20 B4))
    (pad 5 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 21 B3))
  )
  (module mylib:pin_header_5x1_1.27mm_pitch (layer F.Cu) (tedit 5841120E)
    (at 175.768 82.423 180)
    (fp_text reference P5 (at -0.635 1.9685 180) (layer F.SilkS) hide)
    (fp_text value CONN_5m (at 0 2.54 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 22 DE))
    (pad 2 thru_hole circle (at -1.27 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 23 VSYNC))
    (pad 3 thru_hole circle (at 0 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 24 HSYNC))
    (pad 4 thru_hole circle (at 1.27 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 25 DISP))
    (pad 5 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 26 CLOCK))
  )
  (module mylib:62684-401100ALF (layer F.Cu) (tedit 58417BC9)
    (at 166.32682 87.70366)
    (fp_text reference P7 (at -0.061 3.175) (layer F.SilkS))
    (fp_text value RK043FN55HS (at 0.9 2.7) (layer F.Fab) hide)
    (fp_text user 40 (at 10.62318 -0.70366) (layer F.SilkS))
    (fp_text user 1 (at -10.42682 -0.70366) (layer F.SilkS))
    (pad "" connect rect (at 11.6 2.7 180) (size 1.6 2.4) (layers F.Cu F.Mask))
    (pad "" connect rect (at 12.8 3.1 180) (size 0.8 1.6) (layers F.Cu F.Mask))
    (pad "" connect rect (at -12.8 3.1) (size 0.8 1.6) (layers F.Cu F.Mask))
    (pad 1 smd rect (at -9.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 V_LED-))
    (pad 8 smd rect (at -6.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 R3))
    (pad 9 smd rect (at -5.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 R4))
    (pad 7 smd rect (at -6.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 R3))
    (pad 6 smd rect (at -7.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 R3))
    (pad 2 smd rect (at -9.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 V_LED+))
    (pad 3 smd rect (at -8.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -7.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 R3))
    (pad 4 smd rect (at -8.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC_3V3))
    (pad 36 smd rect (at 7.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at 8.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 35 smd rect (at 7.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 34 smd rect (at 6.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 DE))
    (pad 38 smd rect (at 8.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 39 smd rect (at 9.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 40 smd rect (at 9.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at 5.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 HSYNC))
    (pad 33 smd rect (at 6.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 VSYNC))
    (pad 31 smd rect (at 5.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 DISP))
    (pad 30 smd rect (at 4.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 CLOCK))
    (pad 26 smd rect (at 2.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 B5))
    (pad 27 smd rect (at 3.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 B6))
    (pad 29 smd rect (at 4.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 28 smd rect (at 3.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 B7))
    (pad 12 smd rect (at -4.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 R7))
    (pad 13 smd rect (at -3.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 G2))
    (pad 11 smd rect (at -4.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 R6))
    (pad 10 smd rect (at -5.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 R5))
    (pad 14 smd rect (at -3.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 G2))
    (pad 15 smd rect (at -2.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 G2))
    (pad 17 smd rect (at -1.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 G4))
    (pad 16 smd rect (at -2.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 G3))
    (pad 24 smd rect (at 1.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 B3))
    (pad 25 smd rect (at 2.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 B4))
    (pad 23 smd rect (at 1.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 B3))
    (pad 22 smd rect (at 0.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 B3))
    (pad 18 smd rect (at -1.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 G5))
    (pad 19 smd rect (at -0.75 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 G6))
    (pad 21 smd rect (at 0.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 B3))
    (pad 20 smd rect (at -0.25 0) (size 0.3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 G7))
    (pad "" connect rect (at -11.6 2.7) (size 1.6 2.4) (layers F.Cu F.Mask))
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 584275EA)
    (at 148.082 83.439)
    (descr "SMT capacitor, 0402")
    (fp_text reference C1 (at -1.56464 0.10668) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC_3V3))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mylib:8Pin_MLF (layer F.Cu) (tedit 584275F2)
    (at 148.5392 88.2396 180)
    (fp_text reference U1 (at 1.524 -0.42164 450) (layer F.SilkS))
    (fp_text value MIC2289-24YML (at -0.2 7.7 180) (layer F.Fab) hide)
    (pad 8 smd rect (at 0.825 -0.75 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 0.825 -0.25 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(L2-Pad2)"))
    (pad 5 smd rect (at 0.825 0.75 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 0.825 0.25 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 V_LED-))
    (pad 3 smd rect (at -0.825 0.25 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 BACKL_EN))
    (pad 4 smd rect (at -0.825 0.75 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.825 -0.25 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC_3V3))
    (pad 1 smd rect (at -0.825 -0.75 180) (size 0.45 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 V_LED+))
    (pad 9 smd rect (at 0 0 180) (size 0.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 584113BB)
    (at 149.098 82.423)
    (fp_text reference P4 (at 0.5715 -1.27) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 3 VCC_3V3))
  )
  (module mylib:pin_header_1x1_1.27mm_pitch (layer F.Cu) (tedit 584113C1)
    (at 146.558 82.423)
    (fp_text reference P8 (at 0.3302 -1.50368) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0 1.905) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.573) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module mylib:l_1210 (layer F.Cu) (tedit 58419D13)
    (at 147.91436 85.5726)
    (descr "SMT resistor, 1210")
    (fp_text reference L2 (at -2.6924 0.9906 270) (layer F.SilkS))
    (fp_text value 10u (at 0 1.7018) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 3 VCC_3V3))
    (pad 2 smd rect (at -1.397 0) (size 1.6002 2.6924) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(L2-Pad2)"))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 5841B2AE)
    (at 148.87956 90.20556)
    (descr "SMT capacitor, 0805")
    (fp_text reference C5 (at 2.159 0.127 90) (layer F.SilkS))
    (fp_text value 270n (at 0 0.9906) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 4 V_LED+))
    (pad 2 smd rect (at -0.9525 0) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text DE (at 178.3 83.25 90) (layer F.SilkS))
  (gr_line (start 144.5895 91.948) (end 144.5895 81.5975) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.832 91.948) (end 144.5895 91.948) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.832 81.5975) (end 179.832 91.948) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.5895 81.5975) (end 179.832 81.5975) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 3 (at 166.85 83.65) (layer F.SilkS))
  (gr_text 3 (at 152.95 83.65) (layer F.SilkS))
  (gr_text 2 (at 159.25 83.65) (layer F.SilkS))
  (gr_text BL (at 152.146 83.693) (layer F.SilkS))
  (gr_text BLUE (at 169.8 83.65) (layer F.SilkS))
  (gr_text GREEN (at 162.95 83.65) (layer F.SilkS))
  (gr_text RED (at 155.7 83.65) (layer F.SilkS))
  (gr_text "CLOCK\n" (at 173.25 83.3 90) (layer F.SilkS))
  (gr_text DISP (at 174.498 83.312 90) (layer F.SilkS))
  (gr_text HSYNC (at 175.8 83.3 90) (layer F.SilkS))
  (gr_text VSYNC (at 177.05 83.3 90) (layer F.SilkS))
  (gr_text "rockbreak\nrev0.01\nrel/2016" (at 179.2986 88.8238) (layer B.SilkS))
  (gr_text GND (at 145.669 81.788 90) (layer F.SilkS))
  (gr_text 3V3 (at 149.987 81.788 90) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.832 91.948) (xy 144.5895 91.948) (xy 144.5895 81.5975) (xy 179.832 81.5975)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.832 91.948) (xy 144.5895 91.948) (xy 144.5895 81.5975) (xy 179.832 81.5975)
      )
    )
  )
)
