(kicad_pcb (version 20171130) (host pcbnew 5.1.4-e60b266~84~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 277)
    (zones 0)
    (modules 42)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 1.2)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 3v3)
  (net 3 GPIO_1)
  (net 4 GPIO_2)
  (net 5 GPIO_3)
  (net 6 GPIO_4)
  (net 7 CAN_H)
  (net 8 CAN_L)
  (net 9 AVCC)
  (net 10 AGND)
  (net 11 SPI_SCK)
  (net 12 SPI_MISO)
  (net 13 SPI_MOSI)
  (net 14 GPIO_5)
  (net 15 GPIO_6)
  (net 16 GPIO_7)
  (net 17 GPIO_8)
  (net 18 "Net-(J13-Pad1)")
  (net 19 "Net-(J13-Pad2)")
  (net 20 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1.2)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3v3)
    (add_net AGND)
    (add_net AVCC)
    (add_net CAN_H)
    (add_net CAN_L)
    (add_net GND)
    (add_net GPIO_1)
    (add_net GPIO_2)
    (add_net GPIO_3)
    (add_net GPIO_4)
    (add_net GPIO_5)
    (add_net GPIO_6)
    (add_net GPIO_7)
    (add_net GPIO_8)
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J13-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net SPI_MISO)
    (add_net SPI_MOSI)
    (add_net SPI_SCK)
  )
  (module Package_SO:SO-4_7.6x3.6mm_P2.54mm (layer F.Cu) (tedit 5D9FDDD0)
    (at 132.08 156.845 90)
    (descr "4-Lead Plastic Small Outline (SO) (http://www.everlight.com/file/ProductFile/201407061745083848.pdf)")
    (tags "SO SOIC 2.54")
    (attr smd)
    (fp_text reference U1 (at 3.175 3.175 90) (layer F.SilkS))
    (fp_text value EL814 (at 0 2.8 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.065 90) (layer F.Fab))
    (pad 1 smd rect (at -4.5 -1.27 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -4.5 1.27 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (pad 3 smd rect (at 4.5 1.27 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 GPIO_8))
    (pad 4 smd rect (at 4.5 -1.27 90) (size 1.3 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 3v3))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SO-4_7.6x3.6mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D3264CE)
    (at 149.86 92.71)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D3264DA)
    (at 149.86 168.91)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D3264D2)
    (at 160.02 92.71)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5D3264DD)
    (at 160.02 168.91)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 146.685 105.41 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 GPIO_1))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 146.685 110.49 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 AGND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GPIO_2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 148.59 123.825 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 AGND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GPIO_3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 148.59 129.54 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value C (at 0 1.65 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GPIO_4))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 AGND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268ED)
    (at 155.575 163.195)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP1 (at -5.588 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 2 3v3))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268B9)
    (at 132.715 106.68)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP2 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 7 CAN_H))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268BD)
    (at 132.715 110.49)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP3 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 CAN_L))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268C1)
    (at 126.365 164.465)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP4 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268CA)
    (at 144.78 118.11)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP5 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 9 AVCC))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268CD)
    (at 134.62 120.015)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP6 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 10 AGND))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5D3268DB)
    (at 134.62 125.095)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP7 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 11 SPI_SCK))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x20_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 139.7 106.68 180)
    (descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x20 2.54mm single row")
    (fp_text reference J1 (at 0 2.33) (layer B.SilkS))
    (fp_text value Conn_01x20_Male (at 0 -50.59) (layer B.Fab) hide)
    (fp_text user %R (at 0 -24.13 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 3v3))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 CAN_H))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 CAN_L))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 AVCC))
    (pad 7 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 AGND))
    (pad 8 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SPI_SCK))
    (pad 9 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SPI_MISO))
    (pad 10 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 SPI_MOSI))
    (pad 11 thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GPIO_1))
    (pad 12 thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GPIO_2))
    (pad 13 thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GPIO_3))
    (pad 14 thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GPIO_4))
    (pad 15 thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GPIO_5))
    (pad 16 thru_hole oval (at 0 -38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 GPIO_6))
    (pad 17 thru_hole oval (at 0 -40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 GPIO_7))
    (pad 18 thru_hole oval (at 0 -43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 GPIO_8))
    (pad 19 thru_hole oval (at 0 -45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole oval (at 0 -48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 142.875 151.13 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 20k (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 GPIO_8))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 144.78 127 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP8 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 SPI_MISO))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 134.62 128.905 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP9 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 SPI_MOSI))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 144.78 131.445 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP10 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 3 GPIO_1))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 134.62 135.255)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP11 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GPIO_2))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 144.78 137.16 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP12 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GPIO_3))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 134.62 139.7 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP13 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at -0.525001 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 6 GPIO_4))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 144.78 142.24 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP14 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 14 GPIO_5))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 134.62 144.78 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP15 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 15 GPIO_6))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 144.78 147.32 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP16 (at -1.905 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 16 GPIO_7))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Keystone_5015_Micro-Minature (layer F.Cu) (tedit 5A0F774F)
    (at 134.62 148.59 180)
    (descr "SMT Test Point- Micro Miniature 5015, http://www.keyelco.com/product-pdf.cfm?p=1353")
    (tags "Test Point")
    (attr smd)
    (fp_text reference TP17 (at 0 -2.25) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0 0 180) (size 3.4 1.8) (layers F.Cu F.Paste F.Mask)
      (net 17 GPIO_8))
    (model ${KISYS3DMOD}/TestPoint.3dshapes/TestPoint_Keystone_5015_Micro-Minature.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 159.385 102.87 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J2 (at 2.5 -3.55) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 10 AGND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 AVCC))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 GPIO_1))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 159.385 111.76 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J3 (at 2.5 -3.55) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 GPIO_2))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 AVCC))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 10 AGND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 159.385 120.65 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J4 (at 2.5 -3.55) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 10 AGND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 AVCC))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 GPIO_3))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 159.385 129.54 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J5 (at 2.5 -3.55) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 GPIO_4))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 AVCC))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 10 AGND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 125.73 113.665 270)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J6 (at 3.75 -3.55 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 3.75 4.6 90) (layer F.Fab))
    (fp_text user %R (at 3.75 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 3v3))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 GPIO_1))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 GPIO_2))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B6B-XH-A_1x06_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 125.73 127.635 270)
    (descr "JST XH series connector, B6B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J7 (at 6.25 -3.55 90) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 90) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 12.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 GPIO_5))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 13 SPI_MOSI))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 SPI_MISO))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 SPI_SCK))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 3v3))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B6B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 159.385 138.43 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J8 (at 2.5 -3.55) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 3v3))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 14 GPIO_5))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 159.385 147.32 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J9 (at 2.5 -3.55) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 15 GPIO_6))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 3v3))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 159.385 156.21 180)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J10 (at 5.08 -3.81) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 3v3))
    (pad 3 thru_hole oval (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 GPIO_7))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 147.32 156.845 270)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J11 (at -3.81 0.635 180) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 3v3))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 17 GPIO_8))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B6B-XH-A_1x06_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 125.73 146.685 270)
    (descr "JST XH series connector, B6B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J12 (at 0.635 -3.81 90) (layer F.SilkS))
    (fp_text value Conn_01x06 (at 6.25 4.6 90) (layer F.Fab))
    (fp_text user %R (at 6.25 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 3v3))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 SPI_SCK))
    (pad 4 thru_hole oval (at 7.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 12 SPI_MISO))
    (pad 5 thru_hole oval (at 10 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 13 SPI_MOSI))
    (pad 6 thru_hole oval (at 12.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 15 GPIO_6))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B6B-XH-A_1x06_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 138.43 163.83 90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J13 (at 1.25 -3.55 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1.25 4.6 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 2.7 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 18 "Net-(J13-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J13-Pad2)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 125.73 102.235 270)
    (descr "JST XH series connector, B3B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J14 (at 2.5 -3.55 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 2.5 4.6 90) (layer F.Fab))
    (fp_text user %R (at 2.5 2.7 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 8 CAN_L))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 CAN_H))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B3B-XH-A_1x03_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 133.35 165.1 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 220R (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J13-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "By TLA" (at 139.065 97.155) (layer F.SilkS))
  (gr_text "Odrive Aux V1.0\nCC0 License\nLove Everyone" (at 128.27 93.98) (layer F.SilkS))
  (gr_line (start 165.1 169.545) (end 165.1 92.075) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 172.72) (end 161.925 172.72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.745 92.075) (end 118.745 169.545) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.925 88.9) (end 121.92 88.9) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.925 169.545) (end 161.925 172.72) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.92 169.545) (end 118.745 169.545) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.92 92.075) (end 121.92 88.9) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 161.925 92.075) (end 165.1 92.075) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_text CAN_BUS (at 120.65 104.14 90) (layer F.SilkS))
  (gr_text UART (at 120.65 118.11 90) (layer F.SilkS))
  (gr_text SPI_1 (at 120.65 133.985 90) (layer F.SilkS))
  (gr_text SPI_2 (at 120.65 156.21 90) (layer F.SilkS))
  (gr_text ESTOP (at 138.43 167.64) (layer F.SilkS))
  (gr_text GPIO_8 (at 151.13 162.56 90) (layer F.SilkS))
  (gr_text GPIO_7 (at 159.385 160.02) (layer F.SilkS))
  (gr_text GPIO_6 (at 150.495 146.685 90) (layer F.SilkS))
  (gr_text GPIO_5 (at 150.495 137.795 90) (layer F.SilkS))
  (gr_text GPIO_4 (at 150.495 129.54 90) (layer F.SilkS))
  (gr_text GPIO_3 (at 150.495 119.38 90) (layer F.SilkS))
  (gr_text GPIO_2 (at 150.495 111.76 90) (layer F.SilkS))
  (gr_text "Design licensed CC0 - Public Domain. Use this information for any purpose.\nCreated by Taylor Alexander for Twisted Fields Llc.\nThanks to Daniel Theobald for funding the work." (at 100.33 195.58) (layer Dwgs.User))
  (gr_text GND (at 125.095 167.005) (layer F.SilkS))
  (gr_text GPIO_1 (at 150.495 102.87 90) (layer F.SilkS))
  (gr_text 3v3 (at 159.385 163.195) (layer F.SilkS))
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.0048 91.5162) (xy 140.1064 91.5162) (xy 140.1064 91.5416) (xy 140.1826 91.5416) (xy 140.1826 91.567)
        (xy 140.2334 91.567) (xy 140.2334 91.5924) (xy 140.3096 91.5924) (xy 140.3096 91.6178) (xy 140.3604 91.6178)
        (xy 140.3604 91.6432) (xy 140.3858 91.6432) (xy 140.3858 91.6686) (xy 140.4366 91.6686) (xy 140.4366 91.694)
        (xy 140.4874 91.694) (xy 140.4874 91.7194) (xy 140.5128 91.7194) (xy 140.5128 91.7448) (xy 140.5636 91.7448)
        (xy 140.5636 91.7702) (xy 140.589 91.7702) (xy 140.589 91.7956) (xy 140.6144 91.7956) (xy 140.6144 91.821)
        (xy 140.6652 91.821) (xy 140.6652 91.8464) (xy 140.6906 91.8464) (xy 140.6906 91.8718) (xy 140.716 91.8718)
        (xy 140.716 91.8972) (xy 140.7668 91.8972) (xy 140.7668 91.9226) (xy 140.7922 91.9226) (xy 140.7922 91.948)
        (xy 140.8176 91.948) (xy 140.8176 91.9734) (xy 140.843 91.9734) (xy 140.843 91.9988) (xy 140.8684 91.9988)
        (xy 140.8684 92.0242) (xy 140.8938 92.0242) (xy 140.8938 92.0496) (xy 140.9192 92.0496) (xy 140.9192 92.075)
        (xy 140.97 92.075) (xy 140.97 92.0496) (xy 140.9954 92.0496) (xy 140.9954 92.0242) (xy 141.0208 92.0242)
        (xy 141.0208 91.9988) (xy 141.0462 91.9988) (xy 141.0462 91.9734) (xy 141.0716 91.9734) (xy 141.0716 91.948)
        (xy 141.097 91.948) (xy 141.097 91.9226) (xy 141.1224 91.9226) (xy 141.1224 91.8972) (xy 141.1732 91.8972)
        (xy 141.1732 91.8718) (xy 141.1986 91.8718) (xy 141.1986 91.8464) (xy 141.224 91.8464) (xy 141.224 91.821)
        (xy 141.2494 91.821) (xy 141.2494 91.7956) (xy 141.3002 91.7956) (xy 141.3002 91.7702) (xy 141.3256 91.7702)
        (xy 141.3256 91.7448) (xy 141.3764 91.7448) (xy 141.3764 91.7194) (xy 141.4018 91.7194) (xy 141.4018 91.694)
        (xy 141.4526 91.694) (xy 141.4526 91.6686) (xy 141.478 91.6686) (xy 141.478 91.6432) (xy 141.5288 91.6432)
        (xy 141.5288 91.6178) (xy 141.5796 91.6178) (xy 141.5796 91.5924) (xy 141.6558 91.5924) (xy 141.6558 91.567)
        (xy 141.7066 91.567) (xy 141.7066 91.5416) (xy 141.7828 91.5416) (xy 141.7828 91.5162) (xy 141.8844 91.5162)
        (xy 141.8844 91.4908) (xy 142.3924 91.4908) (xy 142.3924 91.5162) (xy 142.5194 91.5162) (xy 142.5194 91.5416)
        (xy 142.5956 91.5416) (xy 142.5956 91.567) (xy 142.6718 91.567) (xy 142.6718 91.5924) (xy 142.7226 91.5924)
        (xy 142.7226 91.6178) (xy 142.7734 91.6178) (xy 142.7734 91.6432) (xy 142.8242 91.6432) (xy 142.8242 91.6686)
        (xy 142.875 91.6686) (xy 142.875 91.694) (xy 142.9258 91.694) (xy 142.9258 91.7194) (xy 142.9512 91.7194)
        (xy 142.9512 91.7448) (xy 142.9766 91.7448) (xy 142.9766 91.7702) (xy 143.002 91.7702) (xy 143.002 91.7956)
        (xy 143.0274 91.7956) (xy 143.0274 91.821) (xy 143.0782 91.821) (xy 143.0782 91.8718) (xy 143.1036 91.8718)
        (xy 143.1036 91.8972) (xy 143.129 91.8972) (xy 143.129 91.9226) (xy 143.1544 91.9226) (xy 143.1544 91.948)
        (xy 143.1798 91.948) (xy 143.1798 91.9988) (xy 143.2052 91.9988) (xy 143.2052 92.0242) (xy 143.2306 92.0242)
        (xy 143.2306 92.075) (xy 143.256 92.075) (xy 143.256 92.1258) (xy 143.2814 92.1258) (xy 143.2814 92.1766)
        (xy 143.3068 92.1766) (xy 143.3068 92.2274) (xy 143.3322 92.2274) (xy 143.3322 92.3036) (xy 143.3576 92.3036)
        (xy 143.3576 92.4306) (xy 143.383 92.4306) (xy 143.383 92.6084) (xy 143.4084 92.6084) (xy 143.4084 92.8878)
        (xy 143.383 92.8878) (xy 143.383 93.0402) (xy 143.3576 93.0402) (xy 143.3576 93.1418) (xy 143.3322 93.1418)
        (xy 143.3322 93.218) (xy 143.3068 93.218) (xy 143.3068 93.2942) (xy 143.2814 93.2942) (xy 143.2814 93.345)
        (xy 143.256 93.345) (xy 143.256 93.3958) (xy 143.2306 93.3958) (xy 143.2306 93.4212) (xy 143.2052 93.4212)
        (xy 143.2052 93.472) (xy 143.1798 93.472) (xy 143.1798 93.5228) (xy 143.1544 93.5228) (xy 143.1544 93.5736)
        (xy 143.129 93.5736) (xy 143.129 93.599) (xy 143.1036 93.599) (xy 143.1036 93.6244) (xy 143.0782 93.6244)
        (xy 143.0782 93.6752) (xy 143.0528 93.6752) (xy 143.0528 93.7006) (xy 143.0274 93.7006) (xy 143.0274 93.726)
        (xy 143.002 93.726) (xy 143.002 93.7768) (xy 142.9766 93.7768) (xy 142.9766 93.8022) (xy 142.9512 93.8022)
        (xy 142.9512 93.8276) (xy 142.9258 93.8276) (xy 142.9258 93.853) (xy 142.9004 93.853) (xy 142.9004 93.8784)
        (xy 142.875 93.8784) (xy 142.875 93.9038) (xy 142.8496 93.9038) (xy 142.8496 93.9292) (xy 142.8242 93.9292)
        (xy 142.8242 93.98) (xy 142.7988 93.98) (xy 142.7988 94.0054) (xy 142.7734 94.0054) (xy 142.7734 94.0308)
        (xy 142.7226 94.0308) (xy 142.7226 94.0562) (xy 142.6972 94.0562) (xy 142.6972 94.0816) (xy 142.6718 94.0816)
        (xy 142.6718 94.107) (xy 142.6464 94.107) (xy 142.6464 94.1324) (xy 142.621 94.1324) (xy 142.621 94.1578)
        (xy 142.5956 94.1578) (xy 142.5956 94.1832) (xy 142.5702 94.1832) (xy 142.5702 94.2086) (xy 142.5448 94.2086)
        (xy 142.5448 94.234) (xy 142.5194 94.234) (xy 142.5194 94.2594) (xy 142.494 94.2594) (xy 142.494 94.2848)
        (xy 142.4686 94.2848) (xy 142.4686 94.3102) (xy 142.4432 94.3102) (xy 142.4432 94.3356) (xy 142.4178 94.3356)
        (xy 142.4178 94.361) (xy 142.3924 94.361) (xy 142.3924 94.3864) (xy 142.367 94.3864) (xy 142.367 94.4118)
        (xy 142.3416 94.4118) (xy 142.3416 94.4372) (xy 142.3162 94.4372) (xy 142.3162 94.4626) (xy 142.2908 94.4626)
        (xy 142.2908 94.488) (xy 142.2654 94.488) (xy 142.2654 94.5134) (xy 142.24 94.5134) (xy 142.24 94.5388)
        (xy 142.2146 94.5388) (xy 142.2146 94.5642) (xy 142.1892 94.5642) (xy 142.1892 94.5896) (xy 142.1638 94.5896)
        (xy 142.1638 94.615) (xy 142.1384 94.615) (xy 142.1384 94.6404) (xy 142.113 94.6404) (xy 142.113 94.6658)
        (xy 142.0622 94.6658) (xy 142.0622 94.6912) (xy 142.0368 94.6912) (xy 142.0368 94.7166) (xy 142.0114 94.7166)
        (xy 142.0114 94.742) (xy 141.986 94.742) (xy 141.986 94.7674) (xy 141.9606 94.7674) (xy 141.9606 94.7928)
        (xy 141.9352 94.7928) (xy 141.9352 94.8182) (xy 141.9098 94.8182) (xy 141.9098 94.8436) (xy 141.8844 94.8436)
        (xy 141.8844 94.869) (xy 141.859 94.869) (xy 141.859 94.8944) (xy 141.8336 94.8944) (xy 141.8336 94.9198)
        (xy 141.8082 94.9198) (xy 141.8082 94.9452) (xy 141.7828 94.9452) (xy 141.7828 94.9706) (xy 141.7574 94.9706)
        (xy 141.7574 94.996) (xy 141.732 94.996) (xy 141.732 95.0214) (xy 141.7066 95.0214) (xy 141.7066 95.0468)
        (xy 141.6812 95.0468) (xy 141.6812 95.0722) (xy 141.6558 95.0722) (xy 141.6558 95.0976) (xy 141.6304 95.0976)
        (xy 141.6304 95.123) (xy 141.605 95.123) (xy 141.605 95.1484) (xy 141.5796 95.1484) (xy 141.5796 95.1738)
        (xy 141.5542 95.1738) (xy 141.5542 95.1992) (xy 141.5288 95.1992) (xy 141.5288 95.2246) (xy 141.5034 95.2246)
        (xy 141.5034 95.25) (xy 141.478 95.25) (xy 141.478 95.2754) (xy 141.4526 95.2754) (xy 141.4526 95.3008)
        (xy 141.4272 95.3008) (xy 141.4272 95.3262) (xy 141.3764 95.3262) (xy 141.3764 95.3516) (xy 141.351 95.3516)
        (xy 141.351 95.377) (xy 141.3256 95.377) (xy 141.3256 95.4024) (xy 141.3002 95.4024) (xy 141.3002 95.4278)
        (xy 141.2748 95.4278) (xy 141.2748 95.4532) (xy 141.2494 95.4532) (xy 141.2494 95.4786) (xy 141.224 95.4786)
        (xy 141.224 95.504) (xy 141.1986 95.504) (xy 141.1986 95.5294) (xy 141.1732 95.5294) (xy 141.1732 95.5548)
        (xy 141.1478 95.5548) (xy 141.1478 95.5802) (xy 141.1224 95.5802) (xy 141.1224 95.6056) (xy 141.097 95.6056)
        (xy 141.097 95.631) (xy 141.0716 95.631) (xy 141.0716 95.6564) (xy 141.0462 95.6564) (xy 141.0462 95.6818)
        (xy 140.9954 95.6818) (xy 140.9954 95.7072) (xy 140.8938 95.7072) (xy 140.8938 95.6818) (xy 140.843 95.6818)
        (xy 140.843 95.6564) (xy 140.8176 95.6564) (xy 140.8176 95.631) (xy 140.7922 95.631) (xy 140.7922 95.6056)
        (xy 140.7668 95.6056) (xy 140.7668 95.5802) (xy 140.7414 95.5802) (xy 140.7414 95.5548) (xy 140.716 95.5548)
        (xy 140.716 95.5294) (xy 140.6906 95.5294) (xy 140.6906 95.504) (xy 140.6652 95.504) (xy 140.6652 95.4786)
        (xy 140.6398 95.4786) (xy 140.6398 95.4532) (xy 140.6144 95.4532) (xy 140.6144 95.4278) (xy 140.589 95.4278)
        (xy 140.589 95.4024) (xy 140.5636 95.4024) (xy 140.5636 95.377) (xy 140.5382 95.377) (xy 140.5382 95.3516)
        (xy 140.5128 95.3516) (xy 140.5128 95.3262) (xy 140.4874 95.3262) (xy 140.4874 95.3008) (xy 140.4366 95.3008)
        (xy 140.4366 95.2754) (xy 140.4112 95.2754) (xy 140.4112 95.25) (xy 140.3858 95.25) (xy 140.3858 95.2246)
        (xy 140.3604 95.2246) (xy 140.3604 95.1992) (xy 140.335 95.1992) (xy 140.335 95.1738) (xy 140.3096 95.1738)
        (xy 140.3096 95.1484) (xy 140.2842 95.1484) (xy 140.2842 95.123) (xy 140.2588 95.123) (xy 140.2588 95.0976)
        (xy 140.2334 95.0976) (xy 140.2334 95.0722) (xy 140.208 95.0722) (xy 140.208 95.0468) (xy 140.1826 95.0468)
        (xy 140.1826 95.0214) (xy 140.1572 95.0214) (xy 140.1572 94.996) (xy 140.1318 94.996) (xy 140.1318 94.9706)
        (xy 140.1064 94.9706) (xy 140.1064 94.9452) (xy 140.081 94.9452) (xy 140.081 94.9198) (xy 140.0556 94.9198)
        (xy 140.0556 94.8944) (xy 140.0302 94.8944) (xy 140.0302 94.869) (xy 140.0048 94.869) (xy 140.0048 94.8436)
        (xy 139.9794 94.8436) (xy 139.9794 94.8182) (xy 139.954 94.8182) (xy 139.954 94.7928) (xy 139.9286 94.7928)
        (xy 139.9286 94.7674) (xy 139.9032 94.7674) (xy 139.9032 94.742) (xy 139.8778 94.742) (xy 139.8778 94.7166)
        (xy 139.8524 94.7166) (xy 139.8524 94.6912) (xy 139.827 94.6912) (xy 139.827 94.6658) (xy 139.7762 94.6658)
        (xy 139.7762 94.6404) (xy 139.7508 94.6404) (xy 139.7508 94.615) (xy 139.7254 94.615) (xy 139.7254 94.5896)
        (xy 139.7 94.5896) (xy 139.7 94.5642) (xy 139.6746 94.5642) (xy 139.6746 94.5388) (xy 139.6492 94.5388)
        (xy 139.6492 94.5134) (xy 139.6238 94.5134) (xy 139.6238 94.488) (xy 139.5984 94.488) (xy 139.5984 94.4626)
        (xy 139.573 94.4626) (xy 139.573 94.4372) (xy 139.5476 94.4372) (xy 139.5476 94.4118) (xy 139.5222 94.4118)
        (xy 139.5222 94.3864) (xy 139.4968 94.3864) (xy 139.4968 94.361) (xy 139.4714 94.361) (xy 139.4714 94.3356)
        (xy 139.446 94.3356) (xy 139.446 94.3102) (xy 139.4206 94.3102) (xy 139.4206 94.2848) (xy 139.3952 94.2848)
        (xy 139.3952 94.2594) (xy 139.3698 94.2594) (xy 139.3698 94.234) (xy 139.3444 94.234) (xy 139.3444 94.2086)
        (xy 139.319 94.2086) (xy 139.319 94.1832) (xy 139.2936 94.1832) (xy 139.2936 94.1578) (xy 139.2682 94.1578)
        (xy 139.2682 94.1324) (xy 139.2428 94.1324) (xy 139.2428 94.107) (xy 139.2174 94.107) (xy 139.2174 94.0816)
        (xy 139.192 94.0816) (xy 139.192 94.0562) (xy 139.1666 94.0562) (xy 139.1666 94.0308) (xy 139.1158 94.0308)
        (xy 139.1158 93.98) (xy 139.065 93.98) (xy 139.065 93.9546) (xy 139.0396 93.9546) (xy 139.0396 93.9292)
        (xy 139.0142 93.9292) (xy 139.0142 93.8784) (xy 138.9888 93.8784) (xy 138.9888 93.853) (xy 138.9634 93.853)
        (xy 138.9634 93.8276) (xy 138.938 93.8276) (xy 138.938 93.8022) (xy 138.9126 93.8022) (xy 138.9126 93.7768)
        (xy 138.8872 93.7768) (xy 138.8872 93.726) (xy 138.8618 93.726) (xy 138.8618 93.7006) (xy 138.8364 93.7006)
        (xy 138.8364 93.6752) (xy 138.811 93.6752) (xy 138.811 93.6244) (xy 138.7856 93.6244) (xy 138.7856 93.599)
        (xy 138.7602 93.599) (xy 138.7602 93.5736) (xy 138.7348 93.5736) (xy 138.7348 93.5228) (xy 138.7094 93.5228)
        (xy 138.7094 93.472) (xy 138.684 93.472) (xy 138.684 93.4212) (xy 138.6586 93.4212) (xy 138.6586 93.3958)
        (xy 138.6332 93.3958) (xy 138.6332 93.345) (xy 138.6078 93.345) (xy 138.6078 93.2688) (xy 138.5824 93.2688)
        (xy 138.5824 93.218) (xy 138.557 93.218) (xy 138.557 93.1418) (xy 138.5316 93.1418) (xy 138.5316 93.0656)
        (xy 138.5062 93.0656) (xy 138.5062 92.9386) (xy 138.4808 92.9386) (xy 138.4808 92.5576) (xy 138.5062 92.5576)
        (xy 138.5062 92.4052) (xy 138.5316 92.4052) (xy 138.5316 92.3036) (xy 138.557 92.3036) (xy 138.557 92.2274)
        (xy 138.5824 92.2274) (xy 138.5824 92.1766) (xy 138.6078 92.1766) (xy 138.6078 92.1258) (xy 138.6332 92.1258)
        (xy 138.6332 92.075) (xy 138.6586 92.075) (xy 138.6586 92.0242) (xy 138.684 92.0242) (xy 138.684 91.9988)
        (xy 138.7094 91.9988) (xy 138.7094 91.948) (xy 138.7348 91.948) (xy 138.7348 91.9226) (xy 138.7602 91.9226)
        (xy 138.7602 91.8972) (xy 138.7856 91.8972) (xy 138.7856 91.8718) (xy 138.811 91.8718) (xy 138.811 91.821)
        (xy 138.8364 91.821) (xy 138.8364 91.7956) (xy 138.8872 91.7956) (xy 138.8872 91.7702) (xy 138.9126 91.7702)
        (xy 138.9126 91.7448) (xy 138.938 91.7448) (xy 138.938 91.7194) (xy 138.9634 91.7194) (xy 138.9634 91.694)
        (xy 139.0142 91.694) (xy 139.0142 91.6686) (xy 139.065 91.6686) (xy 139.065 91.6432) (xy 139.1158 91.6432)
        (xy 139.1158 91.6178) (xy 139.1666 91.6178) (xy 139.1666 91.5924) (xy 139.2174 91.5924) (xy 139.2174 91.567)
        (xy 139.2936 91.567) (xy 139.2936 91.5416) (xy 139.3698 91.5416) (xy 139.3698 91.5162) (xy 139.4968 91.5162)
        (xy 139.4968 91.4908) (xy 140.0048 91.4908)
      )
    )
  )
)
