(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 526)
    (zones 0)
    (modules 53)
    (nets 70)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.15)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(AE1-Pad1)")
  (net 2 GND)
  (net 3 /ANTEN)
  (net 4 VoutCharger)
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 "Net-(C8-Pad1)")
  (net 10 "Net-(C9-Pad1)")
  (net 11 "Net-(C10-Pad1)")
  (net 12 "Net-(C11-Pad1)")
  (net 13 "Net-(C12-Pad1)")
  (net 14 /batteryManagement/batCharg)
  (net 15 /vcpu)
  (net 16 /batteryManagement/Vin)
  (net 17 "Net-(D1-Pad1)")
  (net 18 "Net-(D2-Pad2)")
  (net 19 PG)
  (net 20 "Net-(D3-Pad2)")
  (net 21 STAT1)
  (net 22 "Net-(D4-Pad2)")
  (net 23 STAT2)
  (net 24 "Net-(D5-Pad2)")
  (net 25 /LED)
  (net 26 "Net-(J1-Pad4)")
  (net 27 "Net-(J1-Pad3)")
  (net 28 "Net-(J1-Pad2)")
  (net 29 "Net-(J3-Pad7)")
  (net 30 /RST)
  (net 31 /SWDIO)
  (net 32 /SWDCLK)
  (net 33 /SWO)
  (net 34 "Net-(J3-Pad8)")
  (net 35 "Net-(R1-Pad1)")
  (net 36 "Net-(R2-Pad2)")
  (net 37 "Net-(R3-Pad2)")
  (net 38 "Net-(R4-Pad2)")
  (net 39 /VsupRef)
  (net 40 /button)
  (net 41 /INT1)
  (net 42 "Net-(U1-Pad3)")
  (net 43 "Net-(U1-Pad2)")
  (net 44 /MISO)
  (net 45 /MOSI)
  (net 46 /SCLK)
  (net 47 /CS)
  (net 48 "Net-(U1-Pad11)")
  (net 49 "Net-(U1-Pad10)")
  (net 50 /INT2)
  (net 51 "Net-(U2-Pad47)")
  (net 52 "Net-(U2-Pad44)")
  (net 53 "Net-(U2-Pad43)")
  (net 54 "Net-(U2-Pad42)")
  (net 55 "Net-(U2-Pad41)")
  (net 56 "Net-(U2-Pad40)")
  (net 57 "Net-(U2-Pad39)")
  (net 58 "Net-(U2-Pad38)")
  (net 59 "Net-(U2-Pad29)")
  (net 60 "Net-(U2-Pad28)")
  (net 61 "Net-(U2-Pad23)")
  (net 62 "Net-(U2-Pad22)")
  (net 63 "Net-(U2-Pad20)")
  (net 64 "Net-(U2-Pad12)")
  (net 65 "Net-(U2-Pad11)")
  (net 66 "Net-(U2-Pad6)")
  (net 67 "Net-(U2-Pad4)")
  (net 68 "Net-(Y1-Pad4)")
  (net 69 "Net-(Y1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ANTEN)
    (add_net /CS)
    (add_net /INT1)
    (add_net /INT2)
    (add_net /LED)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCLK)
    (add_net /SWDCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /VsupRef)
    (add_net /batteryManagement/Vin)
    (add_net /batteryManagement/batCharg)
    (add_net /button)
    (add_net /vcpu)
    (add_net GND)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad40)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad42)")
    (add_net "Net-(U2-Pad43)")
    (add_net "Net-(U2-Pad44)")
    (add_net "Net-(U2-Pad47)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(Y1-Pad2)")
    (add_net "Net-(Y1-Pad4)")
    (add_net PG)
    (add_net STAT1)
    (add_net STAT2)
    (add_net VoutCharger)
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 97.7 81.4)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_Vref1 (at 0 1.998) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -2.05) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Mask)
      (net 39 /VsupRef))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 101.4 80.05)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_VChar1 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 4 VoutCharger))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 119 79.5)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_Vcc1 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 15 /vcpu))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 119.3 65.95)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_SCLK1 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 46 /SCLK))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 119.15 70.7)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_MOSI1 (at 0 1.998) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -2.05) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Mask)
      (net 45 /MOSI))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 119.45 74.85)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_MISO1 (at 0 1.998) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -2.05) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Mask)
      (net 44 /MISO))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 119.25 70.55)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_INT2 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 50 /INT2))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 119.75 74.75)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_INT1 (at 0 -1.998) (layer F.SilkS))
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers F.Cu F.Mask)
      (net 41 /INT1))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 97.3 90.8)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_GND1 (at 0 1.998) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -2.05) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module TestPoint:TestPoint_Pad_2.0x2.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 119.3 66.1)
    (descr "SMD rectangular pad as test Point, square 2.0mm side length")
    (tags "test point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP_CS1 (at 0 1.998) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -2.05) (layer B.Fab))
    (fp_text user %R (at 0 2) (layer B.Fab))
    (pad 1 smd rect (at 0 0) (size 2 2) (layers B.Cu B.Mask)
      (net 47 /CS))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 99.5 85.25)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS))
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad_TopBottom (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers B.Cu B.Mask))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers F.Cu F.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module AllardFootPrints:Crystal_SMD_3215-2Pin_3.2x1.5mm_3d (layer F.Cu) (tedit 6060C419)
    (at 105.355 81.3)
    (descr "SMD Crystal FC-135 https://support.epson.biz/td/api/doc_check.php?dl=brief_FC-135R_en.pdf")
    (tags "SMD SMT Crystal")
    (attr smd)
    (fp_text reference Y2 (at 0 -2) (layer F.SilkS))
    (fp_text value "32.768kHz Crystal" (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at -1.2954 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C10-Pad1)"))
    (pad 1 smd rect (at 1.2954 0) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_3215-2Pin_3.2x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/allard/Documents/kicad/3dModels/ABS07AIG-32.768KHZ-D-T.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module AllardFootPrints:Crystal_SMD_2016-4Pin_2.0x1.6mm_3d (layer F.Cu) (tedit 6060C2A7)
    (at 102.1 68.65)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -2) (layer F.SilkS))
    (fp_text value "32MHz Crystal" (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -0.7 -0.55) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(Y1-Pad4)"))
    (pad 3 smd rect (at 0.7 -0.55) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 0.7 0.55) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(Y1-Pad2)"))
    (pad 1 smd rect (at -0.7 0.55) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_2016-4Pin_2.0x1.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "/home/allard/Documents/kicad/3dModels/FA-128 32.0000MF20X-K5--3DModel-STEP-56544.STEP"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module AllardFootPrints:PQFN50P300X250X97-14N (layer F.Cu) (tedit 6060C14A)
    (at 114.85 76.6)
    (fp_text reference U1 (at -0.176 -2.0048) (layer F.SilkS))
    (fp_text value ICM-42688-P (at 4.7008 1.9952) (layer F.Fab))
    (pad 4 smd rect (at -1.165 0.75) (size 0.59 0.35) (layers F.Cu F.Paste)
      (net 41 /INT1))
    (pad 3 smd rect (at -1.165 0.25) (size 0.59 0.35) (layers F.Cu F.Paste)
      (net 42 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -1.165 -0.25) (size 0.59 0.35) (layers F.Cu F.Paste)
      (net 43 "Net-(U1-Pad2)"))
    (pad 1 smd rect (at -1.165 -0.75) (size 0.59 0.35) (layers F.Cu F.Paste)
      (net 44 /MISO))
    (pad 14 smd rect (at -0.5 -0.915) (size 0.35 0.59) (layers F.Cu F.Paste)
      (net 45 /MOSI))
    (pad 13 smd rect (at 0 -0.915) (size 0.35 0.59) (layers F.Cu F.Paste)
      (net 46 /SCLK))
    (pad 12 smd rect (at 0.5 -0.915) (size 0.35 0.59) (layers F.Cu F.Paste)
      (net 47 /CS))
    (pad 11 smd rect (at 1.165 -0.75) (size 0.59 0.35) (layers F.Cu F.Paste)
      (net 48 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at 1.165 -0.25) (size 0.59 0.35) (layers F.Cu F.Paste)
      (net 49 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at 1.165 0.25) (size 0.59 0.35) (layers F.Cu F.Paste)
      (net 50 /INT2))
    (pad 8 smd rect (at 1.165 0.75) (size 0.59 0.35) (layers F.Cu F.Paste)
      (net 15 /vcpu))
    (pad 7 smd rect (at 0.5 0.915) (size 0.35 0.59) (layers F.Cu F.Paste)
      (net 2 GND))
    (pad 6 smd rect (at 0 0.915) (size 0.35 0.59) (layers F.Cu F.Paste)
      (net 2 GND))
    (pad 5 smd rect (at -0.5 0.915) (size 0.35 0.59) (layers F.Cu F.Paste)
      (net 15 /vcpu))
    (model /home/allard/Documents/kicad/3dModels/ICM-42688-P.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm (layer F.Cu) (tedit 6060C0B9)
    (at 107.7 74 90)
    (descr "QFN, 48 Pin (http://infocenter.nordicsemi.com/pdf/nRF51822_PS_v3.3.pdf#page=67), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U2 (at 0 -4.3 90) (layer F.SilkS))
    (fp_text value nRF52832-QFAA (at 0 4.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" smd roundrect (at 1.53 1.53 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad "" smd roundrect (at 1.53 0 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad "" smd roundrect (at 1.53 -1.53 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad "" smd roundrect (at 0 1.53 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad "" smd roundrect (at 0 0 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad "" smd roundrect (at 0 -1.53 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad "" smd roundrect (at -1.53 1.53 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad "" smd roundrect (at -1.53 0 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad "" smd roundrect (at -1.53 -1.53 90) (size 1.24 1.24) (layers F.Paste) (roundrect_rratio 0.2016120967741936))
    (pad 49 smd rect (at 0 0 90) (size 4.6 4.6) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 48 smd roundrect (at -2.2 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /vcpu))
    (pad 47 smd roundrect (at -1.8 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(U2-Pad47)"))
    (pad 46 smd roundrect (at -1.4 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C4-Pad1)"))
    (pad 45 smd roundrect (at -1 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 44 smd roundrect (at -0.6 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(U2-Pad44)"))
    (pad 43 smd roundrect (at -0.2 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(U2-Pad43)"))
    (pad 42 smd roundrect (at 0.2 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "Net-(U2-Pad42)"))
    (pad 41 smd roundrect (at 0.6 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(U2-Pad41)"))
    (pad 40 smd roundrect (at 1 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(U2-Pad40)"))
    (pad 39 smd roundrect (at 1.4 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(U2-Pad39)"))
    (pad 38 smd roundrect (at 1.8 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(U2-Pad38)"))
    (pad 37 smd roundrect (at 2.2 -2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /LED))
    (pad 36 smd roundrect (at 2.95 -2.2 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /vcpu))
    (pad 35 smd roundrect (at 2.95 -1.8 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad1)"))
    (pad 34 smd roundrect (at 2.95 -1.4 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C8-Pad1)"))
    (pad 33 smd roundrect (at 2.95 -1 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C6-Pad1)"))
    (pad 32 smd roundrect (at 2.95 -0.6 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C7-Pad1)"))
    (pad 31 smd roundrect (at 2.95 -0.2 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 30 smd roundrect (at 2.95 0.2 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /ANTEN))
    (pad 29 smd roundrect (at 2.95 0.6 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 "Net-(U2-Pad29)"))
    (pad 28 smd roundrect (at 2.95 1 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 "Net-(U2-Pad28)"))
    (pad 27 smd roundrect (at 2.95 1.4 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 /button))
    (pad 26 smd roundrect (at 2.95 1.8 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /SWDIO))
    (pad 25 smd roundrect (at 2.95 2.2 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /SWDCLK))
    (pad 24 smd roundrect (at 2.2 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /RST))
    (pad 23 smd roundrect (at 1.8 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(U2-Pad23)"))
    (pad 22 smd roundrect (at 1.4 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(U2-Pad22)"))
    (pad 21 smd roundrect (at 1 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /SWO))
    (pad 20 smd roundrect (at 0.6 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(U2-Pad20)"))
    (pad 19 smd roundrect (at 0.2 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 /MOSI))
    (pad 18 smd roundrect (at -0.2 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 /SCLK))
    (pad 17 smd roundrect (at -0.6 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 /MISO))
    (pad 16 smd roundrect (at -1 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 /CS))
    (pad 15 smd roundrect (at -1.4 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 /INT2))
    (pad 14 smd roundrect (at -1.8 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 /INT1))
    (pad 13 smd roundrect (at -2.2 2.95 90) (size 0.2 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /vcpu))
    (pad 12 smd roundrect (at -2.95 2.2 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(U2-Pad12)"))
    (pad 11 smd roundrect (at -2.95 1.8 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(U2-Pad11)"))
    (pad 10 smd roundrect (at -2.95 1.4 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 STAT2))
    (pad 9 smd roundrect (at -2.95 1 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 STAT1))
    (pad 8 smd roundrect (at -2.95 0.6 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 PG))
    (pad 7 smd roundrect (at -2.95 0.2 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /vcpu))
    (pad 6 smd roundrect (at -2.95 -0.2 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 "Net-(U2-Pad6)"))
    (pad 5 smd roundrect (at -2.95 -0.6 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /VsupRef))
    (pad 4 smd roundrect (at -2.95 -1 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 "Net-(U2-Pad4)"))
    (pad 3 smd roundrect (at -2.95 -1.4 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C11-Pad1)"))
    (pad 2 smd roundrect (at -2.95 -1.8 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C10-Pad1)"))
    (pad 1 smd roundrect (at -2.95 -2.2 90) (size 0.8 0.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /home/allard/Documents/kicad/3dModels/NRF52832-QFAA-R--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 116.1 84.4)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 0 -2.9) (layer F.SilkS))
    (fp_text value LP2985-2.5 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 /vcpu))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C12-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VoutCharger))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 VoutCharger))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm (layer F.Cu) (tedit 5DC5F6A3)
    (at 107.4 89.6)
    (descr "QFN, 20 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=274), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U3 (at 0 -3.3) (layer F.SilkS))
    (fp_text value MCP73871 (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" smd roundrect (at 0.625 0.625) (size 1.01 1.01) (layers F.Paste) (roundrect_rratio 0.2475237623762376))
    (pad "" smd roundrect (at 0.625 -0.625) (size 1.01 1.01) (layers F.Paste) (roundrect_rratio 0.2475237623762376))
    (pad "" smd roundrect (at -0.625 0.625) (size 1.01 1.01) (layers F.Paste) (roundrect_rratio 0.2475237623762376))
    (pad "" smd roundrect (at -0.625 -0.625) (size 1.01 1.01) (layers F.Paste) (roundrect_rratio 0.2475237623762376))
    (pad 21 smd rect (at 0 0) (size 2.5 2.5) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 20 smd roundrect (at -1 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VoutCharger))
    (pad 19 smd roundrect (at -0.5 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D1-Pad1)"))
    (pad 18 smd roundrect (at 0 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D1-Pad1)"))
    (pad 17 smd roundrect (at 0.5 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D1-Pad1)"))
    (pad 16 smd roundrect (at 1 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /batteryManagement/batCharg))
    (pad 15 smd roundrect (at 1.9375 -1) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /batteryManagement/batCharg))
    (pad 14 smd roundrect (at 1.9375 -0.5) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /batteryManagement/batCharg))
    (pad 13 smd roundrect (at 1.9375 0) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R3-Pad2)"))
    (pad 12 smd roundrect (at 1.9375 0.5) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(R1-Pad1)"))
    (pad 11 smd roundrect (at 1.9375 1) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 10 smd roundrect (at 1 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 9 smd roundrect (at 0.5 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D1-Pad1)"))
    (pad 8 smd roundrect (at 0 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 STAT1))
    (pad 7 smd roundrect (at -0.5 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 STAT2))
    (pad 6 smd roundrect (at -1 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 PG))
    (pad 5 smd roundrect (at -1.9375 1) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R4-Pad2)"))
    (pad 4 smd roundrect (at -1.9375 0.5) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D1-Pad1)"))
    (pad 3 smd roundrect (at -1.9375 0) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at -1.9375 -0.5) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -1.9375 -1) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VoutCharger))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AllardFootPrints:microTactSwitch (layer F.Cu) (tedit 5E8E662C)
    (at 95.8 67.1 90)
    (attr smd)
    (fp_text reference SW1 (at 0 0.5 90) (layer F.SilkS))
    (fp_text value SW_MEC_5E (at 0 -0.5 90) (layer F.Fab))
    (pad 3 smd rect (at 2.1 -0.8 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 2.1 0.8 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.1 0.8 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 40 /button))
    (pad 1 smd rect (at -2.1 -0.8 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 40 /button))
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 95.8125 72.5)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 20 (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /vcpu))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 96.3375 82.35)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /VsupRef))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 100.788 82.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VoutCharger))
    (pad 1 smd roundrect (at -0.9125 0) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 /VsupRef))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 108.7 98.8125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VoutCharger))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 111.6 98.8125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VoutCharger))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 105.7 98.8125 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VoutCharger))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 101.288 88.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 270k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 101.212 94.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 113.988 92.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 2k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 101.188 91.7 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder (layer F.Cu) (tedit 5F68FEEE)
    (at 112.2 89.3875 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0402_1005Metric_Pad0.77x0.64mm_HandSolder (layer F.Cu) (tedit 5F6BBB3E)
    (at 108.072 63.05)
    (descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (attr smd)
    (fp_text reference L1 (at 0 -1.17) (layer F.SilkS))
    (fp_text value 3.9nH (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5725 0) (size 0.765 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /ANTEN))
    (pad 1 smd roundrect (at -0.5725 0) (size 0.765 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(AE1-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AllardFootPrints:2X5-PTH-1.27MM (layer F.Cu) (tedit 5EA36CA7)
    (at 114.915 69.29 270)
    (descr "<h3>ARM Cortex Debug Connector (10-pin)</h3>\n<p>For debuggers and/or programemrs that support the Cortex Debug Connector (10-pin) interface.</p>\n<p>tDoc (51) layer border represents maximum dimensions of plastic housing.</p>\n<p><a href=\"http://www.digikey.com/product-detail/en/20021111-00010T4LF/609-3712-ND/2209072\">Example Digikey Part</a></p>")
    (fp_text reference J3 (at -1.5748 -1.9304 90) (layer F.SilkS))
    (fp_text value Conn_ARM_JTAG_SWD_10_Full (at -1.8288 2.4638 90) (layer F.Fab))
    (pad 9 thru_hole circle (at 2.54 0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -2.54 0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 15 /vcpu) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at -1.27 0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 0 0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 2 GND) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 1.27 0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad7)") (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 2.54 -0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 30 /RST) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -2.54 -0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 31 /SWDIO) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at -1.27 -0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 32 /SWDCLK) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 0 -0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 33 /SWO) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 1.27 -0.635 270) (size 1 1) (drill 0.508) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad8)") (solder_mask_margin 0.1016))
    (model ${HOME}/Documents/kicad/3dModels/FTSH-105-01-F-D-K.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical (layer F.Cu) (tedit 5B7745C2)
    (at 118.1 98.5 180)
    (descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH side entry")
    (fp_text reference J2 (at 1 -2.9) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 1 4) (layer F.Fab))
    (fp_text user %R (at 1 1.5) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 /batteryManagement/batCharg))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.2083325)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AllardFootPrints:GCT_USB3075-30-A (layer F.Cu) (tedit 5EA36CE1)
    (at 96.875 97.95)
    (fp_text reference J1 (at -0.08593 -2.49759) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 6.86562 6.57223) (layer F.Fab))
    (fp_text user PCB~EDGE (at 5.71554 4.05494) (layer F.Fab))
    (pad 6 thru_hole oval (at 4.875 2.65) (size 1.05 2.1) (drill oval 0.45 1.25) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.275 2.65) (size 1.05 2.1) (drill oval 0.45 1.25) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 3.62 0.42) (size 1.15 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -1.02 0.42) (size 1.15 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.425 2.65) (size 1.75 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.175 2.65) (size 1.75 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.6 0) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.95 0) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 1.3 0) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at 0.65 0) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at 0 0) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 16 /batteryManagement/Vin))
    (model ${HOME}/Documents/kicad/3dModels/gct_usb3075MicroConnector.step
      (offset (xyz 1.32 -2.65 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 100.088 72.5 180)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value Green (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 "Net-(D5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /LED))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 108.7 94.7875 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D4 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value DNP (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 STAT2))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 111.6 94.8125 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D3 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value RED (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 STAT1))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5F68FEF1)
    (at 105.7 94.7875 270)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags LED)
    (attr smd)
    (fp_text reference D2 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value DNP (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 PG))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SMB_Handsoldering (layer F.Cu) (tedit 590B3D55)
    (at 95.9 91.3 270)
    (descr "Diode SMB (DO-214AA) Handsoldering")
    (tags "Diode SMB (DO-214AA) Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 -3 90) (layer F.SilkS))
    (fp_text value Diode (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 -3 90) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 270) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /batteryManagement/Vin))
    (pad 1 smd rect (at -2.7 0 270) (size 3.5 2.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 114.35 80.4325 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C14 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /vcpu))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 118 92.375 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.85 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 14 /batteryManagement/batCharg))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 116.632 88.2 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C12 (at 0 -1.16) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.16) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 109.432 80.2)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C11 (at 0 -1.16) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.16) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 103.8 85.3325 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C10 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value 15pF (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 96.7675 78.3 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C9 (at 0 -1.16) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.16) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 180) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 103.05 65.4825 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value 6pF (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 110.65 68.4825 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value DNP (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 105.6 68.4825 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 99.25 66.7325 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value 6pF (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 90) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 97.2 75.2325 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 111.7 84.275 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.85 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.85 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 2 GND))
    (pad 1 smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2173904347826087)
      (net 4 VoutCharger))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder (layer F.Cu) (tedit 5F6BB22C)
    (at 108.7 65.8825 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value 0.8pF (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.5675 0 270) (size 0.735 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /ANTEN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 105.75 65.77 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.16 90) (layer F.SilkS))
    (fp_text value DNP (at 0 1.16 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(AE1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AllardFootPrints:TRACE_ANTENNA_2.4GHZ_15.2MM (layer F.Cu) (tedit 5E8E668E)
    (at 107.6 61.4)
    (descr "<h3>2.4GHz Meander PCB Trace Antenna</h3>\n<p>PCB trace antenna with a 15.2 x 5.7mm footprint.</p>\n<p>Based on layout from <a href=\"http://www.ti.com/lit/an/swra117d/swra117d.pdf\">TI app note AN043</a>.</p>")
    (attr virtual)
    (fp_text reference AE1 (at 0 -1.27) (layer F.SilkS))
    (fp_text value DNP (at 0 -1.016) (layer F.Fab))
    (fp_text user "Board Edge" (at 1.5 -5.5) (layer F.Fab))
    (fp_text user "Ground Plane" (at 1 0.8) (layer F.Fab))
    (pad 1 smd rect (at 0 0.25) (size 0.5 0.5) (layers F.Cu F.Mask)
      (net 1 "Net-(AE1-Pad1)") (solder_mask_margin 0.1016) (zone_connect 2))
    (pad 2 smd rect (at -2.1 0.25) (size 0.9 0.5) (layers F.Cu F.Mask)
      (net 2 GND) (solder_mask_margin 0.1016) (zone_connect 2))
  )
  (gr_text "Designed Andrew Allard\n3/28/2020 MSD PR21380" (at 104.25 96) (layer B.SilkS))
  (gr_line (start 102.95 56.2) (end 121.95 56.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.95 63) (end 102.95 56.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.45 63) (end 102.95 63) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.45 102) (end 92.45 63) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.95 102) (end 92.45 102) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.95 86.55) (end 121.95 102) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 121.95 56.2) (end 121.95 86.55) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.675 61.325) (xy 121.625 101.775) (xy 92.65 101.85) (xy 92.65 63.35) (xy 104.15 63.35)
        (xy 104.15 61.35)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 121.725 61.375) (xy 121.675 101.825) (xy 92.65 101.85) (xy 92.65 63.35) (xy 104.15 63.35)
        (xy 104.15 61.35)
      )
    )
  )
)
