(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 23)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad6)")
  (net 3 "Net-(J1-Pad5)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 VCC)
  (net 6 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net VCC)
  )
  (module 2328702-4:23287024 (layer B.Cu) (tedit 5EE8238A)
    (at 151.9 117)
    (descr 2328702-4-1)
    (tags Connector)
    (attr smd)
    (fp_text reference J2 (at 0 0.9) (layer B.SilkS) hide)
    (fp_text value 2328702-4 (at 0 0.9) (layer B.SilkS) hide)
    (pad 1 smd rect (at 0.75 1.45) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.25 1.45) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad5)"))
    (pad 3 smd rect (at -0.25 1.45) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 VCC))
    (pad 4 smd rect (at -0.75 1.45) (size 0.3 0.8) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad MP1 smd rect (at 1.75 -1.05) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad MP2 smd rect (at -1.75 -1.05) (size 0.4 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module FH19C-6S-0.5SH_05_:FH19C6S05SH05 (layer F.Cu) (tedit 5EC1ED96)
    (at 151.850001 122.500001)
    (descr "FH19C-6S-0.5SH(05)")
    (tags Connector)
    (attr smd)
    (fp_text reference J1 (at 0 -0.2) (layer F.SilkS) hide)
    (fp_text value FH19C-6S-0.5SH_05_ (at 0 -0.2) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.25 -1.45) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.75 -1.45) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -0.25 -1.45) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 4 smd rect (at 0.25 -1.45) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 0.75 -1.45) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 1.25 -1.45) (size 0.3 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -2.25 1.05) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.25 1.05) (size 0.4 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (gr_text "vita stick\nin psp3000" (at 151.8 122.8) (layer B.SilkS))
  (gr_line (start 155.2 114.9) (end 155.2 124.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.4 114.9) (end 155.2 114.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.4 124.9) (end 148.4 114.9) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.2 124.9) (end 148.4 124.9) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.2 124.9) (xy 148.4 124.9) (xy 148.4 114.9) (xy 155.2 114.9)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.2 124.9) (xy 148.4 124.9) (xy 148.4 114.9) (xy 155.2 114.9)
      )
    )
  )
)
