(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/HS")
  (net 2 "GND")
  (net 3 "/-12V")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D4-Pad2)")
  (net 6 "Net-(J1-PadP)")
  (net 7 "Net-(J8-Pad1)")
  (net 8 "Net-(PS1-Pad2)")
  (net 9 "unconnected-(PS1-Pad6)")
  (net 10 "Net-(C5-Pad1)")
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 59 67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_2220_5650Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115.25 69.5 90)
    (descr "Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 5 0 180) (layer "F.SilkS"))
    (fp_text value "47μF" (at 0 3.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 90) (size 1.8 5.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.138889)
      (net 10 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 90) (size 1.8 5.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.138889)
      (net 3 "/-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 110 138)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 72.25 84.9375 -90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at -4.575 -2.885 90) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 110 126)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_2220_5650Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108 69.5 90)
    (descr "Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 5 0.22 180) (layer "F.SilkS"))
    (fp_text value "47μF" (at 0 3.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 90) (size 1.8 5.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.138889)
      (net 10 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 90) (size 1.8 5.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.138889)
      (net 3 "/-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 109 99.975 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.85 -270) (layer "F.SilkS"))
    (fp_text value "1μF" (at 0 1.85 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "/HS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 160 138)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "benbokser:5KP12A" (layer "F.Cu")
    (tedit 0)
    (at 88.9 86 90)
    (descr "15KPA")
    (tags "Diode")
    (property "Description" "Diode TVS Single Uni-Dir 12V 5KW 2-Pin Case P-600 T/R")
    (property "Height" "")
    (property "Manufacturer_Name" "LITTELFUSE")
    (property "Manufacturer_Part_Number" "5KP12A")
    (property "Mouser Part Number" "576-5KP12A")
    (property "Mouser Price/Stock" "https://www.mouser.com/Search/Refine.aspx?Keyword=576-5KP12A")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at -0.25 -2.9 180) (layer "F.SilkS"))
    (fp_text value "5KP12A" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.325 2.325) (drill 1.55) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 20 0.1 90) (size 2.325 2.325) (drill 1.55) (layers *.Cu *.Mask)
      (net 3 "/-12V") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/benbokser.pretty/5KP12A.STEP"
      (offset (xyz 10 0 5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 72.25 102.5375 -90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at -4.575 -2.885 90) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "SamacSys_Parts:2MS6T1B3M2QES" (layer "F.Cu")
    (tedit 0)
    (at 136.1225 103.5 90)
    (descr "2MS6T1B3M2QES-3")
    (tags "Switch")
    (property "Description" "Toggle Switches SPST OFF-ON")
    (property "Height" "23.63")
    (property "Manufacturer_Name" "Dailywell")
    (property "Manufacturer_Part_Number" "2MS6T1B3M2QES")
    (property "Mouser Part Number" "118-2MS6T1B3M2QES")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Dailywell/2MS6T1B3M2QES?qs=B6kkDfuK7%2FCLnLIcqzvQEQ%3D%3D")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "S1" (at 0 -2.123 90) (layer "F.SilkS"))
    (fp_text value "2MS6T1B3M2QES" (at 0 -2.123 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 -2.123 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 -5.08 90) (size 1.635 1.635) (drill 1.09) (layers *.Cu *.Mask)
      (net 8 "Net-(PS1-Pad2)") (pinfunction "3") (pintype "passive"))
    (model "D:\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\2MS6T1B3M2QES.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "XT90PW-M:AMASS_XT90PW-M" (layer "F.Cu")
    (tedit 62CE1481)
    (at 145.5 125)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HIEGHT" "10.3mm")
    (property "PARTREV" "V00")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -0.25 0.25 180) (layer "F.SilkS"))
    (fp_text value "XT90PW-M" (at -1.76 -13.445) (layer "F.Fab"))
    (pad "N" thru_hole circle (at 5.45 -9.4) (size 4.916 4.916) (drill 3.9) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "NEG") (pintype "passive"))
    (pad "P" thru_hole rect (at -5.45 -9.4) (size 4.916 4.916) (drill 3.9) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-PadP)") (pinfunction "POS") (pintype "passive"))
    (pad "S1" thru_hole oval (at -9.45 0) (size 1.3 2.6) (drill oval 0.6 1.6) (layers *.Cu *.Mask))
    (pad "S2" thru_hole oval (at 9.45 0) (size 1.3 2.6) (drill oval 0.6 1.6) (layers *.Cu *.Mask))
    (model "D:/Documents/KiCad/6.0/footprints/XT90PW-M.pretty/XT90PW-M.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_2220_5650Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101 69.5 90)
    (descr "Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 5 0 180) (layer "F.SilkS"))
    (fp_text value "47μF" (at 0 3.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 90) (size 1.8 5.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.138889)
      (net 10 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 90) (size 1.8 5.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.138889)
      (net 3 "/-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 127.5 138)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "SamacSys_Parts:ULT1225D48NMC" (layer "F.Cu")
    (tedit 0)
    (at 116 86 90)
    (descr "ULT-12/2.5-D48NM-C-5")
    (tags "Power Supply")
    (property "Description" "Isolated DC/DC Converters 30W 48VIN 12VOUT 2.5A DC/DC")
    (property "Height" "9.398")
    (property "Manufacturer_Name" "Murata Electronics")
    (property "Manufacturer_Part_Number" "ULT-12/2.5-D48NM-C")
    (property "Mouser Part Number" "580-ULT-12/2.5D48NMC")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Power-Solutions/ULT-12-25-D48NM-C?qs=pygdPweA0RfIXL%2FkWB89cA%3D%3D")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "PS1" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "ULT-12_2.5-D48NM-C" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd circle locked (at -6.82 -7.62 180) (size 1.78 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/HS") (pinfunction "+VIN") (pintype "passive"))
    (pad "2" smd circle locked (at -6.82 0 180) (size 1.78 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(PS1-Pad2)") (pinfunction "ON/OFF_CONTROL") (pintype "passive"))
    (pad "3" smd circle locked (at -6.82 7.62 180) (size 1.78 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "-VIN") (pintype "passive"))
    (pad "4" smd circle locked (at 6.82 7.62 180) (size 1.78 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/-12V") (pinfunction "-VOUT") (pintype "passive"))
    (pad "5" smd circle locked (at 6.82 3.81 180) (size 1.78 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/-12V") (pinfunction "-SENSE") (pintype "passive"))
    (pad "6" smd circle locked (at 6.82 0 180) (size 1.78 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(PS1-Pad6)") (pinfunction "TRIM") (pintype "passive"))
    (pad "7" smd circle locked (at 6.82 -3.81 180) (size 1.78 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C5-Pad1)") (pinfunction "+SENSE") (pintype "passive"))
    (pad "8" smd circle locked (at 6.82 -7.62 180) (size 1.78 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(C5-Pad1)") (pinfunction "+VOUT") (pintype "passive"))
    (model "D:\\Documents\\KiCad\\6.0\\SamacSys_Parts.3dshapes\\ULT-12_2.5-D48NM-C.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 100.369 114.25 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at -0.25 -1.881 90) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 160 67)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.5 99.975 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85 -270) (layer "F.SilkS"))
    (fp_text value "1μF" (at 0 1.85 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "/HS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 72.25 120.2375 -90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at -4.575 -2.885 90) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.6 0 270) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 270) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "SamacSys_Parts:AK3066CY" (layer "F.Cu")
    (tedit 0)
    (at 136 90.5745 90)
    (descr "AK3-066C-Y-1")
    (tags "TVS Diode (Bi-directional)")
    (property "Description" "ESD Suppressors / TVS Diodes TVS DIODE AXIAL")
    (property "Height" "11")
    (property "Manufacturer_Name" "LITTELFUSE")
    (property "Manufacturer_Part_Number" "AK3-066C-Y")
    (property "Mouser Part Number" "576-AK3-066C-Y")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Littelfuse/AK3-066C-Y?qs=P1JMDcb91o7SsHSLqUW48g%3D%3D")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 12.074 0 90) (layer "F.SilkS"))
    (fp_text value "AK3-066C-Y" (at 12.074 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 12.074 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 2.205 2.205) (drill 1.47) (layers *.Cu *.Mask)
      (net 1 "/HS") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 24.15 0 90) (size 2.205 2.205) (drill 1.47) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "B2B-XH-A_LF__SN_:JST_B2B-XH-A(LF)(SN)" (layer "F.Cu")
    (tedit 62CEDF5E)
    (at 99 85)
    (property "AVAILABILITY" "In Stock")
    (property "DESCRIPTION" "Connector Header Through Hole 2 position 0.098 (2.50mm)")
    (property "MF" "JST Sales")
    (property "MP" "B2B-XH-A(LF)(SN)")
    (property "PACKAGE" "None")
    (property "PRICE" "None")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -5 -0.525 180) (layer "F.SilkS"))
    (fp_text value "B2B-XH-A(LF)(SN)" (at 8.75 4.11) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 1.25 0) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -1.25 0) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/-12V") (pinfunction "2") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/B2B-XH-A_LF__SN_.pretty/B2B-XH-A_LF__SN_.step"
      (offset (xyz 0 0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" locked (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 59 138)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_2220_5650Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 99 77.5 180)
    (descr "Capacitor SMD 2220 (5650 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at -5 3) (layer "F.SilkS"))
    (fp_text value "47μF" (at 0 3.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 180) (size 1.8 5.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.138889)
      (net 10 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 180) (size 1.8 5.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.138889)
      (net 3 "/-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_2220_5650Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 127.5 126)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_2.2mm_M2" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (footprint "benbokser:FT Power Switch" (layer "F.Cu")
    (tedit 0)
    (at 119 112.5 90)
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at -4.445 -4.445 90 unlocked) (layer "F.SilkS"))
    (fp_text value "FT_Power_Switch" (at 0 4.445 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 8.89 2.54 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at -3 0 90) (size 3 5.5) (drill oval 1.3 4) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(J1-PadP)") (pintype "passive"))
    (pad "2" thru_hole roundrect (at 3 0 90) (size 3 5.5) (drill oval 1.3 4) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "/HS") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/benbokser.pretty/MINI POWER SWITCH.STEP"
      (offset (xyz 1.9 -0.4 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 90))
    )
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 146.75 84.9625 90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -4.575 -2.885 90) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.6 0 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.6 0 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 90) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 90) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.469 118.45 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 1.969 90) (layer "F.SilkS"))
    (fp_text value "22kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D4-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/HS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.5 99.975 -90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.85 -270) (layer "F.SilkS"))
    (fp_text value "1μF" (at 0 1.85 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 1 "/HS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.475 0 270) (size 1.15 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.217391)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_8x10" (layer "F.Cu")
    (tedit 5BCA39D0)
    (at 97.5 94 180)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 8.0x10mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -5.2) (layer "F.SilkS"))
    (fp_text value "33μF" (at 0 5.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.25 0 180) (size 3.5 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 1 "/HS") (pintype "passive"))
    (pad "2" smd roundrect (at 3.25 0 180) (size 3.5 2.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_8x10.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 95.469 114.25 -90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at -0.25 1.969 90) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "benbokser:AC03000003600JAC00" (layer "F.Cu")
    (tedit 0)
    (at 100 135.5 180)
    (descr "B12")
    (tags "Resistor")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 10 4 180) (layer "F.SilkS"))
    (fp_text value "365Ω" (at 0 0 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 7 "Net-(J8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 20 0 180) (size 1.575 1.575) (drill 1.05) (layers *.Cu *.Mask)
      (net 1 "/HS") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/benbokser.pretty/AC03000003600JAC00.STEP"
      (offset (xyz 10 0 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.369 118.5 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -0.25 -1.881 90) (layer "F.SilkS"))
    (fp_text value "22kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.5 0.8 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "XT60PW-F:AMASS_XT60PW-F" (layer "F.Cu")
    (tedit 62CE43DE)
    (at 146.75 102.6625 90)
    (property "MANUFACTURER" "AMASS")
    (property "MAXIMUM_PACKAGE_HEIGHT" "8.4 mm")
    (property "PARTREV" "V1.2")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at -4.575 -2.885 90) (layer "F.SilkS"))
    (fp_text value "XT60PW-F" (at 1.14 16.385 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.6 0 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 "/HS") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 3.6 0 90) (size 3.716 3.716) (drill 2.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "S1" thru_hole oval (at -6.75 6 90) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S2" thru_hole oval (at 6.75 6 90) (size 1.3 2.6) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "SHIELD") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/XT60PW-F.pretty/XT60PW-F.step"
      (offset (xyz 0 -15.5 4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "B2B-XH-A_LF__SN_:JST_B2B-XH-A(LF)(SN)" (layer "F.Cu")
    (tedit 62CEDF5E)
    (at 97.369 125.5 180)
    (property "AVAILABILITY" "In Stock")
    (property "DESCRIPTION" "Connector Header Through Hole 2 position 0.098 (2.50mm)")
    (property "MF" "JST Sales")
    (property "MP" "B2B-XH-A(LF)(SN)")
    (property "PACKAGE" "None")
    (property "PRICE" "None")
    (property "Sheetfile" "hopper-power-dist.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 5.869 0) (layer "F.SilkS"))
    (fp_text value "B2B-XH-A(LF)(SN)" (at 8.75 4.11) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 1.25 0 180) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J8-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -1.25 0 180) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-PadP)") (pinfunction "2") (pintype "passive"))
    (model "D:/Documents/KiCad/6.0/footprints/B2B-XH-A_LF__SN_.pretty/B2B-XH-A_LF__SN_.step"
      (offset (xyz 0 0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_rect locked (start 55 63) (end 164 142) (layer "Edge.Cuts") (width 0.2) (fill none))
  (gr_text "Bokser\nhopper-power-dist rev01\n07-24-22" (at 79.25 107) (layer "F.SilkS"))
  (zone (net 10) (net_name "Net-(C5-Pad1)") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 85.5)
        (xy 127.5 88)
        (xy 82 88)
        (xy 79.5 85.5)
        (xy 79.5 63)
        (xy 130 63)
      )
    )
  )
  (zone (net 1) (net_name "/HS") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.5 88)
        (xy 79.5 91)
        (xy 130 91)
        (xy 133 88)
        (xy 133 63)
        (xy 164 63)
        (xy 164 142)
        (xy 55 142)
        (xy 55 63)
        (xy 76.5 63)
      )
    )
  )
  (zone (net 3) (net_name "/-12V") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130 85.5)
        (xy 127.5 88)
        (xy 82 88)
        (xy 79.5 85.5)
        (xy 79.5 63)
        (xy 130 63)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.5 88)
        (xy 79.5 91)
        (xy 130 91)
        (xy 133 88)
        (xy 133 63)
        (xy 164 63)
        (xy 164 142)
        (xy 55 142)
        (xy 55 63)
        (xy 76.5 63)
      )
    )
  )
)
