(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 425)
    (no_connects 0)
    (area 103.199999 46.572 166.806223 131.095)
    (thickness 1.6)
    (drawings 6)
    (tracks 3213)
    (zones 0)
    (modules 115)
    (nets 183)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.18)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.5)
    (via_size 0.5)
    (via_drill 0.3302)
    (via_min_size 0.5)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /VCCINT)
  (net 4 +3V3)
  (net 5 +2V8)
  (net 6 +3V3_FLASH)
  (net 7 "Net-(C28-Pad1)")
  (net 8 "Net-(C29-Pad1)")
  (net 9 "Net-(C31-Pad1)")
  (net 10 "Net-(C32-Pad1)")
  (net 11 /SD_RSV/DAT1)
  (net 12 /SD_D0/MISO/DAT0)
  (net 13 /SD_CLK)
  (net 14 /SD_D1/MOSI/CMD)
  (net 15 /SD_CS/DAT3/CD)
  (net 16 /SD_NC/DAT2)
  (net 17 "Net-(D2-Pad2)")
  (net 18 "Net-(D2-Pad1)")
  (net 19 "Net-(D3-Pad2)")
  (net 20 "Net-(D4-Pad2)")
  (net 21 "Net-(D5-Pad2)")
  (net 22 "Net-(D6-Pad2)")
  (net 23 "Net-(D7-Pad2)")
  (net 24 "Net-(D8-Pad2)")
  (net 25 "Net-(D9-Pad2)")
  (net 26 /SCK)
  (net 27 /AVR_F0)
  (net 28 /AVR_MOSI)
  (net 29 /AVR_F4)
  (net 30 /AVR_MISO)
  (net 31 /AVR_F5)
  (net 32 /AVR_F1)
  (net 33 /SR_M1)
  (net 34 /CB_RST_3V3)
  (net 35 "Net-(J5-Pad3)")
  (net 36 /SR_CSI_B)
  (net 37 /CB_PWDN_3V3)
  (net 38 "Net-(J6-Pad3)")
  (net 39 /SR_RDWR)
  (net 40 /CA_PWDN_3V3)
  (net 41 "Net-(J7-Pad3)")
  (net 42 /SR_M0)
  (net 43 /CA_RST_3V3)
  (net 44 "Net-(J8-Pad3)")
  (net 45 /VBUS)
  (net 46 "Net-(P2-Pad2)")
  (net 47 "Net-(P2-Pad3)")
  (net 48 /CAM_GPIO)
  (net 49 /CAM_CLK)
  (net 50 /CAM_SCL)
  (net 51 /CAM_SDA)
  (net 52 "Net-(P3-Pad15)")
  (net 53 /CA_PWDN)
  (net 54 /CA_HREF)
  (net 55 /CAB_SDA)
  (net 56 /CA_D6)
  (net 57 /CA_D4)
  (net 58 /CA_D2)
  (net 59 /CA_D0)
  (net 60 "Net-(P4-Pad13)")
  (net 61 /CA_D7)
  (net 62 /CA_D5)
  (net 63 /CAB_XCLK)
  (net 64 /CA_D3)
  (net 65 /CAB_SCL)
  (net 66 /CA_D1)
  (net 67 /CA_VSYNC)
  (net 68 /CA_PCLK)
  (net 69 "Net-(P4-Pad18)")
  (net 70 /CA_RST)
  (net 71 /CB_PWDN)
  (net 72 /CB_HREF)
  (net 73 /CB_D6)
  (net 74 /CB_D4)
  (net 75 /CB_D2)
  (net 76 /CB_D0)
  (net 77 "Net-(P5-Pad13)")
  (net 78 /CB_D7)
  (net 79 /CB_D5)
  (net 80 /CB_D3)
  (net 81 /CB_D1)
  (net 82 /CB_VSYNC)
  (net 83 /CB_PCLK)
  (net 84 "Net-(P5-Pad18)")
  (net 85 /CB_RST)
  (net 86 /TDI)
  (net 87 /TCK)
  (net 88 /TMS)
  (net 89 /TDO)
  (net 90 /DONE)
  (net 91 /D-)
  (net 92 /D+)
  (net 93 "Net-(R3-Pad1)")
  (net 94 /AVR_RESET)
  (net 95 /CS_FLASH)
  (net 96 "Net-(R8-Pad1)")
  (net 97 "Net-(R17-Pad2)")
  (net 98 "Net-(R18-Pad1)")
  (net 99 "Net-(R19-Pad2)")
  (net 100 "Net-(RN1-Pad8)")
  (net 101 "Net-(RN1-Pad9)")
  (net 102 /PROGRAM_B)
  (net 103 /INIT_B)
  (net 104 /CLK)
  (net 105 /~SR_QE)
  (net 106 /SS)
  (net 107 /D0)
  (net 108 /CCLK)
  (net 109 /AVR_RX)
  (net 110 /AVR_TX)
  (net 111 /SR_SER)
  (net 112 /SR_SRCLK)
  (net 113 /SR_RCLK)
  (net 114 /D3)
  (net 115 /D2)
  (net 116 /D1)
  (net 117 "Net-(U7-Pad36)")
  (net 118 "Net-(U7-Pad37)")
  (net 119 /DR0_A7)
  (net 120 /DR0_A8)
  (net 121 /DR0_A9)
  (net 122 /DR0_A10)
  (net 123 /DR0_A11)
  (net 124 /DR0_A12)
  (net 125 /DR0_DQ0)
  (net 126 /DR0_DQ1)
  (net 127 /DR0_DQ2)
  (net 128 /DR0_DQ3)
  (net 129 /DR0_DQ4)
  (net 130 /DR0_DQ5)
  (net 131 /DR0_DQ6)
  (net 132 /DR0_DQ7)
  (net 133 /DR0_DQ8)
  (net 134 /DR0_DQ9)
  (net 135 /DR0_DQ10)
  (net 136 /DR0_DQ11)
  (net 137 /DR0_DQ12)
  (net 138 /DR0_DQ13)
  (net 139 /DR0_DQ14)
  (net 140 /DR0_DQ15)
  (net 141 /DR0_WE#)
  (net 142 /DR0_CAS#)
  (net 143 /HD0N)
  (net 144 /HD0P)
  (net 145 /HDCEC)
  (net 146 /HDSCL)
  (net 147 /HD1N)
  (net 148 /HD1P)
  (net 149 /HDSDA)
  (net 150 /HDHPD)
  (net 151 /HD2N)
  (net 152 /HD2P)
  (net 153 /DR0_BA0)
  (net 154 /DR0_BA1)
  (net 155 /HDCLKN)
  (net 156 /HDCLKP)
  (net 157 /DR0_RAS#)
  (net 158 /DR0_CKE)
  (net 159 /DR0_CLK)
  (net 160 /DR0_LDQM)
  (net 161 /DR0_UDQM)
  (net 162 /DR0_A0)
  (net 163 /DR0_A1)
  (net 164 /DR0_A2)
  (net 165 /DR0_A3)
  (net 166 /DR0_A4)
  (net 167 /DR0_A5)
  (net 168 /DR0_A6)
  (net 169 /HDCLKP_O)
  (net 170 /HDCLKN_O)
  (net 171 /HD2P_O)
  (net 172 /HD2N_O)
  (net 173 /HD1P_O)
  (net 174 /HD1N_O)
  (net 175 /HD0P_O)
  (net 176 /HD0N_O)
  (net 177 /CAM_D0_N)
  (net 178 /CAM_D0_P)
  (net 179 /CAM_D1_N)
  (net 180 /CAM_D1_P)
  (net 181 /CAM_C_N)
  (net 182 /CAM_C_P)
  (net_class Default "This is the default net class."
    (clearance 0.18)
    (trace_width 0.25)
    (via_dia 0.5)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +2V8)
    (add_net +3V3)
    (add_net +3V3_FLASH)
    (add_net +5V)
    (add_net /AVR_F0)
    (add_net /AVR_F1)
    (add_net /AVR_F4)
    (add_net /AVR_F5)
    (add_net /AVR_MISO)
    (add_net /AVR_MOSI)
    (add_net /AVR_RESET)
    (add_net /AVR_RX)
    (add_net /AVR_TX)
    (add_net /CAB_SCL)
    (add_net /CAB_SDA)
    (add_net /CAB_XCLK)
    (add_net /CAM_CLK)
    (add_net /CAM_GPIO)
    (add_net /CAM_SCL)
    (add_net /CAM_SDA)
    (add_net /CA_D0)
    (add_net /CA_D1)
    (add_net /CA_D2)
    (add_net /CA_D3)
    (add_net /CA_D4)
    (add_net /CA_D5)
    (add_net /CA_D6)
    (add_net /CA_D7)
    (add_net /CA_HREF)
    (add_net /CA_PCLK)
    (add_net /CA_PWDN)
    (add_net /CA_PWDN_3V3)
    (add_net /CA_RST)
    (add_net /CA_RST_3V3)
    (add_net /CA_VSYNC)
    (add_net /CB_D0)
    (add_net /CB_D1)
    (add_net /CB_D2)
    (add_net /CB_D3)
    (add_net /CB_D4)
    (add_net /CB_D5)
    (add_net /CB_D6)
    (add_net /CB_D7)
    (add_net /CB_HREF)
    (add_net /CB_PCLK)
    (add_net /CB_PWDN)
    (add_net /CB_PWDN_3V3)
    (add_net /CB_RST)
    (add_net /CB_RST_3V3)
    (add_net /CB_VSYNC)
    (add_net /CCLK)
    (add_net /CLK)
    (add_net /CS_FLASH)
    (add_net /D+)
    (add_net /D-)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /DONE)
    (add_net /DR0_A0)
    (add_net /DR0_A1)
    (add_net /DR0_A10)
    (add_net /DR0_A11)
    (add_net /DR0_A12)
    (add_net /DR0_A2)
    (add_net /DR0_A3)
    (add_net /DR0_A4)
    (add_net /DR0_A5)
    (add_net /DR0_A6)
    (add_net /DR0_A7)
    (add_net /DR0_A8)
    (add_net /DR0_A9)
    (add_net /DR0_BA0)
    (add_net /DR0_BA1)
    (add_net /DR0_CAS#)
    (add_net /DR0_CKE)
    (add_net /DR0_CLK)
    (add_net /DR0_DQ0)
    (add_net /DR0_DQ1)
    (add_net /DR0_DQ10)
    (add_net /DR0_DQ11)
    (add_net /DR0_DQ12)
    (add_net /DR0_DQ13)
    (add_net /DR0_DQ14)
    (add_net /DR0_DQ15)
    (add_net /DR0_DQ2)
    (add_net /DR0_DQ3)
    (add_net /DR0_DQ4)
    (add_net /DR0_DQ5)
    (add_net /DR0_DQ6)
    (add_net /DR0_DQ7)
    (add_net /DR0_DQ8)
    (add_net /DR0_DQ9)
    (add_net /DR0_LDQM)
    (add_net /DR0_RAS#)
    (add_net /DR0_UDQM)
    (add_net /DR0_WE#)
    (add_net /HD0N)
    (add_net /HD0N_O)
    (add_net /HD0P)
    (add_net /HD0P_O)
    (add_net /HD1N)
    (add_net /HD1N_O)
    (add_net /HD1P)
    (add_net /HD1P_O)
    (add_net /HD2N)
    (add_net /HD2N_O)
    (add_net /HD2P)
    (add_net /HD2P_O)
    (add_net /HDCEC)
    (add_net /HDCLKN)
    (add_net /HDCLKN_O)
    (add_net /HDCLKP)
    (add_net /HDCLKP_O)
    (add_net /HDHPD)
    (add_net /HDSCL)
    (add_net /HDSDA)
    (add_net /INIT_B)
    (add_net /PROGRAM_B)
    (add_net /SCK)
    (add_net /SD_CLK)
    (add_net /SD_CS/DAT3/CD)
    (add_net /SD_D0/MISO/DAT0)
    (add_net /SD_D1/MOSI/CMD)
    (add_net /SD_NC/DAT2)
    (add_net /SD_RSV/DAT1)
    (add_net /SR_CSI_B)
    (add_net /SR_M0)
    (add_net /SR_M1)
    (add_net /SR_RCLK)
    (add_net /SR_RDWR)
    (add_net /SR_SER)
    (add_net /SR_SRCLK)
    (add_net /SS)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /VBUS)
    (add_net /VCCINT)
    (add_net /~SR_QE)
    (add_net GND)
    (add_net "Net-(C28-Pad1)")
    (add_net "Net-(C29-Pad1)")
    (add_net "Net-(C31-Pad1)")
    (add_net "Net-(C32-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J7-Pad3)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P3-Pad15)")
    (add_net "Net-(P4-Pad13)")
    (add_net "Net-(P4-Pad18)")
    (add_net "Net-(P5-Pad13)")
    (add_net "Net-(P5-Pad18)")
    (add_net "Net-(R17-Pad2)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R19-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(RN1-Pad8)")
    (add_net "Net-(RN1-Pad9)")
    (add_net "Net-(U7-Pad36)")
    (add_net "Net-(U7-Pad37)")
  )
  (net_class DPAIR ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CAM_C_N)
    (add_net /CAM_C_P)
    (add_net /CAM_D0_N)
    (add_net /CAM_D0_P)
    (add_net /CAM_D1_N)
    (add_net /CAM_D1_P)
  )
  (module visionFeet:WurthFFC_1mm_15 (layer F.Cu) (tedit 0)
    (at 150.274 122.449)
    (fp_text reference P3 (at 0 2.15) (layer F.SilkS))
    (fp_text value CONN_01X15 (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -7 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -6 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 177 /CAM_D0_N))
    (pad 3 smd rect (at -5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 178 /CAM_D0_P))
    (pad 4 smd rect (at -4 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at -3 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 179 /CAM_D1_N))
    (pad 6 smd rect (at -2 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 180 /CAM_D1_P))
    (pad 7 smd rect (at -1 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 0 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 181 /CAM_C_N))
    (pad 9 smd rect (at 1 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 182 /CAM_C_P))
    (pad 10 smd rect (at 2 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 3 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 48 /CAM_GPIO))
    (pad 12 smd rect (at 4 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 49 /CAM_CLK))
    (pad 13 smd rect (at 5 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 50 /CAM_SCL))
    (pad 14 smd rect (at 6 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 51 /CAM_SDA))
    (pad 15 smd rect (at 7 0) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(P3-Pad15)"))
    (pad 0 smd rect (at -10 2.9) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 10 2.9) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
  )
  (module visionFeet:CON-HDMI-Amphenol-10029449 (layer F.Cu) (tedit 588AE694)
    (at 129.667 58.547 180)
    (fp_text reference U12 (at 0.5 2 180) (layer F.SilkS))
    (fp_text value CON-HDMI (at 0 11 180) (layer F.Fab))
    (pad 1 smd rect (at 4.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 171 /HD2P_O))
    (pad 2 smd rect (at 4.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 3.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 172 /HD2N_O))
    (pad 4 smd rect (at 3.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 173 /HD1P_O))
    (pad 5 smd rect (at 2.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 174 /HD1N_O))
    (pad 7 smd rect (at 1.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 175 /HD0P_O))
    (pad 8 smd rect (at 1.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 0.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 176 /HD0N_O))
    (pad 10 smd rect (at 0.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 169 /HDCLKP_O))
    (pad 11 smd rect (at -0.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -0.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 170 /HDCLKN_O))
    (pad 13 smd rect (at -1.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 145 /HDCEC))
    (pad 14 smd rect (at -1.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at -2.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 146 /HDSCL))
    (pad 16 smd rect (at -2.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 149 /HDSDA))
    (pad 17 smd rect (at -3.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at -3.75 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 19 smd rect (at -4.25 -1 180) (size 0.3 1.9) (layers F.Cu F.Paste F.Mask)
      (net 150 /HDHPD))
    (pad "" thru_hole circle (at -7.25 0 180) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -7.85 4.9 180) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 7.85 4.9 180) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 7.25 0 180) (size 1.8 1.8) (drill 1.3) (layers *.Cu *.Mask))
  )
  (module visionFeet:TQFP-144_20x20mm_0.5mm_HS (layer F.Cu) (tedit 54130A77)
    (at 133.085001 76.75)
    (descr "P/PG-TQFP-144-2, -3, -7 (see MAXIM 21-0087.PDF and 90-0144.PDF)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U8 (at -0.035001 -0.05) (layer F.SilkS))
    (fp_text value XC6SLX9-TQFP144 (at 0 7.07) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -10.8 -8.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 161 /DR0_UDQM))
    (pad 2 smd rect (at -10.8 -8.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 120 /DR0_A8))
    (pad 3 smd rect (at -10.8 -7.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -10.8 -7.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 5 smd rect (at -10.8 -6.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 160 /DR0_LDQM))
    (pad 6 smd rect (at -10.8 -6.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 121 /DR0_A9))
    (pad 7 smd rect (at -10.8 -5.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 123 /DR0_A11))
    (pad 8 smd rect (at -10.8 -5.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 124 /DR0_A12))
    (pad 9 smd rect (at -10.8 -4.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 132 /DR0_DQ7))
    (pad 10 smd rect (at -10.8 -4.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 131 /DR0_DQ6))
    (pad 11 smd rect (at -10.8 -3.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 130 /DR0_DQ5))
    (pad 12 smd rect (at -10.8 -3.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 129 /DR0_DQ4))
    (pad 13 smd rect (at -10.8 -2.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -10.8 -2.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 128 /DR0_DQ3))
    (pad 15 smd rect (at -10.8 -1.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 127 /DR0_DQ2))
    (pad 16 smd rect (at -10.8 -1.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 158 /DR0_CKE))
    (pad 17 smd rect (at -10.8 -0.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 159 /DR0_CLK))
    (pad 18 smd rect (at -10.8 -0.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 19 smd rect (at -10.8 0.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 20 smd rect (at -10.8 0.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 21 smd rect (at -10.8 1.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 133 /DR0_DQ8))
    (pad 22 smd rect (at -10.8 1.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 134 /DR0_DQ9))
    (pad 23 smd rect (at -10.8 2.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 126 /DR0_DQ1))
    (pad 24 smd rect (at -10.8 2.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 125 /DR0_DQ0))
    (pad 25 smd rect (at -10.8 3.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at -10.8 3.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 135 /DR0_DQ10))
    (pad 27 smd rect (at -10.8 4.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 136 /DR0_DQ11))
    (pad 28 smd rect (at -10.8 4.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 29 smd rect (at -10.8 5.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 137 /DR0_DQ12))
    (pad 30 smd rect (at -10.8 5.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 138 /DR0_DQ13))
    (pad 31 smd rect (at -10.8 6.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 32 smd rect (at -10.8 6.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 139 /DR0_DQ14))
    (pad 33 smd rect (at -10.8 7.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 140 /DR0_DQ15))
    (pad 34 smd rect (at -10.8 7.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 /CAM_SDA))
    (pad 35 smd rect (at -10.8 8.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 /CAM_SCL))
    (pad 36 smd rect (at -10.8 8.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 37 smd rect (at -8.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 102 /PROGRAM_B))
    (pad 38 smd rect (at -8.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 /CB_D0))
    (pad 39 smd rect (at -7.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 103 /INIT_B))
    (pad 40 smd rect (at -7.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 177 /CAM_D0_N))
    (pad 41 smd rect (at -6.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 178 /CAM_D0_P))
    (pad 42 smd rect (at -6.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 43 smd rect (at -5.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /SCK))
    (pad 44 smd rect (at -5.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 /AVR_MOSI))
    (pad 45 smd rect (at -4.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 /AVR_MISO))
    (pad 46 smd rect (at -4.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 114 /D3))
    (pad 47 smd rect (at -3.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 /CA_PWDN_3V3))
    (pad 48 smd rect (at -3.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 106 /SS))
    (pad 49 smd rect (at -2.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 50 smd rect (at -2.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 179 /CAM_D1_N))
    (pad 51 smd rect (at -1.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 180 /CAM_D1_P))
    (pad 52 smd rect (at -1.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 53 smd rect (at -0.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 54 smd rect (at -0.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 55 smd rect (at 0.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 110 /AVR_TX))
    (pad 56 smd rect (at 0.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 104 /CLK))
    (pad 57 smd rect (at 1.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 /CAM_GPIO))
    (pad 58 smd rect (at 1.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 /CAM_CLK))
    (pad 59 smd rect (at 2.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 109 /AVR_RX))
    (pad 60 smd rect (at 2.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 /CB_RST_3V3))
    (pad 61 smd rect (at 3.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 115 /D2))
    (pad 62 smd rect (at 3.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 116 /D1))
    (pad 63 smd rect (at 4.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 64 smd rect (at 4.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 /CB_PWDN_3V3))
    (pad 65 smd rect (at 5.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 107 /D0))
    (pad 66 smd rect (at 5.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 181 /CAM_C_N))
    (pad 67 smd rect (at 6.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 182 /CAM_C_P))
    (pad 68 smd rect (at 6.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 69 smd rect (at 7.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 /CA_RST_3V3))
    (pad 70 smd rect (at 7.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 108 /CCLK))
    (pad 71 smd rect (at 8.25 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 90 /DONE))
    (pad 72 smd rect (at 8.75 10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask))
    (pad 73 smd rect (at 10.8 8.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(R3-Pad1)"))
    (pad 74 smd rect (at 10.8 8.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 67 /CA_VSYNC))
    (pad 75 smd rect (at 10.8 7.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 65 /CAB_SCL))
    (pad 76 smd rect (at 10.8 7.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +2V8))
    (pad 77 smd rect (at 10.8 6.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 78 smd rect (at 10.8 6.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 /CA_HREF))
    (pad 79 smd rect (at 10.8 5.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 /CAB_SDA))
    (pad 80 smd rect (at 10.8 5.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /CA_D6))
    (pad 81 smd rect (at 10.8 4.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 /CA_D4))
    (pad 82 smd rect (at 10.8 4.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 /CA_D2))
    (pad 83 smd rect (at 10.8 3.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 /CA_D0))
    (pad 84 smd rect (at 10.8 3.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 61 /CA_D7))
    (pad 85 smd rect (at 10.8 2.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 /CA_D5))
    (pad 86 smd rect (at 10.8 2.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +2V8))
    (pad 87 smd rect (at 10.8 1.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 64 /CA_D3))
    (pad 88 smd rect (at 10.8 1.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 66 /CA_D1))
    (pad 89 smd rect (at 10.8 0.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 90 smd rect (at 10.8 0.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 91 smd rect (at 10.8 -0.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 92 smd rect (at 10.8 -0.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 68 /CA_PCLK))
    (pad 93 smd rect (at 10.8 -1.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 83 /CB_PCLK))
    (pad 94 smd rect (at 10.8 -1.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 82 /CB_VSYNC))
    (pad 95 smd rect (at 10.8 -2.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 /CAB_XCLK))
    (pad 96 smd rect (at 10.8 -2.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 97 smd rect (at 10.8 -3.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 /CB_HREF))
    (pad 98 smd rect (at 10.8 -3.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 /CB_D6))
    (pad 99 smd rect (at 10.8 -4.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 /CB_D4))
    (pad 100 smd rect (at 10.8 -4.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 /CB_D2))
    (pad 101 smd rect (at 10.8 -5.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 /CB_D7))
    (pad 102 smd rect (at 10.8 -5.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 /CB_D5))
    (pad 103 smd rect (at 10.8 -6.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +2V8))
    (pad 104 smd rect (at 10.8 -6.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 80 /CB_D3))
    (pad 105 smd rect (at 10.8 -7.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 81 /CB_D1))
    (pad 106 smd rect (at 10.8 -7.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 89 /TDO))
    (pad 107 smd rect (at 10.8 -8.25) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 88 /TMS))
    (pad 108 smd rect (at 10.8 -8.75) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 109 smd rect (at 8.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 87 /TCK))
    (pad 110 smd rect (at 8.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 86 /TDI))
    (pad 111 smd rect (at 7.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 143 /HD0N))
    (pad 112 smd rect (at 7.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 144 /HD0P))
    (pad 113 smd rect (at 6.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 114 smd rect (at 6.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 150 /HDHPD))
    (pad 115 smd rect (at 5.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 149 /HDSDA))
    (pad 116 smd rect (at 5.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 147 /HD1N))
    (pad 117 smd rect (at 4.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 148 /HD1P))
    (pad 118 smd rect (at 4.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 146 /HDSCL))
    (pad 119 smd rect (at 3.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 145 /HDCEC))
    (pad 120 smd rect (at 3.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 151 /HD2N))
    (pad 121 smd rect (at 2.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 152 /HD2P))
    (pad 122 smd rect (at 2.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 123 smd rect (at 1.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 155 /HDCLKN))
    (pad 124 smd rect (at 1.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 156 /HDCLKP))
    (pad 125 smd rect (at 0.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 126 smd rect (at 0.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 165 /DR0_A3))
    (pad 127 smd rect (at -0.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 164 /DR0_A2))
    (pad 128 smd rect (at -0.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 129 smd rect (at -1.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 130 smd rect (at -1.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 131 smd rect (at -2.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 163 /DR0_A1))
    (pad 132 smd rect (at -2.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 162 /DR0_A0))
    (pad 133 smd rect (at -3.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 122 /DR0_A10))
    (pad 134 smd rect (at -3.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 154 /DR0_BA1))
    (pad 135 smd rect (at -4.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 136 smd rect (at -4.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 137 smd rect (at -5.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 153 /DR0_BA0))
    (pad 138 smd rect (at -5.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 166 /DR0_A4))
    (pad 139 smd rect (at -6.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 167 /DR0_A5))
    (pad 140 smd rect (at -6.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 168 /DR0_A6))
    (pad 141 smd rect (at -7.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 157 /DR0_RAS#))
    (pad 142 smd rect (at -7.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 119 /DR0_A7))
    (pad 143 smd rect (at -8.25 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 141 /DR0_WE#))
    (pad 144 smd rect (at -8.75 -10.8 90) (size 1.95 0.25) (layers F.Cu F.Paste F.Mask)
      (net 142 /DR0_CAS#))
    (model Housings_QFP.3dshapes/TQFP-144_20x20mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 111.05 94.25 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C30 (at 0.1 1.45 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:SOIC-8_3.9x4.9mm_p1.27mm_HS (layer B.Cu) (tedit 54130A77)
    (at 120.036 106.172 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at -0.064 0.022 180) (layer B.SilkS))
    (fp_text value M25P40-VMN6TPBCT-ND (at 0 -3.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2.9 1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 95 /CS_FLASH))
    (pad 2 smd rect (at -2.9 0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 30 /AVR_MISO))
    (pad 3 smd rect (at -2.9 -0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R18-Pad1)"))
    (pad 4 smd rect (at -2.9 -1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.9 -1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /AVR_MOSI))
    (pad 6 smd rect (at 2.9 -0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 26 /SCK))
    (pad 7 smd rect (at 2.9 0.635 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 99 "Net-(R19-Pad2)"))
    (pad 8 smd rect (at 2.9 1.905 180) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3_FLASH))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:TQFP-44_10x10mm_p0.8mm-HS (layer F.Cu) (tedit 588ED7E7)
    (at 113.221 96.666)
    (descr "44-Lead Plastic Thin Quad Flatpack (PT) - 10x10x1.0 mm Body [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U7 (at 0.329 -0.166) (layer F.SilkS))
    (fp_text value ATMEGA32U4-A (at 0 7.45) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -5.95 -4) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 105 /~SR_QE))
    (pad 2 smd rect (at -5.95 -3.2) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -5.95 -2.4) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 91 /D-))
    (pad 4 smd rect (at -5.95 -1.6) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 92 /D+))
    (pad 5 smd rect (at -5.95 -0.8) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -5.95 0) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 7 smd rect (at -5.95 0.8) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /VBUS))
    (pad 8 smd rect (at -5.95 1.6) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 106 /SS))
    (pad 9 smd rect (at -5.95 2.4) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /SCK))
    (pad 10 smd rect (at -5.95 3.2) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /AVR_MOSI))
    (pad 11 smd rect (at -5.95 4) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /AVR_MISO))
    (pad 12 smd rect (at -4 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 107 /D0))
    (pad 13 smd rect (at -3.2 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 94 /AVR_RESET))
    (pad 14 smd rect (at -2.4 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 15 smd rect (at -1.6 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at -0.8 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C31-Pad1)"))
    (pad 17 smd rect (at 0 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C29-Pad1)"))
    (pad 18 smd rect (at 0.8 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 108 /CCLK))
    (pad 19 smd rect (at 1.6 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 95 /CS_FLASH))
    (pad 20 smd rect (at 2.4 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 109 /AVR_RX))
    (pad 21 smd rect (at 3.2 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 110 /AVR_TX))
    (pad 22 smd rect (at 4 5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 103 /INIT_B))
    (pad 23 smd rect (at 5.95 4) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 5.95 3.2) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C28-Pad1)"))
    (pad 25 smd rect (at 5.95 2.4) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 111 /SR_SER))
    (pad 26 smd rect (at 5.95 1.6) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 112 /SR_SRCLK))
    (pad 27 smd rect (at 5.95 0.8) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 113 /SR_RCLK))
    (pad 28 smd rect (at 5.95 0) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 114 /D3))
    (pad 29 smd rect (at 5.95 -0.8) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 115 /D2))
    (pad 30 smd rect (at 5.95 -1.6) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 116 /D1))
    (pad 31 smd rect (at 5.95 -2.4) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 90 /DONE))
    (pad 32 smd rect (at 5.95 -3.2) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 102 /PROGRAM_B))
    (pad 33 smd rect (at 5.95 -4) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(R17-Pad2)"))
    (pad 34 smd rect (at 4 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 35 smd rect (at 3.2 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 36 smd rect (at 2.4 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(U7-Pad36)"))
    (pad 37 smd rect (at 1.6 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(U7-Pad37)"))
    (pad 38 smd rect (at 0.8 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /AVR_F5))
    (pad 39 smd rect (at 0 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /AVR_F4))
    (pad 40 smd rect (at -0.8 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /AVR_F1))
    (pad 41 smd rect (at -1.6 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /AVR_F0))
    (pad 42 smd rect (at -2.4 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C32-Pad1)"))
    (pad 43 smd rect (at -3.2 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd rect (at -4 -5.95 90) (size 2.01 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C28-Pad1)"))
    (model Housings_QFP.3dshapes/TQFP-44_10x10mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 135.8 125.2 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.7 1.4 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 /D-))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 127.2 120.7)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.8 0.7 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /D+))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P2-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 136.398 110.109)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 0 -2.39) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /SR_M0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /CA_RST_3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J8-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-U_EIA-6032-15_Hand (layer F.Cu) (tedit 58910CC0)
    (at 148.64 102.362 180)
    (descr "Tantalum capacitor, Case U, EIA 6032-15, 6.0x3.2x1.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C38 (at 3.69 -3.188 180) (layer F.SilkS))
    (fp_text value 100u (at 0 3.35 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -3.125 0 180) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3_FLASH))
    (pad 2 smd rect (at 3.125 0 180) (size 3.75 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-U_EIA-6032-15.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 146.774 92.202)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.326 -0.002) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58930C68)
    (at 118.021 117.221)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at -1.921 0.029 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58930C61)
    (at 118.021 115.316)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at -1.921 -0.016 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 58930CB1)
    (at 118.021 113.538)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at -1.921 -0.038 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 122.009 116.713 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.25 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 122.009 114.173 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 0 -1.25 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 122.009 112.014 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D8 (at 0 1.214 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 122.25 108.5 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D9 (at 2.05 0.7 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 125.984 100.33)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J1 (at 0 -2.39) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /SCK))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /SD_CLK))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /AVR_F0))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 129.413 100.33)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J2 (at 0 -2.39) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /AVR_MOSI))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SD_D1/MOSI/CMD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /AVR_F4))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 134.874 98.171)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.39) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /AVR_MISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /SD_D0/MISO/DAT0))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /AVR_F5))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 140.081 98.298)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.39) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /SD_CS/DAT3/CD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /AVR_F1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 125.984 110.109)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 -2.39) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /SR_M1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /CB_RST_3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 129.413 110.109)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J6 (at 0 -2.39) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /SR_CSI_B))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /CB_PWDN_3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J6-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 132.969 110.109)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.39) (layer F.SilkS))
    (fp_text value HEADER_3 (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /SR_RDWR))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /CA_PWDN_3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J7-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_smd_inductors:inductor_smd_1008 (layer F.Cu) (tedit 58910E00)
    (at 113.607 109.5 180)
    (descr "Inductor SMD, 1008")
    (fp_text reference L1 (at -1.582 -2.26 180) (layer F.SilkS))
    (fp_text value 10uH (at 0 2.49936 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.143 0 180) (size 1.016 2.54) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.143 0 180) (size 1.016 2.54) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C28-Pad1)"))
    (model walter/smd_inductors/inductor_smd_1008.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_jst-ph:b2b-ph-kl (layer F.Cu) (tedit 58910D49)
    (at 138.44524 120.396 180)
    (descr "JST PH series connector, B2B-PH-KL")
    (fp_text reference P1 (at 0 -2.99974 180) (layer F.SilkS) hide)
    (fp_text value "CON JST 1x2" (at 0 4.20116 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.00076 0 180) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 1.00076 0 180) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model walter/conn_jst-ph/b2b-ph-kl.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 151.13 52.959)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P6 (at -0.127 10.16) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 10.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 /TDI))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 87 /TCK))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /TDO))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 88 /TMS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module w_smd_trans:sot323-6 (layer F.Cu) (tedit 0)
    (at 144.638 89.773)
    (descr SOT323-6)
    (fp_text reference Q1 (at 0 -1.651) (layer F.SilkS))
    (fp_text value MOSFET (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 1) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 90 /DONE) (clearance 0.14))
    (pad 5 smd rect (at 0 -1) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (clearance 0.14))
    (pad 3 smd rect (at 0.65 1) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D2-Pad1)") (clearance 0.14))
    (pad 2 smd rect (at 0 1) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (clearance 0.14))
    (pad 4 smd rect (at 0.65 -1) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (clearance 0.14))
    (pad 6 smd rect (at -0.65 -1) (size 0.5 0.8) (layers F.Cu F.Paste F.Mask)
      (clearance 0.14))
    (model walter/smd_trans/sot323-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 131.9 120.7)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV1 (at 2 1.2) (layer F.SilkS))
    (fp_text value CG0603MLC-05E (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P2-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 118.11 97.112 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference RV2 (at 0.338 1.778 90) (layer B.SilkS))
    (fp_text value CG0603MLC-05E (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(P2-Pad3)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 583F3B4E)
    (at 111.328634 115.83569 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 3.228634 -3.06431 180) (layer F.SilkS))
    (fp_text value NCP1117ST33T3G (at 0 4.5 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 583F3B4E)
    (at 111.540528 83.528204 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 3.290528 3.228204 180) (layer F.SilkS))
    (fp_text value LD1117S12CTR (at 0 4.5 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /VCCINT))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 583F3B4E)
    (at 111.342668 123.791388 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U4 (at 3.342668 -3.008612 180) (layer F.SilkS))
    (fp_text value AP7361-28E-13 (at 0 4.5 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 +2V8))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 583F3B4E)
    (at 120.396 122.936 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U5 (at 3.264 -3.404 360) (layer F.SilkS))
    (fp_text value NCP1117ST33T3G (at 0 4.5 270) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 270) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3_FLASH))
    (pad 3 smd rect (at -3.15 2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Crystals:Crystal_SMD_Abracon_ABM3-2pin_5.0x3.2mm_HandSoldering (layer B.Cu) (tedit 5873B462)
    (at 111.76 85.979 180)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3 http://www.abracon.com/Resonators/abm3.pdf, hand-soldering, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at -3.49 2.629 180) (layer B.SilkS))
    (fp_text value 8MHz (at 0 -2.8 180) (layer B.Fab))
    (pad 1 smd rect (at -2.7625 0 180) (size 3.325 2.4) (layers B.Cu B.Mask)
      (net 9 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 2.7625 0 180) (size 3.325 2.4) (layers B.Cu B.Mask)
      (net 8 "Net-(C29-Pad1)"))
    (model Crystals.3dshapes/Crystal_SMD_Abracon_ABM3-2pin_5.0x3.2mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 111.201634 114.81969 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.632634 -0.87731 180) (layer B.SilkS))
    (fp_text value 4u7 (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 131.485 69.088 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0.548 1.778 180) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 110.47 67.818)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -0.615 -1.778) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 125.857 77.47)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.905 1.651) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 127.762 71.882)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 1.524 1.397) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 111.445 82.169 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 2.987 -0.127 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 111.784668 121.505388 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 3.034668 -0.044612 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 126.238 75.565)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 3.175 1.524) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 112.669 53.467 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 3.195 -0.635 180) (layer F.SilkS))
    (fp_text value 10u (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 126.238 81.915)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 3.462 -0.015) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 134.874 70.993)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 2.032 1.524) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 139.319 77.343 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at -3.81 0.127 180) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 120.142 74.95 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at -1.123 2.032 90) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 139.954 70.485 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 1.9 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 +2V8))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 127.889 84.963)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 1.9) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 111.516634 116.97869 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 3.185634 -1.25831 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 134.112 83.312)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 1.524 -1.524) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 109.22 75.291 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 0 -1.905 270) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 139.827 79.248 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0.254 -1.524 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 +2V8))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 132.654 84.963)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C20 (at 1.396 1.737) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 119.273 122.428)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C21 (at 3.663 0.762) (layer B.SilkS))
    (fp_text value 4u7 (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 115.189 69.215 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C22 (at 0.254 1.397 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 111.526 80.137 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C23 (at -0.869 1.778 180) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /VCCINT))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 111.449668 124.045388 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C24 (at 2.102668 -2.065612 180) (layer B.SilkS))
    (fp_text value 4u7 (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 +2V8))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 116 90.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C25 (at -0.332 -1.575 180) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 140.274 74.422)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C26 (at 3.109 0) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 118.811 125.095)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C27 (at 3.49 0.127) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3_FLASH))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 107.696 91.694 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C28 (at 1.778 1.397 270) (layer B.SilkS))
    (fp_text value 1u (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C28-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 109.281 88.9)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C29 (at -2.581 -0.3 90) (layer B.SilkS))
    (fp_text value 22p (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C29-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 113.218 88.9 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C31 (at 0.618 -1.5 180) (layer B.SilkS))
    (fp_text value 22p (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C31-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 109.027 88.519)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C32 (at 3.523 -0.019) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C32-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 144.338 64.008)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C34 (at 0.012 1.492) (layer F.SilkS))
    (fp_text value 1nF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 541A9B4D)
    (at 139.446 58.862 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C35 (at 3.363 0.127 90) (layer B.SilkS))
    (fp_text value 0.01uF (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 142.875 54.102)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C36 (at 3.175 0.127) (layer F.SilkS))
    (fp_text value 0.01uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 143.129 52.197)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C37 (at 3.683 0) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 149.545 106.75 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C39 (at 0.245 -1.45 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3_FLASH))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 141.478 83.82 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 93 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 110 106.35 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.076 1.923 360) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 94 /AVR_RESET))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 123.25 102.1 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.119 1.584 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 /CS_FLASH))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 138.43 84.963)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0.17 1.837) (layer B.SilkS))
    (fp_text value R (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 90 /DONE))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 145.542 90.424 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.858 1.624 180) (layer B.SilkS))
    (fp_text value 330 (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 148.082 59.309 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.794 -0.127 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 149.86 96.465776 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -3.102224 0.127 90) (layer B.SilkS))
    (fp_text value 1.8k (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 /CA_RST_3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 70 /CA_RST))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 147.955 96.508776 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 3.567224 -0.127 270) (layer B.SilkS))
    (fp_text value 9.6k (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 70 /CA_RST))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 154.686 79.248)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -3.556 0.127) (layer F.SilkS))
    (fp_text value 1.8k (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 /CB_RST_3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 /CB_RST))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 154.686 77.47 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 3.556 0 180) (layer F.SilkS))
    (fp_text value 9.6k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 /CB_RST))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 125.75 117.75 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0.45 -1.65 180) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J5-Pad3)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 130.259 117.729)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 1.821 1.651) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(J6-Pad3)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 132.758 117.729)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0.442 1.371) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J7-Pad3)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58307AEF)
    (at 140.462 115.951)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J8-Pad3)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 119.296 88.011)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0.973 1.524) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 97 "Net-(R17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 113.1 109.75 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 3.372 0.022 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 98 "Net-(R18-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 115.25 104.15 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at -0.127 1.524 270) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3_FLASH))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 99 "Net-(R19-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 143.764 96.635776 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R20 (at 3.440224 0 270) (layer B.SilkS))
    (fp_text value 1.8k (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 40 /CA_PWDN_3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 /CA_PWDN))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 145.923 96.592776 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at 3.483224 -0.254 270) (layer B.SilkS))
    (fp_text value 9.6k (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 53 /CA_PWDN))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 153.289 72.263)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at 4.211 -0.013) (layer B.SilkS))
    (fp_text value 1.8k (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 37 /CB_PWDN_3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 71 /CB_PWDN))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58307AEF)
    (at 153.924 70.485 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at -3.926 -0.015 180) (layer B.SilkS))
    (fp_text value 9.6k (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 71 /CB_PWDN))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:QFN-32-1EP_5x5mm_p0.5mm_HS (layer F.Cu) (tedit 54130A77)
    (at 142.649 59.326 270)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U10 (at 3.424 3.799 360) (layer F.SilkS))
    (fp_text value AD8194 (at 0 3.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2.65 -1.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 151 /HD2N))
    (pad 2 smd rect (at -2.65 -1.25 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 152 /HD2P))
    (pad 3 smd rect (at -2.65 -0.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 4 smd rect (at -2.65 -0.25 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 155 /HDCLKN))
    (pad 5 smd rect (at -2.65 0.25 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 156 /HDCLKP))
    (pad 6 smd rect (at -2.65 0.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 7 smd rect (at -2.65 1.25 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 169 /HDCLKP_O))
    (pad 8 smd rect (at -2.65 1.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 170 /HDCLKN_O))
    (pad 9 smd rect (at -1.75 2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 171 /HD2P_O))
    (pad 10 smd rect (at -1.25 2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 172 /HD2N_O))
    (pad 11 smd rect (at -0.75 2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at -0.25 2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 173 /HD1P_O))
    (pad 13 smd rect (at 0.25 2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 174 /HD1N_O))
    (pad 14 smd rect (at 0.75 2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 15 smd rect (at 1.25 2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 175 /HD0P_O))
    (pad 16 smd rect (at 1.75 2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 176 /HD0N_O))
    (pad 17 smd rect (at 2.65 1.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 18 smd rect (at 2.65 1.25 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 19 smd rect (at 2.65 0.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 20 smd rect (at 2.65 0.25 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 21 smd rect (at 2.65 -0.25 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 22 smd rect (at 2.65 -0.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 23 smd rect (at 2.65 -1.25 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 24 smd rect (at 2.65 -1.75 270) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 25 smd rect (at 1.75 -2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 26 smd rect (at 1.25 -2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(R8-Pad1)"))
    (pad 27 smd rect (at 0.75 -2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 28 smd rect (at 0.25 -2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 143 /HD0N))
    (pad 29 smd rect (at -0.25 -2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 144 /HD0P))
    (pad 30 smd rect (at -0.75 -2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 31 smd rect (at -1.25 -2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 147 /HD1N))
    (pad 32 smd rect (at -1.75 -2.65) (size 1.2 0.25) (layers F.Cu F.Paste F.Mask)
      (net 148 /HD1P))
    (pad 33 smd rect (at 0.8625 0.8625 270) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625 270) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 270) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625 270) (size 1.725 1.725) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:SOD-123FL-HS (layer B.Cu) (tedit 5889E1F2)
    (at 122.439 119.761)
    (fp_text reference D1 (at 3.545 0.127) (layer B.SilkS))
    (fp_text value MBRX120-TP (at 0 -2.54) (layer B.Fab))
    (pad 1 smd rect (at -1.64 0) (size 1.2 1.2192) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.64 0) (size 1.2 1.2192) (layers B.Cu B.Paste B.Mask)
      (net 45 /VBUS))
  )
  (module visionFeet:TSSOP-II-54-HS (layer F.Cu) (tedit 0)
    (at 112.612 66.153 90)
    (tags "TSSOP-II 54")
    (fp_text reference U11 (at -12.31 0 180) (layer F.SilkS))
    (fp_text value AS4C16M16SA (at 0 0 90) (layer F.Fab))
    (pad 54 smd rect (at -10.4 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -10.4 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 53 smd rect (at -9.6 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 140 /DR0_DQ15))
    (pad 2 smd rect (at -9.6 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 125 /DR0_DQ0))
    (pad 52 smd rect (at -8.8 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -8.8 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 51 smd rect (at -8 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 139 /DR0_DQ14))
    (pad 4 smd rect (at -8 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 126 /DR0_DQ1))
    (pad 50 smd rect (at -7.2 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 138 /DR0_DQ13))
    (pad 5 smd rect (at -7.2 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 127 /DR0_DQ2))
    (pad 49 smd rect (at -6.4 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at -6.4 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 48 smd rect (at -5.6 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 137 /DR0_DQ12))
    (pad 7 smd rect (at -5.6 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 128 /DR0_DQ3))
    (pad 47 smd rect (at -4.8 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 136 /DR0_DQ11))
    (pad 8 smd rect (at -4.8 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 129 /DR0_DQ4))
    (pad 46 smd rect (at -4 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -4 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 45 smd rect (at -3.2 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 135 /DR0_DQ10))
    (pad 10 smd rect (at -3.2 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 130 /DR0_DQ5))
    (pad 44 smd rect (at -2.4 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 134 /DR0_DQ9))
    (pad 11 smd rect (at -2.4 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 131 /DR0_DQ6))
    (pad 43 smd rect (at -1.6 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 12 smd rect (at -1.6 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 42 smd rect (at -0.8 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 133 /DR0_DQ8))
    (pad 13 smd rect (at -0.8 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 132 /DR0_DQ7))
    (pad 41 smd rect (at 0 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at 0 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 40 smd rect (at 0.8 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 0.8 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 160 /DR0_LDQM))
    (pad 39 smd rect (at 1.6 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 161 /DR0_UDQM))
    (pad 16 smd rect (at 1.6 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 141 /DR0_WE#))
    (pad 38 smd rect (at 2.4 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 159 /DR0_CLK))
    (pad 17 smd rect (at 2.4 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 142 /DR0_CAS#))
    (pad 37 smd rect (at 3.2 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 158 /DR0_CKE))
    (pad 18 smd rect (at 3.2 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 157 /DR0_RAS#))
    (pad 36 smd rect (at 4 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 124 /DR0_A12))
    (pad 19 smd rect (at 4 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 35 smd rect (at 4.8 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 123 /DR0_A11))
    (pad 20 smd rect (at 4.8 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 153 /DR0_BA0))
    (pad 34 smd rect (at 5.6 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 121 /DR0_A9))
    (pad 21 smd rect (at 5.6 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 154 /DR0_BA1))
    (pad 33 smd rect (at 6.4 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 120 /DR0_A8))
    (pad 22 smd rect (at 6.4 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 122 /DR0_A10))
    (pad 32 smd rect (at 7.2 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 119 /DR0_A7))
    (pad 23 smd rect (at 7.2 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 162 /DR0_A0))
    (pad 31 smd rect (at 8 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 168 /DR0_A6))
    (pad 24 smd rect (at 8 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 163 /DR0_A1))
    (pad 30 smd rect (at 8.8 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 167 /DR0_A5))
    (pad 25 smd rect (at 8.8 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 164 /DR0_A2))
    (pad 29 smd rect (at 9.6 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 166 /DR0_A4))
    (pad 26 smd rect (at 9.6 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 165 /DR0_A3))
    (pad 28 smd rect (at 10.4 -5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 27 smd rect (at 10.4 5.625 90) (size 0.42 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
  )
  (module visionFeet:WurthFFC_1mm_20 (layer F.Cu) (tedit 58910C9B)
    (at 157.226 95.529 90)
    (fp_text reference P4 (at 0 2.15 90) (layer F.SilkS))
    (fp_text value CONN_01X20 (at 0 3.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -9.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 70 /CA_RST))
    (pad 2 smd rect (at -8.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 68 /CA_PCLK))
    (pad 3 smd rect (at -7.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 67 /CA_VSYNC))
    (pad 4 smd rect (at -6.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 65 /CAB_SCL))
    (pad 5 smd rect (at -5.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 53 /CA_PWDN))
    (pad 6 smd rect (at -4.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 63 /CAB_XCLK))
    (pad 7 smd rect (at -3.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 54 /CA_HREF))
    (pad 8 smd rect (at -2.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 55 /CAB_SDA))
    (pad 9 smd rect (at -1.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 56 /CA_D6))
    (pad 10 smd rect (at -0.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 57 /CA_D4))
    (pad 11 smd rect (at 0.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 58 /CA_D2))
    (pad 12 smd rect (at 1.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 59 /CA_D0))
    (pad 13 smd rect (at 2.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(P4-Pad13)"))
    (pad 14 smd rect (at 3.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 61 /CA_D7))
    (pad 15 smd rect (at 4.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 62 /CA_D5))
    (pad 16 smd rect (at 5.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 64 /CA_D3))
    (pad 17 smd rect (at 6.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 66 /CA_D1))
    (pad 18 smd rect (at 7.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(P4-Pad18)"))
    (pad 19 smd rect (at 8.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +2V8))
    (pad 20 smd rect (at 9.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 0 smd rect (at -12.5 2.9 90) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 12.5 2.9 90) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
  )
  (module visionFeet:WurthFFC_1mm_20 (layer F.Cu) (tedit 0)
    (at 157.247 65.732 90)
    (fp_text reference P5 (at 0 2.15 90) (layer F.SilkS))
    (fp_text value CONN_01X20 (at 0 3.5 90) (layer F.Fab))
    (pad 1 smd rect (at -9.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 85 /CB_RST))
    (pad 2 smd rect (at -8.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 83 /CB_PCLK))
    (pad 3 smd rect (at -7.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 82 /CB_VSYNC))
    (pad 4 smd rect (at -6.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 65 /CAB_SCL))
    (pad 5 smd rect (at -5.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 71 /CB_PWDN))
    (pad 6 smd rect (at -4.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 63 /CAB_XCLK))
    (pad 7 smd rect (at -3.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 72 /CB_HREF))
    (pad 8 smd rect (at -2.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 55 /CAB_SDA))
    (pad 9 smd rect (at -1.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 73 /CB_D6))
    (pad 10 smd rect (at -0.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 74 /CB_D4))
    (pad 11 smd rect (at 0.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 75 /CB_D2))
    (pad 12 smd rect (at 1.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 76 /CB_D0))
    (pad 13 smd rect (at 2.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(P5-Pad13)"))
    (pad 14 smd rect (at 3.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 78 /CB_D7))
    (pad 15 smd rect (at 4.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 79 /CB_D5))
    (pad 16 smd rect (at 5.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 80 /CB_D3))
    (pad 17 smd rect (at 6.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 81 /CB_D1))
    (pad 18 smd rect (at 7.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P5-Pad18)"))
    (pad 19 smd rect (at 8.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 5 +2V8))
    (pad 20 smd rect (at 9.5 0 90) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 0 smd rect (at -12.5 2.9 90) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 12.5 2.9 90) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask))
  )
  (module visionFeet:R_Array_Convex_8x0602_HS (layer B.Cu) (tedit 54539007)
    (at 120.269 113.284)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at -3.519 0.316) (layer B.SilkS))
    (fp_text value 330x8 (at 0 -3) (layer B.Fab))
    (pad 1 smd rect (at -1.1 1.75) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 42 /SR_M0))
    (pad 16 smd rect (at 1.1 1.75) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 8 smd rect (at -1.1 -1.75) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 100 "Net-(RN1-Pad8)"))
    (pad 9 smd rect (at 1.1 -1.75) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 101 "Net-(RN1-Pad9)"))
    (pad 2 smd rect (at -1.1 1.25) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 33 /SR_M1))
    (pad 3 smd rect (at -1.1 0.75) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 36 /SR_CSI_B))
    (pad 4 smd rect (at -1.1 0.25) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 39 /SR_RDWR))
    (pad 5 smd rect (at -1.1 -0.25) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 102 /PROGRAM_B))
    (pad 6 smd rect (at -1.1 -0.75) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 103 /INIT_B))
    (pad 7 smd rect (at -1.1 -1.25) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 15 /SD_CS/DAT3/CD))
    (pad 15 smd rect (at 1.1 1.25) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D4-Pad2)"))
    (pad 14 smd rect (at 1.1 0.75) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D5-Pad2)"))
    (pad 13 smd rect (at 1.1 0.25) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D6-Pad2)"))
    (pad 11 smd rect (at 1.1 -0.75) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D8-Pad2)"))
    (pad 12 smd rect (at 1.1 -0.25) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D7-Pad2)"))
    (pad 10 smd rect (at 1.1 -1.25) (size 1.2 0.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_Array_Convex_8x0602.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:Crys_Abracon_ABM3B-4pin_5.0x3.2mmHS (layer F.Cu) (tedit 58910CA1)
    (at 147.447 97.409 180)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3B http://www.abracon.com/Resonators/abm3b.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference U2 (at 0 2.921 180) (layer F.SilkS))
    (fp_text value ASFLMB-50.000MHZ-LC-T (at 0 3.81 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 1.2 180) (size 2.3 1.7) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 1.2 180) (size 2.3 1.7) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2 -1.2 180) (size 2.3 1.7) (layers F.Cu F.Mask)
      (net 104 /CLK))
    (pad 4 smd rect (at -2 -1.2 180) (size 2.3 1.7) (layers F.Cu F.Mask)
      (net 4 +3V3))
    (model Crystals.3dshapes/Crystal_SMD_Abracon_ABM3B-4pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 107.75 107.25)
    (fp_text reference W1 (at -1.85 0 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 94 /AVR_RESET))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 119.55 86.2)
    (fp_text reference W3 (at 0 -3.6 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 117 "Net-(U7-Pad36)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 117.221 84.455)
    (fp_text reference W4 (at 0 -3.6 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 118 "Net-(U7-Pad37)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 160.147 120.396)
    (fp_text reference W10 (at 1.143 -3.556 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /SD_NC/DAT2))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 153.162 107.823)
    (fp_text reference W11 (at 1.905 -0.127 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /SD_RSV/DAT1))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 153.75 81.75)
    (fp_text reference W12 (at -1.45 3.25 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(P4-Pad13)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 156.25 82.25)
    (fp_text reference W13 (at -1.4 3.45 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(P4-Pad18)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 158.877 116.586)
    (fp_text reference W14 (at 0.254 -3.6 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(P3-Pad15)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 156.464 53.467)
    (fp_text reference W15 (at -1.564 3.175 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(P5-Pad13)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 153.924 53.467)
    (fp_text reference W16 (at -0.524 3.233 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(P5-Pad18)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 107.823 111)
    (fp_text reference W17 (at -1.823 0 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 100 "Net-(RN1-Pad8)"))
  )
  (module visionFeet:PAD-2x3.5mm (layer F.Cu) (tedit 588AEA6C)
    (at 110.25 111)
    (fp_text reference W18 (at 0.2 -3.5 90) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 3) (layer F.Fab))
    (pad 1 smd oval (at 0 0) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(RN1-Pad9)"))
  )
  (module visionFeet:TSSOP-16_4.4x5mm_p0.65mm_HS (layer B.Cu) (tedit 54130A77)
    (at 110.465 98.033)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U9 (at 0.025 0.817) (layer B.SilkS))
    (fp_text value 74HC595 (at 0 -3.55) (layer B.Fab))
    (pad 1 smd rect (at -3.2 2.275) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 33 /SR_M1))
    (pad 2 smd rect (at -3.2 1.625) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 36 /SR_CSI_B))
    (pad 3 smd rect (at -3.2 0.975) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 39 /SR_RDWR))
    (pad 4 smd rect (at -3.2 0.325) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -3.2 -0.325) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -3.2 -0.975) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -3.2 -1.625) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -3.2 -2.275) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 3.2 -2.275) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 3.2 -1.625) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 11 smd rect (at 3.2 -0.975) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 112 /SR_SRCLK))
    (pad 12 smd rect (at 3.2 -0.325) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 113 /SR_RCLK))
    (pad 13 smd rect (at 3.2 0.325) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 105 /~SR_QE))
    (pad 14 smd rect (at 3.2 0.975) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 111 /SR_SER))
    (pad 15 smd rect (at 3.2 1.625) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 42 /SR_M0))
    (pad 16 smd rect (at 3.2 2.275) (size 2.01 0.45) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (model Housings_SSOP.3dshapes/TSSOP-16_4.4x5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:Micro_SD_Molex_5031821852 (layer B.Cu) (tedit 58911708)
    (at 149.84222 117.96522)
    (descr "MicroSD Card socket, Molex P/N 502774-0811")
    (fp_text reference CON1 (at -0.89222 -1.21522) (layer B.SilkS))
    (fp_text value Micro_SD_Molex_5031821852 (at 0 9.70026) (layer B.SilkS) hide)
    (pad 8 smd rect (at 4.8006 7.38378) (size 0.8001 1.67894) (layers B.Cu B.Paste B.Mask)
      (net 11 /SD_RSV/DAT1) (clearance 0.20066))
    (pad 7 smd rect (at 3.70078 7.38378) (size 0.8001 1.67894) (layers B.Cu B.Paste B.Mask)
      (net 12 /SD_D0/MISO/DAT0) (clearance 0.20066))
    (pad 6 smd rect (at 2.60096 7.38378) (size 0.8001 1.67894) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (clearance 0.20066))
    (pad 5 smd rect (at 1.50114 7.38378) (size 0.8001 1.67894) (layers B.Cu B.Paste B.Mask)
      (net 13 /SD_CLK) (clearance 0.20066))
    (pad 4 smd rect (at 0.39878 7.38378) (size 0.8001 1.67894) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3_FLASH) (clearance 0.20066))
    (pad 3 smd rect (at -0.70104 7.38378) (size 0.8001 1.67894) (layers B.Cu B.Paste B.Mask)
      (net 14 /SD_D1/MOSI/CMD) (clearance 0.20066))
    (pad 2 smd rect (at -1.80086 7.38378) (size 0.8001 1.67894) (layers B.Cu B.Paste B.Mask)
      (net 15 /SD_CS/DAT3/CD) (clearance 0.20066))
    (pad 1 smd rect (at -2.90068 7.38378) (size 0.8001 1.67894) (layers B.Cu B.Paste B.Mask)
      (net 16 /SD_NC/DAT2) (clearance 0.20066))
    (pad 9 smd rect (at -7 -5.4) (size 2.012 1.701) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 4.7 -6.3) (size 2.012 1.701) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -7 5.9) (size 2.012 1.701) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad "" smd rect (at 7.2 6.4) (size 2.012 1.5) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at 7.2 4.2) (size 2.012 1.701) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at 7.4 -4.9) (size 2.012 1.701) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -2.8 -6.3) (size 2.012 1.701) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model walter/conn_misc/microsd_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module visionFeet:USB_Micro-B-HS_RHOLE (layer F.Cu) (tedit 5891155B)
    (at 129.823 125.01)
    (descr "Micro USB Type B Receptacle")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P2 (at 0.027 1.44) (layer F.SilkS))
    (fp_text value USB-Micro-B (at 0 5.01) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 45 /VBUS))
    (pad 2 smd rect (at -0.65 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(P2-Pad2)"))
    (pad 3 smd rect (at 0 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(P2-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.3 -1.85 90) (size 2.35 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 thru_hole oval (at -2.5 -1.35 90) (size 1.1 1.25) (drill 0.95) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.5 -1.35 90) (size 1.1 1.25) (drill 0.95) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -3.5 1.35 90) (size 1.55 1.55) (drill 1.25) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 3.5 1.35 90) (size 1.55 1.55) (drill 1.25) (layers *.Cu *.Mask))
  )
  (gr_text 2.1.17 (at 109.7 55.3) (layer B.SilkS))
  (gr_text CC02 (at 109.05 53.1) (layer B.SilkS))
  (gr_line (start 162.7 50.7) (end 162.7 128.6) (layer Edge.Cuts) (width 1))
  (gr_line (start 104 50.7) (end 162.7 50.7) (layer Edge.Cuts) (width 1))
  (gr_line (start 103.7 128.6) (end 103.7 50.7) (layer Edge.Cuts) (width 1))
  (gr_line (start 162.7 128.6) (end 103.7 128.6) (layer Edge.Cuts) (width 1))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.3) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 104 50.7) (xy 162.7 50.7) (xy 162.7 128.5) (xy 104.1 128.6)
      )
    )
  )
)
